;======================================================
;======================================================
#Profibus_DP
; HIGHEST Module_Index currently in use: 3
;
; File Version 2.01
; Version R0101 R0201 for UMC100 with ePlug DPV1 (PDP22) modified by Rolf Oestreich
; ** new module for I/O-Data-Profil 2 "UMC100(R0101 R0201)Profil2" added Date 14.11.2013 
;
; File Version 2.00
; Version R0101 R0201 for UMC100 with ePlug DPV1 (PDP22) created by GSD-Generator, Date 08.06.2011 07:36:23 
; ** first version;
;
; File Version: 1.00
; Version V1.13 for UMC100 with ePlug DPV1 (PDP22) created by GSD-Generator, Date 27.04.2010 11:24:29 
; ** first version
;
;
;=============================================================
; Text-definition for User Prm Data  UMC100_FBP (V1.13)
;=============================================================
;
ExtUserPrmData =  1  "Setting Ie 1 [0.01A]"
Unsigned32 50 24-320000
EndExtUserPrmData

ExtUserPrmData =  2  "Setting Ie 2 [0.01A]"
Unsigned32 50 24-320000
EndExtUserPrmData

ExtUserPrmData =  3  "YD Starting Time [0.1s]"
Unsigned16 600 10-36000
EndExtUserPrmData

ExtUserPrmData =  4  "Current Factor [%]"
Unsigned16 100 2-64000
EndExtUserPrmData

ExtUserPrmData =  5  "Cooling Time [s]"
Unsigned16 120 30-64000
EndExtUserPrmData

PrmText = 6 
Text(0) = "English"
Text(1) = "Deutsch"
Text(2) = "Francais"
Text(3) = "Espanol"
Text(4) = "Italiano"
Text(5) = "Portugues"
EndPrmText
ExtUserPrmData =  6  "Language"
Unsigned8 0 0-5
Prm_Text_Ref = 6 
EndExtUserPrmData

ExtUserPrmData =  7  "Rev Lock-Out Time [s]"
Unsigned8 1 1-255
EndExtUserPrmData

PrmText = 8 
Text(0) = "Off"
Text(1) = "Flash DO2"
Text(2) = "On DO2"
Text(3) = "Invert DO2"
Text(4) = "Flash DO3"
Text(5) = "On DO3"
Text(6) = "Invert DO3"
EndPrmText
ExtUserPrmData =  8  "Fault Output"
Unsigned8 0 0-6
Prm_Text_Ref = 8 
EndExtUserPrmData

PrmText = 9 
Text(0) = "Class 5"
Text(1) = "Class 10"
Text(2) = "Class 20"
Text(3) = "Class 30"
Text(4) = "Class 40"
EndPrmText
ExtUserPrmData =  9  "Trip Class"
Unsigned8 1 0-4
Prm_Text_Ref = 9 
EndExtUserPrmData

ExtUserPrmData =  10  "Low Curr Warn Level [5%]"
Unsigned8 10 0-20
EndExtUserPrmData

ExtUserPrmData =  11  "Low Curr Trip Level [5%]"
Unsigned8 0 0-20
EndExtUserPrmData

ExtUserPrmData =  12  "High Curr Warn Level [5%]"
Unsigned8 30 20-160
EndExtUserPrmData

ExtUserPrmData =  13  "High Curr Trip Level [5%]"
Unsigned8 160 20-160
EndExtUserPrmData

ExtUserPrmData =  14  "Locked Rotor Level [5%]"
Unsigned8 160 20-160
EndExtUserPrmData

ExtUserPrmData =  15  "Locked Rotor Delay [0.1s]"
Unsigned8 5 0-255
EndExtUserPrmData

ExtUserPrmData =  16  "Custom App Parameter"
Unsigned8 0 0-255
EndExtUserPrmData

PrmText = 17 
Text(0) = "Off"
Text(1) = "Stop (NC)"
Text(2) = "Stop (NO)"
Text(3) = "Ext. Flt (NC) always"
Text(4) = "Ext. Flt (NO) always"
Text(5) = "Ext. Flt (NC) Motor on"
Text(6) = "Ext. Flt (NO) Motor on"
Text(7) = "Prep. emerg. Start (NC)"
Text(8) = "Prep. emerg. Start (NO)"
Text(9) = "Testposition (NC)"
Text(10) = "Testposition (NO)"
Text(11) = "Force local (NC)"
Text(12) = "Force local (NO)"
Text(13) = "Fault reset (NC)"
Text(14) = "Fault reset (NO)"
Text(15) = "Voltage DIP (NC)"
Text(16) = "Voltage DIP (NO)"
Text(17) = "CEM11 always (Warning)"
Text(18) = "CEM11 after startup (Warning)"
Text(19) = "CEM11 always (Fault)"
Text(20) = "CEM11 after startup time (Fault)"
EndPrmText
ExtUserPrmData =  17  "Multif In 0"
Unsigned8 0 0-20
Prm_Text_Ref = 17 
EndExtUserPrmData

PrmText = 18 
Text(0) = "Off"
Text(1) = "Stop (NC)"
Text(2) = "Stop (NO)"
Text(3) = "Ext. Flt (NC) always"
Text(4) = "Ext. Flt (NO) always"
Text(5) = "Ext. Flt (NC) Motor on"
Text(6) = "Ext. Flt (NO) Motor on"
Text(7) = "Prep. emerg. Start (NC)"
Text(8) = "Prep. emerg. Start (NO)"
Text(9) = "Testposition (NC)"
Text(10) = "Testposition (NO)"
Text(11) = "Force local (NC)"
Text(12) = "Force local (NO)"
Text(13) = "Fault reset (NC)"
Text(14) = "Fault reset (NO)"
Text(15) = "Voltage DIP (NC)"
Text(16) = "Voltage DIP (NO)"
Text(17) = "CEM11 always (Warning)"
Text(18) = "CEM11 after startup (Warning)"
Text(19) = "CEM11 always (Fault)"
Text(20) = "CEM11 after startup time (Fault)"
EndPrmText
ExtUserPrmData =  18  "Multif In 1"
Unsigned8 0 0-20
Prm_Text_Ref = 18 
EndExtUserPrmData

PrmText = 19 
Text(0) = "Off"
Text(1) = "Stop (NC)"
Text(2) = "Stop (NO)"
Text(3) = "Ext. Flt (NC) always"
Text(4) = "Ext. Flt (NO) always"
Text(5) = "Ext. Flt (NC) Motor on"
Text(6) = "Ext. Flt (NO) Motor on"
Text(7) = "Prep. emerg. Start (NC)"
Text(8) = "Prep. emerg. Start (NO)"
Text(9) = "Testposition (NC)"
Text(10) = "Testposition (NO)"
Text(11) = "Force local (NC)"
Text(12) = "Force local (NO)"
Text(13) = "Fault reset (NC)"
Text(14) = "Fault reset (NO)"
Text(15) = "Voltage DIP (NC)"
Text(16) = "Voltage DIP (NO)"
Text(17) = "CEM11 always (Warning)"
Text(18) = "CEM11 after startup (Warning)"
Text(19) = "CEM11 always (Fault)"
Text(20) = "CEM11 after startup time (Fault)"
EndPrmText
ExtUserPrmData =  19  "Multif In 2"
Unsigned8 0 0-20
Prm_Text_Ref = 19 
EndExtUserPrmData

ExtUserPrmData =  20  "Multif In 0 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  21  "Multif In 1 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  22  "Multif In 2 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

PrmText = 23 
Text(1) = "Transparent"
Text(2) = "Overload Relay"
Text(3) = "Direct Starter"
Text(4) = "Reverse Starter"
Text(5) = "Star-delta Starter"
Text(7) = "Pole-Changing Starter"
Text(9) = "Actuator 1"
Text(10) = "Actuator 2"
Text(11) = "Actuator 3"
Text(12) = "Actuator 4"
EndPrmText
ExtUserPrmData =  23  "Control Function"
Unsigned8 3 1-12
Prm_Text_Ref = 23 
EndExtUserPrmData

PrmText = 24 
Text(0) = "Motor Off"
Text(1) = "Retain"
Text(2) = "Start Forward"
Text(3) = "Start Reverse"
EndPrmText
ExtUserPrmData =  24  "Busfault Reaction"
BitArea(0-3) 0 0-3
Prm_Text_Ref = 24 
EndExtUserPrmData

PrmText = 25 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  25  "Aux Inp 1 Reaction"
BitArea(0-3) 0 0-8
Prm_Text_Ref = 25 
EndExtUserPrmData

PrmText = 26 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  26  "Aux Inp 2 Reaction"
BitArea(4-7) 0 0-8
Prm_Text_Ref = 26 
EndExtUserPrmData

PrmText = 27 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  27  "Aux Inp 3 Reaction"
BitArea(0-3) 0 0-8
Prm_Text_Ref = 27 
EndExtUserPrmData

PrmText = 28 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  28  "Aux Inp 4 Reaction"
BitArea(4-7) 0 0-8
Prm_Text_Ref = 28 
EndExtUserPrmData

PrmText = 29 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  29  "Aux Inp 5 Reaction"
BitArea(0-3) 0 0-8
Prm_Text_Ref = 29 
EndExtUserPrmData

PrmText = 30 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  30  "Aux Inp 6 Reaction"
BitArea(4-7) 0 0-8
Prm_Text_Ref = 30 
EndExtUserPrmData

PrmText = 31 
Text(0) = "Disabled"
Text(1) = "Trip"
Text(2) = "Warning"
EndPrmText
ExtUserPrmData =  31  "PTC, Thermistor"
BitArea(0-1) 0 0-2
Prm_Text_Ref = 31 
EndExtUserPrmData

PrmText = 32 
Text(1) = "Contact DI0"
Text(2) = "Current"
Text(3) = "Simulation"
EndPrmText
ExtUserPrmData =  32  "Check-Back"
BitArea(2-3) 2 1-3
Prm_Text_Ref = 32 
EndExtUserPrmData

PrmText = 33 
Text(0) = "Disabled"
Text(1) = "Trip"
Text(2) = "Warning"
EndPrmText
ExtUserPrmData =  33  "Check Phase Sequence"
BitArea(4-5) 0 0-2
Prm_Text_Ref = 33 
EndExtUserPrmData

PrmText = 34 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  34  "Fault Auto Reset"
Bit(0) 0 0-1
Prm_Text_Ref = 34 
EndExtUserPrmData

PrmText = 35 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  35  "Emergency Start"
Bit(1) 0 0-1
Prm_Text_Ref = 35 
EndExtUserPrmData

PrmText = 36 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  36  "Address Check"
Bit(3) 0 0-1
Prm_Text_Ref = 36 
EndExtUserPrmData

PrmText = 37 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  37  "Enable Custom Logic"
Bit(4) 0 0-1
Prm_Text_Ref = 37 
EndExtUserPrmData

PrmText = 38 
Text(0) = "Time"
Text(1) = "Current"
EndPrmText
ExtUserPrmData =  38  "YD Change-Over Mode"
Bit(5) 1 0-1
Prm_Text_Ref = 38 
EndExtUserPrmData

PrmText = 39 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  39  "Phase Loss Prot."
Bit(6) 1 0-1
Prm_Text_Ref = 39 
EndExtUserPrmData

PrmText = 40 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  40  "DX1xx Enabled"
Bit(0) 0 0-1
Prm_Text_Ref = 40 
EndExtUserPrmData

PrmText = 41 
Text(0) = "Error"
Text(1) = "Warning"
EndPrmText
ExtUserPrmData =  41  "Missing Module React."
Bit(7) 0 0-1
Prm_Text_Ref = 41 
EndExtUserPrmData

PrmText = 42 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  42  "Aux Inp 1 Ack Mode"
Bit(0) 0 0-1
Prm_Text_Ref = 42 
EndExtUserPrmData

PrmText = 43 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  43  "Aux Inp 2 Ack Mode"
Bit(1) 0 0-1
Prm_Text_Ref = 43 
EndExtUserPrmData

PrmText = 44 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  44  "Aux Inp 3 Ack Mode"
Bit(2) 0 0-1
Prm_Text_Ref = 44 
EndExtUserPrmData

PrmText = 45 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  45  "Aux Inp 4 Ack Mode"
Bit(3) 0 0-1
Prm_Text_Ref = 45 
EndExtUserPrmData

PrmText = 46 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  46  "Aux Inp 5 Ack Mode"
Bit(4) 0 0-1
Prm_Text_Ref = 46 
EndExtUserPrmData

PrmText = 47 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  47  "Aux Inp 6 Ack Mode"
Bit(5) 0 0-1
Prm_Text_Ref = 47 
EndExtUserPrmData

PrmText = 48 
Text(0) = "Time"
Text(1) = "x% Therm. Load"
EndPrmText
ExtUserPrmData =  48  "Cooling Mode"
Bit(7) 0 0-1
Prm_Text_Ref = 48 
EndExtUserPrmData

PrmText = 49 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  49  "Invert DI Start Inp."
Bit(0) 0 0-1
Prm_Text_Ref = 49 
EndExtUserPrmData

PrmText = 50 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  50  "Invert DI Stop Inp."
Bit(1) 1 0-1
Prm_Text_Ref = 50 
EndExtUserPrmData

PrmText = 51 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  51  "Inching DI Start Inp"
Bit(4) 0 0-1
Prm_Text_Ref = 51 
EndExtUserPrmData

PrmText = 52 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  52  "Loc 1 Start Bus Cyc"
Bit(0) 0 0-1
Prm_Text_Ref = 52 
EndExtUserPrmData

PrmText = 53 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  53  "Loc 1 Stop Bus Cyc"
Bit(1) 1 0-1
Prm_Text_Ref = 53 
EndExtUserPrmData

PrmText = 54 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  54  "Loc 1 Start DI"
Bit(2) 1 0-1
Prm_Text_Ref = 54 
EndExtUserPrmData

PrmText = 55 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  55  "Loc 1 Stop DI"
Bit(3) 1 0-1
Prm_Text_Ref = 55 
EndExtUserPrmData

PrmText = 56 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  56  "Loc 1 Start LCD"
Bit(4) 1 0-1
Prm_Text_Ref = 56 
EndExtUserPrmData

PrmText = 57 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  57  "Loc 1 Stop LCD"
Bit(5) 1 0-1
Prm_Text_Ref = 57 
EndExtUserPrmData

PrmText = 58 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  58  "Loc 1 Start Bus Acyc"
Bit(6) 0 0-1
Prm_Text_Ref = 58 
EndExtUserPrmData

PrmText = 59 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  59  "Loc 1 Stop Bus Acyc"
Bit(7) 1 0-1
Prm_Text_Ref = 59 
EndExtUserPrmData

PrmText = 60 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  60  "Auto Start Bus Cyc"
Bit(0) 1 0-1
Prm_Text_Ref = 60 
EndExtUserPrmData

PrmText = 61 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  61  "Auto Stop Bus Cyc"
Bit(1) 1 0-1
Prm_Text_Ref = 61 
EndExtUserPrmData

PrmText = 62 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  62  "Auto Start DI"
Bit(2) 0 0-1
Prm_Text_Ref = 62 
EndExtUserPrmData

PrmText = 63 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  63  "Auto Stop DI"
Bit(3) 1 0-1
Prm_Text_Ref = 63 
EndExtUserPrmData

PrmText = 64 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  64  "Auto Start LCD"
Bit(4) 0 0-1
Prm_Text_Ref = 64 
EndExtUserPrmData

PrmText = 65 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  65  "Auto Stop LCD"
Bit(5) 1 0-1
Prm_Text_Ref = 65 
EndExtUserPrmData

PrmText = 66 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  66  "Auto Start Bus Acyc"
Bit(6) 1 0-1
Prm_Text_Ref = 66 
EndExtUserPrmData

PrmText = 67 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  67  "Auto Stop Bus Acyc"
Bit(7) 1 0-1
Prm_Text_Ref = 67 
EndExtUserPrmData

PrmText = 68 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  68  "Loc 2 Start Bus Cyc"
Bit(0) 0 0-1
Prm_Text_Ref = 68 
EndExtUserPrmData

PrmText = 69 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  69  "Loc 2 Stop Bus Cyc"
Bit(1) 1 0-1
Prm_Text_Ref = 69 
EndExtUserPrmData

PrmText = 70 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  70  "Loc 2 Start DI"
Bit(2) 1 0-1
Prm_Text_Ref = 70 
EndExtUserPrmData

PrmText = 71 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  71  "Loc 2 Stop DI"
Bit(3) 1 0-1
Prm_Text_Ref = 71 
EndExtUserPrmData

PrmText = 72 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  72  "Loc 2 Start LCD"
Bit(4) 1 0-1
Prm_Text_Ref = 72 
EndExtUserPrmData

PrmText = 73 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  73  "Loc 2 Stop LCD"
Bit(5) 1 0-1
Prm_Text_Ref = 73 
EndExtUserPrmData

PrmText = 74 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  74  "Loc 2 Start Bus Acyc"
Bit(6) 0 0-1
Prm_Text_Ref = 74 
EndExtUserPrmData

PrmText = 75 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  75  "Loc 2 Stop Bus Acyc"
Bit(7) 1 0-1
Prm_Text_Ref = 75 
EndExtUserPrmData

PrmText = 76 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  76  "Multif In 0 Autoreset"
Bit(4) 0 0-1
Prm_Text_Ref = 76 
EndExtUserPrmData

PrmText = 77 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  77  "Multif In 1 Autoreset"
Bit(5) 0 0-1
Prm_Text_Ref = 77 
EndExtUserPrmData

PrmText = 78 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  78  "Multif In 2 Autoreset"
Bit(6) 0 0-1
Prm_Text_Ref = 78 
EndExtUserPrmData

ExtUserPrmData =  79  "Aux Inp 1 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  80  "Aux Inp 2 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  81  "Aux Inp 3 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  82  "Aux Inp 4 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  83  "Aux Inp 5 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  84  "Aux Inp 6 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  85  "Check-Back Time [0.1s]"
Unsigned8 5 1-255
EndExtUserPrmData

ExtUserPrmData =  86  "Low Curr Warn Delay [0.1s]"
Unsigned8 5 0-255
EndExtUserPrmData

ExtUserPrmData =  87  "Low Curr Trip Delay [0.1s]"
Unsigned8 5 0-255
EndExtUserPrmData

ExtUserPrmData =  88  "High Curr Warn Delay [0.1s]"
Unsigned8 5 0-255
EndExtUserPrmData

ExtUserPrmData =  89  "High Curr Trip Delay [0.1s]"
Unsigned8 5 0-255
EndExtUserPrmData

ExtUserPrmData =  90  "Phase Imb Trip Level [%]"
Unsigned8 50 0-100
EndExtUserPrmData

ExtUserPrmData =  91  "Phase Imb Warn Level [%]"
Unsigned8 100 0-100
EndExtUserPrmData

PrmText = 92 
Text(0) = "Phase Sequence L1 L2 L3"
Text(1) = "Phase Sequence L3 L2 L1"
EndPrmText
ExtUserPrmData =  92  "Phase Reversal"
Bit(0) 0 0-1
Prm_Text_Ref = 92 
EndExtUserPrmData

ExtUserPrmData =  93  "Restart Level [%]"
Unsigned8 30 10-100
EndExtUserPrmData

PrmText = 94 
Text(0) = "Thermal Load"
Text(1) = "DX1xx DI"
Text(2) = "DX1xx DO"
Text(3) = "Operating Hours"
Text(4) = "Number of Trips"
Text(5) = "Number of Starts"
Text(6) = "max. Startup Current"
Text(7) = "Real Startup Time"
EndPrmText
ExtUserPrmData =  94  "User Display 1"
Unsigned8 0 0-7
Prm_Text_Ref = 94 
EndExtUserPrmData

PrmText = 95 
Text(0) = "Thermal Load"
Text(1) = "DX1xx DI"
Text(2) = "DX1xx DO"
Text(3) = "Operating Hours"
Text(4) = "Number of Trips"
Text(5) = "Number of Starts"
Text(6) = "max. Startup Current"
Text(7) = "Real Startup Time"
EndPrmText
ExtUserPrmData =  95  "User Display 2"
Unsigned8 6 0-7
Prm_Text_Ref = 95 
EndExtUserPrmData

PrmText = 96 
Text(0) = "Thermal Load"
Text(1) = "DX1xx DI"
Text(2) = "DX1xx DO"
Text(3) = "Operating Hours"
Text(4) = "Number of Trips"
Text(5) = "Number of Starts"
Text(6) = "max. Startup Current"
Text(7) = "Real Startup Time"
EndPrmText
ExtUserPrmData =  96  "User Display 3"
Unsigned8 7 0-7
Prm_Text_Ref = 96 
EndExtUserPrmData

PrmText = 97 
Text(0) = "Binary 0"
Text(1) = "Binary 1"
Text(2) = "Analog 0"
Text(3) = "Analog 1"
Text(4) = "Time to Trip"
Text(5) = "Time to Cool"
EndPrmText
ExtUserPrmData =  97  "User Display 4"
Unsigned8 4 0-5
Prm_Text_Ref = 97 
EndExtUserPrmData

PrmText = 98 
Text(0) = "Binary 0"
Text(1) = "Binary 1"
Text(2) = "Analog 0"
Text(3) = "Analog 1"
Text(4) = "Time to Trip"
Text(5) = "Time to Cool"
EndPrmText
ExtUserPrmData =  98  "User Display 5"
Unsigned8 5 0-5
Prm_Text_Ref = 98 
EndExtUserPrmData

ExtUserPrmData =  99  "Dip Duration [0.1s]"
Unsigned8 5 1-255
EndExtUserPrmData

ExtUserPrmData =  100  "Dip Autorestart Window [0.1s]"
Unsigned8 1 1-10
EndExtUserPrmData

ExtUserPrmData =  101  "Dip Autorestart Delay [s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  102  "Thermal Load Warnlev [%]"
Unsigned8 100 20-100
EndExtUserPrmData

ExtUserPrmData =  103  "DX1xx DI Delay [ms]"
Unsigned8 20 3-200
EndExtUserPrmData

PrmText = 104 
Text(0) = "0-20mA"
Text(1) = "4-20mA"
Text(2) = "0-10mA"
Text(3) = "0-10V"
EndPrmText
ExtUserPrmData =  104  "DX1xx AO Type"
BitArea(0-1) 0 0-3
Prm_Text_Ref = 104 
EndExtUserPrmData

PrmText = 105 
Text(0) = "Disabled"
Text(1) = "Trip"
Text(2) = "Warning"
EndPrmText
ExtUserPrmData =  105  "DX1xx AO Err Reac"
BitArea(2-3) 0 0-2
Prm_Text_Ref = 105 
EndExtUserPrmData

PrmText = 106 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  106  "Backlight"
Bit(0) 1 0-1
Prm_Text_Ref = 106 
EndExtUserPrmData

PrmText = 107 
Text(0) = "Off"
Text(1) = "On for Parameters"
Text(2) = "On for Param. + Motor Control"
EndPrmText
ExtUserPrmData =  107  "Password Protection"
BitArea(1-2) 0 0-2
Prm_Text_Ref = 107 
EndExtUserPrmData

PrmText = 108 
Text(0) = "Off"
Text(1) = "On"
Text(2) = "On + Rapid Cycle Lockout"
EndPrmText
ExtUserPrmData =  108  "Dip Enable"
BitArea(3-4) 0 0-2
Prm_Text_Ref = 108 
EndExtUserPrmData

PrmText = 109 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  109  "Dip Autorestart Enable"
Bit(5) 0 0-1
Prm_Text_Ref = 109 
EndExtUserPrmData

;=============================================================
; Text-definition for User Prm Data  UMC100_FBP (R0101 R0201)
;=============================================================
;
ExtUserPrmData =  201  "Setting Ie 1 [0.01A]"
Unsigned32 50 24-320000
EndExtUserPrmData

ExtUserPrmData =  202  "Setting Ie 2 [0.01A]"
Unsigned32 50 24-320000
EndExtUserPrmData

ExtUserPrmData =  203  "YD Starting Time [0.1s]"
Unsigned16 600 10-36000
EndExtUserPrmData

ExtUserPrmData =  204  "Current Factor [%]"
Unsigned16 100 2-64000
EndExtUserPrmData

ExtUserPrmData =  205  "Cooling Time [s]"
Unsigned16 120 30-64000
EndExtUserPrmData

ExtUserPrmData =  206  "Earth Flt Trip Level [%]"
Unsigned8 255 20-255
EndExtUserPrmData

ExtUserPrmData =  207  "Earth Flt Trip Delay [0.1s]"
Unsigned8 5 0-255
EndExtUserPrmData

PrmText = 208 
Text(0) = "English"
Text(1) = "Deutsch"
Text(2) = "Francais"
Text(3) = "Espanol"
Text(4) = "Italiano"
Text(5) = "Portugues"
Text(6) = "Russian"
EndPrmText
ExtUserPrmData =  208  "Language"
Unsigned8 0 0-6
Prm_Text_Ref = 208 
EndExtUserPrmData

ExtUserPrmData =  209  "Rev Lock-Out Time [s]"
Unsigned8 1 1-255
EndExtUserPrmData

PrmText = 210 
Text(0) = "Off"
Text(1) = "Flash DO2"
Text(2) = "On DO2"
Text(3) = "Invert DO2"
Text(4) = "Flash DO3"
Text(5) = "On DO3"
Text(6) = "Invert DO3"
EndPrmText
ExtUserPrmData =  210  "Fault Output"
Unsigned8 0 0-6
Prm_Text_Ref = 210 
EndExtUserPrmData

PrmText = 211 
Text(0) = "Class 5"
Text(1) = "Class 10"
Text(2) = "Class 20"
Text(3) = "Class 30"
Text(4) = "Class 40"
EndPrmText
ExtUserPrmData =  211  "Trip Class"
Unsigned8 1 0-4
Prm_Text_Ref = 211 
EndExtUserPrmData

ExtUserPrmData =  212  "Low Curr Warn Level [5%]"
Unsigned8 10 0-20
EndExtUserPrmData

ExtUserPrmData =  213  "Low Curr Trip Level [5%]"
Unsigned8 0 0-20
EndExtUserPrmData

ExtUserPrmData =  214  "High Curr Warn Level [5%]"
Unsigned8 30 20-160
EndExtUserPrmData

ExtUserPrmData =  215  "High Curr Trip Level [5%]"
Unsigned8 160 20-160
EndExtUserPrmData

ExtUserPrmData =  216  "Locked Rotor Level [5%]"
Unsigned8 160 20-160
EndExtUserPrmData

ExtUserPrmData =  217  "Locked Rotor Delay [0.1s]"
Unsigned8 5 0-255
EndExtUserPrmData

ExtUserPrmData =  218  "Custom App Parameter"
Unsigned8 0 0-255
EndExtUserPrmData

PrmText = 219 
Text(0) = "Off"
Text(1) = "Stop (NC)"
Text(2) = "Stop (NO)"
Text(3) = "Ext. Flt (NC) always"
Text(4) = "Ext. Flt (NO) always"
Text(5) = "Ext. Flt (NC) Motor on"
Text(6) = "Ext. Flt (NO) Motor on"
Text(7) = "Prep. emerg. Start (NC)"
Text(8) = "Prep. emerg. Start (NO)"
Text(9) = "Testposition (NC)"
Text(10) = "Testposition (NO)"
Text(11) = "Force local (NC)"
Text(12) = "Force local (NO)"
Text(13) = "Fault reset (NC)"
Text(14) = "Fault reset (NO)"
Text(15) = "Voltage DIP (NC)"
Text(16) = "Voltage DIP (NO)"
Text(17) = "CEM11 always (Warning)"
Text(18) = "CEM11 after startup (Warning)"
Text(19) = "CEM11 always (Fault)"
Text(20) = "CEM11 after startup time (Fault)"
EndPrmText
ExtUserPrmData =  219  "Multif In 0"
Unsigned8 0 0-20
Prm_Text_Ref = 219 
EndExtUserPrmData

PrmText = 220 
Text(0) = "Off"
Text(1) = "Stop (NC)"
Text(2) = "Stop (NO)"
Text(3) = "Ext. Flt (NC) always"
Text(4) = "Ext. Flt (NO) always"
Text(5) = "Ext. Flt (NC) Motor on"
Text(6) = "Ext. Flt (NO) Motor on"
Text(7) = "Prep. emerg. Start (NC)"
Text(8) = "Prep. emerg. Start (NO)"
Text(9) = "Testposition (NC)"
Text(10) = "Testposition (NO)"
Text(11) = "Force local (NC)"
Text(12) = "Force local (NO)"
Text(13) = "Fault reset (NC)"
Text(14) = "Fault reset (NO)"
Text(15) = "Voltage DIP (NC)"
Text(16) = "Voltage DIP (NO)"
Text(17) = "CEM11 always (Warning)"
Text(18) = "CEM11 after startup (Warning)"
Text(19) = "CEM11 always (Fault)"
Text(20) = "CEM11 after startup time (Fault)"
EndPrmText
ExtUserPrmData =  220  "Multif In 1"
Unsigned8 0 0-20
Prm_Text_Ref = 220 
EndExtUserPrmData

PrmText = 221 
Text(0) = "Off"
Text(1) = "Stop (NC)"
Text(2) = "Stop (NO)"
Text(3) = "Ext. Flt (NC) always"
Text(4) = "Ext. Flt (NO) always"
Text(5) = "Ext. Flt (NC) Motor on"
Text(6) = "Ext. Flt (NO) Motor on"
Text(7) = "Prep. emerg. Start (NC)"
Text(8) = "Prep. emerg. Start (NO)"
Text(9) = "Testposition (NC)"
Text(10) = "Testposition (NO)"
Text(11) = "Force local (NC)"
Text(12) = "Force local (NO)"
Text(13) = "Fault reset (NC)"
Text(14) = "Fault reset (NO)"
Text(15) = "Voltage DIP (NC)"
Text(16) = "Voltage DIP (NO)"
Text(17) = "CEM11 always (Warning)"
Text(18) = "CEM11 after startup (Warning)"
Text(19) = "CEM11 always (Fault)"
Text(20) = "CEM11 after startup time (Fault)"
EndPrmText
ExtUserPrmData =  221  "Multif In 2"
Unsigned8 0 0-20
Prm_Text_Ref = 221 
EndExtUserPrmData

ExtUserPrmData =  222  "Multif In 0 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  223  "Multif In 1 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  224  "Multif In 2 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

PrmText = 225 
Text(1) = "Transparent"
Text(2) = "Overload Relay"
Text(3) = "Direct Starter"
Text(4) = "Reverse Starter"
Text(5) = "Star-delta Starter"
Text(7) = "Pole-Changing Starter"
Text(9) = "Actuator 1"
Text(10) = "Actuator 2"
Text(11) = "Actuator 3"
Text(12) = "Actuator 4"
EndPrmText
ExtUserPrmData =  225  "Control Function"
Unsigned8 3 1-12
Prm_Text_Ref = 225 
EndExtUserPrmData

PrmText = 226 
Text(0) = "Motor Off"
Text(1) = "Retain"
Text(2) = "Start Forward"
Text(3) = "Start Reverse"
EndPrmText
ExtUserPrmData =  226  "Busfault Reaction"
BitArea(0-3) 0 0-3
Prm_Text_Ref = 226 
EndExtUserPrmData

PrmText = 227 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  227  "Aux Inp 1 Reaction"
BitArea(0-3) 0 0-8
Prm_Text_Ref = 227 
EndExtUserPrmData

PrmText = 228 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  228  "Aux Inp 2 Reaction"
BitArea(4-7) 0 0-8
Prm_Text_Ref = 228 
EndExtUserPrmData

PrmText = 229 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  229  "Aux Inp 3 Reaction"
BitArea(0-3) 0 0-8
Prm_Text_Ref = 229 
EndExtUserPrmData

PrmText = 230 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  230  "Aux Inp 4 Reaction"
BitArea(4-7) 0 0-8
Prm_Text_Ref = 230 
EndExtUserPrmData

PrmText = 231 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  231  "Aux Inp 5 Reaction"
BitArea(0-3) 0 0-8
Prm_Text_Ref = 231 
EndExtUserPrmData

PrmText = 232 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  232  "Aux Inp 6 Reaction"
BitArea(4-7) 0 0-8
Prm_Text_Ref = 232 
EndExtUserPrmData

PrmText = 233 
Text(0) = "Disabled"
Text(1) = "Trip"
Text(2) = "Warning"
EndPrmText
ExtUserPrmData =  233  "PTC, Thermistor"
BitArea(0-1) 0 0-2
Prm_Text_Ref = 233 
EndExtUserPrmData

PrmText = 234 
Text(1) = "Contact DI0"
Text(2) = "Current"
Text(3) = "Simulation"
EndPrmText
ExtUserPrmData =  234  "Check-Back"
BitArea(2-3) 2 1-3
Prm_Text_Ref = 234 
EndExtUserPrmData

PrmText = 235 
Text(0) = "Disabled"
Text(1) = "Trip"
Text(2) = "Warning"
EndPrmText
ExtUserPrmData =  235  "Check Phase Sequence"
BitArea(4-5) 0 0-2
Prm_Text_Ref = 235 
EndExtUserPrmData

PrmText = 236 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  236  "Fault Auto Reset"
Bit(0) 0 0-1
Prm_Text_Ref = 236 
EndExtUserPrmData

PrmText = 237 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  237  "Emergency Start"
Bit(1) 0 0-1
Prm_Text_Ref = 237 
EndExtUserPrmData

PrmText = 238 
Text(0) = "Always"
Text(1) = "After Startup"
EndPrmText
ExtUserPrmData =  238  "Earth Flt Detection"
Bit(2) 1 0-1
Prm_Text_Ref = 238 
EndExtUserPrmData

PrmText = 239 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  239  "Address Check"
Bit(3) 0 0-1
Prm_Text_Ref = 239 
EndExtUserPrmData

PrmText = 240 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  240  "Enable Custom Logic"
Bit(4) 0 0-1
Prm_Text_Ref = 240 
EndExtUserPrmData

PrmText = 241 
Text(0) = "Time"
Text(1) = "Current"
EndPrmText
ExtUserPrmData =  241  "YD Change-Over Mode"
Bit(5) 1 0-1
Prm_Text_Ref = 241 
EndExtUserPrmData

PrmText = 242 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  242  "Phase Loss Prot."
Bit(6) 1 0-1
Prm_Text_Ref = 242 
EndExtUserPrmData

PrmText = 243 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  243  "DX1xx Enabled"
Bit(0) 0 0-1
Prm_Text_Ref = 243 
EndExtUserPrmData

PrmText = 244 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  244  "VI15x Enabled"
Bit(3) 0 0-1
Prm_Text_Ref = 244 
EndExtUserPrmData

PrmText = 245 
Text(0) = "Error"
Text(1) = "Warning"
EndPrmText
ExtUserPrmData =  245  "Missing Module React."
Bit(7) 0 0-1
Prm_Text_Ref = 245 
EndExtUserPrmData

PrmText = 246 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  246  "Aux Inp 1 Ack Mode"
Bit(0) 0 0-1
Prm_Text_Ref = 246 
EndExtUserPrmData

PrmText = 247 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  247  "Aux Inp 2 Ack Mode"
Bit(1) 0 0-1
Prm_Text_Ref = 247 
EndExtUserPrmData

PrmText = 248 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  248  "Aux Inp 3 Ack Mode"
Bit(2) 0 0-1
Prm_Text_Ref = 248 
EndExtUserPrmData

PrmText = 249 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  249  "Aux Inp 4 Ack Mode"
Bit(3) 0 0-1
Prm_Text_Ref = 249 
EndExtUserPrmData

PrmText = 250 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  250  "Aux Inp 5 Ack Mode"
Bit(4) 0 0-1
Prm_Text_Ref = 250 
EndExtUserPrmData

PrmText = 251 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  251  "Aux Inp 6 Ack Mode"
Bit(5) 0 0-1
Prm_Text_Ref = 251 
EndExtUserPrmData

PrmText = 252 
Text(0) = "Time"
Text(1) = "x% Therm. Load"
EndPrmText
ExtUserPrmData =  252  "Cooling Mode"
Bit(7) 0 0-1
Prm_Text_Ref = 252 
EndExtUserPrmData

PrmText = 253 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  253  "Invert DI Start Inp."
Bit(0) 0 0-1
Prm_Text_Ref = 253 
EndExtUserPrmData

PrmText = 254 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  254  "Invert DI Stop Inp."
Bit(1) 1 0-1
Prm_Text_Ref = 254 
EndExtUserPrmData

PrmText = 255 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  255  "Inching DI Start Inp"
Bit(4) 0 0-1
Prm_Text_Ref = 255 
EndExtUserPrmData

PrmText = 256 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  256  "Loc 1 Start Bus Cyc"
Bit(0) 0 0-1
Prm_Text_Ref = 256 
EndExtUserPrmData

PrmText = 257 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  257  "Loc 1 Stop Bus Cyc"
Bit(1) 1 0-1
Prm_Text_Ref = 257 
EndExtUserPrmData

PrmText = 258 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  258  "Loc 1 Start DI"
Bit(2) 1 0-1
Prm_Text_Ref = 258 
EndExtUserPrmData

PrmText = 259 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  259  "Loc 1 Stop DI"
Bit(3) 1 0-1
Prm_Text_Ref = 259 
EndExtUserPrmData

PrmText = 260 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  260  "Loc 1 Start LCD"
Bit(4) 1 0-1
Prm_Text_Ref = 260 
EndExtUserPrmData

PrmText = 261 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  261  "Loc 1 Stop LCD"
Bit(5) 1 0-1
Prm_Text_Ref = 261 
EndExtUserPrmData

PrmText = 262 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  262  "Loc 1 Start Bus Acyc"
Bit(6) 0 0-1
Prm_Text_Ref = 262 
EndExtUserPrmData

PrmText = 263 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  263  "Loc 1 Stop Bus Acyc"
Bit(7) 1 0-1
Prm_Text_Ref = 263 
EndExtUserPrmData

PrmText = 264 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  264  "Auto Start Bus Cyc"
Bit(0) 1 0-1
Prm_Text_Ref = 264 
EndExtUserPrmData

PrmText = 265 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  265  "Auto Stop Bus Cyc"
Bit(1) 1 0-1
Prm_Text_Ref = 265 
EndExtUserPrmData

PrmText = 266 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  266  "Auto Start DI"
Bit(2) 0 0-1
Prm_Text_Ref = 266 
EndExtUserPrmData

PrmText = 267 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  267  "Auto Stop DI"
Bit(3) 1 0-1
Prm_Text_Ref = 267 
EndExtUserPrmData

PrmText = 268 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  268  "Auto Start LCD"
Bit(4) 0 0-1
Prm_Text_Ref = 268 
EndExtUserPrmData

PrmText = 269 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  269  "Auto Stop LCD"
Bit(5) 1 0-1
Prm_Text_Ref = 269 
EndExtUserPrmData

PrmText = 270 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  270  "Auto Start Bus Acyc"
Bit(6) 1 0-1
Prm_Text_Ref = 270 
EndExtUserPrmData

PrmText = 271 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  271  "Auto Stop Bus Acyc"
Bit(7) 1 0-1
Prm_Text_Ref = 271 
EndExtUserPrmData

PrmText = 272 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  272  "Loc 2 Start Bus Cyc"
Bit(0) 0 0-1
Prm_Text_Ref = 272 
EndExtUserPrmData

PrmText = 273 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  273  "Loc 2 Stop Bus Cyc"
Bit(1) 1 0-1
Prm_Text_Ref = 273 
EndExtUserPrmData

PrmText = 274 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  274  "Loc 2 Start DI"
Bit(2) 1 0-1
Prm_Text_Ref = 274 
EndExtUserPrmData

PrmText = 275 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  275  "Loc 2 Stop DI"
Bit(3) 1 0-1
Prm_Text_Ref = 275 
EndExtUserPrmData

PrmText = 276 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  276  "Loc 2 Start LCD"
Bit(4) 1 0-1
Prm_Text_Ref = 276 
EndExtUserPrmData

PrmText = 277 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  277  "Loc 2 Stop LCD"
Bit(5) 1 0-1
Prm_Text_Ref = 277 
EndExtUserPrmData

PrmText = 278 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  278  "Loc 2 Start Bus Acyc"
Bit(6) 0 0-1
Prm_Text_Ref = 278 
EndExtUserPrmData

PrmText = 279 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  279  "Loc 2 Stop Bus Acyc"
Bit(7) 1 0-1
Prm_Text_Ref = 279 
EndExtUserPrmData

PrmText = 280 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  280  "Multif In 0 Autoreset"
Bit(4) 0 0-1
Prm_Text_Ref = 280 
EndExtUserPrmData

PrmText = 281 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  281  "Multif In 1 Autoreset"
Bit(5) 0 0-1
Prm_Text_Ref = 281 
EndExtUserPrmData

PrmText = 282 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  282  "Multif In 2 Autoreset"
Bit(6) 0 0-1
Prm_Text_Ref = 282 
EndExtUserPrmData

ExtUserPrmData =  283  "Aux Inp 1 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  284  "Aux Inp 2 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  285  "Aux Inp 3 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  286  "Aux Inp 4 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  287  "Aux Inp 5 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  288  "Aux Inp 6 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  289  "Check-Back Time [0.1s]"
Unsigned8 5 1-255
EndExtUserPrmData

ExtUserPrmData =  290  "Low Curr Warn Delay [0.1s]"
Unsigned8 5 0-255
EndExtUserPrmData

ExtUserPrmData =  291  "Low Curr Trip Delay [0.1s]"
Unsigned8 5 0-255
EndExtUserPrmData

ExtUserPrmData =  292  "High Curr Warn Delay [0.1s]"
Unsigned8 5 0-255
EndExtUserPrmData

ExtUserPrmData =  293  "High Curr Trip Delay [0.1s]"
Unsigned8 5 0-255
EndExtUserPrmData

ExtUserPrmData =  294  "Curr Imb Trip Level [%]"
Unsigned8 50 0-100
EndExtUserPrmData

ExtUserPrmData =  295  "Curr Imb Warn Level [%]"
Unsigned8 100 0-100
EndExtUserPrmData

PrmText = 296 
Text(0) = "Phase Sequence L1 L2 L3"
Text(1) = "Phase Sequence L3 L2 L1"
EndPrmText
ExtUserPrmData =  296  "Phase Reversal"
Bit(0) 0 0-1
Prm_Text_Ref = 296 
EndExtUserPrmData

ExtUserPrmData =  297  "Restart Level [%]"
Unsigned8 30 10-100
EndExtUserPrmData

PrmText = 298 
Text(0) = "Thermal Load"
Text(1) = "DX1xx DI"
Text(2) = "DX1xx DO"
Text(3) = "Operating Hours"
Text(4) = "Number of Trips"
Text(5) = "Number of Starts"
Text(6) = "max. Startup Current"
Text(7) = "Real Startup Time"
EndPrmText
ExtUserPrmData =  298  "User Display 1"
Unsigned8 0 0-7
Prm_Text_Ref = 298 
EndExtUserPrmData

PrmText = 299 
Text(0) = "Thermal Load"
Text(1) = "DX1xx DI"
Text(2) = "DX1xx DO"
Text(3) = "Operating Hours"
Text(4) = "Number of Trips"
Text(5) = "Number of Starts"
Text(6) = "max. Startup Current"
Text(7) = "Real Startup Time"
EndPrmText
ExtUserPrmData =  299  "User Display 2"
Unsigned8 6 0-7
Prm_Text_Ref = 299 
EndExtUserPrmData

PrmText = 300 
Text(0) = "Thermal Load"
Text(1) = "DX1xx DI"
Text(2) = "DX1xx DO"
Text(3) = "Operating Hours"
Text(4) = "Number of Trips"
Text(5) = "Number of Starts"
Text(6) = "max. Startup Current"
Text(7) = "Real Startup Time"
EndPrmText
ExtUserPrmData =  300  "User Display 3"
Unsigned8 7 0-7
Prm_Text_Ref = 300 
EndExtUserPrmData

PrmText = 301 
Text(0) = "Binary 0"
Text(1) = "Binary 1"
Text(2) = "Analog 0"
Text(3) = "Analog 1"
Text(4) = "Time to Trip"
Text(5) = "Time to Cool"
Text(6) = "Current to earth"
EndPrmText
ExtUserPrmData =  301  "User Display 4"
Unsigned8 4 0-6
Prm_Text_Ref = 301 
EndExtUserPrmData

PrmText = 302 
Text(0) = "Binary 0"
Text(1) = "Binary 1"
Text(2) = "Analog 0"
Text(3) = "Analog 1"
Text(4) = "Time to Trip"
Text(5) = "Time to Cool"
Text(6) = "Current to earth"
EndPrmText
ExtUserPrmData =  302  "User Display 5"
Unsigned8 5 0-6
Prm_Text_Ref = 302 
EndExtUserPrmData

ExtUserPrmData =  303  "Dip Duration [0.1s]"
Unsigned8 5 1-255
EndExtUserPrmData

ExtUserPrmData =  304  "Dip Autorestart Window [0.1s]"
Unsigned8 1 1-10
EndExtUserPrmData

ExtUserPrmData =  305  "Dip Autorestart Delay [s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  306  "Thermal Load Warnlev [%]"
Unsigned8 100 20-100
EndExtUserPrmData

ExtUserPrmData =  307  "Num Starts Allowed"
Unsigned8 0 0-32
EndExtUserPrmData

ExtUserPrmData =  308  "Num Starts Window [1 min.]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  309  "Num Starts Pause [1 min.]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  310  "Earth Flt Warn Level [%]"
Unsigned8 255 20-255
EndExtUserPrmData

ExtUserPrmData =  311  "Earth Flt Warn Delay [0.1s]"
Unsigned8 5 0-255
EndExtUserPrmData

ExtUserPrmData =  312  "Dip Restart Level [%]"
Unsigned8 90 50-115
EndExtUserPrmData

ExtUserPrmData =  313  "Dip Level [%]"
Unsigned8 70 50-115
EndExtUserPrmData

ExtUserPrmData =  314  "DX1xx DI Delay [ms]"
Unsigned8 20 3-200
EndExtUserPrmData

ExtUserPrmData =  315  "U Low Trip Level [%]"
Unsigned8 70 70-100
EndExtUserPrmData

ExtUserPrmData =  316  "U Low Trip Delay [0.1s]"
Unsigned8 30 0-255
EndExtUserPrmData

ExtUserPrmData =  317  "U Low Warn Level [%]"
Unsigned8 70 70-100
EndExtUserPrmData

ExtUserPrmData =  318  "U Low Warn Delay [0.1s]"
Unsigned8 30 0-255
EndExtUserPrmData

ExtUserPrmData =  319  "U High Trip Level [%]"
Unsigned8 116 100-116
EndExtUserPrmData

ExtUserPrmData =  320  "U High Trip Delay [0.1s]"
Unsigned8 30 0-255
EndExtUserPrmData

ExtUserPrmData =  321  "U High Warn Level [%]"
Unsigned8 116 100-116
EndExtUserPrmData

ExtUserPrmData =  322  "U High Warn Delay [0.1s]"
Unsigned8 30 0-255
EndExtUserPrmData

PrmText = 323 
Text(0) = "0-20mA"
Text(1) = "4-20mA"
Text(2) = "0-10mA"
Text(3) = "0-10V"
EndPrmText
ExtUserPrmData =  323  "DX1xx AO Type"
BitArea(0-1) 0 0-3
Prm_Text_Ref = 323 
EndExtUserPrmData

PrmText = 324 
Text(0) = "Disabled"
Text(1) = "Trip"
Text(2) = "Warning"
EndPrmText
ExtUserPrmData =  324  "DX1xx AO Err Reac"
BitArea(2-3) 0 0-2
Prm_Text_Ref = 324 
EndExtUserPrmData

PrmText = 325 
Text(0) = "Disabled"
Text(1) = "Trip"
Text(2) = "Warning"
EndPrmText
ExtUserPrmData =  325  "Num Starts Overrun"
BitArea(2-3) 0 0-2
Prm_Text_Ref = 325 
EndExtUserPrmData

PrmText = 326 
Text(0) = "Disabled"
Text(1) = "Trip"
Text(2) = "Warning"
EndPrmText
ExtUserPrmData =  326  "Num Starts Prewarn"
BitArea(4-5) 0 0-2
Prm_Text_Ref = 326 
EndExtUserPrmData

PrmText = 327 
Text(0) = "Power Scale Factor = 1"
Text(1) = "Power Scale Factor = 10"
Text(2) = "Power Scale Factor = 100"
Text(3) = "Power Scale Factor = 1000"
EndPrmText
ExtUserPrmData =  327  "Power Scale Factor"
BitArea(6-7) 1 0-3
Prm_Text_Ref = 327 
EndExtUserPrmData

PrmText = 328 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  328  "Backlight"
Bit(0) 1 0-1
Prm_Text_Ref = 328 
EndExtUserPrmData

PrmText = 329 
Text(0) = "Off"
Text(1) = "On for Parameters"
Text(2) = "On for Param. + Motor Control"
EndPrmText
ExtUserPrmData =  329  "Password Protection"
BitArea(1-2) 0 0-2
Prm_Text_Ref = 329 
EndExtUserPrmData

PrmText = 330 
Text(0) = "Off"
Text(1) = "On"
Text(2) = "On + Rapid Cycle Lockout"
EndPrmText
ExtUserPrmData =  330  "Dip Enable"
BitArea(3-4) 0 0-2
Prm_Text_Ref = 330 
EndExtUserPrmData

PrmText = 331 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  331  "Dip Autorestart Enable"
Bit(5) 0 0-1
Prm_Text_Ref = 331 
EndExtUserPrmData

ExtUserPrmData =  332  "Nominal Line Voltage [V]"
Unsigned16 400 150-690
EndExtUserPrmData

ExtUserPrmData =  333  "PwrFactor Trip Level"
Unsigned8 30 30-100
EndExtUserPrmData

ExtUserPrmData =  334  "PwrFactor Trip Delay [0.1s]"
Unsigned8 30 0-255
EndExtUserPrmData

ExtUserPrmData =  335  "PwrFactor Warn Level"
Unsigned8 30 30-100
EndExtUserPrmData

ExtUserPrmData =  336  "PwrFactor Warn Delay [0.1s]"
Unsigned8 30 0-255
EndExtUserPrmData

ExtUserPrmData =  337  "U Imb. Trip Level [0.1%]"
Unsigned8 200 2-200
EndExtUserPrmData

ExtUserPrmData =  338  "U Imb. Trip Delay [0.1s]"
Unsigned8 10 0-255
EndExtUserPrmData

ExtUserPrmData =  339  "U Imb. Warn Level [0.1%]"
Unsigned8 200 2-200
EndExtUserPrmData

ExtUserPrmData =  340  "U Imb. Warn Delay [0.1s]"
Unsigned8 10 0-255
EndExtUserPrmData

ExtUserPrmData =  341  "P Low Trip Level [%]"
Unsigned8 20 20-100
EndExtUserPrmData

ExtUserPrmData =  342  "P Low Trip Delay [s]"
Unsigned8 5 0-255
EndExtUserPrmData

ExtUserPrmData =  343  "P Low Warn Level [%]"
Unsigned8 20 20-100
EndExtUserPrmData

ExtUserPrmData =  344  "P Low Warn Delay [s]"
Unsigned8 5 0-255
EndExtUserPrmData

ExtUserPrmData =  345  "P High Trip Level [5%]"
Unsigned8 200 20-200
EndExtUserPrmData

ExtUserPrmData =  346  "P High Trip Delay [s]"
Unsigned8 10 0-255
EndExtUserPrmData

ExtUserPrmData =  347  "P High Warn Level [5%]"
Unsigned8 200 20-200
EndExtUserPrmData

ExtUserPrmData =  348  "P High Warn Delay [s]"
Unsigned8 10 0-255
EndExtUserPrmData

ExtUserPrmData =  349  "Nominal Power Factor"
Unsigned8 100 1-100
EndExtUserPrmData

ExtUserPrmData =  350  "THD Warning Level [%]"
Unsigned8 10 3-10
EndExtUserPrmData

ExtUserPrmData =  351  "Load Startup Delay [s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  352  "THD Warning Delay [s]"
Unsigned8 5 0-255
EndExtUserPrmData

;
;=====================================================================
; special Parameter-Definitions for DPV1-Plug PDP22
;=====================================================================
PrmText = 10000
Text(0) ="Use Block-Parameters"
Text(1) ="Ignore Block-Parameters"
EndPrmText

PrmText = 10001
Text(0) ="DPV0 Diagnosis Format"
Text(1) ="DPV1 Diagnosis Format"
EndPrmText

ExtUserPrmData = 10000 "Block - Parameter"
Unsigned8 0 0-1
Prm_Text_Ref = 10000
EndExtUserPrmData

ExtUserPrmData = 10001 "Diagnosis Format"
Unsigned8 0 0-1
Prm_Text_Ref = 10001
EndExtUserPrmData

;
;===========================================================
;General parameters
;===========================================================
;
GSD_Revision = 3
Vendor_Name ="ABB"
Model_Name ="PDP22-FBP with UMC100"
Revision ="2.01"
Ident_Number   =0x34E0
Protocol_Ident = 0
Station_Type = 0
FMS_supp = 0
Hardware_Release ="V 1.0"
Software_Release ="V 1.0"
9.6_supp       =1
19.2_supp      =1
31.25_supp     =0
45.45_supp     =1
93.75_supp     =1
187.5_supp     =1
500_supp       =1
1.5M_supp      =1
3M_supp = 1
6M_supp = 1
12M_supp = 1
MaxTsdr_9.6 = 15
MaxTsdr_19.2 = 15
MaxTsdr_31.25 = 15
MaxTsdr_45.45 = 15
MaxTsdr_93.75 = 15
MaxTsdr_187.5 = 15
MaxTsdr_500 = 15
MaxTsdr_1.5M   =20
MaxTsdr_3M = 35
MaxTsdr_6M = 50
MaxTsdr_12M = 95
Redundancy = 0
Repeater_Ctrl_Sig = 0
24V_Pins = 1
Implementation_Type ="VPC3 solution"
Bitmap_Device ="FBP_N"
Bitmap_Diag ="FBP_DIAG"
Bitmap_SF ="FBP_RUN"
;
;================================
; Slave-Specification:
;================================
;
Freeze_Mode_supp = 1
Sync_Mode_supp = 1
Set_Slave_Add_Supp = 0
Auto_Baud_supp = 1
Min_Slave_Intervall = 1
Fail_Safe = 1
Max_Diag_Data_Len = 19
Modul_Offset = 0
Slave_Family=9@FieldBusPlug@ProfibusDP
Modular_Station = 1
Max_Module = 1
Max_Input_len = 48
Max_Output_len = 48
Max_Data_len = 96

;=======================================
; Device specific diagnostic data (DPV1)
;=======================================
;

Unit_Diag_Area = 0 - 7
; Diag Status available
Value(129) ="UMC100 Diag status available"
Unit_Diag_Area_End

Unit_Diag_Area = 24 - 31
; Comm-State-Info
Value(0) ="Communication OK"
Value(1) ="Lost Communication to UMC100"
Unit_Diag_Area_End

Unit_Diag_bit(32) = "Thermal Overload Trip"
Unit_Diag_bit(33) = "Phase Loss"
Unit_Diag_bit(34) = "Phase Imbalance"
Unit_Diag_bit(35) = "Locked Rotor"
Unit_Diag_bit(36) = "Thermal Load Prewarn."
Unit_Diag_bit(37) = "PTC Temperature High"
Unit_Diag_bit(38) = "PTC Wiring Problem"
Unit_Diag_bit(39) = "Check-Back Error"

Unit_Diag_bit(40) = "I below Trip Level"
Unit_Diag_bit(41) = "I below Warn Level"
Unit_Diag_bit(42) = "I above Trip Level"
Unit_Diag_bit(43) = "I above Warn Level"
Unit_Diag_bit(44) = "Earthfault Trip"
Unit_Diag_bit(45) = "Earthfault Warning"
Unit_Diag_bit(46) = "UMC Selftest Error"
Unit_Diag_bit(47) = "Actuator"

Unit_Diag_bit(48) = "IO-Module Missing"
Unit_Diag_bit(49) = "Application Error"
Unit_Diag_bit(50) = "IO-Module Warning/Error"
Unit_Diag_bit(51) = "Auxiliary Input 1"
Unit_Diag_bit(52) = "Auxiliary Input 2"
Unit_Diag_bit(53) = "Auxiliary Input 3"
Unit_Diag_bit(54) = "Auxiliary Input 4"
Unit_Diag_bit(55) = "Auxiliary Input 5"

Unit_Diag_bit(56) = "Auxiliary Input 6"
Unit_Diag_bit(57) = "Ext. Fault Multif. DI0"
Unit_Diag_bit(58) = "Ext. Fault Multif. DI1"
Unit_Diag_bit(59) = "Ext. Fault Multif. DI2"
Unit_Diag_bit(60) = "reserved"
Unit_Diag_bit(61) = "reserved"
Unit_Diag_bit(62) = "reserved"
Unit_Diag_bit(63) = "reserved"

Unit_Diag_bit(64) = "reserved"
Unit_Diag_bit(65) = "reserved"
Unit_Diag_bit(66) = "Underload Power"
Unit_Diag_bit(67) = "Overload Power"
Unit_Diag_bit(68) = "Voltage out of spec."
Unit_Diag_bit(69) = "THD Warning"
Unit_Diag_bit(70) = "reserved"
Unit_Diag_bit(71) = "reserved"

Unit_Diag_bit(72) = "reserved"
Unit_Diag_bit(73) = "reserved"
Unit_Diag_bit(74) = "reserved"
Unit_Diag_bit(75) = "Num Starts Overrun"
Unit_Diag_bit(76) = "Just one start left"
Unit_Diag_bit(77) = "Cooling Time Running"
Unit_Diag_bit(78) = "reserved"
Unit_Diag_bit(79) = "reserved"

Unit_Diag_bit(80) = "reserved"
Unit_Diag_bit(81) = "reserved"
Unit_Diag_bit(82) = "reserved"
Unit_Diag_bit(83) = "reserved"
Unit_Diag_bit(84) = "reserved"
Unit_Diag_bit(85) = "reserved"
Unit_Diag_bit(86) = "Parameter out of range"
Unit_Diag_bit(87) = "Ext. Diag. Available"

Unit_Diag_bit(88) = "Bit0 ext. UMC-Diagnosis"
Unit_Diag_bit(89) = "Bit1 ext. UMC-Diagnosis"
Unit_Diag_bit(90) = "Bit2 ext. UMC-Diagnosis"
Unit_Diag_bit(91) = "Bit3 ext. UMC-Diagnosis"
Unit_Diag_bit(92) = "Bit4 ext. UMC-Diagnosis"
Unit_Diag_bit(93) = "Bit5 ext. UMC-Diagnosis"
Unit_Diag_bit(94) = "Bit6 ext. UMC-Diagnosis"
Unit_Diag_bit(95) = "Bit7 ext. UMC-Diagnosis"

;=============================================
; User Prm Data: Length and Preset:
;=============================================
;
Max_User_Prm_Data_Len   = 232             ;   number of parameter of UMC100 (max 224)
;                                        + number of parameter for the FBP itself (8)
Ext_User_Prm_Data_Const(0) = 0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00    ; constant values for ASIC
;DPV1 status1 = 0x00 =>
;       Bit2 = 0 WD_Base=10ms (1ms=1)
;       Bit7 = 1 DPV1 Enable (Disable=0)
;DPV1 status2 = 0x00 =>
;       Bit0 = 0 ChkCfg nach EN50170(User specific=1)
;DPV1 status3 = 0x00 =>
;       alarm not implemented

Ext_User_Prm_Data_Ref(3) = 10000        ; use/ignore Block-Parameters
Ext_User_Prm_Data_Ref(4) = 10001        ; Diag-Format DPV0/V1
;
;=============================================
; Module Definition List
;=============================================
;

Module="UMC100-FBP (V1.13)"0x11, 0x23, 0x56, 0x63      ; 16DI, 32DO, 7AI, 4AO
1
Ext_Module_Prm_Data_Len= 224                        ; number of used data byte
Ext_User_Prm_Data_Const(0) =    \                 ; initialising of param data
    0x00, 0x00, 0x00, 0x32, 0x00, 0x00, 0x00, 0x32, 0x02, 0x58,  \
    0x00, 0x64, 0x00, 0x78, 0x00, 0x05, 0x00, 0x01, 0x00, 0x01,  \
    0x0A, 0x00, 0x1E, 0xA0, 0xA0, 0x05, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x03, 0x00, 0x00, 0x00, 0x00, 0x08, 0x60,  \
    0x00, 0x00, 0x02, 0xBE, 0xEB, 0xBE, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x05, 0x05, 0x05, 0x05,  \
    0x05, 0x32, 0x64, 0x00, 0x1E, 0x00, 0x06, 0x07, 0x04, 0x05,  \
    0x00, 0x05, 0x01, 0x00, 0x64, 0x00, 0x64, 0x0A, 0x00, 0x05,  \
    0x64, 0x64, 0x00, 0x14, 0x14, 0x14, 0x14, 0x00, 0x00, 0x05,  \
    0x0A, 0x05, 0x78, 0x05, 0x64, 0x05, 0xE0, 0x05, 0xE0, 0x05,  \
    0xE0, 0x05, 0xE0, 0x05, 0xE0, 0x05, 0xE0, 0x05, 0x00, 0x14,  \
    0x00, 0x14, 0x40, 0x44, 0x00, 0x00, 0x00, 0x01, 0x01, 0x7C,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00
Ext_User_Prm_Data_Ref( 0 ) = 1 ;   Setting Ie 1
Ext_User_Prm_Data_Ref( 4 ) = 2 ;   Setting Ie 2
Ext_User_Prm_Data_Ref( 8 ) = 3 ;   YD Starting Time
Ext_User_Prm_Data_Ref( 10 ) = 4 ;   Current Factor
Ext_User_Prm_Data_Ref( 12 ) = 5 ;   Cooling Time
Ext_User_Prm_Data_Ref( 16 ) = 6 ;   Language
Ext_User_Prm_Data_Ref( 17 ) = 7 ;   Rev Lock-Out Time
Ext_User_Prm_Data_Ref( 18 ) = 8 ;   Fault Output
Ext_User_Prm_Data_Ref( 19 ) = 9 ;   Trip Class
Ext_User_Prm_Data_Ref( 20 ) = 10 ;   Low Curr Warn Level
Ext_User_Prm_Data_Ref( 21 ) = 11 ;   Low Curr Trip Level
Ext_User_Prm_Data_Ref( 22 ) = 12 ;   High Curr Warn Level
Ext_User_Prm_Data_Ref( 23 ) = 13 ;   High Curr Trip Level
Ext_User_Prm_Data_Ref( 24 ) = 14 ;   Locked Rotor Level
Ext_User_Prm_Data_Ref( 25 ) = 15 ;   Locked Rotor Delay
Ext_User_Prm_Data_Ref( 26 ) = 16 ;   Custom App Parameter
Ext_User_Prm_Data_Ref( 27 ) = 17 ;   Multif In 0
Ext_User_Prm_Data_Ref( 28 ) = 18 ;   Multif In 1
Ext_User_Prm_Data_Ref( 29 ) = 19 ;   Multif In 2
Ext_User_Prm_Data_Ref( 30 ) = 20 ;   Multif In 0 Delay
Ext_User_Prm_Data_Ref( 31 ) = 21 ;   Multif In 1 Delay
Ext_User_Prm_Data_Ref( 32 ) = 22 ;   Multif In 2 Delay
Ext_User_Prm_Data_Ref( 33 ) = 23 ;   Control Function
Ext_User_Prm_Data_Ref( 34 ) = 24 ;   Busfault Reaction
Ext_User_Prm_Data_Ref( 35 ) = 25 ;   Aux Inp 1 Reaction
Ext_User_Prm_Data_Ref( 35 ) = 26 ;   Aux Inp 2 Reaction
Ext_User_Prm_Data_Ref( 36 ) = 27 ;   Aux Inp 3 Reaction
Ext_User_Prm_Data_Ref( 36 ) = 28 ;   Aux Inp 4 Reaction
Ext_User_Prm_Data_Ref( 37 ) = 29 ;   Aux Inp 5 Reaction
Ext_User_Prm_Data_Ref( 37 ) = 30 ;   Aux Inp 6 Reaction
Ext_User_Prm_Data_Ref( 38 ) = 31 ;   PTC, Thermistor
Ext_User_Prm_Data_Ref( 38 ) = 32 ;   Check-Back
Ext_User_Prm_Data_Ref( 38 ) = 33 ;   Check Phase Sequence
Ext_User_Prm_Data_Ref( 39 ) = 34 ;   Fault Auto Reset
Ext_User_Prm_Data_Ref( 39 ) = 35 ;   Emergency Start
Ext_User_Prm_Data_Ref( 39 ) = 36 ;   Address Check
Ext_User_Prm_Data_Ref( 39 ) = 37 ;   Enable Custom Logic
Ext_User_Prm_Data_Ref( 39 ) = 38 ;   YD Change-Over Mode
Ext_User_Prm_Data_Ref( 39 ) = 39 ;   Phase Loss Prot.
Ext_User_Prm_Data_Ref( 40 ) = 40 ;   DX1xx Enabled
Ext_User_Prm_Data_Ref( 40 ) = 41 ;   Missing Module React.
Ext_User_Prm_Data_Ref( 41 ) = 42 ;   Aux Inp 1 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 43 ;   Aux Inp 2 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 44 ;   Aux Inp 3 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 45 ;   Aux Inp 4 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 46 ;   Aux Inp 5 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 47 ;   Aux Inp 6 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 48 ;   Cooling Mode
Ext_User_Prm_Data_Ref( 42 ) = 49 ;   Invert DI Start Inp.
Ext_User_Prm_Data_Ref( 42 ) = 50 ;   Invert DI Stop Inp.
Ext_User_Prm_Data_Ref( 42 ) = 51 ;   Inching DI Start Inp
Ext_User_Prm_Data_Ref( 43 ) = 52 ;   Loc 1 Start Bus Cyc
Ext_User_Prm_Data_Ref( 43 ) = 53 ;   Loc 1 Stop Bus Cyc
Ext_User_Prm_Data_Ref( 43 ) = 54 ;   Loc 1 Start DI
Ext_User_Prm_Data_Ref( 43 ) = 55 ;   Loc 1 Stop DI
Ext_User_Prm_Data_Ref( 43 ) = 56 ;   Loc 1 Start LCD
Ext_User_Prm_Data_Ref( 43 ) = 57 ;   Loc 1 Stop LCD
Ext_User_Prm_Data_Ref( 43 ) = 58 ;   Loc 1 Start Bus Acyc
Ext_User_Prm_Data_Ref( 43 ) = 59 ;   Loc 1 Stop Bus Acyc
Ext_User_Prm_Data_Ref( 44 ) = 60 ;   Auto Start Bus Cyc
Ext_User_Prm_Data_Ref( 44 ) = 61 ;   Auto Stop Bus Cyc
Ext_User_Prm_Data_Ref( 44 ) = 62 ;   Auto Start DI
Ext_User_Prm_Data_Ref( 44 ) = 63 ;   Auto Stop DI
Ext_User_Prm_Data_Ref( 44 ) = 64 ;   Auto Start LCD
Ext_User_Prm_Data_Ref( 44 ) = 65 ;   Auto Stop LCD
Ext_User_Prm_Data_Ref( 44 ) = 66 ;   Auto Start Bus Acyc
Ext_User_Prm_Data_Ref( 44 ) = 67 ;   Auto Stop Bus Acyc
Ext_User_Prm_Data_Ref( 45 ) = 68 ;   Loc 2 Start Bus Cyc
Ext_User_Prm_Data_Ref( 45 ) = 69 ;   Loc 2 Stop Bus Cyc
Ext_User_Prm_Data_Ref( 45 ) = 70 ;   Loc 2 Start DI
Ext_User_Prm_Data_Ref( 45 ) = 71 ;   Loc 2 Stop DI
Ext_User_Prm_Data_Ref( 45 ) = 72 ;   Loc 2 Start LCD
Ext_User_Prm_Data_Ref( 45 ) = 73 ;   Loc 2 Stop LCD
Ext_User_Prm_Data_Ref( 45 ) = 74 ;   Loc 2 Start Bus Acyc
Ext_User_Prm_Data_Ref( 45 ) = 75 ;   Loc 2 Stop Bus Acyc
Ext_User_Prm_Data_Ref( 46 ) = 76 ;   Multif In 0 Autoreset
Ext_User_Prm_Data_Ref( 46 ) = 77 ;   Multif In 1 Autoreset
Ext_User_Prm_Data_Ref( 46 ) = 78 ;   Multif In 2 Autoreset
Ext_User_Prm_Data_Ref( 50 ) = 79 ;   Aux Inp 1 Delay
Ext_User_Prm_Data_Ref( 51 ) = 80 ;   Aux Inp 2 Delay
Ext_User_Prm_Data_Ref( 52 ) = 81 ;   Aux Inp 3 Delay
Ext_User_Prm_Data_Ref( 53 ) = 82 ;   Aux Inp 4 Delay
Ext_User_Prm_Data_Ref( 54 ) = 83 ;   Aux Inp 5 Delay
Ext_User_Prm_Data_Ref( 55 ) = 84 ;   Aux Inp 6 Delay
Ext_User_Prm_Data_Ref( 56 ) = 85 ;   Check-Back Time
Ext_User_Prm_Data_Ref( 57 ) = 86 ;   Low Curr Warn Delay
Ext_User_Prm_Data_Ref( 58 ) = 87 ;   Low Curr Trip Delay
Ext_User_Prm_Data_Ref( 59 ) = 88 ;   High Curr Warn Delay
Ext_User_Prm_Data_Ref( 60 ) = 89 ;   High Curr Trip Delay
Ext_User_Prm_Data_Ref( 61 ) = 90 ;   Phase Imb Trip Level
Ext_User_Prm_Data_Ref( 62 ) = 91 ;   Phase Imb Warn Level
Ext_User_Prm_Data_Ref( 63 ) = 92 ;   Phase Reversal
Ext_User_Prm_Data_Ref( 64 ) = 93 ;   Restart Level
Ext_User_Prm_Data_Ref( 65 ) = 94 ;   User Display 1
Ext_User_Prm_Data_Ref( 66 ) = 95 ;   User Display 2
Ext_User_Prm_Data_Ref( 67 ) = 96 ;   User Display 3
Ext_User_Prm_Data_Ref( 68 ) = 97 ;   User Display 4
Ext_User_Prm_Data_Ref( 69 ) = 98 ;   User Display 5
Ext_User_Prm_Data_Ref( 71 ) = 99 ;   Dip Duration
Ext_User_Prm_Data_Ref( 72 ) = 100 ;   Dip Autorestart Window
Ext_User_Prm_Data_Ref( 73 ) = 101 ;   Dip Autorestart Delay
Ext_User_Prm_Data_Ref( 74 ) = 102 ;   Thermal Load Warnlev
Ext_User_Prm_Data_Ref( 83 ) = 103 ;   DX1xx DI Delay
Ext_User_Prm_Data_Ref( 112 ) = 104 ;   DX1xx AO Type
Ext_User_Prm_Data_Ref( 112 ) = 105 ;   DX1xx AO Err Reac
Ext_User_Prm_Data_Ref( 117 ) = 106 ;   Backlight
Ext_User_Prm_Data_Ref( 117 ) = 107 ;   Password Protection
Ext_User_Prm_Data_Ref( 117 ) = 108 ;   Dip Enable
Ext_User_Prm_Data_Ref( 117 ) = 109 ;   Dip Autorestart Enable
EndModule


Module="UMC100-FBP (R0101 R0201)"0x11, 0x23, 0x56, 0x63      ; 16DI, 32DO, 7AI, 4AO
2
Ext_Module_Prm_Data_Len= 224                        ; number of used data byte
Ext_User_Prm_Data_Const(0) =    \                 ; initialising of param data
    0x00, 0x00, 0x00, 0x32, 0x00, 0x00, 0x00, 0x32, 0x02, 0x58,  \
    0x00, 0x64, 0x00, 0x78, 0xFF, 0x05, 0x00, 0x01, 0x00, 0x01,  \
    0x0A, 0x00, 0x1E, 0xA0, 0xA0, 0x05, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x03, 0x00, 0x00, 0x00, 0x00, 0x08, 0x64,  \
    0x00, 0x00, 0x02, 0xBE, 0xEB, 0xBE, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x05, 0x05, 0x05, 0x05,  \
    0x05, 0x32, 0x64, 0x00, 0x1E, 0x00, 0x06, 0x07, 0x04, 0x05,  \
    0x00, 0x05, 0x01, 0x00, 0x64, 0x00, 0x00, 0x00, 0xFF, 0x05,  \
    0x5A, 0x46, 0x00, 0x14, 0x14, 0x14, 0x14, 0x00, 0x46, 0x1E,  \
    0x46, 0x1E, 0x74, 0x1E, 0x74, 0x1E, 0xE0, 0x05, 0xE0, 0x05,  \
    0xE0, 0x05, 0xE0, 0x05, 0xE0, 0x05, 0xE0, 0x05, 0x00, 0x14,  \
    0x00, 0x14, 0x40, 0x44, 0x00, 0x00, 0x40, 0x01, 0x01, 0x90,  \
    0x1E, 0x1E, 0x1E, 0x1E, 0xC8, 0x0A, 0xC8, 0x0A, 0x14, 0x05,  \
    0x14, 0x05, 0xC8, 0x0A, 0xC8, 0x0A, 0x64, 0x00, 0x00, 0x0A,  \
    0x00, 0x05, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00
Ext_User_Prm_Data_Ref( 0 ) = 201 ;   Setting Ie 1
Ext_User_Prm_Data_Ref( 4 ) = 202 ;   Setting Ie 2
Ext_User_Prm_Data_Ref( 8 ) = 203 ;   YD Starting Time
Ext_User_Prm_Data_Ref( 10 ) = 204 ;   Current Factor
Ext_User_Prm_Data_Ref( 12 ) = 205 ;   Cooling Time
Ext_User_Prm_Data_Ref( 14 ) = 206 ;   Earth Flt Trip Level
Ext_User_Prm_Data_Ref( 15 ) = 207 ;   Earth Flt Trip Delay
Ext_User_Prm_Data_Ref( 16 ) = 208 ;   Language
Ext_User_Prm_Data_Ref( 17 ) = 209 ;   Rev Lock-Out Time
Ext_User_Prm_Data_Ref( 18 ) = 210 ;   Fault Output
Ext_User_Prm_Data_Ref( 19 ) = 211 ;   Trip Class
Ext_User_Prm_Data_Ref( 20 ) = 212 ;   Low Curr Warn Level
Ext_User_Prm_Data_Ref( 21 ) = 213 ;   Low Curr Trip Level
Ext_User_Prm_Data_Ref( 22 ) = 214 ;   High Curr Warn Level
Ext_User_Prm_Data_Ref( 23 ) = 215 ;   High Curr Trip Level
Ext_User_Prm_Data_Ref( 24 ) = 216 ;   Locked Rotor Level
Ext_User_Prm_Data_Ref( 25 ) = 217 ;   Locked Rotor Delay
Ext_User_Prm_Data_Ref( 26 ) = 218 ;   Custom App Parameter
Ext_User_Prm_Data_Ref( 27 ) = 219 ;   Multif In 0
Ext_User_Prm_Data_Ref( 28 ) = 220 ;   Multif In 1
Ext_User_Prm_Data_Ref( 29 ) = 221 ;   Multif In 2
Ext_User_Prm_Data_Ref( 30 ) = 222 ;   Multif In 0 Delay
Ext_User_Prm_Data_Ref( 31 ) = 223 ;   Multif In 1 Delay
Ext_User_Prm_Data_Ref( 32 ) = 224 ;   Multif In 2 Delay
Ext_User_Prm_Data_Ref( 33 ) = 225 ;   Control Function
Ext_User_Prm_Data_Ref( 34 ) = 226 ;   Busfault Reaction
Ext_User_Prm_Data_Ref( 35 ) = 227 ;   Aux Inp 1 Reaction
Ext_User_Prm_Data_Ref( 35 ) = 228 ;   Aux Inp 2 Reaction
Ext_User_Prm_Data_Ref( 36 ) = 229 ;   Aux Inp 3 Reaction
Ext_User_Prm_Data_Ref( 36 ) = 230 ;   Aux Inp 4 Reaction
Ext_User_Prm_Data_Ref( 37 ) = 231 ;   Aux Inp 5 Reaction
Ext_User_Prm_Data_Ref( 37 ) = 232 ;   Aux Inp 6 Reaction
Ext_User_Prm_Data_Ref( 38 ) = 233 ;   PTC, Thermistor
Ext_User_Prm_Data_Ref( 38 ) = 234 ;   Check-Back
Ext_User_Prm_Data_Ref( 38 ) = 235 ;   Check Phase Sequence
Ext_User_Prm_Data_Ref( 39 ) = 236 ;   Fault Auto Reset
Ext_User_Prm_Data_Ref( 39 ) = 237 ;   Emergency Start
Ext_User_Prm_Data_Ref( 39 ) = 238 ;   Earth Flt Detection
Ext_User_Prm_Data_Ref( 39 ) = 239 ;   Address Check
Ext_User_Prm_Data_Ref( 39 ) = 240 ;   Enable Custom Logic
Ext_User_Prm_Data_Ref( 39 ) = 241 ;   YD Change-Over Mode
Ext_User_Prm_Data_Ref( 39 ) = 242 ;   Phase Loss Prot.
Ext_User_Prm_Data_Ref( 40 ) = 243 ;   DX1xx Enabled
Ext_User_Prm_Data_Ref( 40 ) = 244 ;   VI15x Enabled
Ext_User_Prm_Data_Ref( 40 ) = 245 ;   Missing Module React.
Ext_User_Prm_Data_Ref( 41 ) = 246 ;   Aux Inp 1 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 247 ;   Aux Inp 2 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 248 ;   Aux Inp 3 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 249 ;   Aux Inp 4 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 250 ;   Aux Inp 5 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 251 ;   Aux Inp 6 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 252 ;   Cooling Mode
Ext_User_Prm_Data_Ref( 42 ) = 253 ;   Invert DI Start Inp.
Ext_User_Prm_Data_Ref( 42 ) = 254 ;   Invert DI Stop Inp.
Ext_User_Prm_Data_Ref( 42 ) = 255 ;   Inching DI Start Inp
Ext_User_Prm_Data_Ref( 43 ) = 256 ;   Loc 1 Start Bus Cyc
Ext_User_Prm_Data_Ref( 43 ) = 257 ;   Loc 1 Stop Bus Cyc
Ext_User_Prm_Data_Ref( 43 ) = 258 ;   Loc 1 Start DI
Ext_User_Prm_Data_Ref( 43 ) = 259 ;   Loc 1 Stop DI
Ext_User_Prm_Data_Ref( 43 ) = 260 ;   Loc 1 Start LCD
Ext_User_Prm_Data_Ref( 43 ) = 261 ;   Loc 1 Stop LCD
Ext_User_Prm_Data_Ref( 43 ) = 262 ;   Loc 1 Start Bus Acyc
Ext_User_Prm_Data_Ref( 43 ) = 263 ;   Loc 1 Stop Bus Acyc
Ext_User_Prm_Data_Ref( 44 ) = 264 ;   Auto Start Bus Cyc
Ext_User_Prm_Data_Ref( 44 ) = 265 ;   Auto Stop Bus Cyc
Ext_User_Prm_Data_Ref( 44 ) = 266 ;   Auto Start DI
Ext_User_Prm_Data_Ref( 44 ) = 267 ;   Auto Stop DI
Ext_User_Prm_Data_Ref( 44 ) = 268 ;   Auto Start LCD
Ext_User_Prm_Data_Ref( 44 ) = 269 ;   Auto Stop LCD
Ext_User_Prm_Data_Ref( 44 ) = 270 ;   Auto Start Bus Acyc
Ext_User_Prm_Data_Ref( 44 ) = 271 ;   Auto Stop Bus Acyc
Ext_User_Prm_Data_Ref( 45 ) = 272 ;   Loc 2 Start Bus Cyc
Ext_User_Prm_Data_Ref( 45 ) = 273 ;   Loc 2 Stop Bus Cyc
Ext_User_Prm_Data_Ref( 45 ) = 274 ;   Loc 2 Start DI
Ext_User_Prm_Data_Ref( 45 ) = 275 ;   Loc 2 Stop DI
Ext_User_Prm_Data_Ref( 45 ) = 276 ;   Loc 2 Start LCD
Ext_User_Prm_Data_Ref( 45 ) = 277 ;   Loc 2 Stop LCD
Ext_User_Prm_Data_Ref( 45 ) = 278 ;   Loc 2 Start Bus Acyc
Ext_User_Prm_Data_Ref( 45 ) = 279 ;   Loc 2 Stop Bus Acyc
Ext_User_Prm_Data_Ref( 46 ) = 280 ;   Multif In 0 Autoreset
Ext_User_Prm_Data_Ref( 46 ) = 281 ;   Multif In 1 Autoreset
Ext_User_Prm_Data_Ref( 46 ) = 282 ;   Multif In 2 Autoreset
Ext_User_Prm_Data_Ref( 50 ) = 283 ;   Aux Inp 1 Delay
Ext_User_Prm_Data_Ref( 51 ) = 284 ;   Aux Inp 2 Delay
Ext_User_Prm_Data_Ref( 52 ) = 285 ;   Aux Inp 3 Delay
Ext_User_Prm_Data_Ref( 53 ) = 286 ;   Aux Inp 4 Delay
Ext_User_Prm_Data_Ref( 54 ) = 287 ;   Aux Inp 5 Delay
Ext_User_Prm_Data_Ref( 55 ) = 288 ;   Aux Inp 6 Delay
Ext_User_Prm_Data_Ref( 56 ) = 289 ;   Check-Back Time
Ext_User_Prm_Data_Ref( 57 ) = 290 ;   Low Curr Warn Delay
Ext_User_Prm_Data_Ref( 58 ) = 291 ;   Low Curr Trip Delay
Ext_User_Prm_Data_Ref( 59 ) = 292 ;   High Curr Warn Delay
Ext_User_Prm_Data_Ref( 60 ) = 293 ;   High Curr Trip Delay
Ext_User_Prm_Data_Ref( 61 ) = 294 ;   Curr Imb Trip Level
Ext_User_Prm_Data_Ref( 62 ) = 295 ;   Curr Imb Warn Level
Ext_User_Prm_Data_Ref( 63 ) = 296 ;   Phase Reversal
Ext_User_Prm_Data_Ref( 64 ) = 297 ;   Restart Level
Ext_User_Prm_Data_Ref( 65 ) = 298 ;   User Display 1
Ext_User_Prm_Data_Ref( 66 ) = 299 ;   User Display 2
Ext_User_Prm_Data_Ref( 67 ) = 300 ;   User Display 3
Ext_User_Prm_Data_Ref( 68 ) = 301 ;   User Display 4
Ext_User_Prm_Data_Ref( 69 ) = 302 ;   User Display 5
Ext_User_Prm_Data_Ref( 71 ) = 303 ;   Dip Duration
Ext_User_Prm_Data_Ref( 72 ) = 304 ;   Dip Autorestart Window
Ext_User_Prm_Data_Ref( 73 ) = 305 ;   Dip Autorestart Delay
Ext_User_Prm_Data_Ref( 74 ) = 306 ;   Thermal Load Warnlev
Ext_User_Prm_Data_Ref( 75 ) = 307 ;   Num Starts Allowed
Ext_User_Prm_Data_Ref( 76 ) = 308 ;   Num Starts Window
Ext_User_Prm_Data_Ref( 77 ) = 309 ;   Num Starts Pause
Ext_User_Prm_Data_Ref( 78 ) = 310 ;   Earth Flt Warn Level
Ext_User_Prm_Data_Ref( 79 ) = 311 ;   Earth Flt Warn Delay
Ext_User_Prm_Data_Ref( 80 ) = 312 ;   Dip Restart Level
Ext_User_Prm_Data_Ref( 81 ) = 313 ;   Dip Level
Ext_User_Prm_Data_Ref( 83 ) = 314 ;   DX1xx DI Delay
Ext_User_Prm_Data_Ref( 88 ) = 315 ;   U Low Trip Level
Ext_User_Prm_Data_Ref( 89 ) = 316 ;   U Low Trip Delay
Ext_User_Prm_Data_Ref( 90 ) = 317 ;   U Low Warn Level
Ext_User_Prm_Data_Ref( 91 ) = 318 ;   U Low Warn Delay
Ext_User_Prm_Data_Ref( 92 ) = 319 ;   U High Trip Level
Ext_User_Prm_Data_Ref( 93 ) = 320 ;   U High Trip Delay
Ext_User_Prm_Data_Ref( 94 ) = 321 ;   U High Warn Level
Ext_User_Prm_Data_Ref( 95 ) = 322 ;   U High Warn Delay
Ext_User_Prm_Data_Ref( 112 ) = 323 ;   DX1xx AO Type
Ext_User_Prm_Data_Ref( 112 ) = 324 ;   DX1xx AO Err Reac
Ext_User_Prm_Data_Ref( 116 ) = 325 ;   Num Starts Overrun
Ext_User_Prm_Data_Ref( 116 ) = 326 ;   Num Starts Prewarn
Ext_User_Prm_Data_Ref( 116 ) = 327 ;   Power Scale Factor
Ext_User_Prm_Data_Ref( 117 ) = 328 ;   Backlight
Ext_User_Prm_Data_Ref( 117 ) = 329 ;   Password Protection
Ext_User_Prm_Data_Ref( 117 ) = 330 ;   Dip Enable
Ext_User_Prm_Data_Ref( 117 ) = 331 ;   Dip Autorestart Enable
Ext_User_Prm_Data_Ref( 118 ) = 332 ;   Nominal Line Voltage
Ext_User_Prm_Data_Ref( 120 ) = 333 ;   PwrFactor Trip Level
Ext_User_Prm_Data_Ref( 121 ) = 334 ;   PwrFactor Trip Delay
Ext_User_Prm_Data_Ref( 122 ) = 335 ;   PwrFactor Warn Level
Ext_User_Prm_Data_Ref( 123 ) = 336 ;   PwrFactor Warn Delay
Ext_User_Prm_Data_Ref( 124 ) = 337 ;   U Imb. Trip Level
Ext_User_Prm_Data_Ref( 125 ) = 338 ;   U Imb. Trip Delay
Ext_User_Prm_Data_Ref( 126 ) = 339 ;   U Imb. Warn Level
Ext_User_Prm_Data_Ref( 127 ) = 340 ;   U Imb. Warn Delay
Ext_User_Prm_Data_Ref( 128 ) = 341 ;   P Low Trip Level
Ext_User_Prm_Data_Ref( 129 ) = 342 ;   P Low Trip Delay
Ext_User_Prm_Data_Ref( 130 ) = 343 ;   P Low Warn Level
Ext_User_Prm_Data_Ref( 131 ) = 344 ;   P Low Warn Delay
Ext_User_Prm_Data_Ref( 132 ) = 345 ;   P High Trip Level
Ext_User_Prm_Data_Ref( 133 ) = 346 ;   P High Trip Delay
Ext_User_Prm_Data_Ref( 134 ) = 347 ;   P High Warn Level
Ext_User_Prm_Data_Ref( 135 ) = 348 ;   P High Warn Delay
Ext_User_Prm_Data_Ref( 136 ) = 349 ;   Nominal Power Factor
Ext_User_Prm_Data_Ref( 139 ) = 350 ;   THD Warning Level
Ext_User_Prm_Data_Ref( 140 ) = 351 ;   Load Startup Delay
Ext_User_Prm_Data_Ref( 141 ) = 352 ;   THD Warning Delay
EndModule

Module="UMC 100-FBP (R0101 R0201)Profil2" 0x11, 0x21, 0x50   	; 16DI, 16DO, 1AI, I/O-Data-Profil 2
3
Ext_Module_Prm_Data_Len= 224                        ; number of used data byte
Ext_User_Prm_Data_Const(0) =    \                 ; initialising of param data
    0x00, 0x00, 0x00, 0x32, 0x00, 0x00, 0x00, 0x32, 0x02, 0x58,  \
    0x00, 0x64, 0x00, 0x78, 0xFF, 0x05, 0x00, 0x01, 0x00, 0x01,  \
    0x0A, 0x00, 0x1E, 0xA0, 0xA0, 0x05, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x03, 0x00, 0x00, 0x00, 0x00, 0x08, 0x64,  \
    0x00, 0x00, 0x02, 0xBE, 0xEB, 0xBE, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x05, 0x05, 0x05, 0x05,  \
    0x05, 0x32, 0x64, 0x00, 0x1E, 0x00, 0x06, 0x07, 0x04, 0x05,  \
    0x00, 0x05, 0x01, 0x00, 0x64, 0x00, 0x00, 0x00, 0xFF, 0x05,  \
    0x5A, 0x46, 0x00, 0x14, 0x14, 0x14, 0x14, 0x00, 0x46, 0x1E,  \
    0x46, 0x1E, 0x74, 0x1E, 0x74, 0x1E, 0xE0, 0x05, 0xE0, 0x05,  \
    0xE0, 0x05, 0xE0, 0x05, 0xE0, 0x05, 0xE0, 0x05, 0x00, 0x14,  \
    0x00, 0x14, 0x40, 0x44, 0x00, 0x00, 0x40, 0x01, 0x01, 0x90,  \
    0x1E, 0x1E, 0x1E, 0x1E, 0xC8, 0x0A, 0xC8, 0x0A, 0x14, 0x05,  \
    0x14, 0x05, 0xC8, 0x0A, 0xC8, 0x0A, 0x64, 0x00, 0x00, 0x0A,  \
    0x00, 0x05, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00
Ext_User_Prm_Data_Ref( 0 ) = 201 ;   Setting Ie 1
Ext_User_Prm_Data_Ref( 4 ) = 202 ;   Setting Ie 2
Ext_User_Prm_Data_Ref( 8 ) = 203 ;   YD Starting Time
Ext_User_Prm_Data_Ref( 10 ) = 204 ;   Current Factor
Ext_User_Prm_Data_Ref( 12 ) = 205 ;   Cooling Time
Ext_User_Prm_Data_Ref( 14 ) = 206 ;   Earth Flt Trip Level
Ext_User_Prm_Data_Ref( 15 ) = 207 ;   Earth Flt Trip Delay
Ext_User_Prm_Data_Ref( 16 ) = 208 ;   Language
Ext_User_Prm_Data_Ref( 17 ) = 209 ;   Rev Lock-Out Time
Ext_User_Prm_Data_Ref( 18 ) = 210 ;   Fault Output
Ext_User_Prm_Data_Ref( 19 ) = 211 ;   Trip Class
Ext_User_Prm_Data_Ref( 20 ) = 212 ;   Low Curr Warn Level
Ext_User_Prm_Data_Ref( 21 ) = 213 ;   Low Curr Trip Level
Ext_User_Prm_Data_Ref( 22 ) = 214 ;   High Curr Warn Level
Ext_User_Prm_Data_Ref( 23 ) = 215 ;   High Curr Trip Level
Ext_User_Prm_Data_Ref( 24 ) = 216 ;   Locked Rotor Level
Ext_User_Prm_Data_Ref( 25 ) = 217 ;   Locked Rotor Delay
Ext_User_Prm_Data_Ref( 26 ) = 218 ;   Custom App Parameter
Ext_User_Prm_Data_Ref( 27 ) = 219 ;   Multif In 0
Ext_User_Prm_Data_Ref( 28 ) = 220 ;   Multif In 1
Ext_User_Prm_Data_Ref( 29 ) = 221 ;   Multif In 2
Ext_User_Prm_Data_Ref( 30 ) = 222 ;   Multif In 0 Delay
Ext_User_Prm_Data_Ref( 31 ) = 223 ;   Multif In 1 Delay
Ext_User_Prm_Data_Ref( 32 ) = 224 ;   Multif In 2 Delay
Ext_User_Prm_Data_Ref( 33 ) = 225 ;   Control Function
Ext_User_Prm_Data_Ref( 34 ) = 226 ;   Busfault Reaction
Ext_User_Prm_Data_Ref( 35 ) = 227 ;   Aux Inp 1 Reaction
Ext_User_Prm_Data_Ref( 35 ) = 228 ;   Aux Inp 2 Reaction
Ext_User_Prm_Data_Ref( 36 ) = 229 ;   Aux Inp 3 Reaction
Ext_User_Prm_Data_Ref( 36 ) = 230 ;   Aux Inp 4 Reaction
Ext_User_Prm_Data_Ref( 37 ) = 231 ;   Aux Inp 5 Reaction
Ext_User_Prm_Data_Ref( 37 ) = 232 ;   Aux Inp 6 Reaction
Ext_User_Prm_Data_Ref( 38 ) = 233 ;   PTC, Thermistor
Ext_User_Prm_Data_Ref( 38 ) = 234 ;   Check-Back
Ext_User_Prm_Data_Ref( 38 ) = 235 ;   Check Phase Sequence
Ext_User_Prm_Data_Ref( 39 ) = 236 ;   Fault Auto Reset
Ext_User_Prm_Data_Ref( 39 ) = 237 ;   Emergency Start
Ext_User_Prm_Data_Ref( 39 ) = 238 ;   Earth Flt Detection
Ext_User_Prm_Data_Ref( 39 ) = 239 ;   Address Check
Ext_User_Prm_Data_Ref( 39 ) = 240 ;   Enable Custom Logic
Ext_User_Prm_Data_Ref( 39 ) = 241 ;   YD Change-Over Mode
Ext_User_Prm_Data_Ref( 39 ) = 242 ;   Phase Loss Prot.
Ext_User_Prm_Data_Ref( 40 ) = 243 ;   DX1xx Enabled
Ext_User_Prm_Data_Ref( 40 ) = 244 ;   VI15x Enabled
Ext_User_Prm_Data_Ref( 40 ) = 245 ;   Missing Module React.
Ext_User_Prm_Data_Ref( 41 ) = 246 ;   Aux Inp 1 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 247 ;   Aux Inp 2 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 248 ;   Aux Inp 3 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 249 ;   Aux Inp 4 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 250 ;   Aux Inp 5 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 251 ;   Aux Inp 6 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 252 ;   Cooling Mode
Ext_User_Prm_Data_Ref( 42 ) = 253 ;   Invert DI Start Inp.
Ext_User_Prm_Data_Ref( 42 ) = 254 ;   Invert DI Stop Inp.
Ext_User_Prm_Data_Ref( 42 ) = 255 ;   Inching DI Start Inp
Ext_User_Prm_Data_Ref( 43 ) = 256 ;   Loc 1 Start Bus Cyc
Ext_User_Prm_Data_Ref( 43 ) = 257 ;   Loc 1 Stop Bus Cyc
Ext_User_Prm_Data_Ref( 43 ) = 258 ;   Loc 1 Start DI
Ext_User_Prm_Data_Ref( 43 ) = 259 ;   Loc 1 Stop DI
Ext_User_Prm_Data_Ref( 43 ) = 260 ;   Loc 1 Start LCD
Ext_User_Prm_Data_Ref( 43 ) = 261 ;   Loc 1 Stop LCD
Ext_User_Prm_Data_Ref( 43 ) = 262 ;   Loc 1 Start Bus Acyc
Ext_User_Prm_Data_Ref( 43 ) = 263 ;   Loc 1 Stop Bus Acyc
Ext_User_Prm_Data_Ref( 44 ) = 264 ;   Auto Start Bus Cyc
Ext_User_Prm_Data_Ref( 44 ) = 265 ;   Auto Stop Bus Cyc
Ext_User_Prm_Data_Ref( 44 ) = 266 ;   Auto Start DI
Ext_User_Prm_Data_Ref( 44 ) = 267 ;   Auto Stop DI
Ext_User_Prm_Data_Ref( 44 ) = 268 ;   Auto Start LCD
Ext_User_Prm_Data_Ref( 44 ) = 269 ;   Auto Stop LCD
Ext_User_Prm_Data_Ref( 44 ) = 270 ;   Auto Start Bus Acyc
Ext_User_Prm_Data_Ref( 44 ) = 271 ;   Auto Stop Bus Acyc
Ext_User_Prm_Data_Ref( 45 ) = 272 ;   Loc 2 Start Bus Cyc
Ext_User_Prm_Data_Ref( 45 ) = 273 ;   Loc 2 Stop Bus Cyc
Ext_User_Prm_Data_Ref( 45 ) = 274 ;   Loc 2 Start DI
Ext_User_Prm_Data_Ref( 45 ) = 275 ;   Loc 2 Stop DI
Ext_User_Prm_Data_Ref( 45 ) = 276 ;   Loc 2 Start LCD
Ext_User_Prm_Data_Ref( 45 ) = 277 ;   Loc 2 Stop LCD
Ext_User_Prm_Data_Ref( 45 ) = 278 ;   Loc 2 Start Bus Acyc
Ext_User_Prm_Data_Ref( 45 ) = 279 ;   Loc 2 Stop Bus Acyc
Ext_User_Prm_Data_Ref( 46 ) = 280 ;   Multif In 0 Autoreset
Ext_User_Prm_Data_Ref( 46 ) = 281 ;   Multif In 1 Autoreset
Ext_User_Prm_Data_Ref( 46 ) = 282 ;   Multif In 2 Autoreset
Ext_User_Prm_Data_Ref( 50 ) = 283 ;   Aux Inp 1 Delay
Ext_User_Prm_Data_Ref( 51 ) = 284 ;   Aux Inp 2 Delay
Ext_User_Prm_Data_Ref( 52 ) = 285 ;   Aux Inp 3 Delay
Ext_User_Prm_Data_Ref( 53 ) = 286 ;   Aux Inp 4 Delay
Ext_User_Prm_Data_Ref( 54 ) = 287 ;   Aux Inp 5 Delay
Ext_User_Prm_Data_Ref( 55 ) = 288 ;   Aux Inp 6 Delay
Ext_User_Prm_Data_Ref( 56 ) = 289 ;   Check-Back Time
Ext_User_Prm_Data_Ref( 57 ) = 290 ;   Low Curr Warn Delay
Ext_User_Prm_Data_Ref( 58 ) = 291 ;   Low Curr Trip Delay
Ext_User_Prm_Data_Ref( 59 ) = 292 ;   High Curr Warn Delay
Ext_User_Prm_Data_Ref( 60 ) = 293 ;   High Curr Trip Delay
Ext_User_Prm_Data_Ref( 61 ) = 294 ;   Curr Imb Trip Level
Ext_User_Prm_Data_Ref( 62 ) = 295 ;   Curr Imb Warn Level
Ext_User_Prm_Data_Ref( 63 ) = 296 ;   Phase Reversal
Ext_User_Prm_Data_Ref( 64 ) = 297 ;   Restart Level
Ext_User_Prm_Data_Ref( 65 ) = 298 ;   User Display 1
Ext_User_Prm_Data_Ref( 66 ) = 299 ;   User Display 2
Ext_User_Prm_Data_Ref( 67 ) = 300 ;   User Display 3
Ext_User_Prm_Data_Ref( 68 ) = 301 ;   User Display 4
Ext_User_Prm_Data_Ref( 69 ) = 302 ;   User Display 5
Ext_User_Prm_Data_Ref( 71 ) = 303 ;   Dip Duration
Ext_User_Prm_Data_Ref( 72 ) = 304 ;   Dip Autorestart Window
Ext_User_Prm_Data_Ref( 73 ) = 305 ;   Dip Autorestart Delay
Ext_User_Prm_Data_Ref( 74 ) = 306 ;   Thermal Load Warnlev
Ext_User_Prm_Data_Ref( 75 ) = 307 ;   Num Starts Allowed
Ext_User_Prm_Data_Ref( 76 ) = 308 ;   Num Starts Window
Ext_User_Prm_Data_Ref( 77 ) = 309 ;   Num Starts Pause
Ext_User_Prm_Data_Ref( 78 ) = 310 ;   Earth Flt Warn Level
Ext_User_Prm_Data_Ref( 79 ) = 311 ;   Earth Flt Warn Delay
Ext_User_Prm_Data_Ref( 80 ) = 312 ;   Dip Restart Level
Ext_User_Prm_Data_Ref( 81 ) = 313 ;   Dip Level
Ext_User_Prm_Data_Ref( 83 ) = 314 ;   DX1xx DI Delay
Ext_User_Prm_Data_Ref( 88 ) = 315 ;   U Low Trip Level
Ext_User_Prm_Data_Ref( 89 ) = 316 ;   U Low Trip Delay
Ext_User_Prm_Data_Ref( 90 ) = 317 ;   U Low Warn Level
Ext_User_Prm_Data_Ref( 91 ) = 318 ;   U Low Warn Delay
Ext_User_Prm_Data_Ref( 92 ) = 319 ;   U High Trip Level
Ext_User_Prm_Data_Ref( 93 ) = 320 ;   U High Trip Delay
Ext_User_Prm_Data_Ref( 94 ) = 321 ;   U High Warn Level
Ext_User_Prm_Data_Ref( 95 ) = 322 ;   U High Warn Delay
Ext_User_Prm_Data_Ref( 112 ) = 323 ;   DX1xx AO Type
Ext_User_Prm_Data_Ref( 112 ) = 324 ;   DX1xx AO Err Reac
Ext_User_Prm_Data_Ref( 116 ) = 325 ;   Num Starts Overrun
Ext_User_Prm_Data_Ref( 116 ) = 326 ;   Num Starts Prewarn
Ext_User_Prm_Data_Ref( 116 ) = 327 ;   Power Scale Factor
Ext_User_Prm_Data_Ref( 117 ) = 328 ;   Backlight
Ext_User_Prm_Data_Ref( 117 ) = 329 ;   Password Protection
Ext_User_Prm_Data_Ref( 117 ) = 330 ;   Dip Enable
Ext_User_Prm_Data_Ref( 117 ) = 331 ;   Dip Autorestart Enable
Ext_User_Prm_Data_Ref( 118 ) = 332 ;   Nominal Line Voltage
Ext_User_Prm_Data_Ref( 120 ) = 333 ;   PwrFactor Trip Level
Ext_User_Prm_Data_Ref( 121 ) = 334 ;   PwrFactor Trip Delay
Ext_User_Prm_Data_Ref( 122 ) = 335 ;   PwrFactor Warn Level
Ext_User_Prm_Data_Ref( 123 ) = 336 ;   PwrFactor Warn Delay
Ext_User_Prm_Data_Ref( 124 ) = 337 ;   U Imb. Trip Level
Ext_User_Prm_Data_Ref( 125 ) = 338 ;   U Imb. Trip Delay
Ext_User_Prm_Data_Ref( 126 ) = 339 ;   U Imb. Warn Level
Ext_User_Prm_Data_Ref( 127 ) = 340 ;   U Imb. Warn Delay
Ext_User_Prm_Data_Ref( 128 ) = 341 ;   P Low Trip Level
Ext_User_Prm_Data_Ref( 129 ) = 342 ;   P Low Trip Delay
Ext_User_Prm_Data_Ref( 130 ) = 343 ;   P Low Warn Level
Ext_User_Prm_Data_Ref( 131 ) = 344 ;   P Low Warn Delay
Ext_User_Prm_Data_Ref( 132 ) = 345 ;   P High Trip Level
Ext_User_Prm_Data_Ref( 133 ) = 346 ;   P High Trip Delay
Ext_User_Prm_Data_Ref( 134 ) = 347 ;   P High Warn Level
Ext_User_Prm_Data_Ref( 135 ) = 348 ;   P High Warn Delay
Ext_User_Prm_Data_Ref( 136 ) = 349 ;   Nominal Power Factor
Ext_User_Prm_Data_Ref( 139 ) = 350 ;   THD Warning Level
Ext_User_Prm_Data_Ref( 140 ) = 351 ;   Load Startup Delay
Ext_User_Prm_Data_Ref( 141 ) = 352 ;   THD Warning Delay
EndModule



; DPV1 Alarm
DPV1_Slave = 1
C1_Read_Write_supp = 1
C1_Max_Data_Len                     = 8         ;The parameter specifies the maximum length of user data excluding
                                                ;Function_Num, Slot_number, Index, Length, transferred on the
                                                ;MSAC_1 communication channel.
                                                ;Type: Unsigned8 (0 .. 240)
C1_Response_Timeout = 300
Diagnostic_Alarm_supp = 0
Process_Alarm_supp = 0
Pull_Plug_Alarm_supp = 0
Status_Alarm_supp = 0
Update_Alarm_supp = 0
Manufacturer_Specific_Alarm_supp = 0
Alarm_Sequence_Mode_Count = 0
Alarm_Type_Mode_supp = 0
Diagnostic_Alarm_required = 0

C2_Read_Write_supp = 1
C2_Max_Data_Len                     = 48        ;The parameter specifies the maximum length of user data excluding
                                                ;Function_Num, Slot_number, Index, Length, transferred on the
                                                ;MSAC_2 communication channel.
                                                ;Type: Unsigned8 (0,48 .. 240)
C2_Response_Timeout = 300
C2_Read_Write_required = 1
C2_Max_Count_Channels = 3
Max_Initiate_PDU_Length             = 52        ;The parameter specifies the maximum length of an Initiate Request
                                                ;PDU including the Function_Num to the Resource Manager.
                                                ;Type: Unsigned8 (0,52.. 244)
DPV1_Data_Types                     = 0             ;

