;======================================================
;======================================================
#Profibus_DP
; HIGHEST Module_Index currently in use: 37
;
; Version: 2.07 for ePlug DPV1 (PDP22) modified by Mattias Abelsson Date 2011-06-16
; ** new PST Softstarter CU 06.00.00 added (module_index = 36)
; ** minor corrections to older CU versions of PST
;
; Version: 2.06 for ePlug DPV1 (PDP22) modified Brigitte Dien Date 2011-02-01
; ** minor corrections
;
; Version: 2.05 for ePlug DPV1 (PDP22) modified by Taji Kuruvilla/Brigitte Dien Date 2010-09-17
; ** new PSE Softstarter fw rev. 01.02.01 added (module_index = 35)
;
; Version: 2.04 for ePlug DPV1 (PDP22) modified by Tore Sandberg/Brigitte Dien Date 2010-03-19
; ** added new module with config. data for the ABB XR ITS unit 
;
; Version: 2.03 for ePlug DPV1 (PDP22) modified by Josef R. Kalinski  Date 2009-07-14
; ** new PST Softstarter CU 05.05.00 added (module_index = 33)
; ** for all modules UMC22-FBP: value of block current changed from 0x0A to 0xA0
;
; Version: 2.02 for ePlug DPV1 (PDP22) modified by Brigitte Dien Date 2008-11-19
; ** Config String for UFD Modules was wrong
;
; Version: 2.01 for ePlug DPV1 (PDP22) modified by Brigitte Dien Date 2008-08-28
; ** new module Lincoln LMC1_Glas added (module_index = 32)
;
; Version: 2.00 for ePlug DPV1 (PDP22) modified by Josef R. Kalinski  Date 2008-07-04
; ** new PST Softstarter CU 05.04.04 added (module_index = 31)
;
; 
;
; GSD file for the Plug PDP22 valid for:
;
;	DEVICE / ID / firmware-version / device index
;-----------------------------------------------------
;	Sensor (direct)	  / -                        / -          / all
; 	MSD11             / 1SAJ 310000 Rxxxx        / -          / all
;	MSR22             / 1SAJ 320000 Rxxxx        / -          / all
;	MFI21             / 1SAJ 410000 R0100        / -          / all
;	UMC22 V3.0, 3.10  / 1SAJ 510000 R0100        / V3.0 V3.10 / a30  a31
; 	UMC22 V3.10, 3.20 / 1SAJ 510000 R0200        / V3.20      / b32
; 	UMC22 V3.30       / 1SAJ 510000 R0300        / V3.30      / b33
; 	UMC22 V3.40       / 1SAJ 510000 R0400        / V3.40      / c34
; 	UMC22 V4.00       / 1SAJ 510000 R0600        / V4.00      / c40
;	PST Softstarter   / CU 01.00.00, CU 01.01.00 / -          / -
;	PST Softstarter   / CU 02.00.01, CU 02.01.00 / -          / -
;	PST Softstarter   / CU 03.03.02              / -          / -
;	PST Softstarter   / CU 03.04.01, CU 03.05.00 / -          / -
;	PST Softstarter	 / CU 04.00.02
;	PST Softstarter	 / CU 05.02.02
;	PST Softstarter	 / CU 05.03.03
;	PST Softstarter	 / CU 05.04.04
;	PST Softstarter	 / CU 05.05.00
;	PST Softstarter	 / CU 06.00.00
;	Wireless WDI100   / -                        / WDI100_Ver0_Rev9_5 / -
;	Wireless WDIO100  / WDX / WDP / WDI          / 
;	PR222DS		  / 1SDA059469R1             / EP010 V2.0 / - (TMAX)
;	PR223EF		  / 1SDA064515R1             / EP010 V1.0 / - (TMAX)
;	PR122/PR123/PR332/PR333	/ 1SDA060198R1       / EP010 V2.0 / - (EMAX)
;	Sensopart         / -                        / Revision 1.50 / -
;	Willy Vogel AG    / UFD10                    / -          / -
;	Willy Vogel AG    / UFD20                    / -          / -
;	SS91 Heat Control /
;	PSE Softstarter	 / 
;	PSTX Softstarter / Fieldbus Revision 1.1
;
; 
;	If additional "Ext_User_Prm_Data_Ref" numbers for new devices are defined,
;	they must fit into the following predefined ranges:
;	STO Heidelberg		range 0...999
;	Sweden 					range 1000...1999
;	Italy					range 2000...2999 
;
; 				
;=============================================================
; Text-definition for User Prm Data  "UMC22_FBP (V3.0)"
;=============================================================
;
PrmText = 2
Text(0)   = "Acknowledge"
Text(1)   = "Auto"
EndPrmText
;PrmText = 4
;Text(1)   = "Trip"
;EndPrmText
PrmText = 5
Text(0)   = "Relays Off"
Text(1)   = "Outputs Retain Status"
EndPrmText
PrmText = 6
Text(0)  = "Class  5"
Text(1)  = "Class 10"
Text(2)  = "Class 20"
Text(3)  = "Class 30"
EndPrmText
PrmText = 7
Text(1)  = "Transparent"
Text(2)  = "Overload Relay"
Text(3)  = "Direct Starter"
Text(4)  = "Reversing Starter"
Text(5)  = "Star-Delta Starter 1"
Text(6)  = "Pole-Changing Starter 1"
EndPrmText
PrmText = 16
Text(0)   = "Off"
Text(1)   = "On"
EndPrmText
PrmText = 17
Text(1)   = "Auxiliary Contacts"
Text(2)   = "Motor Current"
Text(3)   = "Simulation"
EndPrmText
PrmText = 18
Text(0)   = "Time"
Text(1)   = "Current"
EndPrmText

ExtUserPrmData =  1 "0301 Set Current 1=10mA*"
Unsigned32 50 24-6300
EndExtUserPrmData
;ExtUserPrmData =  2 "Factor for Current Transformer"
;Unsigned16 1 0-200
;EndExtUserPrmData
ExtUserPrmData =  3 "0401 Trip Class"
Unsigned8 1 0-3
Prm_Text_Ref = 6
EndExtUserPrmData
;ExtUserPrmData =  4 "Overload Behaviour"
;Unsigned8 1 1-1
;Prm_Text_Ref = 4
;EndExtUserPrmData
ExtUserPrmData =  5 "0402 Phase Loss Protection"
Unsigned8 1 0-1
Prm_Text_Ref = 16
EndExtUserPrmData
ExtUserPrmData =  6 "0407 Low Current Threshold=5%*"
Unsigned8 10 6-20
EndExtUserPrmData
ExtUserPrmData =  7 "0408 High Current Threshold=5%*"
Unsigned8 30 20-160
EndExtUserPrmData
ExtUserPrmData =  8 "0403 Cooling Time=0.1s*"
Unsigned16 1200 300-36000
EndExtUserPrmData
ExtUserPrmData =  9 "0404 Automatic fault reset"
Unsigned8 0 0-1
Prm_Text_Ref = 2
EndExtUserPrmData
ExtUserPrmData = 10 "0101 Control Function"
Unsigned8 1 1-6
Prm_Text_Ref = 7
EndExtUserPrmData
ExtUserPrmData = 11 "0202 Check Back"
Unsigned8 2 1-3
Prm_Text_Ref = 17
EndExtUserPrmData
ExtUserPrmData = 12 "0207 Star-Delta Start.Time=0.1s*"
Unsigned16 600 10-36000
EndExtUserPrmData
ExtUserPrmData = 13 "0205 Revers. Lockout Time=0.1s*"
Unsigned16 20 2-36000
EndExtUserPrmData
;ExtUserPrmData = 14 "0601 Operating Hours of Motor"
;Unsigned32 0 0-15000000
;EndExtUserPrmData
;ExtUserPrmData = 15 "0602 Number of Starts"
;Unsigned32 0 0-15000000
;EndExtUserPrmData
ExtUserPrmData = 16 "0501 Commun. fault reaction"
Unsigned8 0 0-1
Prm_Text_Ref = 5
EndExtUserPrmData
ExtUserPrmData = 17 "0405 Start Up Time=0.1s*"
Unsigned16 1200 0-6000
EndExtUserPrmData
ExtUserPrmData = 18 "0201 Local Control via DIs"
Unsigned8 0 0-1
Prm_Text_Ref = 16
EndExtUserPrmData
ExtUserPrmData = 19 "0406 Block.Current Threshold=5%*"
Unsigned8 160 0-160
EndExtUserPrmData
ExtUserPrmData = 20 "0204 Fault Output"
Unsigned8 0 0-1
Prm_Text_Ref = 16
EndExtUserPrmData
ExtUserPrmData = 21 "0206 Star-Delta Changeover Mode"
Unsigned8 1 0-1
Prm_Text_Ref = 18
EndExtUserPrmData
ExtUserPrmData = 23 "0302 Set Current 2=10mA*"
Unsigned32 50 24-6300
EndExtUserPrmData
ExtUserPrmData = 24 "0203 Fault Input"
Unsigned8 0 0-1
Prm_Text_Ref = 16
EndExtUserPrmData
ExtUserPrmData = 25 "0502 Address Check"
Unsigned8 0 0-1
Prm_Text_Ref = 16
EndExtUserPrmData
;
;=============================================================
; Text-definition for User Prm Data  "UMC22_FBP (V3.10, V3.20)"
;=============================================================
;
PrmText = 102
Text(0)   = "Disabled"
Text(1)   = "Autoreset"
EndPrmText
;PrmText = 104
;Text(1)   = "Trip"
;EndPrmText
PrmText = 105
Text(0)   = "Relays Off"
Text(1)   = "Outputs Retain Status"
EndPrmText
PrmText = 106
Text(0)  = "Class  5"
Text(1)  = "Class 10"
Text(2)  = "Class 20"
Text(3)  = "Class 30"
EndPrmText
PrmText = 107
Text(1)  = "Transparent"
Text(2)  = "Overload Relay"
Text(3)  = "Direct Starter"
Text(4)  = "Reversing Starter"
Text(5)  = "Star-Delta Starter 1"
Text(6)  = "Pole-Changing Starter 1"
EndPrmText
PrmText = 116
Text(0)   = "Off"
Text(1)   = "On"
EndPrmText
PrmText = 117
Text(1)   = "Auxiliary Contacts"
Text(2)   = "Motor Current"
Text(3)   = "Simulation"
EndPrmText
PrmText = 118
Text(0)   = "Time"
Text(1)   = "Current"
EndPrmText

ExtUserPrmData = 101 "01 Set Current 1=10mA*"
Unsigned32 50 24-320000
EndExtUserPrmData
ExtUserPrmData = 102 "02 Current Factor"
Unsigned16 100 100-64000
EndExtUserPrmData
ExtUserPrmData = 103 "04 Trip Class"
Unsigned8 1 0-3
Prm_Text_Ref = 106
EndExtUserPrmData
;ExtUserPrmData =  104 "05 Overload Behaviour"
;Unsigned8 1 1-1
;Prm_Text_Ref = 4
;EndExtUserPrmData
ExtUserPrmData =  105 "06 Phase Loss Protection"
Unsigned8 1 0-1
Prm_Text_Ref = 116
EndExtUserPrmData
ExtUserPrmData =  106 "08 Low Current Threshold=5%*"
Unsigned8 10 6-20
EndExtUserPrmData
ExtUserPrmData =  107 "09 High Current Threshold=5%*"
Unsigned8 30 20-160
EndExtUserPrmData
ExtUserPrmData =  108 "10 Cooling Time=0.1s*"
Unsigned16 1200 300-36000
EndExtUserPrmData
ExtUserPrmData =  109 "11 Automatic fault reset"
Unsigned8 0 0-1
Prm_Text_Ref = 102
EndExtUserPrmData
ExtUserPrmData = 110 "12 Control Function"
Unsigned8 1 1-6
Prm_Text_Ref = 107
EndExtUserPrmData
ExtUserPrmData = 111 "13 Check-Back"
Unsigned8 2 1-3
Prm_Text_Ref = 117
EndExtUserPrmData
ExtUserPrmData = 112 "16 Star-Delta Start.Time=0.1s*"
Unsigned16 600 10-36000
EndExtUserPrmData
ExtUserPrmData = 113 "17 Reverse Lockout Time=0.1s*"
Unsigned16 20 2-36000
EndExtUserPrmData
ExtUserPrmData = 114 "18 Operating Hours of Motor"
Unsigned16 0 0-65535
EndExtUserPrmData
ExtUserPrmData = 115 "19 Number of Starts"
Unsigned32 0 0-1000000
EndExtUserPrmData
ExtUserPrmData = 116 "20 Bus fault reaction"
Unsigned8 0 0-1
Prm_Text_Ref = 105
EndExtUserPrmData
ExtUserPrmData = 117 "14 Start-Up Time=0.1s*"
Unsigned16 1200 0-6000
EndExtUserPrmData
ExtUserPrmData = 118 "22 Local Control via DIs"
Unsigned8 0 0-1
Prm_Text_Ref = 116
EndExtUserPrmData
ExtUserPrmData = 119 "23 Block.Current Threshold=5%*"
Unsigned8 160 0-160
EndExtUserPrmData
ExtUserPrmData = 120 "24 Fault Output"
Unsigned8 0 0-1
Prm_Text_Ref = 116
EndExtUserPrmData
ExtUserPrmData = 121 "15 Star-Delta Changeover Mode"
Unsigned8 1 0-1
Prm_Text_Ref = 118
EndExtUserPrmData
ExtUserPrmData = 123 "03 Set Current 2=10mA*"
Unsigned32 50 24-320000
EndExtUserPrmData
ExtUserPrmData = 124 "21 Fault Input"
Unsigned8 0 0-1
Prm_Text_Ref = 116
EndExtUserPrmData
ExtUserPrmData = 125 "26 Address Check"
Unsigned8 0 0-1
Prm_Text_Ref = 116
EndExtUserPrmData
ExtUserPrmData = 126 "25 Number of Trips"
Unsigned8 0 0-255
EndExtUserPrmData
;
;
;=============================================================
; Text-definition for User Prm Data  "UMC22_FBP (V3.30)"
;=============================================================
;
PrmText = 152
Text(0)   = "Disabled"
Text(1)   = "Autoreset"
EndPrmText
;PrmText = 154
;Text(1)   = "Trip"
;EndPrmText
PrmText = 155
Text(0)   = "Relays Off"
Text(1)   = "Outputs Retain Status"
EndPrmText
PrmText = 156
Text(0)  = "Class  5"
Text(1)  = "Class 10"
Text(2)  = "Class 20"
Text(3)  = "Class 30"
EndPrmText
PrmText = 157
Text(1)  = "Transparent"
Text(2)  = "Overload Relay"
Text(3)  = "Direct Starter"
Text(4)  = "Reversing Starter"
Text(5)  = "Star-Delta Starter 1"
Text(6)  = "Pole-Changing Starter 1"
Text(7)  = "Actuator 1"
Text(8)  = "Actuator 2"
Text(9)  = "Actuator 3"
Text(10) = "Actuator 4"
EndPrmText
PrmText = 166
Text(0)   = "Off"
Text(1)   = "On"
EndPrmText
PrmText = 167
Text(1)   = "Auxiliary Contacts"
Text(2)   = "Motor Current"
Text(3)   = "Simulation"
EndPrmText
PrmText = 168
Text(0)   = "Time"
Text(1)   = "Current"
EndPrmText
PrmText = 169
Text(0)   = "Off"
Text(1)   = "On"
Text(2)   = "002"
Text(3)   = "003"
Text(4)   = "004"
Text(5)   = "005"
EndPrmText
ExtUserPrmData = 151 "01 Set Current 1=10mA*"
Unsigned32 50 24-320000
EndExtUserPrmData
ExtUserPrmData = 152 "02 Current Factor (%)" 
Unsigned16 100 100-64000
EndExtUserPrmData
ExtUserPrmData = 153 "04 Trip Class"
Unsigned8 1 0-3
Prm_Text_Ref = 156
EndExtUserPrmData
ExtUserPrmData =  154 "05 DI0 Multi Function Input" 
Unsigned8 0 0-255
EndExtUserPrmData
ExtUserPrmData =  155 "06 Phase Loss Protection"
Unsigned8 1 0-1
Prm_Text_Ref = 166
EndExtUserPrmData
ExtUserPrmData =  156 "08 Low Current Threshold=5%*"
Unsigned8 10 1-20				   
EndExtUserPrmData
ExtUserPrmData =  157 "09 High Current Threshold=5%*"
Unsigned8 30 20-160
EndExtUserPrmData
ExtUserPrmData =  158 "10 Cooling Time=0.1s*"
Unsigned16 1200 300-36000
EndExtUserPrmData
ExtUserPrmData =  159 "11 Automatic fault reset"
Unsigned8 0 0-1
Prm_Text_Ref = 152
EndExtUserPrmData
ExtUserPrmData = 160 "12 Control Function"
Unsigned8 1 1-10
Prm_Text_Ref = 157
EndExtUserPrmData
ExtUserPrmData = 161 "13 Check-Back"
Unsigned8 2 1-3
Prm_Text_Ref = 167
EndExtUserPrmData
ExtUserPrmData = 162 "16 Star-Delta Start.Time=0.1s*"
Unsigned16 600 10-36000
EndExtUserPrmData
ExtUserPrmData = 163 "17 Reverse Lockout Time=0.1s*"
Unsigned16 20 2-36000
EndExtUserPrmData
ExtUserPrmData = 164 "18 Operating Hours of Motor"
Unsigned16 0 0-65535
EndExtUserPrmData
ExtUserPrmData = 165 "19 Number of Starts"
Unsigned32 0 0-1000000
EndExtUserPrmData
ExtUserPrmData = 166 "20 Bus fault reaction"
Unsigned8 0 0-1
Prm_Text_Ref = 155
EndExtUserPrmData
ExtUserPrmData = 167 "14 Start-Up Time=0.1s*"
Unsigned16 1200 0-6000
EndExtUserPrmData
ExtUserPrmData = 168 "22 Local Control" 
Unsigned8 0 0-5
Prm_Text_Ref = 169
EndExtUserPrmData
ExtUserPrmData = 169 "23 Block.Current Threshold=5%*"
Unsigned8 160 0-160
EndExtUserPrmData
ExtUserPrmData = 170 "24 Fault Output"
Unsigned8 0 0-1
Prm_Text_Ref = 166
EndExtUserPrmData
ExtUserPrmData = 171 "15 Star-Delta Changeover Mode"
Unsigned8 1 0-1
Prm_Text_Ref = 168
EndExtUserPrmData
ExtUserPrmData = 173 "03 Set Current 2=10mA*"
Unsigned32 50 24-320000
EndExtUserPrmData
ExtUserPrmData = 174 "21 DI2 Multi Function Input"
Unsigned8 0 0-255
EndExtUserPrmData
ExtUserPrmData = 175 "26 Address Check"
Unsigned8 0 0-1
Prm_Text_Ref = 166
EndExtUserPrmData
ExtUserPrmData = 176 "25 Number of Trips"
Unsigned8 0 0-255
EndExtUserPrmData
ExtUserPrmData = 177 "07 DI1 Multi Function Input"
Unsigned8 0 0-255
EndExtUserPrmData
ExtUserPrmData = 178 "27 Emergency by PLC"
Unsigned8 0 0-1
Prm_Text_Ref = 166
EndExtUserPrmData
;
;=============================================================
; Text-definition for User Prm Data  "UMC22_FBP (V3.40)"
;=============================================================
;
PrmText = 170
Text(0)   = "Off"
Text(1)   = "On"
Text(2)   = "Off+PTC Warn"
Text(3)   = "On+PTC Warn"
;Text(4)   = "004"
;Text(5)   = "005"
Text(6)   = "Off+PTC Trip"
Text(7)   = "On+PTC Trip"
EndPrmText

PrmText = 171
Text(1)  = "Transparent"
Text(2)  = "Overload Relay"
Text(3)  = "Direct Starter"
Text(4)  = "Reversing Starter"
Text(5)  = "Star-Delta Starter 1"
Text(6)  = "Pole-Changing Starter 1"
Text(7)  = "Actuator 1"
Text(8)  = "Actuator 2"
Text(9)  = "Actuator 3"
Text(10) = "Actuator 4"
Text(11) = "Star-Delta Starter 2"
EndPrmText

PrmText = 172
Text(0)   = "Off"
Text(1)   = "On"
Text(3)   = "blink"
EndPrmText



ExtUserPrmData = 181 "01 Set Current 1=10mA*"
Unsigned32 50 24-320000
EndExtUserPrmData
ExtUserPrmData = 182 "02 Current Factor (%)" 
Unsigned16 100 100-64000
EndExtUserPrmData
ExtUserPrmData = 183 "04 Trip Class"
Unsigned8 1 0-3
Prm_Text_Ref = 156
EndExtUserPrmData
ExtUserPrmData =  184 "05 DI0 Multi Function Input" 
Unsigned8 0 0-255
EndExtUserPrmData
ExtUserPrmData =  185 "06 Phase Loss Protection"
Unsigned8 1 0-7
Prm_Text_Ref = 170
EndExtUserPrmData

ExtUserPrmData =  186 "08 Low Current Threshold=5%*"
Unsigned8 10 1-20				   
EndExtUserPrmData
ExtUserPrmData =  187 "09 High Current Threshold=5%*"
Unsigned8 30 20-160
EndExtUserPrmData
ExtUserPrmData =  188 "10 Cooling Time=0.1s*"
Unsigned16 1200 300-36000
EndExtUserPrmData
ExtUserPrmData =  189 "11 Automatic fault reset"
Unsigned8 0 0-1
Prm_Text_Ref = 152
EndExtUserPrmData

ExtUserPrmData = 190 "12 Control Function"
Unsigned8 1 1-11
Prm_Text_Ref = 171
EndExtUserPrmData

ExtUserPrmData = 191 "13 Check-Back"
Unsigned8 2 1-3
Prm_Text_Ref = 167
EndExtUserPrmData
ExtUserPrmData = 192 "16 Star-Delta Start.Time=0.1s*"
Unsigned16 600 10-36000
EndExtUserPrmData
ExtUserPrmData = 193 "17 Reverse Lockout Time=0.1s*"
Unsigned16 20 2-36000
EndExtUserPrmData
ExtUserPrmData = 194 "18 Operating Hours of Motor"
Unsigned16 0 0-65535
EndExtUserPrmData
ExtUserPrmData = 195 "19 Number of Starts"
Unsigned32 0 0-1000000
EndExtUserPrmData
ExtUserPrmData = 196 "20 Bus fault reaction"
Unsigned8 0 0-1
Prm_Text_Ref = 155
EndExtUserPrmData
ExtUserPrmData = 197 "14 Start-Up Time=0.1s*"
Unsigned16 1200 0-6000
EndExtUserPrmData
ExtUserPrmData = 198 "22 Local Control" 
Unsigned8 0 0-5
Prm_Text_Ref = 169
EndExtUserPrmData
ExtUserPrmData = 199 "23 Block.Current Threshold=5%*"
Unsigned8 160 0-160
EndExtUserPrmData

ExtUserPrmData = 200 "24 Fault Output"
Unsigned8 0 0-3
Prm_Text_Ref = 172
EndExtUserPrmData

ExtUserPrmData = 201 "15 Star-Delta Changeover Mode"
Unsigned8 1 0-1
Prm_Text_Ref = 168
EndExtUserPrmData
ExtUserPrmData = 203 "03 Set Current 2=10mA*"
Unsigned32 50 24-320000
EndExtUserPrmData
ExtUserPrmData = 204 "21 DI2 Multi Function Input"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 205 "26 Address Check"
Unsigned8 0 0-1
Prm_Text_Ref = 166
EndExtUserPrmData
ExtUserPrmData = 206 "25 Number of Trips"
Unsigned8 0 0-255
EndExtUserPrmData
ExtUserPrmData = 207 "07 DI1 Multi Function Input"
Unsigned8 0 0-255
EndExtUserPrmData
ExtUserPrmData = 208 "27 Emergency by PLC"
Unsigned8 0 0-1
Prm_Text_Ref = 166
EndExtUserPrmData

;
;=============================================================
; Text-definition for User Prm Data  "UMC22_FBP (V4.00)"
; only changes compared to "UMC22_FBP (V3.40)"
;=============================================================
;
PrmText = 173
Text(0)   = "Off"
Text(1)   = "On"
Text(2)   = "002"
Text(3)   = "003"
Text(4)   = "004"
Text(5)   = "005"
Text(6)   = "006"
Text(7)   = "007"
Text(8)   = "008"
Text(9)   = "009"
EndPrmText
;
ExtUserPrmData = 210 "22 Local Control" 
Unsigned8 0 0-9
Prm_Text_Ref = 173
EndExtUserPrmData
;
ExtUserPrmData = 211 "02 Current Factor (%)" 
Unsigned16 100 2-64000
EndExtUserPrmData


;=============================================================
; Text-definition for User Prm Data "MFI21-FBP"
;=============================================================
;
PrmText=50
Text(0)= "No Configuration"
Text(1)= "Direct, FB=Off"
Text(2)= "Direct, FB=On"
Text(3)= "Reverse, FB=Off"
Text(4)= "Reverse, FB=On"
Text(5)= "Star-Delta, FB=Off"
Text(6)= "Star-Delta, FB=On"
Text(7)= "MFI Transparent"
EndPrmText

ExtUserPrmData=50	"MFI Mode"			; MFI application mode
Unsigned8 0 0-7								; Default 0, range 0..7
Prm_Text_Ref=50								; Reference to PrmText 50
EndExtUserPrmData

ExtUserPrmData=51   "Start-Delta Time = 1ms*"	; MFI delay time in ms
Unsigned32 50 50-260100		   	; Default 50 ms, range 50..260100 ms
EndExtUserPrmData


;=============================================================
; Text-definition for User Prm Data "Softstarter PST(V01)"
; Compatible with CU-version 01.00.00 and 01.01.00.
;=============================================================
;
PrmText = 1008
Text(0)   = "Disable"
Text(1)   = "Enable"
EndPrmText
PrmText = 1011
Text(0)   = "1-30s"
Text(1)   = "1-120s"
EndPrmText
PrmText = 1012
Text(0)   = "0-30s"
Text(1)   = "0-120s"
EndPrmText
PrmText = 1013
Text(0)   = "No"
Text(1)   = "Normal"
Text(2)   = "Dual"
EndPrmText
PrmText = 1014
Text(0)   = "Class 5"
Text(1)  = "Class 10"
Text(2)  = "Class 20"
Text(3)  = "Class 30"
EndPrmText
PrmText = 1017
Text(0)   = "Stop-M"
Text(1)   = "Stop-A"
Text(2)   = "Ind"
EndPrmText
PrmText = 1036
Text(0)   = "Stop-M"
Text(1)   = "Stop-A"
EndPrmText
PrmText = 1049
Text(0)  = "None"
Text(1)  = "Reset"
Text(2)  = "Enable"
Text(3)  = "Jog"
Text(4)  = "DOL-On"
Text(5)  = "Start2"
EndPrmText
PrmText = 1050
Text(0)  = "None"
Text(1)  = "Reset"
Text(2)  = "Enable"
Text(3)  = "Jog"
Text(4)  = "DOL-On"
Text(5)  = "Start3"
EndPrmText
PrmText = 1051
Text(0)   = "Run"
Text(1)   = "TOR"
Text(2)   = "Event"
EndPrmText
PrmText = 1060
Text(0)   = "AS-I"
Text(1)   = "Other"
EndPrmText
PrmText = 1062
Text(0)   = "No"
Text(1)   = "2"
Text(2)   = "3"
EndPrmText
PrmText = 1075
Text(0)  = "US/UK"
Text(1)  = "FI"
Text(2)  = "SE"
Text(3)  = "PT"
Text(4)  = "NL"
Text(5)  = "IT"
Text(6)  = "FR"
Text(7)  = "ES"
Text(8)  = "DE"
Text(9)  = "CN"
EndPrmText
PrmText = 1079
Text(0)   = "ISO"
Text(1)   = "CE"
Text(2)   = "US"
EndPrmText

ExtUserPrmData = 1001 "Setting Ie = 0.1A *"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 1002 "Start Ramp [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 1003 "Stop Ramp  [s]"
Unsigned16 0 0-120
EndExtUserPrmData

ExtUserPrmData = 1004 "Init Volt  [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 1005 "End Volt   [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 1006 "Step Down  [%]"
Unsigned16 100 30-100
EndExtUserPrmData

ExtUserPrmData = 1007 "Current Lim = 0.1 * Ie *"
Unsigned16 40 20-50
EndExtUserPrmData

ExtUserPrmData = 1008 "Kick Start"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData = 1009 "Kick Level  [%]"
Unsigned16 50 50-100
EndExtUserPrmData

ExtUserPrmData = 1010 "Kick Time = 0.01s *"
Unsigned16 20 10-150
EndExtUserPrmData

ExtUserPrmData = 1011 "Start Range"
Unsigned16 0 0-1
Prm_Text_Ref=1011
EndExtUserPrmData

ExtUserPrmData = 1012 "Stop Range"
Unsigned16 0 0-1
Prm_Text_Ref=1012
EndExtUserPrmData

ExtUserPrmData = 1013 "Overload"
Unsigned16 1 0-2
Prm_Text_Ref=1013
EndExtUserPrmData

ExtUserPrmData = 1014 "OL Class"
Unsigned16 1 0-3
Prm_Text_Ref=1014
EndExtUserPrmData

ExtUserPrmData= 1015 "OL Class S"
Unsigned16 1 0-3
Prm_Text_Ref=1014
EndExtUserPrmData

ExtUserPrmData= 1016 "OL Class R"
Unsigned16 1 0-3
Prm_Text_Ref=1014
EndExtUserPrmData

ExtUserPrmData= 1017 "OL Op"
Unsigned16 0 0-2
Prm_Text_Ref=1017
EndExtUserPrmData

ExtUserPrmData= 1018 "Locked Rotor"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData= 1019 "Lock R Lev = 0.1 * Ie *"
Unsigned16 40 30-80
EndExtUserPrmData

ExtUserPrmData= 1020 "Lock R Time = 0.1s *"
Unsigned16 10 2-100
EndExtUserPrmData

ExtUserPrmData= 1021 "Lock R Op"
Unsigned16 0 0-2
Prm_Text_Ref=1017
EndExtUserPrmData

ExtUserPrmData= 1022 "Underload"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData= 1023 "Underl Lev = 0.1 * Ie *"
Unsigned16 8 4-8
EndExtUserPrmData

ExtUserPrmData= 1024 "Underl Time  [s]"
Unsigned16 10 1-30
EndExtUserPrmData

ExtUserPrmData=1025 "Underl Op"
Unsigned16 0 0-2
Prm_Text_Ref=1017
EndExtUserPrmData

ExtUserPrmData = 1026 "Phase Imb"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData= 1027 "Ph Imb Lev [%]"
Unsigned16 80 10-80
EndExtUserPrmData

ExtUserPrmData= 1028 "Ph Imb Op"
Unsigned16 0 0-2
Prm_Text_Ref=1017
EndExtUserPrmData

ExtUserPrmData = 1029 "High I"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData=1030 "High I Op"
Unsigned16 0 0-2
Prm_Text_Ref=1017
EndExtUserPrmData

ExtUserPrmData = 1031 "Phase Rev"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData=1032 "Ph Rev Op"
Unsigned16 0 0-2
Prm_Text_Ref=1017
EndExtUserPrmData

ExtUserPrmData = 1033 "PTC"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData=1034 "PTC Op"
Unsigned16 0 0-2
Prm_Text_Ref=1017
EndExtUserPrmData

ExtUserPrmData=1035 "Ext ByPass"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData
;36
ExtUserPrmData=1036 "BP Fault Op"
Unsigned16 0 0-2
Prm_Text_Ref=1036
EndExtUserPrmData

ExtUserPrmData = 1037 "Warn I=High"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData=1038 "Wa I=H Lev = 0.1* Ie *"
Unsigned16 12 5-50
EndExtUserPrmData

ExtUserPrmData = 1039 "Warn I=Low"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData= 1040 "Wa I=L Lev = 0.1 * Ie *"
Unsigned16 5 4-10
EndExtUserPrmData

ExtUserPrmData = 1041 "Warn OL"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData= 1042 "Wa OL Lev   [%]"
Unsigned16 90 40-99
EndExtUserPrmData

ExtUserPrmData = 1043 "Warn SCR OL"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData= 1044 "Ph Loss Op"
Unsigned16 0 0-1
Prm_Text_Ref=1036
EndExtUserPrmData

ExtUserPrmData= 1045 "FB Fault Op"
Unsigned16 0 0-1
Prm_Text_Ref=1036
EndExtUserPrmData

ExtUserPrmData= 1046 "Freq F Op"
Unsigned16 0 0-1
Prm_Text_Ref=1036
EndExtUserPrmData

ExtUserPrmData=1047 "Overtemp Op"
Unsigned16 0 0-1
Prm_Text_Ref=1036
EndExtUserPrmData

ExtUserPrmData=1048 "SCR SC Op"
Unsigned16 0 0-1
Prm_Text_Ref=1036
EndExtUserPrmData

ExtUserPrmData = 1049 "In0 - Read only"
Unsigned16 0 0-5
Prm_Text_Ref=1049
EndExtUserPrmData

ExtUserPrmData = 1050 "In1 - Read only"
Unsigned16 0 0-5
Prm_Text_Ref=1050
EndExtUserPrmData

ExtUserPrmData= 1051 "Relay K4"
Unsigned16 0 0-2
Prm_Text_Ref=1051
EndExtUserPrmData

ExtUserPrmData= 1052 "Relay K5"
Unsigned16 1 0-2
Prm_Text_Ref=1051
EndExtUserPrmData

ExtUserPrmData= 1053 "Relay K6"
Unsigned16 2 0-2
Prm_Text_Ref=1051
EndExtUserPrmData

ExtUserPrmData = 1054 "SW Outp V7"
Unsigned16 2 0-2
Prm_Text_Ref=1051
EndExtUserPrmData

ExtUserPrmData= 1055 "Event K4"
Unsigned16 0 0-65535
EndExtUserPrmData
;57
ExtUserPrmData= 1056 "Event K5"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData= 1057 "Event K6"
Unsigned16 7 0-65535
EndExtUserPrmData

ExtUserPrmData= 1058 "Event V7"
Unsigned16 7 0-65535
EndExtUserPrmData

ExtUserPrmData = 1059 "Fieldb Ctrl - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData = 1060 "Fieldb Type - Read only"
Unsigned16 1 0-1
Prm_Text_Ref=1060
EndExtUserPrmData

ExtUserPrmData = 1061 "Fieldb Addr - Read only"
Unsigned16 0 0-1000
EndExtUserPrmData

ExtUserPrmData = 1062 "No of Seq"
Unsigned16 0 0-2
Prm_Text_Ref=1062
EndExtUserPrmData

ExtUserPrmData= 1063 "StartRamp1 [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData= 1064 "Init Volt1 [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData= 1065 "Curr Lim1 = 0.1 * Ie *"
Unsigned16 40 20-50
EndExtUserPrmData

ExtUserPrmData= 1066 "1st Set Ie = 0.1A *"
Unsigned16 1000 0-10000
EndExtUserPrmData

ExtUserPrmData= 1067 "StartRamp2   [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData= 1068 "Init Volt2[%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData= 1069 "Curr Lim2 = 0.1 * Ie *"
Unsigned16 40 20-50
EndExtUserPrmData

ExtUserPrmData= 1070 "2nd Set Ie = 0.1A *"
Unsigned16 1000 0-10000
EndExtUserPrmData

ExtUserPrmData= 1071 "StartRamp3   [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData= 1072 "Init Volt3[%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData= 1073 "Curr Lim3 = 0.1 * Ie *"
Unsigned16 40 20-50
EndExtUserPrmData

ExtUserPrmData= 1074 "3rd Set Ie = 0.1A *"
Unsigned16 1000 0-10000
EndExtUserPrmData

ExtUserPrmData = 1075 "Language - Read only"
Unsigned16 0 0-9
Prm_Text_Ref=1075
EndExtUserPrmData

ExtUserPrmData = 1076 "Dummy76 - Read only"
Unsigned16 0 0-0
EndExtUserPrmData

ExtUserPrmData = 1077 "LCD Auto Off - Read only [min]"
Unsigned16 15 1-255
EndExtUserPrmData

ExtUserPrmData = 1078 "Password - Read only"
Unsigned16 0 0-255
EndExtUserPrmData

ExtUserPrmData = 1079 "Date Type - Read only"
Unsigned16 0 0-2
Prm_Text_Ref=1079
EndExtUserPrmData

ExtUserPrmData = 1080 "Date Year - Read only"
Unsigned16 2003 2001-2060
EndExtUserPrmData

ExtUserPrmData = 1081 "Date Month - Read only"
Unsigned16 6 1-12
EndExtUserPrmData

ExtUserPrmData = 1082 "Date Day - Read only"
Unsigned16 15 1-31
EndExtUserPrmData

ExtUserPrmData = 1083 "Time Hour - Read only"
Unsigned16 12 0-23
EndExtUserPrmData

ExtUserPrmData = 1084 "Time Min - Read only"
Unsigned16 30 0-59
EndExtUserPrmData

ExtUserPrmData = 1085 "S Port Ctrl - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData = 1086 "S Port Addr1 - Read only"
Unsigned16 123 0-255
EndExtUserPrmData

ExtUserPrmData = 1087 "S Port Addr2 - Read only"
Unsigned16 123 0-255
EndExtUserPrmData

ExtUserPrmData = 1088 "S Port Addr3 - Read only"
Unsigned16 123 0-255
EndExtUserPrmData

ExtUserPrmData = 1089 "S Port Addr4 - Read only"
Unsigned16 123 0-255
EndExtUserPrmData

ExtUserPrmData = 1090 "CT Ratio Ir [A] - Read only"
Unsigned16 0 0-2500
EndExtUserPrmData

ExtUserPrmData = 1091 "IntByPass - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData = 1092 "ByPass AC3 [A] - Read only"
Unsigned16 0 0-2500
EndExtUserPrmData

ExtUserPrmData = 1093 "SOP1= 0.01*  - Read only"
Unsigned16 100 70-120
EndExtUserPrmData

ExtUserPrmData = 1094 "SOP2= 0.01*  - Read only"
Unsigned16 100 5-2000
EndExtUserPrmData

ExtUserPrmData = 1095 "SOP3= 0.001*  - Read only"
Unsigned16 100 11-1200
EndExtUserPrmData

ExtUserPrmData = 1096 "SOP4= 0.1*  - Read only"
Unsigned16 100 10-200
EndExtUserPrmData
;
;=============================================================
; Text-definition for User Prm Data "Softstarter PST(V02)"
; Compatible with CU-version 02.00.01 and 02.01.00.
;=============================================================
;
PrmText = 1108
Text(0)   = "No"
Text(1)   = "Yes"
EndPrmText
PrmText = 1111
Text(0)   = "1-30s"
Text(1)   = "1-120s"
EndPrmText
PrmText = 1112
Text(0)   = "0-30s"
Text(1)   = "0-120s"
EndPrmText
PrmText = 1113
Text(0)   = "No"
Text(1)   = "Normal"
Text(2)   = "Dual"
EndPrmText
PrmText = 1114
Text(0)  = "Class 10A"
Text(1)  = "Class 10"
Text(2)  = "Class 20"
Text(3)  = "Class 30"
EndPrmText
PrmText = 1117
Text(0)   = "Stop-M"
Text(1)   = "Stop-A"
Text(2)   = "Ind"
EndPrmText
PrmText = 1136
Text(0)   = "Stop-M"
Text(1)   = "Stop-A"
EndPrmText
PrmText = 1149
Text(0)  = "None"
Text(1)  = "Reset"
Text(2)  = "Enable"
Text(3)  = "Jog"
Text(4)  = "DOL-On"
Text(5)  = "Start2"
Text(6)  = "FB-Dis"
EndPrmText
PrmText = 1150
Text(0)  = "None"
Text(1)  = "Reset"
Text(2)  = "Enable"
Text(3)  = "Jog"
Text(4)  = "DOL-On"
Text(5)  = "Start3"
Text(6)  = "FB-Dis"
EndPrmText
PrmText = 1151
Text(0)   = "Run"
Text(1)   = "TOR"
Text(2)   = "Event"
EndPrmText
PrmText = 1160
Text(0)   = "AS-Int"
Text(1)   = "Other"
EndPrmText
PrmText = 1162
Text(1)   = "No"
Text(2)   = "2"
Text(3)   = "3"
EndPrmText
PrmText = 1175
Text(1)  = "US/UK"
Text(2)  = "FI"
Text(3)  = "SE"
Text(4)  = "PT"
Text(5)  = "NL"
Text(6)  = "IT"
Text(7)  = "FR"
Text(8)  = "ES"
Text(9)  = "DE"
Text(10)  = "CN"
Text(11)  = "RU"
EndPrmText
PrmText = 1179
Text(0)   = "ISO"
Text(1)   = "CE"
Text(2)   = "US"
EndPrmText

ExtUserPrmData = 1101 "Setting Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 1102 "Start Ramp [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 1103 "Stop Ramp  [s]"
Unsigned16 0 0-120
EndExtUserPrmData

ExtUserPrmData = 1104 "Init Volt  [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 1105 "End Volt   [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 1106 "Step Down  [%]"
Unsigned16 100 30-100
EndExtUserPrmData

ExtUserPrmData = 1107 "Current Lim [0.1*Ie]"
Unsigned16 40 20-50
EndExtUserPrmData

ExtUserPrmData = 1108 "Kick Start"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData = 1109 "Kick Level  [%]"
Unsigned16 50 50-100
EndExtUserPrmData

ExtUserPrmData = 1110 "Kick Time [0.01s]"
Unsigned16 20 10-150
EndExtUserPrmData

ExtUserPrmData = 1111 "Start Range"
Unsigned16 0 0-1
Prm_Text_Ref=1111
EndExtUserPrmData

ExtUserPrmData = 1112 "Stop Range"
Unsigned16 0 0-1
Prm_Text_Ref=1112
EndExtUserPrmData

ExtUserPrmData = 1113 "Overload"
Unsigned16 1 0-2
Prm_Text_Ref=1113
EndExtUserPrmData

ExtUserPrmData = 1114 "OL Class"
Unsigned16 1 0-3
Prm_Text_Ref=1114
EndExtUserPrmData

ExtUserPrmData= 1115 "OL Class S"
Unsigned16 1 0-3
Prm_Text_Ref=1114
EndExtUserPrmData

ExtUserPrmData= 1116 "OL Class R"
Unsigned16 1 0-3
Prm_Text_Ref=1114
EndExtUserPrmData

ExtUserPrmData= 1117 "OL Op"
Unsigned16 0 0-2
Prm_Text_Ref=1117
EndExtUserPrmData

ExtUserPrmData= 1118 "Locked Rotor"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData= 1119 "Lock R Lev [0.1*Ie]"
Unsigned16 40 30-80
EndExtUserPrmData

ExtUserPrmData= 1120 "Lock R Time [0.1s]"
Unsigned16 10 2-100
EndExtUserPrmData

ExtUserPrmData= 1121 "Lock R Op"
Unsigned16 0 0-2
Prm_Text_Ref=1117
EndExtUserPrmData

ExtUserPrmData= 1122 "Underload"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData= 1123 "Underl Lev [0.1*Ie]"
Unsigned16 8 4-8
EndExtUserPrmData

ExtUserPrmData= 1124 "Underl Time [s]"
Unsigned16 10 1-30
EndExtUserPrmData

ExtUserPrmData=1125 "Underl Op"
Unsigned16 0 0-2
Prm_Text_Ref=1117
EndExtUserPrmData

ExtUserPrmData = 1126 "Phase Imb"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData= 1127 "Ph Imb Lev [%]"
Unsigned16 80 10-80
EndExtUserPrmData

ExtUserPrmData= 1128 "Ph Imb Op"
Unsigned16 0 0-2
Prm_Text_Ref=1117
EndExtUserPrmData

ExtUserPrmData = 1129 "High I"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData=1130 "High I Op"
Unsigned16 0 0-2
Prm_Text_Ref=1117
EndExtUserPrmData

ExtUserPrmData = 1131 "Phase Rev"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData=1132 "Ph Rev Op"
Unsigned16 0 0-2
Prm_Text_Ref=1117
EndExtUserPrmData

ExtUserPrmData = 1133 "PTC"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData=1134 "PTC Op"
Unsigned16 0 0-2
Prm_Text_Ref=1117
EndExtUserPrmData

ExtUserPrmData=1135 "Ext ByPass"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData
;36
ExtUserPrmData=1136 "BP Fault Op"
Unsigned16 0 0-1
Prm_Text_Ref=1136
EndExtUserPrmData

ExtUserPrmData = 1137 "Warn I=High"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData=1138 "Wa I=H Lev [0.1*Ie]"
Unsigned16 12 5-50
EndExtUserPrmData

ExtUserPrmData = 1139 "Warn I=Low"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData= 1140 "Wa I=L Lev [0.1*Ie]"
Unsigned16 5 4-10
EndExtUserPrmData

ExtUserPrmData = 1141 "Warn OL"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData= 1142 "Wa OL Lev  [%]"
Unsigned16 90 40-99
EndExtUserPrmData

ExtUserPrmData = 1143 "Warn SCR OL"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData= 1144 "Ph Loss Op"
Unsigned16 0 0-1
Prm_Text_Ref=1136
EndExtUserPrmData

ExtUserPrmData= 1145 "FB Fault Op"
Unsigned16 0 0-1
Prm_Text_Ref=1136
EndExtUserPrmData

ExtUserPrmData= 1146 "Freq F Op"
Unsigned16 0 0-1
Prm_Text_Ref=1136
EndExtUserPrmData

ExtUserPrmData=1147 "HC Temp Op"
Unsigned16 0 0-1
Prm_Text_Ref=1136
EndExtUserPrmData

ExtUserPrmData=1148 "SCR SC Op"
Unsigned16 0 0-1
Prm_Text_Ref=1136
EndExtUserPrmData

ExtUserPrmData = 1149 "In0 - Read only"
Unsigned16 1 0-6
Prm_Text_Ref=1149
EndExtUserPrmData

ExtUserPrmData = 1150 "In1 - Read only"
Unsigned16 1 0-6
Prm_Text_Ref=1150
EndExtUserPrmData

ExtUserPrmData= 1151 "Relay K4"
Unsigned16 0 0-2
Prm_Text_Ref=1151
EndExtUserPrmData

ExtUserPrmData= 1152 "Relay K5"
Unsigned16 1 0-2
Prm_Text_Ref=1151
EndExtUserPrmData

ExtUserPrmData= 1153 "Relay K6"
Unsigned16 2 0-2
Prm_Text_Ref=1151
EndExtUserPrmData

ExtUserPrmData = 1154 "SW Outp V7"
Unsigned16 2 0-2
Prm_Text_Ref=1151
EndExtUserPrmData

ExtUserPrmData= 1155 "Event K4"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData= 1156 "Event K5"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData= 1157 "Event K6"
Unsigned16 7 0-65535
EndExtUserPrmData

ExtUserPrmData= 1158 "Event V7"
Unsigned16 7 0-65535
EndExtUserPrmData

ExtUserPrmData = 1159 "Fieldb Ctrl - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData = 1160 "Fieldb Type - Read only"
Unsigned16 1 0-1
Prm_Text_Ref=1160
EndExtUserPrmData

ExtUserPrmData = 1161 "Fieldb Addr - Read only"
Unsigned16 0 0-1000
EndExtUserPrmData

ExtUserPrmData = 1162 "No of Seq"
Unsigned16 1 1-3
Prm_Text_Ref=1162
EndExtUserPrmData

ExtUserPrmData= 1163 "StartRamp1 [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData= 1164 "Init Volt1 [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData= 1165 "Curr Lim1 [0.1*Ie]"
Unsigned16 40 20-70
EndExtUserPrmData

ExtUserPrmData= 1166 "1st Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData= 1167 "StartRamp2  [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData= 1168 "Init Volt2 [%]"
Unsigned16 30 30-70
EndExtUserPrmData
;75
ExtUserPrmData= 1169 "Curr Lim2 [0.1*Ie]"
Unsigned16 40 20-70
EndExtUserPrmData

ExtUserPrmData= 1170 "2nd Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData= 1171 "StartRamp3  [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData= 1172 "Init Volt3[%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData= 1173 "Curr Lim3 [0.1*Ie]"
Unsigned16 40 20-70
EndExtUserPrmData

ExtUserPrmData= 1174 "3rd Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 1175 "Language - Read only"
Unsigned16 1 1-11
Prm_Text_Ref=1175
EndExtUserPrmData

ExtUserPrmData = 1176 "Dummy76 - Read only"
Unsigned16 0 0-15
EndExtUserPrmData

ExtUserPrmData = 1177 "LCD Auto Off - Read only [min]"
Unsigned16 15 1-255
EndExtUserPrmData

ExtUserPrmData = 1178 "Password - Read only"
Unsigned16 0 0-255
EndExtUserPrmData

ExtUserPrmData = 1179 "Date Type - Read only"
Unsigned16 0 0-2
Prm_Text_Ref=1179
EndExtUserPrmData

ExtUserPrmData = 1180 "Date Year - Read only"
Unsigned16 2002 2001-2060
EndExtUserPrmData

ExtUserPrmData = 1181 "Date Month - Read only"
Unsigned16 6 1-12
EndExtUserPrmData

ExtUserPrmData = 1182 "Date Day - Read only"
Unsigned16 15 1-31
EndExtUserPrmData

ExtUserPrmData = 1183 "Time Hour - Read only"
Unsigned16 12 0-23
EndExtUserPrmData

ExtUserPrmData = 1184 "Time Min - Read only"
Unsigned16 30 0-59
EndExtUserPrmData

ExtUserPrmData = 1185 "S Port Ctrl - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData = 1186 "S Port Addr1 - Read only"
Unsigned16 192 0-255
EndExtUserPrmData

ExtUserPrmData = 1187 "S Port Addr2 - Read only"
Unsigned16 168 0-255
EndExtUserPrmData

ExtUserPrmData = 1188 "S Port Addr3 - Read only"
Unsigned16 0 0-255
EndExtUserPrmData

ExtUserPrmData = 1189 "S Port Addr4 - Read only"
Unsigned16 2 0-255
EndExtUserPrmData

ExtUserPrmData = 1190 "CT Ratio Ir [A] - Read only"
Unsigned16 100 1-2500
EndExtUserPrmData

ExtUserPrmData = 1191 "IntByPass - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData = 1192 "ByPass AC3 [A] - Read only"
Unsigned16 0 0-2500
EndExtUserPrmData

ExtUserPrmData = 1193 "SOP1 [0.01] - Read only"
Unsigned16 95 70-120
EndExtUserPrmData

ExtUserPrmData = 1194 "SOP2 [0.01] - Read only"
Unsigned16 1000 5-2000
EndExtUserPrmData

ExtUserPrmData = 1195 "SOP3 [0.001] - Read only"
Unsigned16 600 11-1200
EndExtUserPrmData

ExtUserPrmData = 1196 "SOP4 [0.1] - Read only"
Unsigned16 40 10-200
EndExtUserPrmData
;
;=============================================================
; Text-definition for User Prm Data "Softstarter PST(V03)"
; Compatible with CU-version 03.03.02.
;=============================================================
;
PrmText = 1208
Text(0)   = "No"
Text(1)   = "Yes"
EndPrmText
PrmText = 1211
Text(0)   = "1-30s"
Text(1)   = "1-120s"
EndPrmText
PrmText = 1212
Text(0)   = "0-30s"
Text(1)   = "0-120s"
EndPrmText
PrmText = 1213
Text(0)   = "No"
Text(1)   = "Normal"
Text(2)   = "Dual"
EndPrmText
PrmText = 1214
Text(0)  = "Class 10A"
Text(1)  = "Class 10"
Text(2)  = "Class 20"
Text(3)  = "Class 30"
EndPrmText
PrmText = 1217
Text(0)   = "Stop-M"
Text(1)   = "Stop-A"
Text(2)   = "Ind"
EndPrmText
PrmText = 1236
Text(0)   = "Stop-M"
Text(1)   = "Stop-A"
EndPrmText
PrmText = 1249
Text(0)  = "None"
Text(1)  = "Reset"
Text(2)  = "Enable"
Text(3)  = "Jog"
Text(4)  = "DOL-On"
Text(5)  = "Start2"
Text(6)  = "FB-Dis"
EndPrmText
PrmText = 1250
Text(0)  = "None"
Text(1)  = "Reset"
Text(2)  = "Enable"
Text(3)  = "Jog"
Text(4)  = "DOL-On"
Text(5)  = "Start3"
Text(6)  = "FB-Dis"
EndPrmText
PrmText = 1251
Text(0)   = "Run"
Text(1)   = "TOR"
Text(2)   = "Event"
EndPrmText
PrmText = 1260
Text(0)   = "AS-Int"
Text(1)   = "Other"
EndPrmText
PrmText = 1262
Text(1)   = "No"
Text(2)   = "2"
Text(3)   = "3"
EndPrmText
PrmText = 1275
Text(1)  = "US/UK"
Text(2)  = "FI"
Text(3)  = "SE"
Text(4)  = "PT"
Text(5)  = "NL"
Text(6)  = "IT"
Text(7)  = "FR"
Text(8)  = "ES"
Text(9)  = "DE"
Text(10)  = "CN"
Text(11)  = "RU"
Text(12)  = "TR"
EndPrmText
PrmText = 1279
Text(0)   = "ISO"
Text(1)   = "CE"
Text(2)   = "US"
EndPrmText

ExtUserPrmData = 1201 "Setting Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 1202 "Start Ramp [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 1203 "Stop Ramp  [s]"
Unsigned16 0 0-120
EndExtUserPrmData

ExtUserPrmData = 1204 "Init Volt  [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 1205 "End Volt   [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 1206 "Step Down  [%]"
Unsigned16 100 30-100
EndExtUserPrmData

ExtUserPrmData = 1207 "Current Lim [0.1*Ie]"
Unsigned16 40 20-70
EndExtUserPrmData

ExtUserPrmData = 1208 "Kick Start"
Unsigned16 0 0-1
Prm_Text_Ref=1208
EndExtUserPrmData

ExtUserPrmData = 1209 "Kick Level  [%]"
Unsigned16 50 50-100
EndExtUserPrmData

ExtUserPrmData = 1210 "Kick Time [0.01s]"
Unsigned16 20 10-150
EndExtUserPrmData

ExtUserPrmData = 1211 "Start Range"
Unsigned16 0 0-1
Prm_Text_Ref=1211
EndExtUserPrmData

ExtUserPrmData = 1212 "Stop Range"
Unsigned16 0 0-1
Prm_Text_Ref=1212
EndExtUserPrmData

ExtUserPrmData = 1213 "Overload"
Unsigned16 1 0-2
Prm_Text_Ref=1213
EndExtUserPrmData

ExtUserPrmData = 1214 "OL Class"
Unsigned16 1 0-3
Prm_Text_Ref=1214
EndExtUserPrmData

ExtUserPrmData= 1215 "OL Class S"
Unsigned16 1 0-3
Prm_Text_Ref=1214
EndExtUserPrmData

ExtUserPrmData= 1216 "OL Class R"
Unsigned16 1 0-3
Prm_Text_Ref=1214
EndExtUserPrmData

ExtUserPrmData= 1217 "OL Op"
Unsigned16 0 0-2
Prm_Text_Ref=1217
EndExtUserPrmData

ExtUserPrmData= 1218 "Locked Rotor"
Unsigned16 0 0-1
Prm_Text_Ref=1208
EndExtUserPrmData

ExtUserPrmData= 1219 "Lock R Lev [0.1*Ie]"
Unsigned16 40 5-80
EndExtUserPrmData

ExtUserPrmData= 1220 "Lock R Time [0.1s]"
Unsigned16 10 2-100
EndExtUserPrmData

ExtUserPrmData= 1221 "Lock R Op"
Unsigned16 0 0-2
Prm_Text_Ref=1217
EndExtUserPrmData

ExtUserPrmData= 1222 "Underload"
Unsigned16 0 0-1
Prm_Text_Ref=1208
EndExtUserPrmData

ExtUserPrmData= 1223 "Underl Lev [0.1*Ie]"
Unsigned16 5 4-8
EndExtUserPrmData

ExtUserPrmData= 1224 "Underl Time [s]"
Unsigned16 10 1-30
EndExtUserPrmData

ExtUserPrmData=1225 "Underl Op"
Unsigned16 0 0-2
Prm_Text_Ref=1217
EndExtUserPrmData

ExtUserPrmData = 1226 "Phase Imb"
Unsigned16 0 0-1
Prm_Text_Ref=1208
EndExtUserPrmData

ExtUserPrmData= 1227 "Ph Imb Lev [%]"
Unsigned16 80 10-80
EndExtUserPrmData

ExtUserPrmData= 1228 "Ph Imb Op"
Unsigned16 0 0-2
Prm_Text_Ref=1217
EndExtUserPrmData

ExtUserPrmData = 1229 "High I"
Unsigned16 0 0-1
Prm_Text_Ref=1208
EndExtUserPrmData

ExtUserPrmData=1230 "High I Op"
Unsigned16 0 0-2
Prm_Text_Ref=1217
EndExtUserPrmData

ExtUserPrmData = 1231 "Phase Rev"
Unsigned16 0 0-1
Prm_Text_Ref=1208
EndExtUserPrmData

ExtUserPrmData=1232 "Ph Rev Op"
Unsigned16 0 0-2
Prm_Text_Ref=1217
EndExtUserPrmData

ExtUserPrmData = 1233 "PTC"
Unsigned16 0 0-1
Prm_Text_Ref=1208
EndExtUserPrmData

ExtUserPrmData=1234 "PTC Op"
Unsigned16 0 0-2
Prm_Text_Ref=1217
EndExtUserPrmData

ExtUserPrmData=1235 "Ext ByPass"
Unsigned16 0 0-1
Prm_Text_Ref=1208
EndExtUserPrmData
;36
ExtUserPrmData=1236 "Dummy36 - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1236
EndExtUserPrmData

ExtUserPrmData = 1237 "Warn I=High"
Unsigned16 0 0-1
Prm_Text_Ref=1208
EndExtUserPrmData

ExtUserPrmData=1238 "Wa I=H Lev [0.1*Ie]"
Unsigned16 12 5-50
EndExtUserPrmData

ExtUserPrmData = 1239 "Warn I=Low"
Unsigned16 0 0-1
Prm_Text_Ref=1208
EndExtUserPrmData

ExtUserPrmData= 1240 "Wa I=L Lev [0.1*Ie]"
Unsigned16 5 4-10
EndExtUserPrmData

ExtUserPrmData = 1241 "Warn OL"
Unsigned16 0 0-1
Prm_Text_Ref=1208
EndExtUserPrmData

ExtUserPrmData= 1242 "Wa OL Lev  [%]"
Unsigned16 90 40-99
EndExtUserPrmData

ExtUserPrmData = 1243 "Warn SCR OL"
Unsigned16 0 0-1
Prm_Text_Ref=1208
EndExtUserPrmData

ExtUserPrmData= 1244 "Ph Loss Op"
Unsigned16 0 0-1
Prm_Text_Ref=1236
EndExtUserPrmData

ExtUserPrmData= 1245 "FB Fault Op"
Unsigned16 0 0-1
Prm_Text_Ref=1236
EndExtUserPrmData

ExtUserPrmData= 1246 "Freq F Op"
Unsigned16 0 0-1
Prm_Text_Ref=1236
EndExtUserPrmData

ExtUserPrmData=1247 "HC Temp Op"
Unsigned16 0 0-1
Prm_Text_Ref=1236
EndExtUserPrmData

ExtUserPrmData=1248 "SCR SC Op"
Unsigned16 0 0-1
Prm_Text_Ref=1236
EndExtUserPrmData

ExtUserPrmData = 1249 "In0 - Read only"
Unsigned16 1 0-6
Prm_Text_Ref=1249
EndExtUserPrmData

ExtUserPrmData = 1250 "In1 - Read only"
Unsigned16 1 0-6
Prm_Text_Ref=1250
EndExtUserPrmData

ExtUserPrmData= 1251 "Relay K4"
Unsigned16 0 0-2
Prm_Text_Ref=1251
EndExtUserPrmData

ExtUserPrmData= 1252 "Relay K5"
Unsigned16 1 0-2
Prm_Text_Ref=1251
EndExtUserPrmData

ExtUserPrmData= 1253 "Relay K6"
Unsigned16 2 0-2
Prm_Text_Ref=1251
EndExtUserPrmData

ExtUserPrmData = 1254 "SW Outp V7"
Unsigned16 2 0-2
Prm_Text_Ref=1251
EndExtUserPrmData

ExtUserPrmData= 1255 "Event K4"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData= 1256 "Event K5"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData= 1257 "Event K6"
Unsigned16 7 0-65535
EndExtUserPrmData

ExtUserPrmData= 1258 "Event V7"
Unsigned16 7 0-65535
EndExtUserPrmData

ExtUserPrmData = 1259 "Fieldb Ctrl - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1208
EndExtUserPrmData

ExtUserPrmData = 1260 "Fieldb Type - Read only"
Unsigned16 1 0-1
Prm_Text_Ref=1260
EndExtUserPrmData

ExtUserPrmData = 1261 "Fieldb Addr - Read only"
Unsigned16 0 0-1000
EndExtUserPrmData

ExtUserPrmData = 1262 "No of Seq"
Unsigned16 1 1-3
Prm_Text_Ref=1262
EndExtUserPrmData

ExtUserPrmData= 1263 "StartRamp1 [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData= 1264 "Init Volt1 [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData= 1265 "Curr Lim1 [0.1*Ie]"
Unsigned16 40 20-70
EndExtUserPrmData

ExtUserPrmData= 1266 "1st Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData= 1267 "StartRamp2  [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData= 1268 "Init Volt2 [%]"
Unsigned16 30 30-70
EndExtUserPrmData
;75
ExtUserPrmData= 1269 "Curr Lim2 [0.1*Ie]"
Unsigned16 40 20-70
EndExtUserPrmData

ExtUserPrmData= 1270 "2nd Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData= 1271 "StartRamp3  [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData= 1272 "Init Volt3[%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData= 1273 "Curr Lim3 [0.1*Ie]"
Unsigned16 40 20-70
EndExtUserPrmData

ExtUserPrmData= 1274 "3rd Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 1275 "Language - Read only"
Unsigned16 1 1-12
Prm_Text_Ref=1275
EndExtUserPrmData

ExtUserPrmData = 1276 "Dummy76 - Read only"
Unsigned16 0 0-15
EndExtUserPrmData

ExtUserPrmData = 1277 "LCD Auto Off - Read only [min]"
Unsigned16 15 1-255
EndExtUserPrmData

ExtUserPrmData = 1278 "Password - Read only"
Unsigned16 0 0-255
EndExtUserPrmData

ExtUserPrmData = 1279 "Date Type - Read only"
Unsigned16 0 0-2
Prm_Text_Ref=1279
EndExtUserPrmData

ExtUserPrmData = 1280 "Date Year - Read only"
Unsigned16 2002 2001-2060
EndExtUserPrmData

ExtUserPrmData = 1281 "Date Month - Read only"
Unsigned16 6 1-12
EndExtUserPrmData

ExtUserPrmData = 1282 "Date Day - Read only"
Unsigned16 15 1-31
EndExtUserPrmData

ExtUserPrmData = 1283 "Time Hour - Read only"
Unsigned16 12 0-23
EndExtUserPrmData

ExtUserPrmData = 1284 "Time Min - Read only"
Unsigned16 30 0-59
EndExtUserPrmData

ExtUserPrmData = 1285 "S Port Ctrl - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1208
EndExtUserPrmData

ExtUserPrmData = 1286 "S Port Addr1 - Read only"
Unsigned16 192 0-255
EndExtUserPrmData

ExtUserPrmData = 1287 "S Port Addr2 - Read only"
Unsigned16 168 0-255
EndExtUserPrmData

ExtUserPrmData = 1288 "S Port Addr3 - Read only"
Unsigned16 0 0-255
EndExtUserPrmData

ExtUserPrmData = 1289 "S Port Addr4 - Read only"
Unsigned16 2 0-255
EndExtUserPrmData

ExtUserPrmData = 1290 "CT Ratio Ir [A] - Read only"
Unsigned16 100 1-2500
EndExtUserPrmData

ExtUserPrmData = 1291 "IntByPass - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1208
EndExtUserPrmData

ExtUserPrmData = 1292 "ByPass AC3 [A] - Read only"
Unsigned16 0 0-2500
EndExtUserPrmData

ExtUserPrmData = 1293 "SOP1 [0.01] - Read only"
Unsigned16 95 70-120
EndExtUserPrmData

ExtUserPrmData = 1294 "SOP2 [0.01] - Read only"
Unsigned16 1000 5-2000
EndExtUserPrmData

ExtUserPrmData = 1295 "SOP3 [0.001] - Read only"
Unsigned16 600 12-1200
EndExtUserPrmData

ExtUserPrmData = 1296 "SOP4 [0.1] - Read only"
Unsigned16 40 10-200
EndExtUserPrmData

ExtUserPrmData = 1297 "BP Close Op"
Unsigned16 0 0-1
Prm_Text_Ref=1236
EndExtUserPrmData

ExtUserPrmData = 1298 "BP Open Op"
Unsigned16 0 0-1
Prm_Text_Ref=1236
EndExtUserPrmData

ExtUserPrmData = 1299 "Dummy99 - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1208
EndExtUserPrmData

ExtUserPrmData = 1300 "FCODE1 - Read only"
Unsigned16 0 0-10
EndExtUserPrmData

ExtUserPrmData = 1301 "FCODE2 - Read only"
Unsigned16 0 0-10
EndExtUserPrmData

ExtUserPrmData = 1302 "FCODE3 - Read only"
Unsigned16 0 0-10
EndExtUserPrmData

ExtUserPrmData = 1303 "FCODE4 - Read only"
Unsigned16 0 0-10
EndExtUserPrmData

ExtUserPrmData = 1304 "FCODE5 - Read only"
Unsigned16 0 0-100
EndExtUserPrmData

ExtUserPrmData = 1305 "FCODE6 - Read only"
Unsigned16 0 0-100
EndExtUserPrmData

ExtUserPrmData = 1306 "PST(B) [A] - Read only"
Unsigned16 100 1-2500
EndExtUserPrmData

ExtUserPrmData = 1307 "FCODE7 - Read only"
Unsigned16 1 0-1
Prm_Text_Ref=1208
EndExtUserPrmData

ExtUserPrmData = 1308 "FCODE8 - Read only"
Unsigned16 1 0-1
Prm_Text_Ref=1208
EndExtUserPrmData

ExtUserPrmData = 1309 "FCODE9 - Read only"
Unsigned16 1 0-1
Prm_Text_Ref=1208
EndExtUserPrmData
;
;=============================================================
; Text-definition for User Prm Data "Softstarter PST(V04)"
; Compatible with CU-version 03.04.01 and 03.05.00 
; also used for CU-version 04.00.02
;=============================================================
;
PrmText = 1408
Text(0)   = "No"
Text(1)   = "Yes"
EndPrmText
PrmText = 1411
Text(0)   = "1-30s"
Text(1)   = "1-120s"
EndPrmText
PrmText = 1412
Text(0)   = "0-30s"
Text(1)   = "0-120s"
EndPrmText
PrmText = 1413
Text(0)   = "No"
Text(1)   = "Normal"
Text(2)   = "Dual"
EndPrmText
PrmText = 1414
Text(0)  = "Class 10A"
Text(1)  = "Class 10"
Text(2)  = "Class 20"
Text(3)  = "Class 30"
EndPrmText
PrmText = 1417
Text(0)   = "Stop-M"
Text(1)   = "Stop-A"
Text(2)   = "Ind"
EndPrmText
PrmText = 1436
Text(0)   = "Stop-M"
Text(1)   = "Stop-A"
EndPrmText
PrmText = 1449
Text(0)  = "None"
Text(1)  = "Reset"
Text(2)  = "Enable"
Text(3)  = "Jog"
Text(4)  = "DOL-On"
Text(5)  = "Start2"
Text(6)  = "FB-Dis"
EndPrmText
PrmText = 1450
Text(0)  = "None"
Text(1)  = "Reset"
Text(2)  = "Enable"
Text(3)  = "Jog"
Text(4)  = "DOL-On"
Text(5)  = "Start3"
Text(6)  = "FB-Dis"
EndPrmText
PrmText = 1451
Text(0)   = "Run"
Text(1)   = "TOR"
Text(2)   = "Event"
EndPrmText
PrmText = 1460
Text(0)   = "AS-Int"
Text(1)   = "Other"
EndPrmText
PrmText = 1462
Text(1)   = "No"
Text(2)   = "2"
Text(3)   = "3"
EndPrmText
PrmText = 1475
Text(1)  = "US/UK"
Text(2)  = "FI"
Text(3)  = "SE"
Text(4)  = "PT"
Text(5)  = "NL"
Text(6)  = "IT"
Text(7)  = "FR"
Text(8)  = "ES"
Text(9)  = "DE"
Text(10)  = "CN"
Text(11)  = "RU"
Text(12)  = "TR"
EndPrmText
PrmText = 1479
Text(0)   = "ISO"
Text(1)   = "CE"
Text(2)   = "US"
EndPrmText

ExtUserPrmData = 1401 "Setting Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 1402 "Start Ramp [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 1403 "Stop Ramp  [s]"
Unsigned16 0 0-120
EndExtUserPrmData

ExtUserPrmData = 1404 "Init Volt  [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 1405 "End Volt   [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 1406 "Step Down  [%]"
Unsigned16 100 30-100
EndExtUserPrmData

ExtUserPrmData = 1407 "Current Lim [0.1*Ie]"
Unsigned16 40 20-70
EndExtUserPrmData

ExtUserPrmData = 1408 "Kick Start"
Unsigned16 0 0-1
Prm_Text_Ref=1408
EndExtUserPrmData

ExtUserPrmData = 1409 "Kick Level  [%]"
Unsigned16 50 50-100
EndExtUserPrmData

ExtUserPrmData = 1410 "Kick Time [0.01s]"
Unsigned16 20 10-150
EndExtUserPrmData

ExtUserPrmData = 1411 "Start Range"
Unsigned16 0 0-1
Prm_Text_Ref=1411
EndExtUserPrmData

ExtUserPrmData = 1412 "Stop Range"
Unsigned16 0 0-1
Prm_Text_Ref=1412
EndExtUserPrmData

ExtUserPrmData = 1413 "Overload"
Unsigned16 1 0-2
Prm_Text_Ref=1413
EndExtUserPrmData

ExtUserPrmData = 1414 "OL Class"
Unsigned16 1 0-3
Prm_Text_Ref=1414
EndExtUserPrmData

ExtUserPrmData= 1415 "OL Class S"
Unsigned16 1 0-3
Prm_Text_Ref=1414
EndExtUserPrmData

ExtUserPrmData= 1416 "OL Class R"
Unsigned16 1 0-3
Prm_Text_Ref=1414
EndExtUserPrmData

ExtUserPrmData= 1417 "OL Op"
Unsigned16 0 0-2
Prm_Text_Ref=1417
EndExtUserPrmData

ExtUserPrmData= 1418 "Locked Rotor"
Unsigned16 0 0-1
Prm_Text_Ref=1408
EndExtUserPrmData

ExtUserPrmData= 1419 "Lock R Lev [0.1*Ie]"
Unsigned16 40 5-80
EndExtUserPrmData

ExtUserPrmData= 1420 "Lock R Time [0.1s]"
Unsigned16 10 2-100
EndExtUserPrmData

ExtUserPrmData= 1421 "Lock R Op"
Unsigned16 0 0-2
Prm_Text_Ref=1417
EndExtUserPrmData

ExtUserPrmData= 1422 "Underload"
Unsigned16 0 0-1
Prm_Text_Ref=1408
EndExtUserPrmData

ExtUserPrmData= 1423 "Underl Lev [0.1*Ie]"
Unsigned16 5 4-8
EndExtUserPrmData

ExtUserPrmData= 1424 "Underl Time [s]"
Unsigned16 10 1-30
EndExtUserPrmData

ExtUserPrmData=1425 "Underl Op"
Unsigned16 0 0-2
Prm_Text_Ref=1417
EndExtUserPrmData

ExtUserPrmData = 1426 "Phase Imb"
Unsigned16 0 0-1
Prm_Text_Ref=1408
EndExtUserPrmData

ExtUserPrmData= 1427 "Ph Imb Lev [%]"
Unsigned16 80 10-80
EndExtUserPrmData

ExtUserPrmData= 1428 "Ph Imb Op"
Unsigned16 0 0-2
Prm_Text_Ref=1417
EndExtUserPrmData

ExtUserPrmData = 1429 "High I"
Unsigned16 0 0-1
Prm_Text_Ref=1408
EndExtUserPrmData

ExtUserPrmData=1430 "High I Op"
Unsigned16 0 0-2
Prm_Text_Ref=1417
EndExtUserPrmData

ExtUserPrmData = 1431 "Phase Rev"
Unsigned16 0 0-1
Prm_Text_Ref=1408
EndExtUserPrmData

ExtUserPrmData=1432 "Ph Rev Op"
Unsigned16 0 0-2
Prm_Text_Ref=1417
EndExtUserPrmData

ExtUserPrmData = 1433 "PTC"
Unsigned16 0 0-1
Prm_Text_Ref=1408
EndExtUserPrmData

ExtUserPrmData=1434 "PTC Op"
Unsigned16 0 0-2
Prm_Text_Ref=1417
EndExtUserPrmData

ExtUserPrmData=1435 "Ext ByPass"
Unsigned16 0 0-1
Prm_Text_Ref=1408
EndExtUserPrmData
;36
ExtUserPrmData=1436 "Dummy36 - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1436
EndExtUserPrmData

ExtUserPrmData = 1437 "Warn I=High"
Unsigned16 0 0-1
Prm_Text_Ref=1408
EndExtUserPrmData

ExtUserPrmData=1438 "Wa I=H Lev [0.1*Ie]"
Unsigned16 14 5-50
EndExtUserPrmData

ExtUserPrmData = 1439 "Warn I=Low"
Unsigned16 0 0-1
Prm_Text_Ref=1408
EndExtUserPrmData

ExtUserPrmData= 1440 "Wa I=L Lev [0.1*Ie]"
Unsigned16 5 4-10
EndExtUserPrmData

ExtUserPrmData = 1441 "Warn OL"
Unsigned16 0 0-1
Prm_Text_Ref=1408
EndExtUserPrmData

ExtUserPrmData= 1442 "Wa OL Lev  [%]"
Unsigned16 90 40-99
EndExtUserPrmData

ExtUserPrmData = 1443 "Warn SCR OL"
Unsigned16 0 0-1
Prm_Text_Ref=1408
EndExtUserPrmData

ExtUserPrmData= 1444 "Ph Loss Op"
Unsigned16 0 0-1
Prm_Text_Ref=1436
EndExtUserPrmData

ExtUserPrmData= 1445 "FB Fault Op"
Unsigned16 0 0-1
Prm_Text_Ref=1436
EndExtUserPrmData

ExtUserPrmData= 1446 "Freq F Op"
Unsigned16 0 0-1
Prm_Text_Ref=1436
EndExtUserPrmData

ExtUserPrmData=1447 "HC Temp Op"
Unsigned16 0 0-1
Prm_Text_Ref=1436
EndExtUserPrmData

ExtUserPrmData=1448 "SCR SC Op"
Unsigned16 0 0-1
Prm_Text_Ref=1436
EndExtUserPrmData

ExtUserPrmData = 1449 "In0 - Read only"
Unsigned16 1 0-6
Prm_Text_Ref=1449
EndExtUserPrmData

ExtUserPrmData = 1450 "In1 - Read only"
Unsigned16 1 0-6
Prm_Text_Ref=1450
EndExtUserPrmData

ExtUserPrmData= 1451 "Relay K4"
Unsigned16 0 0-2
Prm_Text_Ref=1451
EndExtUserPrmData

ExtUserPrmData= 1452 "Relay K5"
Unsigned16 1 0-2
Prm_Text_Ref=1451
EndExtUserPrmData

ExtUserPrmData= 1453 "Relay K6"
Unsigned16 2 0-2
Prm_Text_Ref=1451
EndExtUserPrmData

ExtUserPrmData = 1454 "SW Outp V7"
Unsigned16 2 0-2
Prm_Text_Ref=1451
EndExtUserPrmData

ExtUserPrmData= 1455 "Event K4"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData= 1456 "Event K5"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData= 1457 "Event K6"
Unsigned16 7 0-65535
EndExtUserPrmData

ExtUserPrmData= 1458 "Event V7"
Unsigned16 7 0-65535
EndExtUserPrmData

ExtUserPrmData = 1459 "Fieldb Ctrl - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1408
EndExtUserPrmData

ExtUserPrmData = 1460 "Fieldb Type - Read only"
Unsigned16 1 0-1
Prm_Text_Ref=1460
EndExtUserPrmData

ExtUserPrmData = 1461 "Fieldb Addr - Read only"
Unsigned16 0 0-1000
EndExtUserPrmData

ExtUserPrmData = 1462 "No of Seq"
Unsigned16 1 1-3
Prm_Text_Ref=1462
EndExtUserPrmData

ExtUserPrmData= 1463 "StartRamp1 [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData= 1464 "Init Volt1 [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData= 1465 "Curr Lim1 [0.1*Ie]"
Unsigned16 40 20-70
EndExtUserPrmData

ExtUserPrmData= 1466 "1st Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData= 1467 "StartRamp2  [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData= 1468 "Init Volt2 [%]"
Unsigned16 30 30-70
EndExtUserPrmData
;75
ExtUserPrmData= 1469 "Curr Lim2 [0.1*Ie]"
Unsigned16 40 20-70
EndExtUserPrmData

ExtUserPrmData= 1470 "2nd Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData= 1471 "StartRamp3  [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData= 1472 "Init Volt3[%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData= 1473 "Curr Lim3 [0.1*Ie]"
Unsigned16 40 20-70
EndExtUserPrmData

ExtUserPrmData= 1474 "3rd Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 1475 "Language - Read only"
Unsigned16 1 1-12
Prm_Text_Ref=1475
EndExtUserPrmData

ExtUserPrmData = 1476 "Dummy76 - Read only"
Unsigned16 0 0-15
EndExtUserPrmData

ExtUserPrmData = 1477 "LCD Auto Off - Read only [min]"
Unsigned16 15 1-255
EndExtUserPrmData

ExtUserPrmData = 1478 "Password - Read only"
Unsigned16 0 0-255
EndExtUserPrmData

ExtUserPrmData = 1479 "Date Type - Read only"
Unsigned16 0 0-2
Prm_Text_Ref=1479
EndExtUserPrmData

ExtUserPrmData = 1480 "Date Year - Read only"
Unsigned16 2002 2001-2060
EndExtUserPrmData

ExtUserPrmData = 1481 "Date Month - Read only"
Unsigned16 6 1-12
EndExtUserPrmData

ExtUserPrmData = 1482 "Date Day - Read only"
Unsigned16 15 1-31
EndExtUserPrmData

ExtUserPrmData = 1483 "Time Hour - Read only"
Unsigned16 12 0-23
EndExtUserPrmData

ExtUserPrmData = 1484 "Time Min - Read only"
Unsigned16 30 0-59
EndExtUserPrmData

ExtUserPrmData = 1485 "S Port Ctrl - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1408
EndExtUserPrmData

ExtUserPrmData = 1486 "S Port Addr1 - Read only"
Unsigned16 192 0-255
EndExtUserPrmData

ExtUserPrmData = 1487 "S Port Addr2 - Read only"
Unsigned16 168 0-255
EndExtUserPrmData

ExtUserPrmData = 1488 "S Port Addr3 - Read only"
Unsigned16 0 0-255
EndExtUserPrmData

ExtUserPrmData = 1489 "S Port Addr4 - Read only"
Unsigned16 2 0-255
EndExtUserPrmData

ExtUserPrmData = 1490 "CT Ratio Ir [A] - Read only"
Unsigned16 100 1-2500
EndExtUserPrmData

ExtUserPrmData = 1491 "IntByPass - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1408
EndExtUserPrmData

ExtUserPrmData = 1492 "ByPass AC3 [A] - Read only"
Unsigned16 0 0-2500
EndExtUserPrmData

ExtUserPrmData = 1493 "SOP1 [0.01] - Read only"
Unsigned16 95 70-120
EndExtUserPrmData

ExtUserPrmData = 1494 "SOP2 [0.01] - Read only"
Unsigned16 1000 5-2000
EndExtUserPrmData

ExtUserPrmData = 1495 "SOP3 [0.001] - Read only"
Unsigned16 600 12-1200
EndExtUserPrmData

ExtUserPrmData = 1496 "SOP4 [0.1] - Read only"
Unsigned16 40 10-200
EndExtUserPrmData

ExtUserPrmData = 1497 "BP Close Op"
Unsigned16 0 0-1
Prm_Text_Ref=1436
EndExtUserPrmData

ExtUserPrmData = 1498 "BP Open Op"
Unsigned16 0 0-1
Prm_Text_Ref=1436
EndExtUserPrmData

ExtUserPrmData = 1499 "Dummy99 - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1408
EndExtUserPrmData

ExtUserPrmData = 1500 "FCODE1 - Read only"
Unsigned16 0 0-10
EndExtUserPrmData

ExtUserPrmData = 1501 "FCODE2 - Read only"
Unsigned16 0 0-10
EndExtUserPrmData

ExtUserPrmData = 1502 "FCODE3 - Read only"
Unsigned16 0 0-10
EndExtUserPrmData

ExtUserPrmData = 1503 "FCODE4 - Read only"
Unsigned16 0 0-10
EndExtUserPrmData

ExtUserPrmData = 1504 "FCODE5 - Read only"
Unsigned16 0 0-100
EndExtUserPrmData

ExtUserPrmData = 1505 "FCODE6 - Read only"
Unsigned16 0 0-100
EndExtUserPrmData

ExtUserPrmData = 1506 "PST(B) [A] - Read only"
Unsigned16 100 1-2500
EndExtUserPrmData

ExtUserPrmData = 1507 "FCODE7 - Read only"
Unsigned16 1 0-1
Prm_Text_Ref=1408
EndExtUserPrmData

ExtUserPrmData = 1508 "FCODE8 - Read only"
Unsigned16 1 0-1
Prm_Text_Ref=1408
EndExtUserPrmData

ExtUserPrmData = 1509 "FCODE9 - Read only"
Unsigned16 1 0-1
Prm_Text_Ref=1408
EndExtUserPrmData

ExtUserPrmData = 1510 "FCODE10 - Read only"
Unsigned16 14 0-25
EndExtUserPrmData

;=============================================================
; Additional parameters for CU 04.00.02
; Text-definition for User Prm Data "Softstarter PST(V04)"
;=============================================================
;
PrmText = 1575
Text(1)  = "US/UK"
Text(2)  = "FI"
Text(3)  = "SE"
Text(4)  = "PT"
Text(5)  = "NL"
Text(6)  = "IT"
Text(7)  = "FR"
Text(8)  = "ES"
Text(9)  = "DE"
Text(10) = "CN"
Text(11) = "RU"
Text(12) = "TR"
Text(13) = "PL"
EndPrmText

ExtUserPrmData = 1575 "Language - Read only"
Unsigned16 1 1-13
Prm_Text_Ref=1575
EndExtUserPrmData

ExtUserPrmData = 1511 "Current Limit Y Time [s]"
Unsigned16 0 0-120
EndExtUserPrmData

ExtUserPrmData = 1512 "Current Limit Y Level [0.1*Ie]"
Unsigned16 40 20-70
EndExtUserPrmData

ExtUserPrmData = 1513 "FB Auto Disable - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1408
EndExtUserPrmData


;=============================================================
; Text-definition for User Prm Data "Softstarter PST(V05)"
; Compatible with CU-version 05.02.02.
;=============================================================
;
PrmText = 1608
Text(0)   = "No"
Text(1)   = "Yes"
EndPrmText
PrmText = 1611
Text(0)   = "1-30s"
Text(1)   = "1-120s"
EndPrmText
PrmText = 1612
Text(0)   = "0-30s"
Text(1)   = "0-120s"
EndPrmText
PrmText = 1613
Text(0)   = "No"
Text(1)   = "Normal"
Text(2)   = "Dual"
EndPrmText
PrmText = 1614
Text(0)  = "Class 10A"
Text(1)  = "Class 10"
Text(2)  = "Class 20"
Text(3)  = "Class 30"
EndPrmText
PrmText = 1617
Text(0)   = "Stop-M"
Text(1)   = "Stop-A"
Text(2)   = "Ind"
EndPrmText
PrmText = 1644
Text(0)   = "Stop-M"
Text(1)   = "Stop-A"
EndPrmText
PrmText = 1649
Text(0)  = "None"
Text(1)  = "Reset"
Text(2)  = "Enable"
Text(3)  = "Jog"
Text(4)  = "DOL-On"
Text(5)  = "Start2"
Text(6)  = "FB-Dis"
EndPrmText
PrmText = 1650
Text(0)  = "None"
Text(1)  = "Reset"
Text(2)  = "Enable"
Text(3)  = "Jog"
Text(4)  = "DOL-On"
Text(5)  = "Start3"
Text(6)  = "FB-Dis"
EndPrmText
PrmText = 1651
Text(0)   = "Run"
Text(1)   = "TOR"
Text(2)   = "Event"
EndPrmText
PrmText = 1660
Text(0)   = "AS-Int"
Text(1)   = "Other"
EndPrmText
PrmText = 1662
Text(1)   = "No"
Text(2)   = "2"
Text(3)   = "3"
EndPrmText
PrmText = 1675
Text(1)  = "US/UK"
Text(2)  = "FI"
Text(3)  = "SE"
Text(4)  = "PT"
Text(5)  = "NL"
Text(6)  = "IT"
Text(7)  = "FR"
Text(8)  = "ES"
Text(9)  = "DE"
Text(10) = "CN"
Text(11) = "RU"
Text(12) = "TR"
Text(13) = "PL"
EndPrmText
PrmText = 1679
Text(0)   = "ISO"
Text(1)   = "CE"
Text(2)   = "US"
EndPrmText
PrmText = 1714
Text(0)   = "Volt"
Text(1)   = "Torque"
EndPrmText
PrmText = 1724
Text(0)   = "0-20mA"
Text(1)   = "4-20mA"
Text(2)   = "0-10V"
EndPrmText
PrmText = 1725
Text(0)   = "I Amp"
Text(1)   = "U Volt"
Text(2)   = "P kW"
Text(3)   = "P hp"
Text(4)   = "Q kVAr"
Text(5)   = "S kVA"
Text(6)   = "TmpMot"
Text(7)   = "TmpSCR"
Text(8)   = "cosPhi"
EndPrmText


ExtUserPrmData = 1601 "Setting Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 1602 "Start Ramp [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 1603 "Stop Ramp [s]"
Unsigned16 0 0-120
EndExtUserPrmData

ExtUserPrmData = 1604 "Init Volt [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 1605 "End Volt [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 1606 "Step Down [%]"
Unsigned16 100 30-100
EndExtUserPrmData

ExtUserPrmData = 1607 "Current Lim [0.1*Ie]"
Unsigned16 40 20-70
EndExtUserPrmData

ExtUserPrmData = 1608 "Kick Start"
Unsigned16 0 0-1
Prm_Text_Ref=1608
EndExtUserPrmData

ExtUserPrmData = 1609 "Kick Level [%]"
Unsigned16 50 50-100
EndExtUserPrmData

ExtUserPrmData = 1610 "Kick Time [0.01s]"
Unsigned16 20 10-150
EndExtUserPrmData

ExtUserPrmData = 1611 "Start Range"
Unsigned16 0 0-1
Prm_Text_Ref=1611
EndExtUserPrmData

ExtUserPrmData = 1612 "Stop Range"
Unsigned16 0 0-1
Prm_Text_Ref=1612
EndExtUserPrmData

ExtUserPrmData = 1613 "Overload"
Unsigned16 1 0-2
Prm_Text_Ref=1613
EndExtUserPrmData

ExtUserPrmData = 1614 "OL Class"
Unsigned16 1 0-3
Prm_Text_Ref=1614
EndExtUserPrmData

ExtUserPrmData = 1615 "OL Class S"
Unsigned16 1 0-3
Prm_Text_Ref=1614
EndExtUserPrmData

ExtUserPrmData = 1616 "OL Class R"
Unsigned16 1 0-3
Prm_Text_Ref=1614
EndExtUserPrmData

ExtUserPrmData = 1617 "OL Op"
Unsigned16 0 0-2
Prm_Text_Ref=1617
EndExtUserPrmData

ExtUserPrmData = 1618 "Locked Rotor"
Unsigned16 0 0-1
Prm_Text_Ref=1608
EndExtUserPrmData

ExtUserPrmData = 1619 "Lock R Lev [0.1*Ie]"
Unsigned16 40 5-80
EndExtUserPrmData

ExtUserPrmData = 1620 "Lock R Time [0.1s]"
Unsigned16 10 2-100
EndExtUserPrmData

ExtUserPrmData = 1621 "Lock R Op"
Unsigned16 0 0-2
Prm_Text_Ref=1617
EndExtUserPrmData

ExtUserPrmData = 1622 "Underload"
Unsigned16 0 0-1
Prm_Text_Ref=1608
EndExtUserPrmData

ExtUserPrmData = 1623 "Underl Lev [0.1*Ie]"
Unsigned16 5 4-8
EndExtUserPrmData

ExtUserPrmData = 1624 "Underl Time [s]"
Unsigned16 10 1-30
EndExtUserPrmData

ExtUserPrmData =1625 "Underl Op"
Unsigned16 0 0-2
Prm_Text_Ref=1617
EndExtUserPrmData

ExtUserPrmData = 1626 "Phase Imb"
Unsigned16 0 0-1
Prm_Text_Ref=1608
EndExtUserPrmData

ExtUserPrmData = 1627 "Ph Imb Lev [%]"
Unsigned16 80 10-80
EndExtUserPrmData

ExtUserPrmData = 1628 "Ph Imb Op"
Unsigned16 0 0-2
Prm_Text_Ref=1617
EndExtUserPrmData

ExtUserPrmData = 1629 "High I"
Unsigned16 0 0-1
Prm_Text_Ref=1608
EndExtUserPrmData

ExtUserPrmData = 1630 "High I Op"
Unsigned16 0 0-2
Prm_Text_Ref=1617
EndExtUserPrmData

ExtUserPrmData = 1631 "Phase Rev"
Unsigned16 0 0-1
Prm_Text_Ref=1608
EndExtUserPrmData

ExtUserPrmData = 1632 "Ph Rev Op"
Unsigned16 0 0-2
Prm_Text_Ref=1617
EndExtUserPrmData

ExtUserPrmData = 1633 "PTC"
Unsigned16 0 0-1
Prm_Text_Ref=1608
EndExtUserPrmData

ExtUserPrmData = 1634 "PTC Op"
Unsigned16 0 0-2
Prm_Text_Ref=1617
EndExtUserPrmData

ExtUserPrmData = 1635 "Ext ByPass"
Unsigned16 0 0-1
Prm_Text_Ref=1608
EndExtUserPrmData

ExtUserPrmData = 1637 "Warn I=High"
Unsigned16 0 0-1
Prm_Text_Ref=1608
EndExtUserPrmData

ExtUserPrmData = 1638 "Wa I=H Lev [0.1*Ie]"
Unsigned16 12 5-50
EndExtUserPrmData

ExtUserPrmData = 1639 "Warn I=Low"
Unsigned16 0 0-1
Prm_Text_Ref=1608
EndExtUserPrmData

ExtUserPrmData = 1640 "Wa I=L Lev [0.1*Ie]"
Unsigned16 5 4-10
EndExtUserPrmData

ExtUserPrmData = 1641 "Warn OL"
Unsigned16 0 0-1
Prm_Text_Ref=1608
EndExtUserPrmData

ExtUserPrmData = 1642 "Wa OL Lev [%]"
Unsigned16 90 40-99
EndExtUserPrmData

ExtUserPrmData = 1643 "Warn SCR OL"
Unsigned16 0 0-1
Prm_Text_Ref=1608
EndExtUserPrmData

ExtUserPrmData = 1644 "Ph Loss Op"
Unsigned16 0 0-1
Prm_Text_Ref=1644
EndExtUserPrmData

ExtUserPrmData = 1645 "FB Fault Op"
Unsigned16 0 0-1
Prm_Text_Ref=1644
EndExtUserPrmData

ExtUserPrmData = 1646 "Freq F Op"
Unsigned16 0 0-1
Prm_Text_Ref=1644
EndExtUserPrmData

ExtUserPrmData = 1647 "HC Temp Op"
Unsigned16 0 0-1
Prm_Text_Ref=1644
EndExtUserPrmData

ExtUserPrmData = 1648 "SCR SC Op"
Unsigned16 0 0-1
Prm_Text_Ref=1644
EndExtUserPrmData

ExtUserPrmData = 1649 "In0 - Read only"
Unsigned16 1 0-6
Prm_Text_Ref=1649
EndExtUserPrmData

ExtUserPrmData = 1650 "In1 - Read only"
Unsigned16 1 0-6
Prm_Text_Ref=1650
EndExtUserPrmData

ExtUserPrmData = 1651 "Relay K4"
Unsigned16 0 0-2
Prm_Text_Ref=1651
EndExtUserPrmData

ExtUserPrmData = 1652 "Relay K5"
Unsigned16 1 0-2
Prm_Text_Ref=1651
EndExtUserPrmData

ExtUserPrmData = 1653 "Relay K6"
Unsigned16 2 0-2
Prm_Text_Ref=1651
EndExtUserPrmData

ExtUserPrmData = 1654 "SW Outp V7"
Unsigned16 2 0-2
Prm_Text_Ref=1651
EndExtUserPrmData

ExtUserPrmData = 1655 "Event K4"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 1656 "Event K5"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 1657 "Event K6"
Unsigned16 7 0-65535
EndExtUserPrmData

ExtUserPrmData = 1658 "Event V7"
Unsigned16 7 0-65535
EndExtUserPrmData

ExtUserPrmData = 1659 "Fieldb Ctrl - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1608
EndExtUserPrmData

ExtUserPrmData = 1660 "Fieldb Type - Read only"
Unsigned16 1 0-1
Prm_Text_Ref=1660
EndExtUserPrmData

ExtUserPrmData = 1661 "Fieldb Addr - Read only"
Unsigned16 0 0-1000
EndExtUserPrmData

ExtUserPrmData = 1662 "No of Seq"
Unsigned16 1 1-3
Prm_Text_Ref=1662
EndExtUserPrmData

ExtUserPrmData = 1663 "StartRamp1 [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 1664 "Init Volt1 [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 1665 "Curr Lim1 [0.1*Ie]"
Unsigned16 40 20-70
EndExtUserPrmData

ExtUserPrmData = 1666 "1st Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 1667 "StartRamp2 [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 1668 "Init Volt2 [%]"
Unsigned16 30 30-70
EndExtUserPrmData
;75
ExtUserPrmData = 1669 "Curr Lim2 [0.1*Ie]"
Unsigned16 40 20-70
EndExtUserPrmData

ExtUserPrmData = 1670 "2nd Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 1671 "StartRamp3 [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 1672 "Init Volt3 [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 1673 "Curr Lim3 [0.1*Ie]"
Unsigned16 40 20-70
EndExtUserPrmData

ExtUserPrmData = 1674 "3rd Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 1675 "Language - Read only"
Unsigned16 1 1-13
Prm_Text_Ref=1675
EndExtUserPrmData

ExtUserPrmData = 1679 "Date Type - Read only"
Unsigned16 0 0-2
Prm_Text_Ref=1679
EndExtUserPrmData

ExtUserPrmData = 1680 "Date Year - Read only"
Unsigned16 2002 1901-2038
EndExtUserPrmData

ExtUserPrmData = 1681 "Date Month - Read only"
Unsigned16 6 1-12
EndExtUserPrmData

ExtUserPrmData = 1682 "Date Day - Read only"
Unsigned16 15 1-31
EndExtUserPrmData

ExtUserPrmData = 1683 "Time Hour - Read only"
Unsigned16 12 0-23
EndExtUserPrmData

ExtUserPrmData = 1684 "Time Min - Read only"
Unsigned16 30 0-59
EndExtUserPrmData

ExtUserPrmData = 1697 "BP Close Op"
Unsigned16 0 0-1
Prm_Text_Ref=1644
EndExtUserPrmData

ExtUserPrmData = 1698 "BP Open Op"
Unsigned16 0 0-1
Prm_Text_Ref=1644
EndExtUserPrmData

ExtUserPrmData = 1706 "PST(B) [A] - Read only"
Unsigned16 100 1-2500
EndExtUserPrmData

ExtUserPrmData = 1711 "Current Limit Y Time [s]"
Unsigned16 0 0-120
EndExtUserPrmData

ExtUserPrmData = 1712 "Current Limit Y Level [0.1*Ie]"
Unsigned16 40 20-70
EndExtUserPrmData

ExtUserPrmData = 1713 "FB Auto Disable - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1608
EndExtUserPrmData

ExtUserPrmData = 1714 "Start Mode"
Unsigned16 0 0-1
Prm_Text_Ref=1714
EndExtUserPrmData

ExtUserPrmData = 1715 "Stop Mode"
Unsigned16 0 0-1
Prm_Text_Ref=1714
EndExtUserPrmData

ExtUserPrmData = 1716 "Torque Limit [%]"
Unsigned16 150 20-200
EndExtUserPrmData

ExtUserPrmData = 1717 "Tune T-Ctrl [%]"
Unsigned16 100 30-300
EndExtUserPrmData

ExtUserPrmData = 1723 "Analogue Out"
Unsigned16 0 0-1
Prm_Text_Ref=1608
EndExtUserPrmData

ExtUserPrmData = 1724 "Anl Ref"
Unsigned16 1 0-2
Prm_Text_Ref=1724
EndExtUserPrmData

ExtUserPrmData = 1725 "Anl Type"
Unsigned16 0 0-8
Prm_Text_Ref=1725
EndExtUserPrmData

ExtUserPrmData = 1726 "I Range Max [A]"
Unsigned16 11000 1-20000
EndExtUserPrmData

ExtUserPrmData = 1727 "U Range Max [V]"
Unsigned16 600 10-1000
EndExtUserPrmData

ExtUserPrmData = 1728 "kW Range Max [0.1kW]"
Unsigned16 15000 1-30000
EndExtUserPrmData

ExtUserPrmData = 1729 "hp Range Max [0.1hp]"
Unsigned16 15000 1-30000
EndExtUserPrmData

ExtUserPrmData = 1730 "Q Range Max [0.1kVAr]"
Unsigned16 15000 1-30000
EndExtUserPrmData

ExtUserPrmData = 1731 "S Range Max [0.1kVA]"
Unsigned16 15000 1-30000
EndExtUserPrmData


;=============================================================
; Text-definition for User Prm Data "Softstarter PST(V06)"
; Compatible with CU-version 05.03.03.
;=============================================================
;
PrmText = 1808
Text(0)   = "No"
Text(1)   = "Yes"
EndPrmText
PrmText = 1811
Text(0)   = "1-30s"
Text(1)   = "1-120s"
EndPrmText
PrmText = 1812
Text(0)   = "0-30s"
Text(1)   = "0-120s"
EndPrmText
PrmText = 1813
Text(0)   = "No"
Text(1)   = "Normal"
Text(2)   = "Dual"
EndPrmText
PrmText = 1814
Text(0)  = "No"
Text(1)  = "Class 10A"
Text(2)  = "Class 10"
Text(3)  = "Class 20"
Text(4)  = "Class 30"
EndPrmText
PrmText = 1817
Text(0)   = "Stop-M"
Text(1)   = "Stop-A"
Text(2)   = "Ind"
EndPrmText
PrmText = 1844
Text(0)   = "Stop-M"
Text(1)   = "Stop-A"
EndPrmText
PrmText = 1849
Text(0)  = "None"
Text(1)  = "Reset"
Text(2)  = "Enable"
Text(3)  = "Jog"
Text(4)  = "DOL-On"
Text(5)  = "Start2"
Text(6)  = "FB-Dis"
EndPrmText
PrmText = 1850
Text(0)  = "None"
Text(1)  = "Reset"
Text(2)  = "Enable"
Text(3)  = "Jog"
Text(4)  = "DOL-On"
Text(5)  = "Start3"
Text(6)  = "FB-Dis"
EndPrmText
PrmText = 1851
Text(0)   = "Run"
Text(1)   = "TOR"
Text(2)   = "Event"
EndPrmText
PrmText = 1860
Text(0)   = "AS-Int"
Text(1)   = "Other"
EndPrmText
PrmText = 1862
Text(1)   = "No"
Text(2)   = "2"
Text(3)   = "3"
EndPrmText
PrmText = 1875
Text(1)  = "US/UK"
Text(2)  = "FI"
Text(3)  = "SE"
Text(4)  = "PT"
Text(5)  = "NL"
Text(6)  = "IT"
Text(7)  = "FR"
Text(8)  = "ES"
Text(9)  = "DE"
Text(10) = "CN"
Text(11) = "RU"
Text(12) = "TR"
Text(13) = "PL"
Text(14) = "CZ"
EndPrmText
PrmText = 1879
Text(0)   = "ISO"
Text(1)   = "CE"
Text(2)   = "US"
EndPrmText
PrmText = 1914
Text(0)   = "Volt"
Text(1)   = "Torque"
EndPrmText
PrmText = 1924
Text(0)   = "0-20mA"
Text(1)   = "4-20mA"
Text(2)   = "0-10V"
EndPrmText
PrmText = 1925
Text(0)   = "I Amp"
Text(1)   = "U Volt"
Text(2)   = "P kW"
Text(3)   = "P hp"
Text(4)   = "Q kVAr"
Text(5)   = "S kVA"
Text(6)   = "TmpMot"
Text(7)   = "TmpSCR"
Text(8)   = "cosPhi"
EndPrmText


ExtUserPrmData = 1801 "Setting Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 1802 "Start Ramp [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 1803 "Stop Ramp [s]"
Unsigned16 0 0-120
EndExtUserPrmData

ExtUserPrmData = 1804 "Init Volt [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 1805 "End Volt [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 1806 "Step Down [%]"
Unsigned16 100 30-100
EndExtUserPrmData

ExtUserPrmData = 1807 "Current Lim [0.1*Ie]"
Unsigned16 40 20-70
EndExtUserPrmData

ExtUserPrmData = 1808 "Kick Start"
Unsigned16 0 0-1
Prm_Text_Ref=1808
EndExtUserPrmData

ExtUserPrmData = 1809 "Kick Level [%]"
Unsigned16 50 50-100
EndExtUserPrmData

ExtUserPrmData = 1810 "Kick Time [0.01s]"
Unsigned16 20 10-150
EndExtUserPrmData

ExtUserPrmData = 1811 "Start Range"
Unsigned16 0 0-1
Prm_Text_Ref=1811
EndExtUserPrmData

ExtUserPrmData = 1812 "Stop Range"
Unsigned16 0 0-1
Prm_Text_Ref=1812
EndExtUserPrmData

ExtUserPrmData = 1813 "Overload"
Unsigned16 1 0-2
Prm_Text_Ref=1813
EndExtUserPrmData

ExtUserPrmData = 1814 "OL Class"
Unsigned16 2 1-4
Prm_Text_Ref=1814
EndExtUserPrmData

ExtUserPrmData = 1815 "OL Class S"
Unsigned16 2 0-4
Prm_Text_Ref=1814
EndExtUserPrmData

ExtUserPrmData = 1816 "OL Class R"
Unsigned16 2 0-4
Prm_Text_Ref=1814
EndExtUserPrmData

ExtUserPrmData = 1817 "OL Op"
Unsigned16 0 0-2
Prm_Text_Ref=1817
EndExtUserPrmData

ExtUserPrmData = 1818 "Locked Rotor"
Unsigned16 0 0-1
Prm_Text_Ref=1808
EndExtUserPrmData

ExtUserPrmData = 1819 "Lock R Lev [0.1*Ie]"
Unsigned16 40 5-80
EndExtUserPrmData

ExtUserPrmData = 1820 "Lock R Time [0.1s]"
Unsigned16 10 2-100
EndExtUserPrmData

ExtUserPrmData = 1821 "Lock R Op"
Unsigned16 0 0-2
Prm_Text_Ref=1817
EndExtUserPrmData

ExtUserPrmData = 1822 "Underload"
Unsigned16 0 0-1
Prm_Text_Ref=1808
EndExtUserPrmData

ExtUserPrmData = 1823 "Underl Lev [0.1*Ie]"
Unsigned16 5 4-8
EndExtUserPrmData

ExtUserPrmData = 1824 "Underl Time [s]"
Unsigned16 10 1-30
EndExtUserPrmData

ExtUserPrmData =1825 "Underl Op"
Unsigned16 0 0-2
Prm_Text_Ref=1817
EndExtUserPrmData

ExtUserPrmData = 1826 "Phase Imb"
Unsigned16 0 0-1
Prm_Text_Ref=1808
EndExtUserPrmData

ExtUserPrmData = 1827 "Ph Imb Lev [%]"
Unsigned16 80 10-80
EndExtUserPrmData

ExtUserPrmData = 1828 "Ph Imb Op"
Unsigned16 0 0-2
Prm_Text_Ref=1817
EndExtUserPrmData

ExtUserPrmData = 1829 "High I"
Unsigned16 0 0-1
Prm_Text_Ref=1808
EndExtUserPrmData

ExtUserPrmData = 1830 "High I Op"
Unsigned16 0 0-2
Prm_Text_Ref=1817
EndExtUserPrmData

ExtUserPrmData = 1831 "Phase Rev"
Unsigned16 0 0-1
Prm_Text_Ref=1808
EndExtUserPrmData

ExtUserPrmData = 1832 "Ph Rev Op"
Unsigned16 0 0-2
Prm_Text_Ref=1817
EndExtUserPrmData

ExtUserPrmData = 1833 "PTC"
Unsigned16 0 0-1
Prm_Text_Ref=1808
EndExtUserPrmData

ExtUserPrmData = 1834 "PTC Op"
Unsigned16 0 0-2
Prm_Text_Ref=1817
EndExtUserPrmData

ExtUserPrmData = 1835 "Ext ByPass"
Unsigned16 0 0-1
Prm_Text_Ref=1808
EndExtUserPrmData

ExtUserPrmData = 1837 "Warn I=High"
Unsigned16 0 0-1
Prm_Text_Ref=1808
EndExtUserPrmData

ExtUserPrmData = 1838 "Wa I=H Lev [0.1*Ie]"
Unsigned16 12 5-50
EndExtUserPrmData

ExtUserPrmData = 1839 "Warn I=Low"
Unsigned16 0 0-1
Prm_Text_Ref=1808
EndExtUserPrmData

ExtUserPrmData = 1840 "Wa I=L Lev [0.1*Ie]"
Unsigned16 5 4-10
EndExtUserPrmData

ExtUserPrmData = 1841 "Warn OL"
Unsigned16 0 0-1
Prm_Text_Ref=1808
EndExtUserPrmData

ExtUserPrmData = 1842 "Wa OL Lev [%]"
Unsigned16 90 40-99
EndExtUserPrmData

ExtUserPrmData = 1843 "Warn SCR OL"
Unsigned16 0 0-1
Prm_Text_Ref=1808
EndExtUserPrmData

ExtUserPrmData = 1844 "Ph Loss Op"
Unsigned16 0 0-1
Prm_Text_Ref=1844
EndExtUserPrmData

ExtUserPrmData = 1845 "FB Fault Op"
Unsigned16 0 0-1
Prm_Text_Ref=1844
EndExtUserPrmData

ExtUserPrmData = 1846 "Freq F Op"
Unsigned16 0 0-1
Prm_Text_Ref=1844
EndExtUserPrmData

ExtUserPrmData = 1847 "HC Temp Op"
Unsigned16 0 0-1
Prm_Text_Ref=1844
EndExtUserPrmData

ExtUserPrmData = 1848 "SCR SC Op"
Unsigned16 0 0-1
Prm_Text_Ref=1844
EndExtUserPrmData

ExtUserPrmData = 1849 "In0 - Read only"
Unsigned16 1 0-6
Prm_Text_Ref=1849
EndExtUserPrmData

ExtUserPrmData = 1850 "In1 - Read only"
Unsigned16 1 0-6
Prm_Text_Ref=1850
EndExtUserPrmData

ExtUserPrmData = 1851 "Relay K4"
Unsigned16 0 0-2
Prm_Text_Ref=1851
EndExtUserPrmData

ExtUserPrmData = 1852 "Relay K5"
Unsigned16 1 0-2
Prm_Text_Ref=1851
EndExtUserPrmData

ExtUserPrmData = 1853 "Relay K6"
Unsigned16 2 0-2
Prm_Text_Ref=1851
EndExtUserPrmData

ExtUserPrmData = 1854 "SW Outp V7"
Unsigned16 2 0-2
Prm_Text_Ref=1851
EndExtUserPrmData

ExtUserPrmData = 1855 "Event K4"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 1856 "Event K5"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 1857 "Event K6"
Unsigned16 7 0-65535
EndExtUserPrmData

ExtUserPrmData = 1858 "Event V7"
Unsigned16 7 0-65535
EndExtUserPrmData

ExtUserPrmData = 1859 "Fieldb Ctrl - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1808
EndExtUserPrmData

ExtUserPrmData = 1860 "Fieldb Type - Read only"
Unsigned16 1 0-1
Prm_Text_Ref=1860
EndExtUserPrmData

ExtUserPrmData = 1861 "Fieldb Addr - Read only"
Unsigned16 0 0-1000
EndExtUserPrmData

ExtUserPrmData = 1862 "No of Seq"
Unsigned16 1 1-3
Prm_Text_Ref=1862
EndExtUserPrmData

ExtUserPrmData = 1863 "StartRamp1 [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 1864 "Init Volt1 [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 1865 "Curr Lim1 [0.1*Ie]"
Unsigned16 40 20-70
EndExtUserPrmData

ExtUserPrmData = 1866 "1st Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 1867 "StartRamp2 [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 1868 "Init Volt2 [%]"
Unsigned16 30 30-70
EndExtUserPrmData
;75
ExtUserPrmData = 1869 "Curr Lim2 [0.1*Ie]"
Unsigned16 40 20-70
EndExtUserPrmData

ExtUserPrmData = 1870 "2nd Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 1871 "StartRamp3 [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 1872 "Init Volt3 [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 1873 "Curr Lim3 [0.1*Ie]"
Unsigned16 40 20-70
EndExtUserPrmData

ExtUserPrmData = 1874 "3rd Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 1875 "Language - Read only"
Unsigned16 1 1-14
Prm_Text_Ref=1875
EndExtUserPrmData

ExtUserPrmData = 1879 "Date Type - Read only"
Unsigned16 0 0-2
Prm_Text_Ref=1879
EndExtUserPrmData

ExtUserPrmData = 1880 "Date Year - Read only"
Unsigned16 2002 1901-2038
EndExtUserPrmData

ExtUserPrmData = 1881 "Date Month - Read only"
Unsigned16 6 1-12
EndExtUserPrmData

ExtUserPrmData = 1882 "Date Day - Read only"
Unsigned16 15 1-31
EndExtUserPrmData

ExtUserPrmData = 1883 "Time Hour - Read only"
Unsigned16 12 0-23
EndExtUserPrmData

ExtUserPrmData = 1884 "Time Min - Read only"
Unsigned16 30 0-59
EndExtUserPrmData

ExtUserPrmData = 1897 "BP Close Op"
Unsigned16 0 0-1
Prm_Text_Ref=1844
EndExtUserPrmData

ExtUserPrmData = 1898 "BP Open Op"
Unsigned16 0 0-1
Prm_Text_Ref=1844
EndExtUserPrmData

ExtUserPrmData = 1906 "PST(B) [A] - Read only"
Unsigned16 100 1-2500
EndExtUserPrmData

ExtUserPrmData = 1911 "Current Limit Y Time [s]"
Unsigned16 0 0-120
EndExtUserPrmData

ExtUserPrmData = 1912 "Current Limit Y Level [0.1*Ie]"
Unsigned16 40 20-70
EndExtUserPrmData

ExtUserPrmData = 1913 "FB Auto Disable - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1808
EndExtUserPrmData

ExtUserPrmData = 1914 "Start Mode"
Unsigned16 0 0-1
Prm_Text_Ref=1914
EndExtUserPrmData

ExtUserPrmData = 1915 "Stop Mode"
Unsigned16 0 0-1
Prm_Text_Ref=1914
EndExtUserPrmData

ExtUserPrmData = 1916 "Torque Limit [%]"
Unsigned16 150 20-200
EndExtUserPrmData

ExtUserPrmData = 1917 "Tune T-Ctrl [%]"
Unsigned16 100 30-300
EndExtUserPrmData

ExtUserPrmData = 1923 "Analogue Out"
Unsigned16 0 0-1
Prm_Text_Ref=1808
EndExtUserPrmData

ExtUserPrmData = 1924 "Anl Ref"
Unsigned16 1 0-2
Prm_Text_Ref=1924
EndExtUserPrmData

ExtUserPrmData = 1925 "Anl Type"
Unsigned16 0 0-8
Prm_Text_Ref=1925
EndExtUserPrmData

ExtUserPrmData = 1926 "I Range Max [A]"
Unsigned16 11000 1-20000
EndExtUserPrmData

ExtUserPrmData = 1927 "U Range Max [V]"
Unsigned16 600 10-1000
EndExtUserPrmData

ExtUserPrmData = 1928 "kW Range Max [0.1kW]"
Unsigned16 15000 1-30000
EndExtUserPrmData

ExtUserPrmData = 1929 "hp Range Max [0.1hp]"
Unsigned16 15000 1-30000
EndExtUserPrmData

ExtUserPrmData = 1930 "Q Range Max [0.1kVAr]"
Unsigned16 15000 1-30000
EndExtUserPrmData

ExtUserPrmData = 1931 "S Range Max [0.1kVA]"
Unsigned16 15000 1-30000
EndExtUserPrmData


;=============================================================
; Text-definition for User Prm Data "Softstarter PST(V07)"
; Compatible with CU-version 05.04.04.
;=============================================================
;
PrmText = 5008
Text(0)   = "No"
Text(1)   = "Yes"
EndPrmText
PrmText = 5011
Text(0)   = "1-30s"
Text(1)   = "1-120s"
EndPrmText
PrmText = 5012
Text(0)   = "0-30s"
Text(1)   = "0-120s"
EndPrmText
PrmText = 5013
Text(0)   = "No"
Text(1)   = "Normal"
Text(2)   = "Dual"
EndPrmText
PrmText = 5014
Text(0)  = "Class 10A"
Text(1)  = "Class 10"
Text(2)  = "Class 20"
Text(3)  = "Class 30"
Text(4)  = "No"
EndPrmText
PrmText = 5017
Text(0)   = "Stop-M"
Text(1)   = "Stop-A"
Text(2)   = "Ind"
EndPrmText
PrmText = 5044
Text(0)   = "Stop-M"
Text(1)   = "Stop-A"
EndPrmText
PrmText = 5049
Text(0)  = "None"
Text(1)  = "Reset"
Text(2)  = "Enable"
Text(3)  = "Jog"
Text(4)  = "DOL-On"
Text(5)  = "Start2"
Text(6)  = "FB-Dis"
EndPrmText
PrmText = 5050
Text(0)  = "None"
Text(1)  = "Reset"
Text(2)  = "Enable"
Text(3)  = "Jog"
Text(4)  = "DOL-On"
Text(5)  = "Start3"
Text(6)  = "FB-Dis"
EndPrmText
PrmText = 5051
Text(0)   = "Run"
Text(1)   = "TOR"
Text(2)   = "Event"
EndPrmText
PrmText = 5060
Text(0)   = "AS-Int"
Text(1)   = "Other"
EndPrmText
PrmText = 5062
Text(1)   = "No"
Text(2)   = "2"
Text(3)   = "3"
EndPrmText
PrmText = 5075
Text(1)  = "US/UK"
Text(2)  = "FI"
Text(3)  = "SE"
Text(4)  = "PT"
Text(5)  = "NL"
Text(6)  = "IT"
Text(7)  = "FR"
Text(8)  = "ES"
Text(9)  = "DE"
Text(10) = "CN"
Text(11) = "RU"
Text(12) = "TR"
Text(13) = "PL"
Text(14) = "CZ"
EndPrmText
PrmText = 5079
Text(0)   = "ISO"
Text(1)   = "CE"
Text(2)   = "US"
EndPrmText
PrmText = 5114
Text(0)   = "Volt"
Text(1)   = "Torque"
EndPrmText
PrmText = 5124
Text(0)   = "0-20mA"
Text(1)   = "4-20mA"
Text(2)   = "0-10V"
EndPrmText
PrmText = 5125
Text(0)   = "I Amp"
Text(1)   = "U Volt"
Text(2)   = "P kW"
Text(3)   = "P hp"
Text(4)   = "Q kVAr"
Text(5)   = "S kVA"
Text(6)   = "TmpMot"
Text(7)   = "TmpSCR"
Text(8)   = "cosPhi"
EndPrmText
PrmText = 5132
Text(0)   = "010000"
Text(1)   = "010100"
Text(2)   = "020001"
Text(3)   = "030302"
Text(4)   = "030401"
Text(5)   = "030500"
Text(6)   = "040002"
Text(7)   = "050202"
Text(8)   = "050404"
EndPrmText

ExtUserPrmData = 5001 "Setting Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 5002 "Start Ramp [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 5003 "Stop Ramp [s]"
Unsigned16 0 0-120
EndExtUserPrmData

ExtUserPrmData = 5004 "Init Volt [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 5005 "End Volt [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 5006 "Step Down [%]"
Unsigned16 100 30-100
EndExtUserPrmData

ExtUserPrmData = 5007 "Current Lim [0.1*Ie]"
Unsigned16 40 15-70
EndExtUserPrmData

ExtUserPrmData = 5008 "Kick Start"
Unsigned16 0 0-1
Prm_Text_Ref=5008
EndExtUserPrmData

ExtUserPrmData = 5009 "Kick Level [%]"
Unsigned16 50 50-100
EndExtUserPrmData

ExtUserPrmData = 5010 "Kick Time [0.01s]"
Unsigned16 20 10-150
EndExtUserPrmData

ExtUserPrmData = 5011 "Start Range"
Unsigned16 0 0-1
Prm_Text_Ref=5011
EndExtUserPrmData

ExtUserPrmData = 5012 "Stop Range"
Unsigned16 0 0-1
Prm_Text_Ref=5012
EndExtUserPrmData

ExtUserPrmData = 5013 "Overload"
Unsigned16 1 0-2
Prm_Text_Ref=5013
EndExtUserPrmData

ExtUserPrmData = 5014 "OL Class"
Unsigned16 1 0-3
Prm_Text_Ref=5014
EndExtUserPrmData

ExtUserPrmData = 5015 "OL Class S"
Unsigned16 1 0-4
Prm_Text_Ref=5014
EndExtUserPrmData

ExtUserPrmData = 5016 "OL Class R"
Unsigned16 1 0-4
Prm_Text_Ref=5014
EndExtUserPrmData

ExtUserPrmData = 5017 "OL Op"
Unsigned16 0 0-2
Prm_Text_Ref=5017
EndExtUserPrmData

ExtUserPrmData = 5018 "Locked Rotor"
Unsigned16 0 0-1
Prm_Text_Ref=5008
EndExtUserPrmData

ExtUserPrmData = 5019 "Lock R Lev [0.1*Ie]"
Unsigned16 40 5-80
EndExtUserPrmData

ExtUserPrmData = 5020 "Lock R Time [0.1s]"
Unsigned16 10 2-100
EndExtUserPrmData

ExtUserPrmData = 5021 "Lock R Op"
Unsigned16 0 0-2
Prm_Text_Ref=5017
EndExtUserPrmData

ExtUserPrmData = 5022 "Underload"
Unsigned16 0 0-1
Prm_Text_Ref=5008
EndExtUserPrmData

ExtUserPrmData = 5023 "Underl Lev [0.1*Ie]"
Unsigned16 5 4-8
EndExtUserPrmData

ExtUserPrmData = 5024 "Underl Time [s]"
Unsigned16 10 1-30
EndExtUserPrmData

ExtUserPrmData =5025 "Underl Op"
Unsigned16 0 0-2
Prm_Text_Ref=5017
EndExtUserPrmData

ExtUserPrmData = 5026 "Phase Imb"
Unsigned16 0 0-1
Prm_Text_Ref=5008
EndExtUserPrmData

ExtUserPrmData = 5027 "Ph Imb Lev [%]"
Unsigned16 80 10-80
EndExtUserPrmData

ExtUserPrmData = 5028 "Ph Imb Op"
Unsigned16 0 0-2
Prm_Text_Ref=5017
EndExtUserPrmData

ExtUserPrmData = 5029 "High I"
Unsigned16 0 0-1
Prm_Text_Ref=5008
EndExtUserPrmData

ExtUserPrmData = 5030 "High I Op"
Unsigned16 0 0-2
Prm_Text_Ref=5017
EndExtUserPrmData

ExtUserPrmData = 5031 "Phase Rev"
Unsigned16 0 0-1
Prm_Text_Ref=5008
EndExtUserPrmData

ExtUserPrmData = 5032 "Ph Rev Op"
Unsigned16 0 0-2
Prm_Text_Ref=5017
EndExtUserPrmData

ExtUserPrmData = 5033 "PTC"
Unsigned16 0 0-1
Prm_Text_Ref=5008
EndExtUserPrmData

ExtUserPrmData = 5034 "PTC Op"
Unsigned16 0 0-2
Prm_Text_Ref=5017
EndExtUserPrmData

ExtUserPrmData = 5035 "Ext ByPass"
Unsigned16 0 0-1
Prm_Text_Ref=5008
EndExtUserPrmData

ExtUserPrmData = 5037 "Warn I=High"
Unsigned16 0 0-1
Prm_Text_Ref=5008
EndExtUserPrmData

ExtUserPrmData = 5038 "Wa I=H Lev [0.1*Ie]"
Unsigned16 12 5-80
EndExtUserPrmData

ExtUserPrmData = 5039 "Warn I=Low"
Unsigned16 0 0-1
Prm_Text_Ref=5008
EndExtUserPrmData

ExtUserPrmData = 5040 "Wa I=L Lev [0.1*Ie]"
Unsigned16 8 4-10
EndExtUserPrmData

ExtUserPrmData = 5041 "Warn OL"
Unsigned16 0 0-1
Prm_Text_Ref=5008
EndExtUserPrmData

ExtUserPrmData = 5042 "Wa OL Lev [%]"
Unsigned16 90 40-99
EndExtUserPrmData

ExtUserPrmData = 5043 "Warn SCR OL"
Unsigned16 0 0-1
Prm_Text_Ref=5008
EndExtUserPrmData

ExtUserPrmData = 5044 "Ph Loss Op"
Unsigned16 0 0-1
Prm_Text_Ref=5044
EndExtUserPrmData

ExtUserPrmData = 5045 "FB Fault Op"
Unsigned16 0 0-1
Prm_Text_Ref=5044
EndExtUserPrmData

ExtUserPrmData = 5046 "Freq F Op"
Unsigned16 0 0-1
Prm_Text_Ref=5044
EndExtUserPrmData

ExtUserPrmData = 5047 "HC Temp Op"
Unsigned16 0 0-1
Prm_Text_Ref=5044
EndExtUserPrmData

ExtUserPrmData = 5048 "SCR SC Op"
Unsigned16 0 0-1
Prm_Text_Ref=5044
EndExtUserPrmData

ExtUserPrmData = 5049 "In0 - Read only"
Unsigned16 1 0-6
Prm_Text_Ref=5049
EndExtUserPrmData

ExtUserPrmData = 5050 "In1 - Read only"
Unsigned16 1 0-6
Prm_Text_Ref=5050
EndExtUserPrmData

ExtUserPrmData = 5051 "Relay K4"
Unsigned16 0 0-2
Prm_Text_Ref=5051
EndExtUserPrmData

ExtUserPrmData = 5052 "Relay K5"
Unsigned16 1 0-2
Prm_Text_Ref=5051
EndExtUserPrmData

ExtUserPrmData = 5053 "Relay K6"
Unsigned16 2 0-2
Prm_Text_Ref=5051
EndExtUserPrmData

ExtUserPrmData = 5054 "SW Outp V7"
Unsigned16 2 0-2
Prm_Text_Ref=5051
EndExtUserPrmData

ExtUserPrmData = 5055 "Event K4"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 5056 "Event K5"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 5057 "Event K6"
Unsigned16 7 0-65535
EndExtUserPrmData

ExtUserPrmData = 5058 "Event V7"
Unsigned16 7 0-65535
EndExtUserPrmData

ExtUserPrmData = 5059 "Fieldb Ctrl - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=5008
EndExtUserPrmData

ExtUserPrmData = 5060 "Fieldb Type - Read only"
Unsigned16 1 0-1
Prm_Text_Ref=5060
EndExtUserPrmData

ExtUserPrmData = 5061 "Fieldb Addr - Read only"
Unsigned16 0 0-1000
EndExtUserPrmData

ExtUserPrmData = 5062 "No of Seq"
Unsigned16 1 1-3
Prm_Text_Ref=5062
EndExtUserPrmData

ExtUserPrmData = 5063 "StartRamp1 [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 5064 "Init Volt1 [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 5065 "Curr Lim1 [0.1*Ie]"
Unsigned16 40 15-70
EndExtUserPrmData

ExtUserPrmData = 5066 "1st Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 5067 "StartRamp2 [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 5068 "Init Volt2 [%]"
Unsigned16 30 30-70
EndExtUserPrmData
;75
ExtUserPrmData = 5069 "Curr Lim2 [0.1*Ie]"
Unsigned16 40 15-70
EndExtUserPrmData

ExtUserPrmData = 5070 "2nd Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 5071 "StartRamp3 [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 5072 "Init Volt3 [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 5073 "Curr Lim3 [0.1*Ie]"
Unsigned16 40 15-70
EndExtUserPrmData

ExtUserPrmData = 5074 "3rd Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 5075 "Language - Read only"
Unsigned16 1 1-14
Prm_Text_Ref=5075
EndExtUserPrmData

ExtUserPrmData = 5079 "Date Type - Read only"
Unsigned16 0 0-2
Prm_Text_Ref=5079
EndExtUserPrmData

ExtUserPrmData = 5080 "Date Year - Read only"
Unsigned16 2002 1901-2038
EndExtUserPrmData

ExtUserPrmData = 5081 "Date Month - Read only"
Unsigned16 6 1-12
EndExtUserPrmData

ExtUserPrmData = 5082 "Date Day - Read only"
Unsigned16 15 1-31
EndExtUserPrmData

ExtUserPrmData = 5083 "Time Hour - Read only"
Unsigned16 12 0-23
EndExtUserPrmData

ExtUserPrmData = 5084 "Time Min - Read only"
Unsigned16 30 0-59
EndExtUserPrmData

ExtUserPrmData = 5097 "BP Close Op"
Unsigned16 0 0-1
Prm_Text_Ref=5044
EndExtUserPrmData

ExtUserPrmData = 5098 "BP Open Op"
Unsigned16 0 0-1
Prm_Text_Ref=5044
EndExtUserPrmData

ExtUserPrmData = 5106 "PST(B) [A] - Read only"
Unsigned16 100 1-2500
EndExtUserPrmData

ExtUserPrmData = 5111 "Current Limit Y Time [s]"
Unsigned16 0 0-120
EndExtUserPrmData

ExtUserPrmData = 5112 "Current Limit Y Level [0.1*Ie]"
Unsigned16 40 15-70
EndExtUserPrmData

ExtUserPrmData = 5113 "FB Auto Disable - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=5008
EndExtUserPrmData

ExtUserPrmData = 5114 "Start Mode"
Unsigned16 0 0-1
Prm_Text_Ref=5114
EndExtUserPrmData

ExtUserPrmData = 5115 "Stop Mode"
Unsigned16 0 0-1
Prm_Text_Ref=5114
EndExtUserPrmData

ExtUserPrmData = 5116 "Torque Limit [%]"
Unsigned16 150 20-200
EndExtUserPrmData

ExtUserPrmData = 5117 "Tune T-Ctrl [%]"
Unsigned16 100 30-300
EndExtUserPrmData

ExtUserPrmData = 5123 "Analogue Out"
Unsigned16 0 0-1
Prm_Text_Ref=5008
EndExtUserPrmData

ExtUserPrmData = 5124 "Anl Ref"
Unsigned16 1 0-2
Prm_Text_Ref=5124
EndExtUserPrmData

ExtUserPrmData = 5125 "Anl Type"
Unsigned16 0 0-8
Prm_Text_Ref=5125
EndExtUserPrmData

ExtUserPrmData = 5126 "I Range Max [A]"
Unsigned16 11000 1-20000
EndExtUserPrmData

ExtUserPrmData = 5127 "U Range Max [V]"
Unsigned16 600 10-1000
EndExtUserPrmData

ExtUserPrmData = 5128 "kW Range Max [0.1kW]"
Unsigned16 15000 1-30000
EndExtUserPrmData

ExtUserPrmData = 5129 "hp Range Max [0.1hp]"
Unsigned16 15000 1-30000
EndExtUserPrmData

ExtUserPrmData = 5130 "Q Range Max [0.1kVAr]"
Unsigned16 15000 1-30000
EndExtUserPrmData

ExtUserPrmData = 5131 "S Range Max [0.1kVA]"
Unsigned16 15000 1-30000
EndExtUserPrmData

ExtUserPrmData = 5132 "Imitate SW"
Unsigned16 8 0-8
Prm_Text_Ref=5132
EndExtUserPrmData


;=============================================================
; Text-definition for User Prm Data "Softstarter PST(V08)"
; Compatible with CU-version 05.05.00.
;=============================================================
;
PrmText = 5208
Text(0)   = "No"
Text(1)   = "Yes"
EndPrmText
PrmText = 5211
Text(0)   = "1-30s"
Text(1)   = "1-120s"
EndPrmText
PrmText = 5212
Text(0)   = "0-30s"
Text(1)   = "0-120s"
EndPrmText
PrmText = 5213
Text(0)   = "No"
Text(1)   = "Normal"
Text(2)   = "Dual"
EndPrmText
PrmText = 5214
Text(0)  = "Class 10A"
Text(1)  = "Class 10"
Text(2)  = "Class 20"
Text(3)  = "Class 30"
Text(4)  = "No"
EndPrmText
PrmText = 5217
Text(0)   = "Stop-M"
Text(1)   = "Stop-A"
Text(2)   = "Ind"
EndPrmText
PrmText = 5244
Text(0)   = "Stop-M"
Text(1)   = "Stop-A"
EndPrmText
PrmText = 5249
Text(0)  = "None"
Text(1)  = "Reset"
Text(2)  = "Enable"
Text(3)  = "Jog"
Text(4)  = "DOL-On"
Text(5)  = "Start2"
Text(6)  = "FB-Dis"
EndPrmText
PrmText = 5250
Text(0)  = "None"
Text(1)  = "Reset"
Text(2)  = "Enable"
Text(3)  = "Jog"
Text(4)  = "DOL-On"
Text(5)  = "Start3"
Text(6)  = "FB-Dis"
EndPrmText
PrmText = 5251
Text(0)   = "Run"
Text(1)   = "TOR"
Text(2)   = "Event"
EndPrmText
PrmText = 5260
Text(0)   = "AS-Int"
Text(1)   = "Other"
EndPrmText
PrmText = 5262
Text(1)   = "No"
Text(2)   = "2"
Text(3)   = "3"
EndPrmText
PrmText = 5275
Text(1)  = "US/UK"
Text(2)  = "FI"
Text(3)  = "SE"
Text(4)  = "PT"
Text(5)  = "NL"
Text(6)  = "IT"
Text(7)  = "FR"
Text(8)  = "ES"
Text(9)  = "DE"
Text(10) = "CN"
Text(11) = "RU"
Text(12) = "TR"
Text(13) = "PL"
Text(14) = "CZ"
EndPrmText
PrmText = 5279
Text(0)   = "ISO"
Text(1)   = "CE"
Text(2)   = "US"
EndPrmText
PrmText = 5314
Text(0)   = "Volt"
Text(1)   = "Torque"
EndPrmText
PrmText = 5324
Text(0)   = "0-20mA"
Text(1)   = "4-20mA"
Text(2)   = "0-10V"
EndPrmText
PrmText = 5325
Text(0)   = "I Amp"
Text(1)   = "U Volt"
Text(2)   = "P kW"
Text(3)   = "P hp"
Text(4)   = "Q kVAr"
Text(5)   = "S kVA"
Text(6)   = "TmpMot"
Text(7)   = "TmpSCR"
Text(8)   = "cosPhi"
EndPrmText
PrmText = 5332
Text(0)   = "010000"
Text(1)   = "010100"
Text(2)   = "020001"
Text(3)   = "030302"
Text(4)   = "030401"
Text(5)   = "030500"
Text(6)   = "040002"
Text(7)   = "050202"
Text(8)   = "050404"
Text(9)   = "050500"
EndPrmText
PrmText = 5333
Text(0)   = "Auto"
Text(1)   = "Line"
Text(2)   = "DeltaUI"
Text(3)   = "DeltaIU"
EndPrmText

ExtUserPrmData = 5201 "Setting Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 5202 "Start Ramp [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 5203 "Stop Ramp [s]"
Unsigned16 0 0-120
EndExtUserPrmData

ExtUserPrmData = 5204 "Init Volt [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 5205 "End Volt [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 5206 "Step Down [%]"
Unsigned16 100 30-100
EndExtUserPrmData

ExtUserPrmData = 5207 "Current Lim [0.1*Ie]"
Unsigned16 40 15-70
EndExtUserPrmData

ExtUserPrmData = 5208 "Kick Start"
Unsigned16 0 0-1
Prm_Text_Ref=5208
EndExtUserPrmData

ExtUserPrmData = 5209 "Kick Level [%]"
Unsigned16 50 50-100
EndExtUserPrmData

ExtUserPrmData = 5210 "Kick Time [0.01s]"
Unsigned16 20 10-150
EndExtUserPrmData

ExtUserPrmData = 5211 "Start Range"
Unsigned16 0 0-1
Prm_Text_Ref=5211
EndExtUserPrmData

ExtUserPrmData = 5212 "Stop Range"
Unsigned16 0 0-1
Prm_Text_Ref=5212
EndExtUserPrmData

ExtUserPrmData = 5213 "Overload"
Unsigned16 1 0-2
Prm_Text_Ref=5213
EndExtUserPrmData

ExtUserPrmData = 5214 "OL Class"
Unsigned16 1 0-3
Prm_Text_Ref=5214
EndExtUserPrmData

ExtUserPrmData = 5215 "OL Class S"
Unsigned16 1 0-4
Prm_Text_Ref=5214
EndExtUserPrmData

ExtUserPrmData = 5216 "OL Class R"
Unsigned16 1 0-4
Prm_Text_Ref=5214
EndExtUserPrmData

ExtUserPrmData = 5217 "OL Op"
Unsigned16 0 0-2
Prm_Text_Ref=5217
EndExtUserPrmData

ExtUserPrmData = 5218 "Locked Rotor"
Unsigned16 0 0-1
Prm_Text_Ref=5208
EndExtUserPrmData

ExtUserPrmData = 5219 "Lock R Lev [0.1*Ie]"
Unsigned16 40 5-80
EndExtUserPrmData

ExtUserPrmData = 5220 "Lock R Time [0.1s]"
Unsigned16 10 2-100
EndExtUserPrmData

ExtUserPrmData = 5221 "Lock R Op"
Unsigned16 0 0-2
Prm_Text_Ref=5217
EndExtUserPrmData

ExtUserPrmData = 5222 "Underload"
Unsigned16 0 0-1
Prm_Text_Ref=5208
EndExtUserPrmData

ExtUserPrmData = 5223 "Underl Lev [0.1*Ie]"
Unsigned16 5 4-8
EndExtUserPrmData

ExtUserPrmData = 5224 "Underl Time [s]"
Unsigned16 10 1-30
EndExtUserPrmData

ExtUserPrmData =5225 "Underl Op"
Unsigned16 0 0-2
Prm_Text_Ref=5217
EndExtUserPrmData

ExtUserPrmData = 5226 "Phase Imb"
Unsigned16 0 0-1
Prm_Text_Ref=5208
EndExtUserPrmData

ExtUserPrmData = 5227 "Ph Imb Lev [%]"
Unsigned16 80 10-80
EndExtUserPrmData

ExtUserPrmData = 5228 "Ph Imb Op"
Unsigned16 0 0-2
Prm_Text_Ref=5217
EndExtUserPrmData

ExtUserPrmData = 5229 "High I"
Unsigned16 0 0-1
Prm_Text_Ref=5208
EndExtUserPrmData

ExtUserPrmData = 5230 "High I Op"
Unsigned16 0 0-2
Prm_Text_Ref=5217
EndExtUserPrmData

ExtUserPrmData = 5231 "Phase Rev"
Unsigned16 0 0-1
Prm_Text_Ref=5208
EndExtUserPrmData

ExtUserPrmData = 5232 "Ph Rev Op"
Unsigned16 0 0-2
Prm_Text_Ref=5217
EndExtUserPrmData

ExtUserPrmData = 5233 "PTC"
Unsigned16 0 0-1
Prm_Text_Ref=5208
EndExtUserPrmData

ExtUserPrmData = 5234 "PTC Op"
Unsigned16 0 0-2
Prm_Text_Ref=5217
EndExtUserPrmData

ExtUserPrmData = 5235 "Ext ByPass"
Unsigned16 0 0-1
Prm_Text_Ref=5208
EndExtUserPrmData

ExtUserPrmData = 5237 "Warn I=High"
Unsigned16 0 0-1
Prm_Text_Ref=5208
EndExtUserPrmData

ExtUserPrmData = 5238 "Wa I=H Lev [0.1*Ie]"
Unsigned16 12 5-80
EndExtUserPrmData

ExtUserPrmData = 5239 "Warn I=Low"
Unsigned16 0 0-1
Prm_Text_Ref=5208
EndExtUserPrmData

ExtUserPrmData = 5240 "Wa I=L Lev [0.1*Ie]"
Unsigned16 8 4-10
EndExtUserPrmData

ExtUserPrmData = 5241 "Warn OL"
Unsigned16 0 0-1
Prm_Text_Ref=5208
EndExtUserPrmData

ExtUserPrmData = 5242 "Wa OL Lev [%]"
Unsigned16 90 40-99
EndExtUserPrmData

ExtUserPrmData = 5243 "Warn SCR OL"
Unsigned16 0 0-1
Prm_Text_Ref=5208
EndExtUserPrmData

ExtUserPrmData = 5244 "Ph Loss Op"
Unsigned16 0 0-1
Prm_Text_Ref=5244
EndExtUserPrmData

ExtUserPrmData = 5245 "FB Fault Op"
Unsigned16 0 0-1
Prm_Text_Ref=5244
EndExtUserPrmData

ExtUserPrmData = 5246 "Freq F Op"
Unsigned16 0 0-1
Prm_Text_Ref=5244
EndExtUserPrmData

ExtUserPrmData = 5247 "HC Temp Op"
Unsigned16 0 0-1
Prm_Text_Ref=5244
EndExtUserPrmData

ExtUserPrmData = 5248 "SCR SC Op"
Unsigned16 0 0-1
Prm_Text_Ref=5244
EndExtUserPrmData

ExtUserPrmData = 5249 "In0 - Read only"
Unsigned16 1 0-6
Prm_Text_Ref=5249
EndExtUserPrmData

ExtUserPrmData = 5250 "In1 - Read only"
Unsigned16 1 0-6
Prm_Text_Ref=5250
EndExtUserPrmData

ExtUserPrmData = 5251 "Relay K4"
Unsigned16 0 0-2
Prm_Text_Ref=5251
EndExtUserPrmData

ExtUserPrmData = 5252 "Relay K5"
Unsigned16 1 0-2
Prm_Text_Ref=5251
EndExtUserPrmData

ExtUserPrmData = 5253 "Relay K6"
Unsigned16 2 0-2
Prm_Text_Ref=5251
EndExtUserPrmData

ExtUserPrmData = 5254 "SW Outp V7"
Unsigned16 2 0-2
Prm_Text_Ref=5251
EndExtUserPrmData

ExtUserPrmData = 5255 "Event K4"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 5256 "Event K5"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 5257 "Event K6"
Unsigned16 7 0-65535
EndExtUserPrmData

ExtUserPrmData = 5258 "Event V7"
Unsigned16 7 0-65535
EndExtUserPrmData

ExtUserPrmData = 5259 "Fieldb Ctrl - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=5208
EndExtUserPrmData

ExtUserPrmData = 5260 "Fieldb Type - Read only"
Unsigned16 1 0-1
Prm_Text_Ref=5260
EndExtUserPrmData

ExtUserPrmData = 5261 "Fieldb Addr - Read only"
Unsigned16 0 0-1000
EndExtUserPrmData

ExtUserPrmData = 5262 "No of Seq"
Unsigned16 1 1-3
Prm_Text_Ref=5262
EndExtUserPrmData

ExtUserPrmData = 5263 "StartRamp1 [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 5264 "Init Volt1 [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 5265 "Curr Lim1 [0.1*Ie]"
Unsigned16 40 15-70
EndExtUserPrmData

ExtUserPrmData = 5266 "1st Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 5267 "StartRamp2 [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 5268 "Init Volt2 [%]"
Unsigned16 30 30-70
EndExtUserPrmData
;75
ExtUserPrmData = 5269 "Curr Lim2 [0.1*Ie]"
Unsigned16 40 15-70
EndExtUserPrmData

ExtUserPrmData = 5270 "2nd Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 5271 "StartRamp3 [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 5272 "Init Volt3 [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 5273 "Curr Lim3 [0.1*Ie]"
Unsigned16 40 15-70
EndExtUserPrmData

ExtUserPrmData = 5274 "3rd Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 5275 "Language - Read only"
Unsigned16 1 1-14
Prm_Text_Ref=5275
EndExtUserPrmData

ExtUserPrmData = 5279 "Date Type - Read only"
Unsigned16 0 0-2
Prm_Text_Ref=5279
EndExtUserPrmData

ExtUserPrmData = 5280 "Date Year - Read only"
Unsigned16 2002 1901-2038
EndExtUserPrmData

ExtUserPrmData = 5281 "Date Month - Read only"
Unsigned16 6 1-12
EndExtUserPrmData

ExtUserPrmData = 5282 "Date Day - Read only"
Unsigned16 15 1-31
EndExtUserPrmData

ExtUserPrmData = 5283 "Time Hour - Read only"
Unsigned16 12 0-23
EndExtUserPrmData

ExtUserPrmData = 5284 "Time Min - Read only"
Unsigned16 30 0-59
EndExtUserPrmData

ExtUserPrmData = 5297 "BP Close Op"
Unsigned16 0 0-1
Prm_Text_Ref=5244
EndExtUserPrmData

ExtUserPrmData = 5298 "BP Open Op"
Unsigned16 0 0-1
Prm_Text_Ref=5244
EndExtUserPrmData

ExtUserPrmData = 5306 "PST(B) [A] - Read only"
Unsigned16 100 1-2500
EndExtUserPrmData

ExtUserPrmData = 5311 "Current Limit Y Time [s]"
Unsigned16 0 0-120
EndExtUserPrmData

ExtUserPrmData = 5312 "Current Limit Y Level [0.1*Ie]"
Unsigned16 40 15-70
EndExtUserPrmData

ExtUserPrmData = 5313 "FB Auto Disable - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=5208
EndExtUserPrmData

ExtUserPrmData = 5314 "Start Mode"
Unsigned16 0 0-1
Prm_Text_Ref=5314
EndExtUserPrmData

ExtUserPrmData = 5315 "Stop Mode"
Unsigned16 0 0-1
Prm_Text_Ref=5314
EndExtUserPrmData

ExtUserPrmData = 5316 "Torque Limit [%]"
Unsigned16 150 20-200
EndExtUserPrmData

ExtUserPrmData = 5317 "Tune T-Ctrl [%]"
Unsigned16 100 30-300
EndExtUserPrmData

ExtUserPrmData = 5323 "Analogue Out"
Unsigned16 0 0-1
Prm_Text_Ref=5208
EndExtUserPrmData

ExtUserPrmData = 5324 "Anl Ref"
Unsigned16 1 0-2
Prm_Text_Ref=5324
EndExtUserPrmData

ExtUserPrmData = 5325 "Anl Type"
Unsigned16 0 0-8
Prm_Text_Ref=5325
EndExtUserPrmData

ExtUserPrmData = 5326 "I Range Max [A]"
Unsigned16 11000 1-20000
EndExtUserPrmData

ExtUserPrmData = 5327 "U Range Max [V]"
Unsigned16 600 10-1000
EndExtUserPrmData

ExtUserPrmData = 5328 "kW Range Max [0.1kW]"
Unsigned16 15000 1-30000
EndExtUserPrmData

ExtUserPrmData = 5329 "hp Range Max [0.1hp]"
Unsigned16 15000 1-30000
EndExtUserPrmData

ExtUserPrmData = 5330 "Q Range Max [0.1kVAr]"
Unsigned16 15000 1-30000
EndExtUserPrmData

ExtUserPrmData = 5331 "S Range Max [0.1kVA]"
Unsigned16 15000 1-30000
EndExtUserPrmData

ExtUserPrmData = 5332 "Imitate SW"
Unsigned16 9 0-9
Prm_Text_Ref=5332
EndExtUserPrmData

ExtUserPrmData = 5333 "Connection"
Unsigned16 0 0-3
Prm_Text_Ref=5333
EndExtUserPrmData


;=============================================================
; Text-definition for User Prm Data "Softstarter PST(V09)"
; Compatible with CU-version 06.00.00.
;=============================================================
;
PrmText = 5508
Text(0)   = "No"
Text(1)   = "Yes"
EndPrmText
PrmText = 5511
Text(0)   = "1-30s"
Text(1)   = "1-120s"
EndPrmText
PrmText = 5512
Text(0)   = "0-30s"
Text(1)   = "0-120s"
EndPrmText
PrmText = 5513
Text(0)   = "No"
Text(1)   = "Normal"
Text(2)   = "Dual"
EndPrmText
PrmText = 5514
Text(0)  = "Class 10A"
Text(1)  = "Class 10"
Text(2)  = "Class 20"
Text(3)  = "Class 30"
Text(4)  = "No"
EndPrmText
PrmText = 5517
Text(0)   = "Stop-M"
Text(1)   = "Stop-A"
Text(2)   = "Ind"
EndPrmText
PrmText = 5544
Text(0)   = "Stop-M"
Text(1)   = "Stop-A"
EndPrmText
PrmText = 5549
Text(0)  = "None"
Text(1)  = "Reset"
Text(2)  = "Enable"
Text(3)  = "Jog"
Text(4)  = "DOL-On"
Text(5)  = "Start2"
Text(6)  = "FB-Dis"
EndPrmText
PrmText = 5550
Text(0)  = "None"
Text(1)  = "Reset"
Text(2)  = "Enable"
Text(3)  = "Jog"
Text(4)  = "DOL-On"
Text(5)  = "Start3"
Text(6)  = "FB-Dis"
EndPrmText
PrmText = 5551
Text(0)   = "Run"
Text(1)   = "TOR"
Text(2)   = "Event"
EndPrmText
PrmText = 5560
Text(0)   = "AS-Int"
Text(1)   = "Other"
EndPrmText
PrmText = 5562
Text(1)   = "No"
Text(2)   = "2"
Text(3)   = "3"
EndPrmText
PrmText = 5575
Text(1)  = "US/UK"
Text(2)  = "FI"
Text(3)  = "SE"
Text(4)  = "PT"
Text(5)  = "NL"
Text(6)  = "IT"
Text(7)  = "FR"
Text(8)  = "ES"
Text(9)  = "DE"
Text(10) = "CN"
Text(11) = "RU"
Text(12) = "TR"
Text(13) = "PL"
Text(14) = "CZ"
EndPrmText
PrmText = 5579
Text(0)   = "ISO"
Text(1)   = "CE"
Text(2)   = "US"
EndPrmText
PrmText = 5614
Text(0)   = "Volt"
Text(1)   = "Torque"
EndPrmText
PrmText = 5624
Text(0)   = "0-20mA"
Text(1)   = "4-20mA"
Text(2)   = "0-10V"
EndPrmText
PrmText = 5625
Text(0)   = "I Amp"
Text(1)   = "U Volt"
Text(2)   = "P kW"
Text(3)   = "P hp"
Text(4)   = "Q kVAr"
Text(5)   = "S kVA"
Text(6)   = "TmpMot"
Text(7)   = "TmpSCR"
Text(8)   = "cosPhi"
EndPrmText
PrmText = 5632
Text(0)   = "010000"
Text(1)   = "010100"
Text(2)   = "020001"
Text(3)   = "030302"
Text(4)   = "030401"
Text(5)   = "030500"
Text(6)   = "040002"
Text(7)   = "050202"
Text(8)   = "050404"
Text(9)   = "050500"
Text(10)  = "060000"
EndPrmText
PrmText = 5633
Text(0)   = "Auto"
Text(1)   = "Line"
Text(2)   = "DeltaUI"
Text(3)   = "DeltaIU"
EndPrmText

ExtUserPrmData = 5501 "Setting Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 5502 "Start Ramp [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 5503 "Stop Ramp [s]"
Unsigned16 0 0-120
EndExtUserPrmData

ExtUserPrmData = 5504 "Init Volt [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 5505 "End Volt [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 5506 "Step Down [%]"
Unsigned16 100 30-100
EndExtUserPrmData

ExtUserPrmData = 5507 "Current Lim [0.1*Ie]"
Unsigned16 40 15-70
EndExtUserPrmData

ExtUserPrmData = 5508 "Kick Start"
Unsigned16 0 0-1
Prm_Text_Ref=5508
EndExtUserPrmData

ExtUserPrmData = 5509 "Kick Level [%]"
Unsigned16 50 50-100
EndExtUserPrmData

ExtUserPrmData = 5510 "Kick Time [0.01s]"
Unsigned16 20 10-150
EndExtUserPrmData

ExtUserPrmData = 5511 "Start Range"
Unsigned16 0 0-1
Prm_Text_Ref=5511
EndExtUserPrmData

ExtUserPrmData = 5512 "Stop Range"
Unsigned16 0 0-1
Prm_Text_Ref=5512
EndExtUserPrmData

ExtUserPrmData = 5513 "Overload"
Unsigned16 1 0-2
Prm_Text_Ref=5513
EndExtUserPrmData

ExtUserPrmData = 5514 "OL Class"
Unsigned16 1 0-3
Prm_Text_Ref=5514
EndExtUserPrmData

ExtUserPrmData = 5515 "OL Class S"
Unsigned16 1 0-4
Prm_Text_Ref=5514
EndExtUserPrmData

ExtUserPrmData = 5516 "OL Class R"
Unsigned16 1 0-4
Prm_Text_Ref=5514
EndExtUserPrmData

ExtUserPrmData = 5517 "OL Op"
Unsigned16 0 0-2
Prm_Text_Ref=5517
EndExtUserPrmData

ExtUserPrmData = 5518 "Locked Rotor"
Unsigned16 0 0-1
Prm_Text_Ref=5508
EndExtUserPrmData

ExtUserPrmData = 5519 "Lock R Lev [0.1*Ie]"
Unsigned16 40 5-80
EndExtUserPrmData

ExtUserPrmData = 5520 "Lock R Time [0.1s]"
Unsigned16 10 2-100
EndExtUserPrmData

ExtUserPrmData = 5521 "Lock R Op"
Unsigned16 0 0-2
Prm_Text_Ref=5517
EndExtUserPrmData

ExtUserPrmData = 5522 "Underload"
Unsigned16 0 0-1
Prm_Text_Ref=5508
EndExtUserPrmData

ExtUserPrmData = 5523 "Underl Lev [0.1*Ie]"
Unsigned16 5 4-8
EndExtUserPrmData

ExtUserPrmData = 5524 "Underl Time [s]"
Unsigned16 10 1-30
EndExtUserPrmData

ExtUserPrmData =5525 "Underl Op"
Unsigned16 0 0-2
Prm_Text_Ref=5517
EndExtUserPrmData

ExtUserPrmData = 5526 "Phase Imb"
Unsigned16 0 0-1
Prm_Text_Ref=5508
EndExtUserPrmData

ExtUserPrmData = 5527 "Ph Imb Lev [%]"
Unsigned16 80 10-80
EndExtUserPrmData

ExtUserPrmData = 5528 "Ph Imb Op"
Unsigned16 0 0-2
Prm_Text_Ref=5517
EndExtUserPrmData

ExtUserPrmData = 5529 "High I"
Unsigned16 0 0-1
Prm_Text_Ref=5508
EndExtUserPrmData

ExtUserPrmData = 5530 "High I Op"
Unsigned16 0 0-2
Prm_Text_Ref=5517
EndExtUserPrmData

ExtUserPrmData = 5531 "Phase Rev"
Unsigned16 0 0-1
Prm_Text_Ref=5508
EndExtUserPrmData

ExtUserPrmData = 5532 "Ph Rev Op"
Unsigned16 0 0-2
Prm_Text_Ref=5517
EndExtUserPrmData

ExtUserPrmData = 5533 "PTC"
Unsigned16 0 0-1
Prm_Text_Ref=5508
EndExtUserPrmData

ExtUserPrmData = 5534 "PTC Op"
Unsigned16 0 0-2
Prm_Text_Ref=5517
EndExtUserPrmData

ExtUserPrmData = 5535 "Ext ByPass"
Unsigned16 0 0-1
Prm_Text_Ref=5508
EndExtUserPrmData

ExtUserPrmData = 5537 "Warn I=High"
Unsigned16 0 0-1
Prm_Text_Ref=5508
EndExtUserPrmData

ExtUserPrmData = 5538 "Wa I=H Lev [0.1*Ie]"
Unsigned16 12 5-80
EndExtUserPrmData

ExtUserPrmData = 5539 "Warn I=Low"
Unsigned16 0 0-1
Prm_Text_Ref=5508
EndExtUserPrmData

ExtUserPrmData = 5540 "Wa I=L Lev [0.1*Ie]"
Unsigned16 8 4-10
EndExtUserPrmData

ExtUserPrmData = 5541 "Warn OL"
Unsigned16 0 0-1
Prm_Text_Ref=5508
EndExtUserPrmData

ExtUserPrmData = 5542 "Wa OL Lev [%]"
Unsigned16 90 40-99
EndExtUserPrmData

ExtUserPrmData = 5543 "Warn SCR OL"
Unsigned16 0 0-1
Prm_Text_Ref=5508
EndExtUserPrmData

ExtUserPrmData = 5544 "Ph Loss Op"
Unsigned16 0 0-1
Prm_Text_Ref=5544
EndExtUserPrmData

ExtUserPrmData = 5545 "FB Fault Op"
Unsigned16 0 0-1
Prm_Text_Ref=5544
EndExtUserPrmData

ExtUserPrmData = 5546 "Freq F Op"
Unsigned16 0 0-1
Prm_Text_Ref=5544
EndExtUserPrmData

ExtUserPrmData = 5547 "HC Temp Op"
Unsigned16 0 0-1
Prm_Text_Ref=5544
EndExtUserPrmData

ExtUserPrmData = 5548 "SCR SC Op"
Unsigned16 0 0-1
Prm_Text_Ref=5544
EndExtUserPrmData

ExtUserPrmData = 5549 "In0 - Read only"
Unsigned16 1 0-6
Prm_Text_Ref=5549
EndExtUserPrmData

ExtUserPrmData = 5550 "In1 - Read only"
Unsigned16 1 0-6
Prm_Text_Ref=5550
EndExtUserPrmData

ExtUserPrmData = 5551 "Relay K4"
Unsigned16 0 0-2
Prm_Text_Ref=5551
EndExtUserPrmData

ExtUserPrmData = 5552 "Relay K5"
Unsigned16 1 0-2
Prm_Text_Ref=5551
EndExtUserPrmData

ExtUserPrmData = 5553 "Relay K6"
Unsigned16 2 0-2
Prm_Text_Ref=5551
EndExtUserPrmData

ExtUserPrmData = 5554 "SW Outp V7"
Unsigned16 2 0-2
Prm_Text_Ref=5551
EndExtUserPrmData

ExtUserPrmData = 5555 "Event K4"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 5556 "Event K5"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 5557 "Event K6"
Unsigned16 7 0-65535
EndExtUserPrmData

ExtUserPrmData = 5558 "Event V7"
Unsigned16 7 0-65535
EndExtUserPrmData

ExtUserPrmData = 5559 "Fieldb Ctrl - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=5508
EndExtUserPrmData

ExtUserPrmData = 5560 "Fieldb Type - Read only"
Unsigned16 1 0-1
Prm_Text_Ref=5560
EndExtUserPrmData

ExtUserPrmData = 5561 "Fieldb Addr - Read only"
Unsigned16 0 0-1000
EndExtUserPrmData

ExtUserPrmData = 5562 "No of Seq"
Unsigned16 1 1-3
Prm_Text_Ref=5562
EndExtUserPrmData

ExtUserPrmData = 5563 "StartRamp1 [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 5564 "Init Volt1 [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 5565 "Curr Lim1 [0.1*Ie]"
Unsigned16 40 15-70
EndExtUserPrmData

ExtUserPrmData = 5566 "1st Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 5567 "StartRamp2 [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 5568 "Init Volt2 [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 5569 "Curr Lim2 [0.1*Ie]"
Unsigned16 40 15-70
EndExtUserPrmData

ExtUserPrmData = 5570 "2nd Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 5571 "StartRamp3 [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 5572 "Init Volt3 [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 5573 "Curr Lim3 [0.1*Ie]"
Unsigned16 40 15-70
EndExtUserPrmData

ExtUserPrmData = 5574 "3rd Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 5575 "Language - Read only"
Unsigned16 1 1-14
Prm_Text_Ref=5575
EndExtUserPrmData

ExtUserPrmData = 5579 "Date Type - Read only"
Unsigned16 0 0-2
Prm_Text_Ref=5579
EndExtUserPrmData

ExtUserPrmData = 5580 "Date Year - Read only"
Unsigned16 2000 2000-2065
EndExtUserPrmData

ExtUserPrmData = 5581 "Date Month - Read only"
Unsigned16 1 1-12
EndExtUserPrmData

ExtUserPrmData = 5582 "Date Day - Read only"
Unsigned16 1 1-31
EndExtUserPrmData

ExtUserPrmData = 5583 "Time Hour - Read only"
Unsigned16 0 0-23
EndExtUserPrmData

ExtUserPrmData = 5584 "Time Min - Read only"
Unsigned16 0 0-59
EndExtUserPrmData

ExtUserPrmData = 5597 "BP Close Op"
Unsigned16 0 0-1
Prm_Text_Ref=5544
EndExtUserPrmData

ExtUserPrmData = 5598 "BP Open Op"
Unsigned16 0 0-1
Prm_Text_Ref=5544
EndExtUserPrmData

ExtUserPrmData = 5606 "PST(B) [A] - Read only"
Unsigned16 100 1-2500
EndExtUserPrmData

ExtUserPrmData = 5611 "Current Limit Y Time [s]"
Unsigned16 0 0-120
EndExtUserPrmData

ExtUserPrmData = 5612 "Current Limit Y Level [0.1*Ie]"
Unsigned16 40 15-70
EndExtUserPrmData

ExtUserPrmData = 5613 "FB Auto Disable - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=5508
EndExtUserPrmData

ExtUserPrmData = 5614 "Start Mode"
Unsigned16 0 0-1
Prm_Text_Ref=5614
EndExtUserPrmData

ExtUserPrmData = 5615 "Stop Mode"
Unsigned16 0 0-1
Prm_Text_Ref=5614
EndExtUserPrmData

ExtUserPrmData = 5616 "Torque Limit [%]"
Unsigned16 150 20-200
EndExtUserPrmData

ExtUserPrmData = 5617 "Tune T-Ctrl [%]"
Unsigned16 100 30-300
EndExtUserPrmData

ExtUserPrmData = 5623 "Analogue Out"
Unsigned16 0 0-1
Prm_Text_Ref=5508
EndExtUserPrmData

ExtUserPrmData = 5624 "Anl Ref"
Unsigned16 1 0-2
Prm_Text_Ref=5624
EndExtUserPrmData

ExtUserPrmData = 5625 "Anl Type"
Unsigned16 0 0-8
Prm_Text_Ref=5625
EndExtUserPrmData

ExtUserPrmData = 5626 "I Range Max [A]"
Unsigned16 11000 1-20000
EndExtUserPrmData

ExtUserPrmData = 5627 "U Range Max [V]"
Unsigned16 600 10-1000
EndExtUserPrmData

ExtUserPrmData = 5628 "kW Range Max [0.1kW]"
Unsigned16 15000 1-30000
EndExtUserPrmData

ExtUserPrmData = 5629 "hp Range Max [0.1hp]"
Unsigned16 15000 1-30000
EndExtUserPrmData

ExtUserPrmData = 5630 "Q Range Max [0.1kVAr]"
Unsigned16 15000 1-30000
EndExtUserPrmData

ExtUserPrmData = 5631 "S Range Max [0.1kVA]"
Unsigned16 15000 1-30000
EndExtUserPrmData

ExtUserPrmData = 5632 "Imitate SW"
Unsigned16 10 0-10
Prm_Text_Ref=5632
EndExtUserPrmData

ExtUserPrmData = 5633 "Connection"
Unsigned16 0 0-3
Prm_Text_Ref=5633
EndExtUserPrmData


;=============================================================
; Definition for Ext User Prm Data "Wireless WDI100"
;=============================================================
;
; Cell ID WDI100
; Default 0, Bereich 0__59
ExtUserPrmData = 500 "Cell-ID"
Unsigned16 0 0-59		
EndExtUserPrmData

ExtUserPrmData = 501 "WSIX  15-0"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 502 "WSIX  31-16" 
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 503 "WSIX  47-32"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 504 "WSIX  63-48"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 505 "WSIX  79-64"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 506 "WSIX  95-80"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 507 "WSIX 111-96"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 508 "WSIX 119-112"
Unsigned16 0 0-255
EndExtUserPrmData


;==================================================================
; Definition for Ext User Prm Data "Wireless WDIO100 - WDI/WDX/WDP"
;==================================================================
;
PrmText = 600
Text(0)   = "On"
Text(1)   = "Off"
EndPrmText

PrmText = 601
Text(0)   = "AUTO ACK"
Text(1)   = "WDIO100 ACK"
EndPrmText

PrmText = 602
Text(0)   = "Zero"
Text(1)   = "Keep"
EndPrmText

PrmText = 603
Text(0)   = "1ms"
Text(1)   = "5ms"
Text(2)   = "25ms"
EndPrmText



; Cell ID WDI100
; Default 1, Bereich 1__59
ExtUserPrmData = 604 "Cell-ID"
Unsigned16 1 1-59		
EndExtUserPrmData

ExtUserPrmData = 605 "WSIX  15-0"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 606 "WSIX  31-16" 
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 607 "WSIX  47-32"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 608 "WSIX  63-48"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 609 "WSIX  79-64"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 610 "WSIX  95-80"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 611 "WSIX 111-96"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 612 "WSIX 119-112"
Unsigned16 0 0-255
EndExtUserPrmData

ExtUserPrmData = 616 "ANTENNA SWITCH"
Unsigned16 0 0-1
Prm_Text_Ref=600
EndExtUserPrmData


;=============================================================
; Definition for Ext User Prm Data "Wireless WDIO100-WDX"
;=============================================================
;
; WDIO100 max 7 I/O Pads

ExtUserPrmData = 613 "WSIX  55-48"
Unsigned16 0 0-255
EndExtUserPrmData

ExtUserPrmData = 614 "WDP  6-0"
Unsigned16 0 0-127
EndExtUserPrmData

;=============================================================
; Definition for Ext User Prm Data "Wireless WDIO100-WDP"
;=============================================================
;
; WDIOP100 max 13 I/O Pads

ExtUserPrmData = 615 "WDP  12-0"
Unsigned16 0 0-8191
EndExtUserPrmData

;=============================================================
; Definition for Ext User Prm Data "Wireless WDIO100-WDX/WDP"
;=============================================================
;
ExtUserPrmData = 617 "WDP ERROR ACK"
Unsigned16 0 0-1
Prm_Text_Ref=601
EndExtUserPrmData

ExtUserPrmData = 618 "FAILSAFE MODE"
Unsigned16 0 0-1
Prm_Text_Ref=602
EndExtUserPrmData

ExtUserPrmData = 619 "FILTER TIME"
Unsigned16 0 0-2
Prm_Text_Ref=603
EndExtUserPrmData




;=============================================================
; Text-definition for User Prm Data  "VOGEL_LUB"
;=============================================================
; Anfang System 1
ExtUserPrmData = 4000 "Sys0 P31,parameter 0"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4001 "Sys0 P31,parameter 1"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4002 "Sys0 P31,parameter 2"
Unsigned8 0 0-255 
EndExtUserPrmData

ExtUserPrmData = 4003 "Sys0 P31,parameter 3"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4004 "Sys0 P32,parameter 0"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4005 "Sys0 P32,parameter 1"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4006 "Sys0 P32,parameter 2"
Unsigned8 0 0-255 
EndExtUserPrmData

ExtUserPrmData = 4007 "Sys0 P32,parameter 3"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4008 "Sys0 ADD_PAR_0"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4009 "Sys0 ADD_PAR_1"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4010 "Sys0 ADD_PAR_2"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4011 "Sys0 ADD_PAR_3"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4012 "Sys0 ADD_PAR_4"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4013 "Sys0 ADD_PAR_5"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4014 "Sys0 ADD_PAR_6"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4015 "Sys0 ADD_PAR_7"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4016 "Sys0 ADD_PAR_8"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4017 "Sys0 ADD_PAR_9"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4018 "Sys0 ADD_PAR_10"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4019 "Sys0 ADD_PAR_11"
Unsigned8 0 0-255
EndExtUserPrmData


ExtUserPrmData = 4020 "Sys0 ADD_PAR_12"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4021 "Sys0 ADD_PAR_13"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4022 "Sys0 ADD_PAR_14"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4023 "Sys0 ADD_PAR_15"
Unsigned8 0 0-255
EndExtUserPrmData

;Ende System 1




;Anfang System 2
ExtUserPrmData = 4024 "Sys0 P31,parameter 0"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4025 "Sys0 P31,parameter 1"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4026 "Sys0 P31,parameter 2"
Unsigned8 0 0-255 
EndExtUserPrmData

ExtUserPrmData = 4027 "Sys0 P31,parameter 3"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4028 "Sys0 P32,parameter 0"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4029 "Sys0 P32,parameter 1"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4030 "Sys0 P32,parameter 2"
Unsigned8 0 0-255 
EndExtUserPrmData

ExtUserPrmData = 4031 "Sys0 P32,parameter 3"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4032 "SYS0 ADD_PAR_0"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4033 "SYS0 ADD_PAR_1"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4034 "SYS0 ADD_PAR_2"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4035 "SYS0 ADD_PAR_3"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4036 "SYS0 ADD_PAR_4"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4037 "SYS0 ADD_PAR_5"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4038 "SYS0 ADD_PAR_6"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4039 "SYS0 ADD_PAR_7"
Unsigned8 0 0-255
EndExtUserPrmData


ExtUserPrmData = 4040 "SYS0 ADD_PAR_8"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4041 "SYS0 ADD_PAR_9"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4042 "SYS0 ADD_PAR_10"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4043 "SYS0 ADD_PAR_11"
Unsigned8 0 0-255
EndExtUserPrmData


ExtUserPrmData = 4044 "SYS0 ADD_PAR_12"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4045 "SYS0 ADD_PAR_13"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4046 "SYS0 ADD_PAR_14"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4047 "SYS0 ADD_PAR_15"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4048 "Sys1 P31,parameter 0"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4049 "Sys1 P31,parameter 1"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4050 "Sys1 P31,parameter 2"
Unsigned8 0 0-255 
EndExtUserPrmData

ExtUserPrmData = 4051 "Sys1 P31,parameter 3"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4052 "Sys1 P32,parameter 0"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4053 "Sys1 P32,parameter 1"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4054 "Sys1 P32,parameter 2"
Unsigned8 0 0-255 
EndExtUserPrmData

ExtUserPrmData = 4055 "Sys1 P32,parameter 3"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4056 "SYS1 ADD_PAR_0"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4057 "SYS1 ADD_PAR_1"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4058 "SYS1 ADD_PAR_2"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4059 "SYS1 ADD_PAR_3"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4060 "SYS1 ADD_PAR_4"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4061 "SYS1 ADD_PAR_5"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4062 "SYS1 ADD_PAR_6"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4063 "SYS1 ADD_PAR_7"
Unsigned8 0 0-255
EndExtUserPrmData


ExtUserPrmData = 4064 "SYS1 ADD_PAR_8"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4065 "SYS1 ADD_PAR_9"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4066 "SYS1 ADD_PAR_10"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4067 "SYS1 ADD_PAR_11"
Unsigned8 0 0-255
EndExtUserPrmData


ExtUserPrmData = 4068 "SYS1 ADD_PAR_12"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4069 "SYS1 ADD_PAR_13"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4070 "SYS1 ADD_PAR_14"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4071 "SYS1 ADD_PAR_15"
Unsigned8 0 0-255
EndExtUserPrmData
; Ende System 2

;start analogsystem mit aerosolsensor
;=============================================================
; Text-definition for User Prm Data  "VOGEL_LUB"
;=============================================================
; Anfang System 1
ExtUserPrmData = 4072 "Sys0 P31,parameter 0"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4073 "Sys0 P31,parameter 1"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4074 "Sys0 P31,parameter 2"
Unsigned8 0 0-255 
EndExtUserPrmData

ExtUserPrmData = 4075 "Sys0 P31,parameter 3"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4076 "Sys0 P32,parameter 0"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4077 "Sys0 P32,parameter 1"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4078 "Sys0 P32,parameter 2"
Unsigned8 0 0-255 
EndExtUserPrmData

ExtUserPrmData = 4079 "Sys0 P32,parameter 3"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4080 "Sys0 ADD_PAR_0"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4081 "Sys0 ADD_PAR_1"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4082 "Sys0 ADD_PAR_2"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4083 "Sys0 ADD_PAR_3"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4084 "Sys0 ADD_PAR_4"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4085 "Sys0 ADD_PAR_5"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4086 "Sys0 ADD_PAR_6"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4087 "Sys0 ADD_PAR_7"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4088 "Sys0 ADD_PAR_8"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4089 "Sys0 ADD_PAR_9"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4090 "Sys0 ADD_PAR_10"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4091 "Sys0 ADD_PAR_11"
Unsigned8 0 0-255
EndExtUserPrmData


ExtUserPrmData = 4092 "Sys0 ADD_PAR_12"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4093 "Sys0 ADD_PAR_13"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4094 "Sys0 ADD_PAR_14"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4095 "Sys0 ADD_PAR_15"
Unsigned8 0 0-255
EndExtUserPrmData

;Ende System 1 analog


; Anfang System 2 analog
;Anfang System 2
ExtUserPrmData = 4096 "Sys0 P31,parameter 0"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4097 "Sys0 P31,parameter 1"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4098 "Sys0 P31,parameter 2"
Unsigned8 0 0-255 
EndExtUserPrmData

ExtUserPrmData = 4099 "Sys0 P31,parameter 3"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4100 "Sys0 P32,parameter 0"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4101 "Sys0 P32,parameter 1"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4102 "Sys0 P32,parameter 2"
Unsigned8 0 0-255 
EndExtUserPrmData

ExtUserPrmData = 4103 "Sys0 P32,parameter 3"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4104 "SYS0 ADD_PAR_0"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4105 "SYS0 ADD_PAR_1"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4106 "SYS0 ADD_PAR_2"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4107 "SYS0 ADD_PAR_3"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4108 "SYS0 ADD_PAR_4"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4109 "SYS0 ADD_PAR_5"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4110 "SYS0 ADD_PAR_6"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4111 "SYS0 ADD_PAR_7"
Unsigned8 0 0-255
EndExtUserPrmData


ExtUserPrmData = 4112 "SYS0 ADD_PAR_8"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4113 "SYS0 ADD_PAR_9"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4114 "SYS0 ADD_PAR_10"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4115 "SYS0 ADD_PAR_11"
Unsigned8 0 0-255
EndExtUserPrmData


ExtUserPrmData = 4116 "SYS0 ADD_PAR_12"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4117 "SYS0 ADD_PAR_13"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4118 "SYS0 ADD_PAR_14"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4119 "SYS0 ADD_PAR_15"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4120 "Sys1 P31,parameter 0"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4121 "Sys1 P31,parameter 1"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4122 "Sys1 P31,parameter 2"
Unsigned8 0 0-255 
EndExtUserPrmData

ExtUserPrmData = 4123 "Sys1 P31,parameter 3"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4124 "Sys1 P32,parameter 0"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4125 "Sys1 P32,parameter 1"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4126 "Sys1 P32,parameter 2"
Unsigned8 0 0-255 
EndExtUserPrmData

ExtUserPrmData = 4127 "Sys1 P32,parameter 3"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4128 "SYS1 ADD_PAR_0"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4129 "SYS1 ADD_PAR_1"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4130 "SYS1 ADD_PAR_2"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4131 "SYS1 ADD_PAR_3"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4132 "SYS1 ADD_PAR_4"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4133 "SYS1 ADD_PAR_5"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4134 "SYS1 ADD_PAR_6"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4135 "SYS1 ADD_PAR_7"
Unsigned8 0 0-255
EndExtUserPrmData


ExtUserPrmData = 4136 "SYS1 ADD_PAR_8"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4137 "SYS1 ADD_PAR_9"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4138 "SYS1 ADD_PAR_10"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4139 "SYS1 ADD_PAR_11"
Unsigned8 0 0-255
EndExtUserPrmData


ExtUserPrmData = 4140 "SYS1 ADD_PAR_12"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4141 "SYS1 ADD_PAR_13"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4142 "SYS1 ADD_PAR_14"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 4143 "SYS1 ADD_PAR_15"
Unsigned8 0 0-255
EndExtUserPrmData
; Ende System 2 analog



;==================================================================
; Definition for Ext User Prm Data "Lincoln LMC1_GLAS"
;==================================================================
;
ExtUserPrmData = 4565 "ZyklusV1_UeberwachungS1"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 4566 "ZyklusV2_UeberwachungS2"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 4567 "ZyklusV3_UeberwachungM"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 4568 "Ausschaltverzoegerung"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 4570 "Haltezeit"
Unsigned16 0 0-65535
EndExtUserPrmData


;=============================================================
; Text-definition for User Prm Data "Softstarter PSE"
;=============================================================
;
PrmText = 5403
Text(0)   = "Off"
Text(1)   = "On"
EndPrmText
PrmText = 5414
Text(0)  = "Class 10A"
Text(1)  = "Class 10"
Text(2)  = "Class 20"
Text(3)  = "Class 30"
EndPrmText
PrmText = 5415
Text(0)   = "Hand"
Text(1)   = "Auto"
EndPrmText

ExtUserPrmData = 5401 "Setting Ie [0.1A]"
Unsigned16 1 0-3700
EndExtUserPrmData

ExtUserPrmData = 5402 "Start Ramp [s]"
Unsigned16 10 1-30
EndExtUserPrmData

ExtUserPrmData = 5403 "Stop R On"
Unsigned16 0 0-1
Prm_Text_Ref=5403
EndExtUserPrmData

ExtUserPrmData = 5404 "Stop Ramp [s]"
Unsigned16 1 0-30
EndExtUserPrmData

ExtUserPrmData = 5405 "Init Volt [%]"
Unsigned16 40 30-70
EndExtUserPrmData

ExtUserPrmData = 5406 "End Volt [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 5407 "Curr Lim [0.1*Ie]"
Unsigned16 70 15-70
EndExtUserPrmData

ExtUserPrmData = 5408 "Trq Start"
Unsigned16 0 0-1
Prm_Text_Ref=5403
EndExtUserPrmData

ExtUserPrmData = 5409 "Trq Stop"
Unsigned16 0 0-1
Prm_Text_Ref=5403
EndExtUserPrmData

ExtUserPrmData = 5410 "Kick Start"
Unsigned16 0 0-1
Prm_Text_Ref=5403
EndExtUserPrmData

ExtUserPrmData = 5411 "Kick Time [0.1s]"
Unsigned16 2 1-10
EndExtUserPrmData

ExtUserPrmData = 5412 "Kick Volt [%]"
Unsigned16 50 30-100
EndExtUserPrmData

ExtUserPrmData = 5413 "EOL On"
Unsigned16 1 0-1
Prm_Text_Ref=5403
EndExtUserPrmData

ExtUserPrmData = 5414 "EOL Class"
Unsigned16 1 0-3
Prm_Text_Ref=5414
EndExtUserPrmData

ExtUserPrmData = 5415 "EOL Op"
Unsigned16 0 0-1
Prm_Text_Ref=5415
EndExtUserPrmData

ExtUserPrmData = 5416 "Underload"
Unsigned16 0 0-1
Prm_Text_Ref=5403
EndExtUserPrmData

ExtUserPrmData = 5417 "Underl Lev [0.1*Ie]"
Unsigned16 5 2-10
EndExtUserPrmData

ExtUserPrmData =5418 "Underl Op"
Unsigned16 0 0-1
Prm_Text_Ref=5415
EndExtUserPrmData

ExtUserPrmData = 5419 "Locked R"
Unsigned16 0 0-1
Prm_Text_Ref=5403
EndExtUserPrmData

ExtUserPrmData = 5420 "Lock R Lev [0.1*Ie]"
Unsigned16 12 5-70
EndExtUserPrmData

ExtUserPrmData = 5421 "Lock Op"
Unsigned16 0 0-1
Prm_Text_Ref=5415
EndExtUserPrmData

ExtUserPrmData = 5422 "Bad Net Op"
Unsigned16 0 0-1
Prm_Text_Ref=5415
EndExtUserPrmData



;=====================================================================
; special Parameter-Definitions for DPV1-Plug PDP22
;=====================================================================
PrmText = 10000
Text(0)   = "Use Block-Parameters"
Text(1)   = "Ignore Block-Parameters"
EndPrmText

PrmText = 10001
Text(0)   = "DPV0 Diagnosis Format"
Text(1)   = "DPV1 Diagnosis Format"
EndPrmText

ExtUserPrmData=10000	"Block-Parameter"	
Unsigned8 0 0-1    								
Prm_Text_Ref=10000
EndExtUserPrmData

ExtUserPrmData=10001	"Diagnosis Format"	
Unsigned8 0 0-1    								
Prm_Text_Ref=10001
EndExtUserPrmData

;
;===========================================================
;General parameters
;===========================================================
;
GSD_Revision   =3
Vendor_Name    ="ABB"
Model_Name      ="PDP22-FBP (V1)"
Revision       ="V 2.07"
Ident_Number   =0x082D
Protocol_Ident =0
Station_Type   =0
FMS_supp       =0
Hardware_Release= "V 1.0"
Software_Release= "V 1.0"
9.6_supp       =1
19.2_supp      =1
31.25_supp     =0
45.45_supp     =1
93.75_supp     =1
187.5_supp     =1
500_supp       =1
1.5M_supp      =1
3M_supp        =1
6M_supp        =1
12M_supp       =1
MaxTsdr_9.6    =15
MaxTsdr_19.2   =15
MaxTsdr_31.25  =15
MaxTsdr_45.45  =15
MaxTsdr_93.75  =15
MaxTsdr_187.5  =15
MaxTsdr_500    =15
MaxTsdr_1.5M   =20
MaxTsdr_3M     =35
MaxTsdr_6M     =50
MaxTsdr_12M    =95
Redundancy     =0
Repeater_Ctrl_Sig=0
24V_Pins       =1
Implementation_Type ="VPC3 solution"
Bitmap_Device       ="FBP_N"
Bitmap_Diag         ="FBP_DIAG"
Bitmap_SF           ="FBP_RUN"
;
;================================
; Slave-Specification:
;================================
;
Freeze_Mode_supp    =1
Sync_Mode_supp      =1
Set_Slave_Add_Supp  =0
Auto_Baud_supp      =1
Min_Slave_Intervall =1
Fail_Safe           =1
Max_Diag_Data_Len   =19
Modul_Offset        =0
Slave_Family=9@FieldBusPlug@ProfibusDP
Modular_Station		 =1
Max_Module          =1
Max_Input_len       =48
Max_Output_len      =48
Max_Data_len        =96

;=======================================
; Device specific diagnostic data (DPV1)
;=======================================
;
Unit_Diag_Area = 24-31
; Comm-State-Info
Value(0) = "Communication OK"
Value(1) = "Lost Communication to Device"
Unit_Diag_Area_End

Unit_Diag_bit(32) = "Device Diag Byte 0, Bit 0"
Unit_Diag_bit(33) = "Device Diag Byte 0, Bit 1"
Unit_Diag_bit(34) = "Device Diag Byte 0, Bit 2"
Unit_Diag_bit(35) = "Device Diag Byte 0, Bit 3"
Unit_Diag_bit(36) = "Device Diag Byte 0, Bit 4"
Unit_Diag_bit(37) = "Device Diag Byte 0, Bit 5"
Unit_Diag_bit(38) = "Device Diag Byte 0, Bit 6"
Unit_Diag_bit(39) = "Device Diag Byte 0, Bit 7"

Unit_Diag_bit(40) = "Device Diag Byte 1, Bit 0"
Unit_Diag_bit(41) = "Device Diag Byte 1, Bit 1"
Unit_Diag_bit(42) = "Device Diag Byte 1, Bit 2"
Unit_Diag_bit(43) = "Device Diag Byte 1, Bit 3"
Unit_Diag_bit(44) = "Device Diag Byte 1, Bit 4"
Unit_Diag_bit(45) = "Device Diag Byte 1, Bit 5"
Unit_Diag_bit(46) = "Device Diag Byte 1, Bit 6"
Unit_Diag_bit(47) = "Device Diag Byte 1, Bit 7"

Unit_Diag_bit(48) = "Device Diag Byte 2, Bit 0"
Unit_Diag_bit(49) = "Device Diag Byte 2, Bit 1"
Unit_Diag_bit(50) = "Device Diag Byte 2, Bit 2"
Unit_Diag_bit(51) = "Device Diag Byte 2, Bit 3"
Unit_Diag_bit(52) = "Device Diag Byte 2, Bit 4"
Unit_Diag_bit(53) = "Device Diag Byte 2, Bit 5"
Unit_Diag_bit(54) = "Device Diag Byte 2, Bit 6"
Unit_Diag_bit(55) = "Device Diag Byte 2, Bit 7"

Unit_Diag_bit(56) = "Device Diag Byte 3, Bit 0"
Unit_Diag_bit(57) = "Device Diag Byte 3, Bit 1"
Unit_Diag_bit(58) = "Device Diag Byte 3, Bit 2"
Unit_Diag_bit(59) = "Device Diag Byte 3, Bit 3"
Unit_Diag_bit(60) = "Device Diag Byte 3, Bit 4"
Unit_Diag_bit(61) = "Device Diag Byte 3, Bit 5"
Unit_Diag_bit(62) = "Device Diag Byte 3, Bit 6"
Unit_Diag_bit(63) = "Device Diag Byte 3, Bit 7"

Unit_Diag_bit(64) = "Device Diag Byte 4, Bit 0"
Unit_Diag_bit(65) = "Device Diag Byte 4, Bit 1"
Unit_Diag_bit(66) = "Device Diag Byte 4, Bit 2"
Unit_Diag_bit(67) = "Device Diag Byte 4, Bit 3"
Unit_Diag_bit(68) = "Device Diag Byte 4, Bit 4"
Unit_Diag_bit(69) = "Device Diag Byte 4, Bit 5"
Unit_Diag_bit(70) = "Device Diag Byte 4, Bit 6"
Unit_Diag_bit(71) = "Device Diag Byte 4, Bit 7"

Unit_Diag_bit(72) = "Device Diag Byte 5, Bit 0"
Unit_Diag_bit(73) = "Device Diag Byte 5, Bit 1"
Unit_Diag_bit(74) = "Device Diag Byte 5, Bit 2"
Unit_Diag_bit(75) = "Device Diag Byte 5, Bit 3"
Unit_Diag_bit(76) = "Device Diag Byte 5, Bit 4"
Unit_Diag_bit(77) = "Device Diag Byte 5, Bit 5"
Unit_Diag_bit(78) = "Device Diag Byte 5, Bit 6"
Unit_Diag_bit(79) = "Device Diag Byte 5, Bit 7"

Unit_Diag_bit(80) = "Device Diag Byte 6, Bit 0"
Unit_Diag_bit(81) = "Device Diag Byte 6, Bit 1"
Unit_Diag_bit(82) = "Device Diag Byte 6, Bit 2"
Unit_Diag_bit(83) = "Device Diag Byte 6, Bit 3"
Unit_Diag_bit(84) = "Device Diag Byte 6, Bit 4"
Unit_Diag_bit(85) = "Device Diag Byte 6, Bit 5"
Unit_Diag_bit(86) = "Device Diag Byte 6, Bit 6"
Unit_Diag_bit(87) = "Device Diag Byte 6, Bit 7"

Unit_Diag_bit(88) = "Device Diag Byte 7, Bit 0"
Unit_Diag_bit(89) = "Device Diag Byte 7, Bit 1"
Unit_Diag_bit(90) = "Device Diag Byte 7, Bit 2"
Unit_Diag_bit(91) = "Device Diag Byte 7, Bit 3"
Unit_Diag_bit(92) = "Device Diag Byte 7, Bit 4"
Unit_Diag_bit(93) = "Device Diag Byte 7, Bit 5"
Unit_Diag_bit(94) = "Device Diag Byte 7, Bit 6"
Unit_Diag_bit(95) = "Device Diag Byte 7, Bit 7"


;=============================================
; User Prm Data: Length and Preset:
;=============================================
;
Max_User_Prm_Data_Len	= 237					;   number of parameter of the longest module (max 229)
;                                        + number of parameter for the FBP itself
Ext_User_Prm_Data_Const(0) = 0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00 	; constant values for ASIC
;DPV1 status1 = 0x00 =>
;       Bit2 = 0 WD_Base=10ms (1ms=1)
;       Bit7 = 1 DPV1 Enable (Disable=0)
;DPV1 status2 = 0x00 =>
;       Bit0 = 0 ChkCfg nach EN50170(User specific=1)
;DPV1 status3 = 0x00 =>
;       alarm not implemented

Ext_User_Prm_Data_Ref(3) = 10000		; use/ignore Block-Parameters
Ext_User_Prm_Data_Ref(4) = 10001		; Diag-Format DPV0/V1
;
;=============================================
; Module Definition List
;=============================================
;
Module="Sensor (static mode)" 0x10, 0x20				; 1DO, 2DI
1
EndModule

Module="MSD11-FBP" 0x10, 0x20								; 1DO, 2DI
2
EndModule

Module="MSR22-FBP" 0x10, 0x20								; 2DO, 3DI
3
EndModule

Module="MFI21-FBP" 0x10, 0x20								; 3DO, 4DI
4
Ext_Module_Prm_Data_Len   = 5								; number of used data byte
Ext_User_Prm_Data_Const(0)=0x00,0x00,0x00,0x00,0x32	; initialising of param data
Ext_User_Prm_Data_Ref(0) = 50								; application mode
Ext_User_Prm_Data_Ref(1) = 51								; delay time
EndModule	

Module="UMC22-FBP (V3.0)" 0x11, 0x21, 0x50    	; 16DI, 16DO, 1AI
5
Ext_Module_Prm_Data_Len=42										; number of used data byte
Ext_User_Prm_Data_Const(0) =	\								; initialising of param data
							0x00,0x00,0x00,0x32,0x00,0x01,0x00,0x00,0x00,0x32, \
							0x01,0x01,0x01,0x00,0x0A,0x1E,0x04,0xB0,0x00,0x01, \
							0x02,0x04,0xB0,0x00,0x00,0xC8,0x00,0x14,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0xA0,0x00
Ext_User_Prm_Data_Ref(0)	= 1
;Ext_User_Prm_Data_Ref(4)	= 2
Ext_User_Prm_Data_Ref(6)	= 23
Ext_User_Prm_Data_Ref(10)	= 3
;Ext_User_Prm_Data_Ref(11)	= 4
Ext_User_Prm_Data_Ref(12)	= 5

Ext_User_Prm_Data_Ref(14)	= 6
Ext_User_Prm_Data_Ref(15)	= 7
Ext_User_Prm_Data_Ref(16)	= 8
Ext_User_Prm_Data_Ref(18)	= 9
Ext_User_Prm_Data_Ref(19) = 10
Ext_User_Prm_Data_Ref(20)	= 11
Ext_User_Prm_Data_Ref(21)	= 17
Ext_User_Prm_Data_Ref(23)	= 21
Ext_User_Prm_Data_Ref(24)	= 12
Ext_User_Prm_Data_Ref(26)	= 13
;Ext_User_Prm_Data_Ref(28)	= 14
;Ext_User_Prm_Data_Ref(32)	= 15
Ext_User_Prm_Data_Ref(36) = 25  
Ext_User_Prm_Data_Ref(37)	= 16
Ext_User_Prm_Data_Ref(38)	= 24
Ext_User_Prm_Data_Ref(39)	= 18
Ext_User_Prm_Data_Ref(40)	= 19
Ext_User_Prm_Data_Ref(41)	= 20
EndModule

Module="UMC22-FBP (V3.10, V3.20)" 0x11, 0x21, 0x50   	; 16DI, 16DO, 1AI
6
Ext_Module_Prm_Data_Len=42										; number of used data byte
Ext_User_Prm_Data_Const(0) =	\								; initialising of param data
							0x00,0x00,0x00,0x32,0x00,0x01,0x00,0x00,0x00,0x32, \
							0x01,0x01,0x01,0x00,0x0A,0x1E,0x04,0xB0,0x00,0x01, \
							0x02,0x04,0xB0,0x00,0x00,0xC8,0x00,0x14,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0xA0,0x00
Ext_User_Prm_Data_Ref(0)	= 101
Ext_User_Prm_Data_Ref(4)	= 102
Ext_User_Prm_Data_Ref(6)	= 123
Ext_User_Prm_Data_Ref(10)	= 103
;Ext_User_Prm_Data_Ref(11)	= 104
Ext_User_Prm_Data_Ref(12)	= 105

Ext_User_Prm_Data_Ref(14)	= 106
Ext_User_Prm_Data_Ref(15)	= 107
Ext_User_Prm_Data_Ref(16)	= 108
Ext_User_Prm_Data_Ref(18)	= 109
Ext_User_Prm_Data_Ref(19) = 110
Ext_User_Prm_Data_Ref(20)	= 111
Ext_User_Prm_Data_Ref(21)	= 117
Ext_User_Prm_Data_Ref(23)	= 121
Ext_User_Prm_Data_Ref(24)	= 112
Ext_User_Prm_Data_Ref(26)	= 113
Ext_User_Prm_Data_Ref(28)	= 114
Ext_User_Prm_Data_Ref(30)	= 126
Ext_User_Prm_Data_Ref(32)	= 115
Ext_User_Prm_Data_Ref(36) = 125  
Ext_User_Prm_Data_Ref(37)	= 116
Ext_User_Prm_Data_Ref(38)	= 124
Ext_User_Prm_Data_Ref(39)	= 118
Ext_User_Prm_Data_Ref(40)	= 119
Ext_User_Prm_Data_Ref(41)	= 120
EndModule

Module="UMC22-FBP (V3.30)" 0x11, 0x21, 0x50   	; 16DI, 16DO, 1AI
7
Ext_Module_Prm_Data_Len=42										; number of used data byte
Ext_User_Prm_Data_Const(0) =	\								; initialising of param data
							0x00,0x00,0x00,0x32,0x00,0x64,0x00,0x00,0x00,0x32, \
							0x01,0x00,0x01,0x00,0x0A,0x1E,0x04,0xB0,0x00,0x01, \
							0x02,0x04,0xB0,0x00,0x00,0xC8,0x00,0x14,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0xA0,0x00
Ext_User_Prm_Data_Ref(0)	= 151
Ext_User_Prm_Data_Ref(4)	= 152
Ext_User_Prm_Data_Ref(6)	= 173
Ext_User_Prm_Data_Ref(10)	= 153
Ext_User_Prm_Data_Ref(11)	= 154
Ext_User_Prm_Data_Ref(12)	= 155
Ext_User_Prm_Data_Ref(13)	= 177
Ext_User_Prm_Data_Ref(14)	= 156
Ext_User_Prm_Data_Ref(15)	= 157
Ext_User_Prm_Data_Ref(16)	= 158
Ext_User_Prm_Data_Ref(18)	= 159
Ext_User_Prm_Data_Ref(19) = 160
Ext_User_Prm_Data_Ref(20)	= 161
Ext_User_Prm_Data_Ref(21)	= 167
Ext_User_Prm_Data_Ref(23)	= 171
Ext_User_Prm_Data_Ref(24)	= 162
Ext_User_Prm_Data_Ref(26)	= 163
Ext_User_Prm_Data_Ref(28)	= 164
Ext_User_Prm_Data_Ref(30)	= 176
Ext_User_Prm_Data_Ref(31)	= 178
Ext_User_Prm_Data_Ref(32)	= 165
Ext_User_Prm_Data_Ref(36) = 175  
Ext_User_Prm_Data_Ref(37)	= 166
Ext_User_Prm_Data_Ref(38)	= 174
Ext_User_Prm_Data_Ref(39)	= 168
Ext_User_Prm_Data_Ref(40)	= 169
Ext_User_Prm_Data_Ref(41)	= 170
EndModule

Module="UMC22-FBP (V3.40)" 0x11, 0x21, 0x50   	; 16DI, 16DO, 1AI
8
Ext_Module_Prm_Data_Len=42										; number of used data byte
Ext_User_Prm_Data_Const(0) =	\								; initialising of param data
							0x00,0x00,0x00,0x32,0x00,0x64,0x00,0x00,0x00,0x32, \
							0x01,0x00,0x01,0x00,0x0A,0x1E,0x04,0xB0,0x00,0x01, \
							0x02,0x04,0xB0,0x00,0x00,0xC8,0x00,0x14,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0xA0,0x00
Ext_User_Prm_Data_Ref(0)	= 181
Ext_User_Prm_Data_Ref(4)	= 182
Ext_User_Prm_Data_Ref(6)	= 203
Ext_User_Prm_Data_Ref(10)	= 183
Ext_User_Prm_Data_Ref(11)	= 184
Ext_User_Prm_Data_Ref(12)	= 185
Ext_User_Prm_Data_Ref(13)	= 207
Ext_User_Prm_Data_Ref(14)	= 186
Ext_User_Prm_Data_Ref(15)	= 187
Ext_User_Prm_Data_Ref(16)	= 188
Ext_User_Prm_Data_Ref(18)	= 189
Ext_User_Prm_Data_Ref(19) = 190
Ext_User_Prm_Data_Ref(20)	= 191
Ext_User_Prm_Data_Ref(21)	= 197
Ext_User_Prm_Data_Ref(23)	= 201
Ext_User_Prm_Data_Ref(24)	= 192
Ext_User_Prm_Data_Ref(26)	= 193
Ext_User_Prm_Data_Ref(28)	= 194
Ext_User_Prm_Data_Ref(30)	= 206
Ext_User_Prm_Data_Ref(31)	= 208
Ext_User_Prm_Data_Ref(32)	= 195
Ext_User_Prm_Data_Ref(36) = 205  
Ext_User_Prm_Data_Ref(37)	= 196
Ext_User_Prm_Data_Ref(38)	= 204
Ext_User_Prm_Data_Ref(39)	= 198
Ext_User_Prm_Data_Ref(40)	= 199
Ext_User_Prm_Data_Ref(41)	= 200
EndModule

Module="UMC22-FBP (V4.00)" 0x11, 0x21, 0x50   	; 16DI, 16DO, 1AI
29
Ext_Module_Prm_Data_Len=42										; number of used data byte
Ext_User_Prm_Data_Const(0) =	\								; initialising of param data
							0x00,0x00,0x00,0x32,0x00,0x64,0x00,0x00,0x00,0x32, \
							0x01,0x00,0x01,0x00,0x0A,0x1E,0x04,0xB0,0x00,0x01, \
							0x02,0x04,0xB0,0x00,0x00,0xC8,0x00,0x14,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0xA0,0x00
Ext_User_Prm_Data_Ref(0)	= 181	; Set Current 1
Ext_User_Prm_Data_Ref(4)	= 211	; Current Factor (%) --> changed
Ext_User_Prm_Data_Ref(6)	= 203	; Set Current 2
Ext_User_Prm_Data_Ref(10)	= 183	; Trip Class
Ext_User_Prm_Data_Ref(11)	= 184	; DI0 Multi Function Input
Ext_User_Prm_Data_Ref(12)	= 185	; Phase Loss Protection
Ext_User_Prm_Data_Ref(13)	= 207	; DI1 Multi Function Input
Ext_User_Prm_Data_Ref(14)	= 186	; Low Current Threshold
Ext_User_Prm_Data_Ref(15)	= 187	; High Current Threshold
Ext_User_Prm_Data_Ref(16)	= 188	; Cooling Time
Ext_User_Prm_Data_Ref(18)	= 189	; Automatic fault reset
Ext_User_Prm_Data_Ref(19)	= 190	; Control Function
Ext_User_Prm_Data_Ref(20)	= 191	; Check-Back
Ext_User_Prm_Data_Ref(21)	= 197	; Start-Up Time
Ext_User_Prm_Data_Ref(23)	= 201	; Star-Delta Changeover Mode
Ext_User_Prm_Data_Ref(24)	= 192	; Star-Delta Start Time
Ext_User_Prm_Data_Ref(26)	= 193	; Reverse Lockout Time
Ext_User_Prm_Data_Ref(28)	= 194	; Operating Hours of Motor
Ext_User_Prm_Data_Ref(30)	= 206	; Number of Trips
Ext_User_Prm_Data_Ref(31)	= 208	; Emergency by PLC
Ext_User_Prm_Data_Ref(32)	= 195	; Number of Starts
Ext_User_Prm_Data_Ref(36)	= 205   ; Address Check
Ext_User_Prm_Data_Ref(37)	= 196	; Bus fault reaction
Ext_User_Prm_Data_Ref(38)	= 204	; DI2 Multi Function Input
Ext_User_Prm_Data_Ref(39)	= 210	; Local Control --> changed
Ext_User_Prm_Data_Ref(40)	= 199	; Block Current Threshold
Ext_User_Prm_Data_Ref(41)	= 200	; Fault Output
EndModule

Module="PST (CU 01.00.00, CU 01.01.00)" 0x15, 0x21, 0x58, 0x65			 ;48 DI, 16 DO, 9 AI, 6AO
9
Ext_Module_Prm_Data_Len=192								 ;number of used data bytes
Ext_User_Prm_Data_Const(0)=\								 ;Initialising of Param data
							0x00,0x01,0x00,0x0A,0x00,0x00,0x00,0x1E,0x00,0x1E, \
							0x00,0x64,0x00,0x28,0x00,0x00,0x00,0x32,0x00,0x14, \
							0x00,0x00,0x00,0x00,0x00,0x01,0x00,0x0A,0x00,0x0A, \
							0x00,0x0A,0x00,0x00,0x00,0x00,0x00,0x28,0x00,0x0A, \
							0x00,0x00,0x00,0x00,0x00,0x08,0x00,0x0A,0x00,0x00, \
							0x00,0x00,0x50,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x0C,0x00,0x00,0x00,0x05, \
							0x00,0x00,0x00,0x5A,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x01,0x00,0x02,0x00,0x02,0x00,0x00, \
							0x00,0x00,0x00,0x07,0x00,0x07,0x00,0x00,0x00,0x01, \
							0x00,0x00,0x00,0x00,0x00,0x0A,0x00,0x1E,0x00,0x28, \
							0x03,0xE8,0x00,0x0A,0x00,0x1E,0x00,0x28,0x03,0xE8, \
							0x00,0x0A,0x00,0x1E,0x00,0x28,0x03,0xE8,0x00,0x00, \
							0x00,0x00,0x00,0x0F,0x00,0x00,0x00,0x00,0x0F,0xD3, \
							0x00,0x06,0x00,0x0F,0x00,0x0C,0x00,0x1E,0x00,0x00, \
							0x00,0x7B,0x00,0x7B,0x00,0x7B,0x00,0x7B,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x64,0x00,0x64,0x00,0x64, \
							0x00,0x64

Ext_User_Prm_Data_Ref(0)	= 1001
Ext_User_Prm_Data_Ref(2)	= 1002
Ext_User_Prm_Data_Ref(4)	= 1003
Ext_User_Prm_Data_Ref(6)	= 1004
Ext_User_Prm_Data_Ref(8)	= 1005
Ext_User_Prm_Data_Ref(10)	= 1006
Ext_User_Prm_Data_Ref(12)	= 1007
Ext_User_Prm_Data_Ref(14)	= 1008
Ext_User_Prm_Data_Ref(16)	= 1009
Ext_User_Prm_Data_Ref(18)	= 1010
Ext_User_Prm_Data_Ref(20)	= 1011
Ext_User_Prm_Data_Ref(22)	= 1012
Ext_User_Prm_Data_Ref(24)	= 1013
Ext_User_Prm_Data_Ref(26)	= 1014
Ext_User_Prm_Data_Ref(28)	= 1015
Ext_User_Prm_Data_Ref(30)	= 1016
Ext_User_Prm_Data_Ref(32)	= 1017
Ext_User_Prm_Data_Ref(34)	= 1018
Ext_User_Prm_Data_Ref(36)	= 1019
Ext_User_Prm_Data_Ref(38)	= 1020
Ext_User_Prm_Data_Ref(40)	= 1021
Ext_User_Prm_Data_Ref(42)	= 1022
Ext_User_Prm_Data_Ref(44)	= 1023
Ext_User_Prm_Data_Ref(46)	= 1024
Ext_User_Prm_Data_Ref(48)	= 1025
Ext_User_Prm_Data_Ref(50)	= 1026
Ext_User_Prm_Data_Ref(52)	= 1027
Ext_User_Prm_Data_Ref(54)	= 1028
Ext_User_Prm_Data_Ref(56)	= 1029
Ext_User_Prm_Data_Ref(58)	= 1030
Ext_User_Prm_Data_Ref(60)	= 1031
Ext_User_Prm_Data_Ref(62)	= 1032
Ext_User_Prm_Data_Ref(64)	= 1033
Ext_User_Prm_Data_Ref(66)	= 1034
Ext_User_Prm_Data_Ref(68)	= 1035
Ext_User_Prm_Data_Ref(70)	= 1036
Ext_User_Prm_Data_Ref(72)	= 1037
Ext_User_Prm_Data_Ref(74)	= 1038
Ext_User_Prm_Data_Ref(76)	= 1039
Ext_User_Prm_Data_Ref(78)	= 1040
Ext_User_Prm_Data_Ref(80)	= 1041
Ext_User_Prm_Data_Ref(82)	= 1042
Ext_User_Prm_Data_Ref(84)	= 1043
Ext_User_Prm_Data_Ref(86)	= 1044
Ext_User_Prm_Data_Ref(88)	= 1045
Ext_User_Prm_Data_Ref(90)	= 1046
Ext_User_Prm_Data_Ref(92)	= 1047
Ext_User_Prm_Data_Ref(94)	= 1048
Ext_User_Prm_Data_Ref(96)	= 1049
Ext_User_Prm_Data_Ref(98)	= 1050
Ext_User_Prm_Data_Ref(100)	= 1051
Ext_User_Prm_Data_Ref(102)	= 1052
Ext_User_Prm_Data_Ref(104)	= 1053
Ext_User_Prm_Data_Ref(106)	= 1054
Ext_User_Prm_Data_Ref(108)	= 1055
Ext_User_Prm_Data_Ref(110)	= 1056
Ext_User_Prm_Data_Ref(112)	= 1057
Ext_User_Prm_Data_Ref(114)	= 1058
Ext_User_Prm_Data_Ref(116)	= 1059
Ext_User_Prm_Data_Ref(118)	= 1060
Ext_User_Prm_Data_Ref(120)	= 1061
Ext_User_Prm_Data_Ref(122)	= 1062
Ext_User_Prm_Data_Ref(124)	= 1063
Ext_User_Prm_Data_Ref(126)	= 1064
Ext_User_Prm_Data_Ref(128)	= 1065
Ext_User_Prm_Data_Ref(130)	= 1066
Ext_User_Prm_Data_Ref(132)	= 1067
Ext_User_Prm_Data_Ref(134)	= 1068
Ext_User_Prm_Data_Ref(136)	= 1069
Ext_User_Prm_Data_Ref(138)	= 1070
Ext_User_Prm_Data_Ref(140)	= 1071
Ext_User_Prm_Data_Ref(142)	= 1072
Ext_User_Prm_Data_Ref(144)	= 1073
Ext_User_Prm_Data_Ref(146)	= 1074
Ext_User_Prm_Data_Ref(148)	= 1075
Ext_User_Prm_Data_Ref(150)	= 1076
Ext_User_Prm_Data_Ref(152)	= 1077
Ext_User_Prm_Data_Ref(154)	= 1078
Ext_User_Prm_Data_Ref(156)	= 1079
Ext_User_Prm_Data_Ref(158)	= 1080
Ext_User_Prm_Data_Ref(160)	= 1081
Ext_User_Prm_Data_Ref(162)	= 1082
Ext_User_Prm_Data_Ref(164)	= 1083
Ext_User_Prm_Data_Ref(166)	= 1084
Ext_User_Prm_Data_Ref(168)	= 1085
Ext_User_Prm_Data_Ref(170)	= 1086
Ext_User_Prm_Data_Ref(172)	= 1087
Ext_User_Prm_Data_Ref(174)	= 1088
Ext_User_Prm_Data_Ref(176)	= 1089
Ext_User_Prm_Data_Ref(178)	= 1090
Ext_User_Prm_Data_Ref(180)	= 1091
Ext_User_Prm_Data_Ref(182)	= 1092
Ext_User_Prm_Data_Ref(184)	= 1093
Ext_User_Prm_Data_Ref(186)	= 1094
Ext_User_Prm_Data_Ref(188)	= 1095
Ext_User_Prm_Data_Ref(190)	= 1096						
EndModule

Module="PST (CU 02.00.01, CU 02.01.00)" 0x15, 0x21, 0x58, 0x65			 ;48 DI, 16 DO, 9 AI, 6AO
10
Ext_Module_Prm_Data_Len=192								 ;number of used data bytes
Ext_User_Prm_Data_Const(0)=\								 ;Initialising of Param data
							0x00,0x01,0x00,0x0A,0x00,0x00,0x00,0x1E,0x00,0x1E, \
							0x00,0x64,0x00,0x28,0x00,0x00,0x00,0x32,0x00,0x14, \
							0x00,0x00,0x00,0x00,0x00,0x01,0x00,0x01,0x00,0x01, \
							0x00,0x01,0x00,0x00,0x00,0x00,0x00,0x28,0x00,0x0A, \
							0x00,0x00,0x00,0x00,0x00,0x08,0x00,0x0A,0x00,0x00, \
							0x00,0x00,0x00,0x50,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x0C,0x00,0x00,0x00,0x05, \
							0x00,0x00,0x00,0x5A,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x01,0x00,0x01, \
							0x00,0x00,0x00,0x01,0x00,0x02,0x00,0x02,0x00,0x00, \
							0x00,0x00,0x00,0x07,0x00,0x07,0x00,0x00,0x00,0x01, \
							0x00,0x00,0x00,0x01,0x00,0x0A,0x00,0x1E,0x00,0x28, \
							0x00,0x01,0x00,0x0A,0x00,0x1E,0x00,0x28,0x00,0x01, \
							0x00,0x0A,0x00,0x1E,0x00,0x28,0x00,0x01,0x00,0x01, \
							0x00,0x00,0x00,0x0F,0x00,0x00,0x00,0x00,0x0F,0xD2, \
							0x00,0x06,0x00,0x0F,0x00,0x0C,0x00,0x1E,0x00,0x00, \
							0x00,0xC0,0x00,0xA8,0x00,0x00,0x00,0x02,0x00,0x64, \
							0x00,0x00,0x00,0x00,0x00,0x5F,0x03,0xE8,0x02,0x58, \
							0x00,0x28

Ext_User_Prm_Data_Ref(0)	= 1101
Ext_User_Prm_Data_Ref(2)	= 1102
Ext_User_Prm_Data_Ref(4)	= 1103
Ext_User_Prm_Data_Ref(6)	= 1104
Ext_User_Prm_Data_Ref(8)	= 1105
Ext_User_Prm_Data_Ref(10)	= 1106
Ext_User_Prm_Data_Ref(12)	= 1107
Ext_User_Prm_Data_Ref(14)	= 1108
Ext_User_Prm_Data_Ref(16)	= 1109
Ext_User_Prm_Data_Ref(18)	= 1110
Ext_User_Prm_Data_Ref(20)	= 1111
Ext_User_Prm_Data_Ref(22)	= 1112
Ext_User_Prm_Data_Ref(24)	= 1113
Ext_User_Prm_Data_Ref(26)	= 1114
Ext_User_Prm_Data_Ref(28)	= 1115
Ext_User_Prm_Data_Ref(30)	= 1116
Ext_User_Prm_Data_Ref(32)	= 1117
Ext_User_Prm_Data_Ref(34)	= 1118
Ext_User_Prm_Data_Ref(36)	= 1119
Ext_User_Prm_Data_Ref(38)	= 1120
Ext_User_Prm_Data_Ref(40)	= 1121
Ext_User_Prm_Data_Ref(42)	= 1122
Ext_User_Prm_Data_Ref(44)	= 1123
Ext_User_Prm_Data_Ref(46)	= 1124
Ext_User_Prm_Data_Ref(48)	= 1125
Ext_User_Prm_Data_Ref(50)	= 1126
Ext_User_Prm_Data_Ref(52)	= 1127
Ext_User_Prm_Data_Ref(54)	= 1128
Ext_User_Prm_Data_Ref(56)	= 1129
Ext_User_Prm_Data_Ref(58)	= 1130
Ext_User_Prm_Data_Ref(60)	= 1131
Ext_User_Prm_Data_Ref(62)	= 1132
Ext_User_Prm_Data_Ref(64)	= 1133
Ext_User_Prm_Data_Ref(66)	= 1134
Ext_User_Prm_Data_Ref(68)	= 1135
Ext_User_Prm_Data_Ref(70)	= 1136
Ext_User_Prm_Data_Ref(72)	= 1137
Ext_User_Prm_Data_Ref(74)	= 1138
Ext_User_Prm_Data_Ref(76)	= 1139
Ext_User_Prm_Data_Ref(78)	= 1140
Ext_User_Prm_Data_Ref(80)	= 1141
Ext_User_Prm_Data_Ref(82)	= 1142
Ext_User_Prm_Data_Ref(84)	= 1143
Ext_User_Prm_Data_Ref(86)	= 1144
Ext_User_Prm_Data_Ref(88)	= 1145
Ext_User_Prm_Data_Ref(90)	= 1146
Ext_User_Prm_Data_Ref(92)	= 1147
Ext_User_Prm_Data_Ref(94)	= 1148
Ext_User_Prm_Data_Ref(96)	= 1149
Ext_User_Prm_Data_Ref(98)	= 1150
Ext_User_Prm_Data_Ref(100)	= 1151
Ext_User_Prm_Data_Ref(102)	= 1152
Ext_User_Prm_Data_Ref(104)	= 1153
Ext_User_Prm_Data_Ref(106)	= 1154
Ext_User_Prm_Data_Ref(108)	= 1155
Ext_User_Prm_Data_Ref(110)	= 1156
Ext_User_Prm_Data_Ref(112)	= 1157
Ext_User_Prm_Data_Ref(114)	= 1158
Ext_User_Prm_Data_Ref(116)	= 1159
Ext_User_Prm_Data_Ref(118)	= 1160
Ext_User_Prm_Data_Ref(120)	= 1161
Ext_User_Prm_Data_Ref(122)	= 1162
Ext_User_Prm_Data_Ref(124)	= 1163
Ext_User_Prm_Data_Ref(126)	= 1164
Ext_User_Prm_Data_Ref(128)	= 1165
Ext_User_Prm_Data_Ref(130)	= 1166
Ext_User_Prm_Data_Ref(132)	= 1167
Ext_User_Prm_Data_Ref(134)	= 1168
Ext_User_Prm_Data_Ref(136)	= 1169
Ext_User_Prm_Data_Ref(138)	= 1170
Ext_User_Prm_Data_Ref(140)	= 1171
Ext_User_Prm_Data_Ref(142)	= 1172
Ext_User_Prm_Data_Ref(144)	= 1173
Ext_User_Prm_Data_Ref(146)	= 1174
Ext_User_Prm_Data_Ref(148)	= 1175
Ext_User_Prm_Data_Ref(150)	= 1176
Ext_User_Prm_Data_Ref(152)	= 1177
Ext_User_Prm_Data_Ref(154)	= 1178
Ext_User_Prm_Data_Ref(156)	= 1179
Ext_User_Prm_Data_Ref(158)	= 1180
Ext_User_Prm_Data_Ref(160)	= 1181
Ext_User_Prm_Data_Ref(162)	= 1182
Ext_User_Prm_Data_Ref(164)	= 1183
Ext_User_Prm_Data_Ref(166)	= 1184
Ext_User_Prm_Data_Ref(168)	= 1185
Ext_User_Prm_Data_Ref(170)	= 1186
Ext_User_Prm_Data_Ref(172)	= 1187
Ext_User_Prm_Data_Ref(174)	= 1188
Ext_User_Prm_Data_Ref(176)	= 1189
Ext_User_Prm_Data_Ref(178)	= 1190
Ext_User_Prm_Data_Ref(180)	= 1191
Ext_User_Prm_Data_Ref(182)	= 1192
Ext_User_Prm_Data_Ref(184)	= 1193
Ext_User_Prm_Data_Ref(186)	= 1194
Ext_User_Prm_Data_Ref(188)	= 1195
Ext_User_Prm_Data_Ref(190)	= 1196						
EndModule

Module="PST (CU 03.03.02)" 0x15, 0x21, 0x58, 0x65			 ;48 DI, 16 DO, 9 AI, 6AO, Compatible with CU-version 03.03.02.
11
Ext_Module_Prm_Data_Len=218									 ;number of used data bytes
Ext_User_Prm_Data_Const(0)=\								 ;Initialising of Param data
							0x00,0x01,0x00,0x0A,0x00,0x00,0x00,0x1E,0x00,0x1E, \
							0x00,0x64,0x00,0x28,0x00,0x00,0x00,0x32,0x00,0x14, \
							0x00,0x00,0x00,0x00,0x00,0x01,0x00,0x01,0x00,0x01, \
							0x00,0x01,0x00,0x00,0x00,0x00,0x00,0x28,0x00,0x0A, \
							0x00,0x00,0x00,0x00,0x00,0x05,0x00,0x0A,0x00,0x00, \
							0x00,0x00,0x00,0x50,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x0C,0x00,0x00,0x00,0x05, \
							0x00,0x00,0x00,0x5A,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x01,0x00,0x01, \
							0x00,0x00,0x00,0x01,0x00,0x02,0x00,0x02,0x00,0x00, \
							0x00,0x00,0x00,0x07,0x00,0x07,0x00,0x00,0x00,0x01, \
							0x00,0x00,0x00,0x01,0x00,0x0A,0x00,0x1E,0x00,0x28, \
							0x00,0x01,0x00,0x0A,0x00,0x1E,0x00,0x28,0x00,0x01, \
							0x00,0x0A,0x00,0x1E,0x00,0x28,0x00,0x01,0x00,0x01, \
							0x00,0x00,0x00,0x0F,0x00,0x00,0x00,0x00,0x0F,0xD2, \
							0x00,0x06,0x00,0x0F,0x00,0x0C,0x00,0x1E,0x00,0x00, \
							0x00,0xC0,0x00,0xA8,0x00,0x00,0x00,0x02,0x00,0x64, \
							0x00,0x00,0x00,0x00,0x00,0x5F,0x03,0xE8,0x02,0x58, \
							0x00,0x28,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x64,0x00,0x01,0x00,0x01,0x00,0x01

Ext_User_Prm_Data_Ref(0)	= 1201
Ext_User_Prm_Data_Ref(2)	= 1202
Ext_User_Prm_Data_Ref(4)	= 1203
Ext_User_Prm_Data_Ref(6)	= 1204
Ext_User_Prm_Data_Ref(8)	= 1205
Ext_User_Prm_Data_Ref(10)	= 1206
Ext_User_Prm_Data_Ref(12)	= 1207
Ext_User_Prm_Data_Ref(14)	= 1208
Ext_User_Prm_Data_Ref(16)	= 1209
Ext_User_Prm_Data_Ref(18)	= 1210
Ext_User_Prm_Data_Ref(20)	= 1211
Ext_User_Prm_Data_Ref(22)	= 1212
Ext_User_Prm_Data_Ref(24)	= 1213
Ext_User_Prm_Data_Ref(26)	= 1214
Ext_User_Prm_Data_Ref(28)	= 1215
Ext_User_Prm_Data_Ref(30)	= 1216
Ext_User_Prm_Data_Ref(32)	= 1217
Ext_User_Prm_Data_Ref(34)	= 1218
Ext_User_Prm_Data_Ref(36)	= 1219
Ext_User_Prm_Data_Ref(38)	= 1220
Ext_User_Prm_Data_Ref(40)	= 1221
Ext_User_Prm_Data_Ref(42)	= 1222
Ext_User_Prm_Data_Ref(44)	= 1223
Ext_User_Prm_Data_Ref(46)	= 1224
Ext_User_Prm_Data_Ref(48)	= 1225
Ext_User_Prm_Data_Ref(50)	= 1226
Ext_User_Prm_Data_Ref(52)	= 1227
Ext_User_Prm_Data_Ref(54)	= 1228
Ext_User_Prm_Data_Ref(56)	= 1229
Ext_User_Prm_Data_Ref(58)	= 1230
Ext_User_Prm_Data_Ref(60)	= 1231
Ext_User_Prm_Data_Ref(62)	= 1232
Ext_User_Prm_Data_Ref(64)	= 1233
Ext_User_Prm_Data_Ref(66)	= 1234
Ext_User_Prm_Data_Ref(68)	= 1235
Ext_User_Prm_Data_Ref(70)	= 1236
Ext_User_Prm_Data_Ref(72)	= 1237
Ext_User_Prm_Data_Ref(74)	= 1238
Ext_User_Prm_Data_Ref(76)	= 1239
Ext_User_Prm_Data_Ref(78)	= 1240
Ext_User_Prm_Data_Ref(80)	= 1241
Ext_User_Prm_Data_Ref(82)	= 1242
Ext_User_Prm_Data_Ref(84)	= 1243
Ext_User_Prm_Data_Ref(86)	= 1244
Ext_User_Prm_Data_Ref(88)	= 1245
Ext_User_Prm_Data_Ref(90)	= 1246
Ext_User_Prm_Data_Ref(92)	= 1247
Ext_User_Prm_Data_Ref(94)	= 1248
Ext_User_Prm_Data_Ref(96)	= 1249
Ext_User_Prm_Data_Ref(98)	= 1250
Ext_User_Prm_Data_Ref(100)	= 1251
Ext_User_Prm_Data_Ref(102)	= 1252
Ext_User_Prm_Data_Ref(104)	= 1253
Ext_User_Prm_Data_Ref(106)	= 1254
Ext_User_Prm_Data_Ref(108)	= 1255
Ext_User_Prm_Data_Ref(110)	= 1256
Ext_User_Prm_Data_Ref(112)	= 1257
Ext_User_Prm_Data_Ref(114)	= 1258
Ext_User_Prm_Data_Ref(116)	= 1259
Ext_User_Prm_Data_Ref(118)	= 1260
Ext_User_Prm_Data_Ref(120)	= 1261
Ext_User_Prm_Data_Ref(122)	= 1262
Ext_User_Prm_Data_Ref(124)	= 1263
Ext_User_Prm_Data_Ref(126)	= 1264
Ext_User_Prm_Data_Ref(128)	= 1265
Ext_User_Prm_Data_Ref(130)	= 1266
Ext_User_Prm_Data_Ref(132)	= 1267
Ext_User_Prm_Data_Ref(134)	= 1268
Ext_User_Prm_Data_Ref(136)	= 1269
Ext_User_Prm_Data_Ref(138)	= 1270
Ext_User_Prm_Data_Ref(140)	= 1271
Ext_User_Prm_Data_Ref(142)	= 1272
Ext_User_Prm_Data_Ref(144)	= 1273
Ext_User_Prm_Data_Ref(146)	= 1274
Ext_User_Prm_Data_Ref(148)	= 1275
Ext_User_Prm_Data_Ref(150)	= 1276
Ext_User_Prm_Data_Ref(152)	= 1277
Ext_User_Prm_Data_Ref(154)	= 1278
Ext_User_Prm_Data_Ref(156)	= 1279
Ext_User_Prm_Data_Ref(158)	= 1280
Ext_User_Prm_Data_Ref(160)	= 1281
Ext_User_Prm_Data_Ref(162)	= 1282
Ext_User_Prm_Data_Ref(164)	= 1283
Ext_User_Prm_Data_Ref(166)	= 1284
Ext_User_Prm_Data_Ref(168)	= 1285
Ext_User_Prm_Data_Ref(170)	= 1286
Ext_User_Prm_Data_Ref(172)	= 1287
Ext_User_Prm_Data_Ref(174)	= 1288
Ext_User_Prm_Data_Ref(176)	= 1289
Ext_User_Prm_Data_Ref(178)	= 1290
Ext_User_Prm_Data_Ref(180)	= 1291
Ext_User_Prm_Data_Ref(182)	= 1292
Ext_User_Prm_Data_Ref(184)	= 1293
Ext_User_Prm_Data_Ref(186)	= 1294
Ext_User_Prm_Data_Ref(188)	= 1295
Ext_User_Prm_Data_Ref(190)	= 1296
Ext_User_Prm_Data_Ref(192)	= 1297
Ext_User_Prm_Data_Ref(194)	= 1298
Ext_User_Prm_Data_Ref(196)	= 1299
Ext_User_Prm_Data_Ref(198)	= 1300
Ext_User_Prm_Data_Ref(200)	= 1301
Ext_User_Prm_Data_Ref(202)	= 1302
Ext_User_Prm_Data_Ref(204)	= 1303
Ext_User_Prm_Data_Ref(206)	= 1304
Ext_User_Prm_Data_Ref(208)	= 1305
Ext_User_Prm_Data_Ref(210)	= 1306
Ext_User_Prm_Data_Ref(212)	= 1307
Ext_User_Prm_Data_Ref(214)	= 1308
Ext_User_Prm_Data_Ref(216)	= 1309
EndModule

Module="PST (CU 03.04.01, CU 03.05.00)" 0x15, 0x21, 0x58, 0x65			 ;48 DI, 16 DO, 9 AI, 6AO, Compatible with CU-version 03.04.01 and 03.05.00.
12
Ext_Module_Prm_Data_Len=220									 ;number of used data bytes
Ext_User_Prm_Data_Const(0)=\								 ;Initialising of Param data
							0x00,0x01,0x00,0x0A,0x00,0x00,0x00,0x1E,0x00,0x1E, \
							0x00,0x64,0x00,0x28,0x00,0x00,0x00,0x32,0x00,0x14, \
							0x00,0x00,0x00,0x00,0x00,0x01,0x00,0x01,0x00,0x01, \
							0x00,0x01,0x00,0x00,0x00,0x00,0x00,0x28,0x00,0x0A, \
							0x00,0x00,0x00,0x00,0x00,0x05,0x00,0x0A,0x00,0x00, \
							0x00,0x00,0x00,0x50,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x0C,0x00,0x00,0x00,0x05, \
							0x00,0x00,0x00,0x5A,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x01,0x00,0x01, \
							0x00,0x00,0x00,0x01,0x00,0x02,0x00,0x02,0x00,0x00, \
							0x00,0x00,0x00,0x07,0x00,0x07,0x00,0x00,0x00,0x01, \
							0x00,0x00,0x00,0x01,0x00,0x0A,0x00,0x1E,0x00,0x28, \
							0x00,0x01,0x00,0x0A,0x00,0x1E,0x00,0x28,0x00,0x01, \
							0x00,0x0A,0x00,0x1E,0x00,0x28,0x00,0x01,0x00,0x01, \
							0x00,0x00,0x00,0x0F,0x00,0x00,0x00,0x00,0x0F,0xD2, \
							0x00,0x06,0x00,0x0F,0x00,0x0C,0x00,0x1E,0x00,0x00, \
							0x00,0xC0,0x00,0xA8,0x00,0x00,0x00,0x02,0x00,0x64, \
							0x00,0x00,0x00,0x00,0x00,0x5F,0x03,0xE8,0x02,0x58, \
							0x00,0x28,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x64,0x00,0x01,0x00,0x01,0x00,0x01,0x00,0x0E

Ext_User_Prm_Data_Ref(0)	= 1401
Ext_User_Prm_Data_Ref(2)	= 1402
Ext_User_Prm_Data_Ref(4)	= 1403
Ext_User_Prm_Data_Ref(6)	= 1404
Ext_User_Prm_Data_Ref(8)	= 1405
Ext_User_Prm_Data_Ref(10)	= 1406
Ext_User_Prm_Data_Ref(12)	= 1407
Ext_User_Prm_Data_Ref(14)	= 1408
Ext_User_Prm_Data_Ref(16)	= 1409
Ext_User_Prm_Data_Ref(18)	= 1410
Ext_User_Prm_Data_Ref(20)	= 1411
Ext_User_Prm_Data_Ref(22)	= 1412
Ext_User_Prm_Data_Ref(24)	= 1413
Ext_User_Prm_Data_Ref(26)	= 1414
Ext_User_Prm_Data_Ref(28)	= 1415
Ext_User_Prm_Data_Ref(30)	= 1416
Ext_User_Prm_Data_Ref(32)	= 1417
Ext_User_Prm_Data_Ref(34)	= 1418
Ext_User_Prm_Data_Ref(36)	= 1419
Ext_User_Prm_Data_Ref(38)	= 1420
Ext_User_Prm_Data_Ref(40)	= 1421
Ext_User_Prm_Data_Ref(42)	= 1422
Ext_User_Prm_Data_Ref(44)	= 1423
Ext_User_Prm_Data_Ref(46)	= 1424
Ext_User_Prm_Data_Ref(48)	= 1425
Ext_User_Prm_Data_Ref(50)	= 1426
Ext_User_Prm_Data_Ref(52)	= 1427
Ext_User_Prm_Data_Ref(54)	= 1428
Ext_User_Prm_Data_Ref(56)	= 1429
Ext_User_Prm_Data_Ref(58)	= 1430
Ext_User_Prm_Data_Ref(60)	= 1431
Ext_User_Prm_Data_Ref(62)	= 1432
Ext_User_Prm_Data_Ref(64)	= 1433
Ext_User_Prm_Data_Ref(66)	= 1434
Ext_User_Prm_Data_Ref(68)	= 1435
Ext_User_Prm_Data_Ref(70)	= 1436
Ext_User_Prm_Data_Ref(72)	= 1437
Ext_User_Prm_Data_Ref(74)	= 1438
Ext_User_Prm_Data_Ref(76)	= 1439
Ext_User_Prm_Data_Ref(78)	= 1440
Ext_User_Prm_Data_Ref(80)	= 1441
Ext_User_Prm_Data_Ref(82)	= 1442
Ext_User_Prm_Data_Ref(84)	= 1443
Ext_User_Prm_Data_Ref(86)	= 1444
Ext_User_Prm_Data_Ref(88)	= 1445
Ext_User_Prm_Data_Ref(90)	= 1446
Ext_User_Prm_Data_Ref(92)	= 1447
Ext_User_Prm_Data_Ref(94)	= 1448
Ext_User_Prm_Data_Ref(96)	= 1449
Ext_User_Prm_Data_Ref(98)	= 1450
Ext_User_Prm_Data_Ref(100)	= 1451
Ext_User_Prm_Data_Ref(102)	= 1452
Ext_User_Prm_Data_Ref(104)	= 1453
Ext_User_Prm_Data_Ref(106)	= 1454
Ext_User_Prm_Data_Ref(108)	= 1455
Ext_User_Prm_Data_Ref(110)	= 1456
Ext_User_Prm_Data_Ref(112)	= 1457
Ext_User_Prm_Data_Ref(114)	= 1458
Ext_User_Prm_Data_Ref(116)	= 1459
Ext_User_Prm_Data_Ref(118)	= 1460
Ext_User_Prm_Data_Ref(120)	= 1461
Ext_User_Prm_Data_Ref(122)	= 1462
Ext_User_Prm_Data_Ref(124)	= 1463
Ext_User_Prm_Data_Ref(126)	= 1464
Ext_User_Prm_Data_Ref(128)	= 1465
Ext_User_Prm_Data_Ref(130)	= 1466
Ext_User_Prm_Data_Ref(132)	= 1467
Ext_User_Prm_Data_Ref(134)	= 1468
Ext_User_Prm_Data_Ref(136)	= 1469
Ext_User_Prm_Data_Ref(138)	= 1470
Ext_User_Prm_Data_Ref(140)	= 1471
Ext_User_Prm_Data_Ref(142)	= 1472
Ext_User_Prm_Data_Ref(144)	= 1473
Ext_User_Prm_Data_Ref(146)	= 1474
Ext_User_Prm_Data_Ref(148)	= 1475
Ext_User_Prm_Data_Ref(150)	= 1476
Ext_User_Prm_Data_Ref(152)	= 1477
Ext_User_Prm_Data_Ref(154)	= 1478
Ext_User_Prm_Data_Ref(156)	= 1479
Ext_User_Prm_Data_Ref(158)	= 1480
Ext_User_Prm_Data_Ref(160)	= 1481
Ext_User_Prm_Data_Ref(162)	= 1482
Ext_User_Prm_Data_Ref(164)	= 1483
Ext_User_Prm_Data_Ref(166)	= 1484
Ext_User_Prm_Data_Ref(168)	= 1485
Ext_User_Prm_Data_Ref(170)	= 1486
Ext_User_Prm_Data_Ref(172)	= 1487
Ext_User_Prm_Data_Ref(174)	= 1488
Ext_User_Prm_Data_Ref(176)	= 1489
Ext_User_Prm_Data_Ref(178)	= 1490
Ext_User_Prm_Data_Ref(180)	= 1491
Ext_User_Prm_Data_Ref(182)	= 1492
Ext_User_Prm_Data_Ref(184)	= 1493
Ext_User_Prm_Data_Ref(186)	= 1494
Ext_User_Prm_Data_Ref(188)	= 1495
Ext_User_Prm_Data_Ref(190)	= 1496
Ext_User_Prm_Data_Ref(192)	= 1497
Ext_User_Prm_Data_Ref(194)	= 1498
Ext_User_Prm_Data_Ref(196)	= 1499
Ext_User_Prm_Data_Ref(198)	= 1500
Ext_User_Prm_Data_Ref(200)	= 1501
Ext_User_Prm_Data_Ref(202)	= 1502
Ext_User_Prm_Data_Ref(204)	= 1503
Ext_User_Prm_Data_Ref(206)	= 1504
Ext_User_Prm_Data_Ref(208)	= 1505
Ext_User_Prm_Data_Ref(210)	= 1506
Ext_User_Prm_Data_Ref(212)	= 1507
Ext_User_Prm_Data_Ref(214)	= 1508
Ext_User_Prm_Data_Ref(216)	= 1509
Ext_User_Prm_Data_Ref(218)	= 1510
EndModule


Module="PST (CU 04.00.02)" 0x15, 0x21, 0x58, 0x65			 ;48 DI, 16 DO, 9 AI, 6AO, Compatible with CU-version 04.00.02.
23
Ext_Module_Prm_Data_Len=226									 ;number of used data bytes
Ext_User_Prm_Data_Const(0)=\								 ;Initialising of Param data
							0x00,0x01,0x00,0x0A,0x00,0x00,0x00,0x1E,0x00,0x1E, \
							0x00,0x64,0x00,0x28,0x00,0x00,0x00,0x32,0x00,0x14, \
							0x00,0x00,0x00,0x00,0x00,0x01,0x00,0x01,0x00,0x01, \
							0x00,0x01,0x00,0x00,0x00,0x00,0x00,0x28,0x00,0x0A, \
							0x00,0x00,0x00,0x00,0x00,0x05,0x00,0x0A,0x00,0x00, \
							0x00,0x00,0x00,0x50,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x0C,0x00,0x00,0x00,0x05, \
							0x00,0x00,0x00,0x5A,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x01,0x00,0x01, \
							0x00,0x00,0x00,0x01,0x00,0x02,0x00,0x02,0x00,0x00, \
							0x00,0x00,0x00,0x07,0x00,0x07,0x00,0x00,0x00,0x01, \
							0x00,0x00,0x00,0x01,0x00,0x0A,0x00,0x1E,0x00,0x28, \
							0x00,0x01,0x00,0x0A,0x00,0x1E,0x00,0x28,0x00,0x01, \
							0x00,0x0A,0x00,0x1E,0x00,0x28,0x00,0x01,0x00,0x01, \
							0x00,0x00,0x00,0x0F,0x00,0x00,0x00,0x00,0x0F,0xD2, \
							0x00,0x06,0x00,0x0F,0x00,0x0C,0x00,0x1E,0x00,0x00, \
							0x00,0xC0,0x00,0xA8,0x00,0x00,0x00,0x02,0x00,0x64, \
							0x00,0x00,0x00,0x00,0x00,0x5F,0x03,0xE8,0x02,0x58, \
							0x00,0x28,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x64,0x00,0x01,0x00,0x01,0x00,0x01,0x00,0x0E, \
							0x00,0x00,0x00,0x28,0x00,0x00

Ext_User_Prm_Data_Ref(0)	= 1401
Ext_User_Prm_Data_Ref(2)	= 1402
Ext_User_Prm_Data_Ref(4)	= 1403
Ext_User_Prm_Data_Ref(6)	= 1404
Ext_User_Prm_Data_Ref(8)	= 1405
Ext_User_Prm_Data_Ref(10)	= 1406
Ext_User_Prm_Data_Ref(12)	= 1407
Ext_User_Prm_Data_Ref(14)	= 1408
Ext_User_Prm_Data_Ref(16)	= 1409
Ext_User_Prm_Data_Ref(18)	= 1410
Ext_User_Prm_Data_Ref(20)	= 1411
Ext_User_Prm_Data_Ref(22)	= 1412
Ext_User_Prm_Data_Ref(24)	= 1413
Ext_User_Prm_Data_Ref(26)	= 1414
Ext_User_Prm_Data_Ref(28)	= 1415
Ext_User_Prm_Data_Ref(30)	= 1416
Ext_User_Prm_Data_Ref(32)	= 1417
Ext_User_Prm_Data_Ref(34)	= 1418
Ext_User_Prm_Data_Ref(36)	= 1419
Ext_User_Prm_Data_Ref(38)	= 1420
Ext_User_Prm_Data_Ref(40)	= 1421
Ext_User_Prm_Data_Ref(42)	= 1422
Ext_User_Prm_Data_Ref(44)	= 1423
Ext_User_Prm_Data_Ref(46)	= 1424
Ext_User_Prm_Data_Ref(48)	= 1425
Ext_User_Prm_Data_Ref(50)	= 1426
Ext_User_Prm_Data_Ref(52)	= 1427
Ext_User_Prm_Data_Ref(54)	= 1428
Ext_User_Prm_Data_Ref(56)	= 1429
Ext_User_Prm_Data_Ref(58)	= 1430
Ext_User_Prm_Data_Ref(60)	= 1431
Ext_User_Prm_Data_Ref(62)	= 1432
Ext_User_Prm_Data_Ref(64)	= 1433
Ext_User_Prm_Data_Ref(66)	= 1434
Ext_User_Prm_Data_Ref(68)	= 1435
Ext_User_Prm_Data_Ref(70)	= 1436
Ext_User_Prm_Data_Ref(72)	= 1437
Ext_User_Prm_Data_Ref(74)	= 1438
Ext_User_Prm_Data_Ref(76)	= 1439
Ext_User_Prm_Data_Ref(78)	= 1440
Ext_User_Prm_Data_Ref(80)	= 1441
Ext_User_Prm_Data_Ref(82)	= 1442
Ext_User_Prm_Data_Ref(84)	= 1443
Ext_User_Prm_Data_Ref(86)	= 1444
Ext_User_Prm_Data_Ref(88)	= 1445
Ext_User_Prm_Data_Ref(90)	= 1446
Ext_User_Prm_Data_Ref(92)	= 1447
Ext_User_Prm_Data_Ref(94)	= 1448
Ext_User_Prm_Data_Ref(96)	= 1449
Ext_User_Prm_Data_Ref(98)	= 1450
Ext_User_Prm_Data_Ref(100)	= 1451
Ext_User_Prm_Data_Ref(102)	= 1452
Ext_User_Prm_Data_Ref(104)	= 1453
Ext_User_Prm_Data_Ref(106)	= 1454
Ext_User_Prm_Data_Ref(108)	= 1455
Ext_User_Prm_Data_Ref(110)	= 1456
Ext_User_Prm_Data_Ref(112)	= 1457
Ext_User_Prm_Data_Ref(114)	= 1458
Ext_User_Prm_Data_Ref(116)	= 1459
Ext_User_Prm_Data_Ref(118)	= 1460
Ext_User_Prm_Data_Ref(120)	= 1461
Ext_User_Prm_Data_Ref(122)	= 1462
Ext_User_Prm_Data_Ref(124)	= 1463
Ext_User_Prm_Data_Ref(126)	= 1464
Ext_User_Prm_Data_Ref(128)	= 1465
Ext_User_Prm_Data_Ref(130)	= 1466
Ext_User_Prm_Data_Ref(132)	= 1467
Ext_User_Prm_Data_Ref(134)	= 1468
Ext_User_Prm_Data_Ref(136)	= 1469
Ext_User_Prm_Data_Ref(138)	= 1470
Ext_User_Prm_Data_Ref(140)	= 1471
Ext_User_Prm_Data_Ref(142)	= 1472
Ext_User_Prm_Data_Ref(144)	= 1473
Ext_User_Prm_Data_Ref(146)	= 1474
Ext_User_Prm_Data_Ref(148)	= 1575  ;(!)
Ext_User_Prm_Data_Ref(150)	= 1476
Ext_User_Prm_Data_Ref(152)	= 1477
Ext_User_Prm_Data_Ref(154)	= 1478
Ext_User_Prm_Data_Ref(156)	= 1479
Ext_User_Prm_Data_Ref(158)	= 1480
Ext_User_Prm_Data_Ref(160)	= 1481
Ext_User_Prm_Data_Ref(162)	= 1482
Ext_User_Prm_Data_Ref(164)	= 1483
Ext_User_Prm_Data_Ref(166)	= 1484
Ext_User_Prm_Data_Ref(168)	= 1485
Ext_User_Prm_Data_Ref(170)	= 1486
Ext_User_Prm_Data_Ref(172)	= 1487
Ext_User_Prm_Data_Ref(174)	= 1488
Ext_User_Prm_Data_Ref(176)	= 1489
Ext_User_Prm_Data_Ref(178)	= 1490
Ext_User_Prm_Data_Ref(180)	= 1491
Ext_User_Prm_Data_Ref(182)	= 1492
Ext_User_Prm_Data_Ref(184)	= 1493
Ext_User_Prm_Data_Ref(186)	= 1494
Ext_User_Prm_Data_Ref(188)	= 1495
Ext_User_Prm_Data_Ref(190)	= 1496
Ext_User_Prm_Data_Ref(192)	= 1497
Ext_User_Prm_Data_Ref(194)	= 1498
Ext_User_Prm_Data_Ref(196)	= 1499
Ext_User_Prm_Data_Ref(198)	= 1500
Ext_User_Prm_Data_Ref(200)	= 1501
Ext_User_Prm_Data_Ref(202)	= 1502
Ext_User_Prm_Data_Ref(204)	= 1503
Ext_User_Prm_Data_Ref(206)	= 1504
Ext_User_Prm_Data_Ref(208)	= 1505
Ext_User_Prm_Data_Ref(210)	= 1506
Ext_User_Prm_Data_Ref(212)	= 1507
Ext_User_Prm_Data_Ref(214)	= 1508
Ext_User_Prm_Data_Ref(216)	= 1509
Ext_User_Prm_Data_Ref(218)	= 1510
Ext_User_Prm_Data_Ref(220)	= 1511
Ext_User_Prm_Data_Ref(222)	= 1512
Ext_User_Prm_Data_Ref(224)	= 1513
EndModule


Module="PST (CU 05.02.02)" 0x15, 0x21, 0x58, 0x65			 ;48 DI, 16 DO, 12 AI, 6AO, Compatible with CU-version 05.02.02.
25
Ext_Module_Prm_Data_Len=198									 ;number of used data bytes
Ext_User_Prm_Data_Const(0)=\								 ;Initialising of Param data
							0x00,0x01,0x00,0x0A,0x00,0x00,0x00,0x1E,0x00,0x1E, \
							0x00,0x64,0x00,0x28,0x00,0x00,0x00,0x32,0x00,0x14, \
							0x00,0x00,0x00,0x00,0x00,0x01,0x00,0x01,0x00,0x01, \
							0x00,0x01,0x00,0x00,0x00,0x00,0x00,0x28,0x00,0x0A, \
							0x00,0x00,0x00,0x00,0x00,0x05,0x00,0x0A,0x00,0x00, \
							0x00,0x00,0x00,0x50,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
										 0x00,0x00,0x00,0x0C,0x00,0x00,0x00,0x05, \
							0x00,0x00,0x00,0x5A,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x01,0x00,0x01, \
							0x00,0x00,0x00,0x01,0x00,0x02,0x00,0x02,0x00,0x00, \
							0x00,0x00,0x00,0x07,0x00,0x07,0x00,0x00,0x00,0x01, \
							0x00,0x00,0x00,0x01,0x00,0x0A,0x00,0x1E,0x00,0x28, \
							0x00,0x01,0x00,0x0A,0x00,0x1E,0x00,0x28,0x00,0x01, \
							0x00,0x0A,0x00,0x1E,0x00,0x28,0x00,0x01,0x00,0x01, \
																	0x00,0x00,0x0F,0xD2, \
							0x00,0x06,0x00,0x0F,0x00,0x0C,0x00,0x1E,				\
																								\
																								\
									 0x00,0x00,0x00,0x00,								\
																								\
							0x00,0x64,														\
							0x00,0x00,0x00,0x28,0x00,0x00,0x00,0x00,0x00,0x00,	\
							0x00,0x96,0x00,0x64,											\
													  0x00,0x00,0x00,0x01,0x00,0x00,	\
							0x2A,0xF8,0x02,0x58,0x3A,0x98,0x3A,0x98,0x3A,0x98,	\
							0x3A,0x98

Ext_User_Prm_Data_Ref(0)	= 1601
Ext_User_Prm_Data_Ref(2)	= 1602
Ext_User_Prm_Data_Ref(4)	= 1603
Ext_User_Prm_Data_Ref(6)	= 1604
Ext_User_Prm_Data_Ref(8)	= 1605
Ext_User_Prm_Data_Ref(10)	= 1606
Ext_User_Prm_Data_Ref(12)	= 1607
Ext_User_Prm_Data_Ref(14)	= 1608
Ext_User_Prm_Data_Ref(16)	= 1609
Ext_User_Prm_Data_Ref(18)	= 1610
Ext_User_Prm_Data_Ref(20)	= 1611
Ext_User_Prm_Data_Ref(22)	= 1612
Ext_User_Prm_Data_Ref(24)	= 1613
Ext_User_Prm_Data_Ref(26)	= 1614
Ext_User_Prm_Data_Ref(28)	= 1615
Ext_User_Prm_Data_Ref(30)	= 1616
Ext_User_Prm_Data_Ref(32)	= 1617
Ext_User_Prm_Data_Ref(34)	= 1618
Ext_User_Prm_Data_Ref(36)	= 1619
Ext_User_Prm_Data_Ref(38)	= 1620
Ext_User_Prm_Data_Ref(40)	= 1621
Ext_User_Prm_Data_Ref(42)	= 1622
Ext_User_Prm_Data_Ref(44)	= 1623
Ext_User_Prm_Data_Ref(46)	= 1624
Ext_User_Prm_Data_Ref(48)	= 1625
Ext_User_Prm_Data_Ref(50)	= 1626
Ext_User_Prm_Data_Ref(52)	= 1627
Ext_User_Prm_Data_Ref(54)	= 1628
Ext_User_Prm_Data_Ref(56)	= 1629
Ext_User_Prm_Data_Ref(58)	= 1630
Ext_User_Prm_Data_Ref(60)	= 1631
Ext_User_Prm_Data_Ref(62)	= 1632
Ext_User_Prm_Data_Ref(64)	= 1633
Ext_User_Prm_Data_Ref(66)	= 1634
Ext_User_Prm_Data_Ref(68)	= 1635
Ext_User_Prm_Data_Ref(70)	= 1637
Ext_User_Prm_Data_Ref(72)	= 1638
Ext_User_Prm_Data_Ref(74)	= 1639
Ext_User_Prm_Data_Ref(76)	= 1640
Ext_User_Prm_Data_Ref(78)	= 1641
Ext_User_Prm_Data_Ref(80)	= 1642
Ext_User_Prm_Data_Ref(82)	= 1643
Ext_User_Prm_Data_Ref(84)	= 1644
Ext_User_Prm_Data_Ref(86)	= 1645
Ext_User_Prm_Data_Ref(88)	= 1646
Ext_User_Prm_Data_Ref(90)	= 1647
Ext_User_Prm_Data_Ref(92)	= 1648
Ext_User_Prm_Data_Ref(94)	= 1649
Ext_User_Prm_Data_Ref(96)	= 1650
Ext_User_Prm_Data_Ref(98)	= 1651
Ext_User_Prm_Data_Ref(100)	= 1652
Ext_User_Prm_Data_Ref(102)	= 1653
Ext_User_Prm_Data_Ref(104)	= 1654
Ext_User_Prm_Data_Ref(106)	= 1655
Ext_User_Prm_Data_Ref(108)	= 1656
Ext_User_Prm_Data_Ref(110)	= 1657
Ext_User_Prm_Data_Ref(112)	= 1658
Ext_User_Prm_Data_Ref(114)	= 1659
Ext_User_Prm_Data_Ref(116)	= 1660
Ext_User_Prm_Data_Ref(118)	= 1661
Ext_User_Prm_Data_Ref(120)	= 1662
Ext_User_Prm_Data_Ref(122)	= 1663
Ext_User_Prm_Data_Ref(124)	= 1664
Ext_User_Prm_Data_Ref(126)	= 1665
Ext_User_Prm_Data_Ref(128)	= 1666
Ext_User_Prm_Data_Ref(130)	= 1667
Ext_User_Prm_Data_Ref(132)	= 1668
Ext_User_Prm_Data_Ref(134)	= 1669
Ext_User_Prm_Data_Ref(136)	= 1670
Ext_User_Prm_Data_Ref(138)	= 1671
Ext_User_Prm_Data_Ref(140)	= 1672
Ext_User_Prm_Data_Ref(142)	= 1673
Ext_User_Prm_Data_Ref(144)	= 1674
Ext_User_Prm_Data_Ref(146)	= 1675
Ext_User_Prm_Data_Ref(148)	= 1679
Ext_User_Prm_Data_Ref(150)	= 1680
Ext_User_Prm_Data_Ref(152)	= 1681
Ext_User_Prm_Data_Ref(154)	= 1682
Ext_User_Prm_Data_Ref(156)	= 1683
Ext_User_Prm_Data_Ref(158)	= 1684
Ext_User_Prm_Data_Ref(160)	= 1697
Ext_User_Prm_Data_Ref(162)	= 1698
Ext_User_Prm_Data_Ref(164)	= 1706
Ext_User_Prm_Data_Ref(166)	= 1711
Ext_User_Prm_Data_Ref(168)	= 1712
Ext_User_Prm_Data_Ref(170)	= 1713
Ext_User_Prm_Data_Ref(172)	= 1714
Ext_User_Prm_Data_Ref(174)	= 1715
Ext_User_Prm_Data_Ref(176)	= 1716
Ext_User_Prm_Data_Ref(178)	= 1717
Ext_User_Prm_Data_Ref(180)	= 1723
Ext_User_Prm_Data_Ref(182)	= 1724
Ext_User_Prm_Data_Ref(184)	= 1725
Ext_User_Prm_Data_Ref(186)	= 1726
Ext_User_Prm_Data_Ref(188)	= 1727
Ext_User_Prm_Data_Ref(190)	= 1728
Ext_User_Prm_Data_Ref(192)	= 1729
Ext_User_Prm_Data_Ref(194)	= 1730
Ext_User_Prm_Data_Ref(196)	= 1731
EndModule


Module="PST (CU 05.03.03)" 0x15, 0x21, 0x58, 0x65			 ;48 DI, 16 DO, 9 AI, 6AO, Compatible with CU-version 05.03.03.
26
Ext_Module_Prm_Data_Len=198									 ;number of used data bytes
Ext_User_Prm_Data_Const(0)=\								 ;Initialising of Param data
							0x00,0x01,0x00,0x0A,0x00,0x00,0x00,0x1E,0x00,0x1E, \
							0x00,0x64,0x00,0x28,0x00,0x00,0x00,0x32,0x00,0x14, \
							0x00,0x00,0x00,0x00,0x00,0x01,0x00,0x02,0x00,0x02, \
							0x00,0x02,0x00,0x00,0x00,0x00,0x00,0x28,0x00,0x0A, \
							0x00,0x00,0x00,0x00,0x00,0x05,0x00,0x0A,0x00,0x00, \
							0x00,0x00,0x00,0x50,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
										 0x00,0x00,0x00,0x0C,0x00,0x00,0x00,0x05, \
							0x00,0x00,0x00,0x5A,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x01,0x00,0x01, \
							0x00,0x00,0x00,0x01,0x00,0x02,0x00,0x02,0x00,0x00, \
							0x00,0x00,0x00,0x07,0x00,0x07,0x00,0x00,0x00,0x01, \
							0x00,0x00,0x00,0x01,0x00,0x0A,0x00,0x1E,0x00,0x28, \
							0x00,0x01,0x00,0x0A,0x00,0x1E,0x00,0x28,0x00,0x01, \
							0x00,0x0A,0x00,0x1E,0x00,0x28,0x00,0x01,0x00,0x01, \
																	0x00,0x00,0x0F,0xD2, \
							0x00,0x06,0x00,0x0F,0x00,0x0C,0x00,0x1E,				\
																								\
																								\
									 0x00,0x00,0x00,0x00,								\
																								\
							0x00,0x64,														\
							0x00,0x00,0x00,0x28,0x00,0x00,0x00,0x00,0x00,0x00,	\
							0x00,0x96,0x00,0x64,											\
													  0x00,0x00,0x00,0x01,0x00,0x00,	\
							0x2A,0xF8,0x02,0x58,0x3A,0x98,0x3A,0x98,0x3A,0x98,	\
							0x3A,0x98

Ext_User_Prm_Data_Ref(0)	= 1801
Ext_User_Prm_Data_Ref(2)	= 1802
Ext_User_Prm_Data_Ref(4)	= 1803
Ext_User_Prm_Data_Ref(6)	= 1804
Ext_User_Prm_Data_Ref(8)	= 1805
Ext_User_Prm_Data_Ref(10)	= 1806
Ext_User_Prm_Data_Ref(12)	= 1807
Ext_User_Prm_Data_Ref(14)	= 1808
Ext_User_Prm_Data_Ref(16)	= 1809
Ext_User_Prm_Data_Ref(18)	= 1810
Ext_User_Prm_Data_Ref(20)	= 1811
Ext_User_Prm_Data_Ref(22)	= 1812
Ext_User_Prm_Data_Ref(24)	= 1813
Ext_User_Prm_Data_Ref(26)	= 1814
Ext_User_Prm_Data_Ref(28)	= 1815
Ext_User_Prm_Data_Ref(30)	= 1816
Ext_User_Prm_Data_Ref(32)	= 1817
Ext_User_Prm_Data_Ref(34)	= 1818
Ext_User_Prm_Data_Ref(36)	= 1819
Ext_User_Prm_Data_Ref(38)	= 1820
Ext_User_Prm_Data_Ref(40)	= 1821
Ext_User_Prm_Data_Ref(42)	= 1822
Ext_User_Prm_Data_Ref(44)	= 1823
Ext_User_Prm_Data_Ref(46)	= 1824
Ext_User_Prm_Data_Ref(48)	= 1825
Ext_User_Prm_Data_Ref(50)	= 1826
Ext_User_Prm_Data_Ref(52)	= 1827
Ext_User_Prm_Data_Ref(54)	= 1828
Ext_User_Prm_Data_Ref(56)	= 1829
Ext_User_Prm_Data_Ref(58)	= 1830
Ext_User_Prm_Data_Ref(60)	= 1831
Ext_User_Prm_Data_Ref(62)	= 1832
Ext_User_Prm_Data_Ref(64)	= 1833
Ext_User_Prm_Data_Ref(66)	= 1834
Ext_User_Prm_Data_Ref(68)	= 1835
Ext_User_Prm_Data_Ref(70)	= 1837
Ext_User_Prm_Data_Ref(72)	= 1838
Ext_User_Prm_Data_Ref(74)	= 1839
Ext_User_Prm_Data_Ref(76)	= 1840
Ext_User_Prm_Data_Ref(78)	= 1841
Ext_User_Prm_Data_Ref(80)	= 1842
Ext_User_Prm_Data_Ref(82)	= 1843
Ext_User_Prm_Data_Ref(84)	= 1844
Ext_User_Prm_Data_Ref(86)	= 1845
Ext_User_Prm_Data_Ref(88)	= 1846
Ext_User_Prm_Data_Ref(90)	= 1847
Ext_User_Prm_Data_Ref(92)	= 1848
Ext_User_Prm_Data_Ref(94)	= 1849
Ext_User_Prm_Data_Ref(96)	= 1850
Ext_User_Prm_Data_Ref(98)	= 1851
Ext_User_Prm_Data_Ref(100)	= 1852
Ext_User_Prm_Data_Ref(102)	= 1853
Ext_User_Prm_Data_Ref(104)	= 1854
Ext_User_Prm_Data_Ref(106)	= 1855
Ext_User_Prm_Data_Ref(108)	= 1856
Ext_User_Prm_Data_Ref(110)	= 1857
Ext_User_Prm_Data_Ref(112)	= 1858
Ext_User_Prm_Data_Ref(114)	= 1859
Ext_User_Prm_Data_Ref(116)	= 1860
Ext_User_Prm_Data_Ref(118)	= 1861
Ext_User_Prm_Data_Ref(120)	= 1862
Ext_User_Prm_Data_Ref(122)	= 1863
Ext_User_Prm_Data_Ref(124)	= 1864
Ext_User_Prm_Data_Ref(126)	= 1865
Ext_User_Prm_Data_Ref(128)	= 1866
Ext_User_Prm_Data_Ref(130)	= 1867
Ext_User_Prm_Data_Ref(132)	= 1868
Ext_User_Prm_Data_Ref(134)	= 1869
Ext_User_Prm_Data_Ref(136)	= 1870
Ext_User_Prm_Data_Ref(138)	= 1871
Ext_User_Prm_Data_Ref(140)	= 1872
Ext_User_Prm_Data_Ref(142)	= 1873
Ext_User_Prm_Data_Ref(144)	= 1874
Ext_User_Prm_Data_Ref(146)	= 1875
Ext_User_Prm_Data_Ref(148)	= 1879
Ext_User_Prm_Data_Ref(150)	= 1880
Ext_User_Prm_Data_Ref(152)	= 1881
Ext_User_Prm_Data_Ref(154)	= 1882
Ext_User_Prm_Data_Ref(156)	= 1883
Ext_User_Prm_Data_Ref(158)	= 1884
Ext_User_Prm_Data_Ref(160)	= 1897
Ext_User_Prm_Data_Ref(162)	= 1898
Ext_User_Prm_Data_Ref(164)	= 1906
Ext_User_Prm_Data_Ref(166)	= 1911
Ext_User_Prm_Data_Ref(168)	= 1912
Ext_User_Prm_Data_Ref(170)	= 1913
Ext_User_Prm_Data_Ref(172)	= 1914
Ext_User_Prm_Data_Ref(174)	= 1915
Ext_User_Prm_Data_Ref(176)	= 1916
Ext_User_Prm_Data_Ref(178)	= 1917
Ext_User_Prm_Data_Ref(180)	= 1923
Ext_User_Prm_Data_Ref(182)	= 1924
Ext_User_Prm_Data_Ref(184)	= 1925
Ext_User_Prm_Data_Ref(186)	= 1926
Ext_User_Prm_Data_Ref(188)	= 1927
Ext_User_Prm_Data_Ref(190)	= 1928
Ext_User_Prm_Data_Ref(192)	= 1929
Ext_User_Prm_Data_Ref(194)	= 1930
Ext_User_Prm_Data_Ref(196)	= 1931
EndModule


Module="PST (CU 05.04.04)" 0x15, 0x21, 0x58, 0x65			;48 DI, 16 DO, 9 AI, 6 AO, Compatible with CU-version 05.04.04.
31
Ext_Module_Prm_Data_Len=200												;number of used data bytes
Ext_User_Prm_Data_Const(0)=\								 				;Initialising of Param data
	0x00,0x01,0x00,0x0A,0x00,0x00,0x00,0x1E,0x00,0x1E, \	;1-5, A:1-5, NA:-
	0x00,0x64,0x00,0x28,0x00,0x00,0x00,0x32,0x00,0x14, \	;6-10, A:6-10, NA:-
	0x00,0x00,0x00,0x00,0x00,0x01,0x00,0x01,0x00,0x01, \	;11-15, A:11-15, NA:-
	0x00,0x01,0x00,0x00,0x00,0x00,0x00,0x28,0x00,0x0A, \	;16-20, A:16-20 NA:-
	0x00,0x00,0x00,0x00,0x00,0x05,0x00,0x0A,0x00,0x00, \	;21-25, A:21-25, NA:-
	0x00,0x00,0x00,0x50,0x00,0x00,0x00,0x00,0x00,0x00, \	;26-30, A:26-30, NA:-
	0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \	;31-35, A:31-35, NA:-
					0x00,0x00,0x00,0x0C,0x00,0x00,0x00,0x08, \	;36-40, A:37-40, NA:36
	0x00,0x00,0x00,0x5A,0x00,0x00,0x00,0x00,0x00,0x00, \	;41-45, A:41-45, NA:-
	0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x01,0x00,0x01, \	;46-50, A:46-50, NA:-
	0x00,0x00,0x00,0x01,0x00,0x02,0x00,0x02,0x00,0x00, \	;51-55, A:51-55, NA:-
	0x00,0x00,0x00,0x07,0x00,0x07,0x00,0x00,0x00,0x01, \	;56-60, A:56-60, NA:-
	0x00,0x00,0x00,0x01,0x00,0x0A,0x00,0x1E,0x00,0x28, \	;61-65, A:61-65, NA:-
	0x00,0x01,0x00,0x0A,0x00,0x1E,0x00,0x28,0x00,0x01, \	;66-70, A:66-70, NA:-
	0x00,0x0A,0x00,0x1E,0x00,0x28,0x00,0x01,0x00,0x01, \	;71-75, A:71-75, NA:-
													 0x00,0x00,0x0F,0xD2, \	;76-80, A:79-80, NA:76-78
	0x00,0x06,0x00,0x0F,0x00,0x0C,0x00,0x1E,					\	;81-85, A:81-84, NA:85
																						\	;86-90, A:-, NA:86-90
																						\	;91-95, A:-, NA:91-95
				 	0x00,0x00,0x00,0x00,									\	;96-100, A:97-98, NA:96, 99-100
																						\	;101-105, A:-, NA:101-105
	0x00,0x64,																	\	;106-110, A:106, NA:107-110
	0x00,0x00,0x00,0x28,0x00,0x00,0x00,0x00,0x00,0x00,	\	;111-115, A:111-115, NA:-
	0x00,0x96,0x00,0x64,													\	;116-120, A:116-117, NA:118-120
							  0x00,0x00,0x00,0x01,0x00,0x00,		\	;121-125, A:123-125, NA:121-122
	0x2A,0xF8,0x02,0x58,0x3A,0x98,0x3A,0x98,0x3A,0x98,	\	;126-130, A:126-130, NA:-
	0x3A,0x98,0x00,0x08															;131-132, A:131-132, NA:-

Ext_User_Prm_Data_Ref(0)	= 5001
Ext_User_Prm_Data_Ref(2)	= 5002
Ext_User_Prm_Data_Ref(4)	= 5003
Ext_User_Prm_Data_Ref(6)	= 5004
Ext_User_Prm_Data_Ref(8)	= 5005
Ext_User_Prm_Data_Ref(10)	= 5006
Ext_User_Prm_Data_Ref(12)	= 5007
Ext_User_Prm_Data_Ref(14)	= 5008
Ext_User_Prm_Data_Ref(16)	= 5009
Ext_User_Prm_Data_Ref(18)	= 5010
Ext_User_Prm_Data_Ref(20)	= 5011
Ext_User_Prm_Data_Ref(22)	= 5012
Ext_User_Prm_Data_Ref(24)	= 5013
Ext_User_Prm_Data_Ref(26)	= 5014
Ext_User_Prm_Data_Ref(28)	= 5015
Ext_User_Prm_Data_Ref(30)	= 5016
Ext_User_Prm_Data_Ref(32)	= 5017
Ext_User_Prm_Data_Ref(34)	= 5018
Ext_User_Prm_Data_Ref(36)	= 5019
Ext_User_Prm_Data_Ref(38)	= 5020
Ext_User_Prm_Data_Ref(40)	= 5021
Ext_User_Prm_Data_Ref(42)	= 5022
Ext_User_Prm_Data_Ref(44)	= 5023
Ext_User_Prm_Data_Ref(46)	= 5024
Ext_User_Prm_Data_Ref(48)	= 5025
Ext_User_Prm_Data_Ref(50)	= 5026
Ext_User_Prm_Data_Ref(52)	= 5027
Ext_User_Prm_Data_Ref(54)	= 5028
Ext_User_Prm_Data_Ref(56)	= 5029
Ext_User_Prm_Data_Ref(58)	= 5030
Ext_User_Prm_Data_Ref(60)	= 5031
Ext_User_Prm_Data_Ref(62)	= 5032
Ext_User_Prm_Data_Ref(64)	= 5033
Ext_User_Prm_Data_Ref(66)	= 5034
Ext_User_Prm_Data_Ref(68)	= 5035
Ext_User_Prm_Data_Ref(70)	= 5037
Ext_User_Prm_Data_Ref(72)	= 5038
Ext_User_Prm_Data_Ref(74)	= 5039
Ext_User_Prm_Data_Ref(76)	= 5040
Ext_User_Prm_Data_Ref(78)	= 5041
Ext_User_Prm_Data_Ref(80)	= 5042
Ext_User_Prm_Data_Ref(82)	= 5043
Ext_User_Prm_Data_Ref(84)	= 5044
Ext_User_Prm_Data_Ref(86)	= 5045
Ext_User_Prm_Data_Ref(88)	= 5046
Ext_User_Prm_Data_Ref(90)	= 5047
Ext_User_Prm_Data_Ref(92)	= 5048
Ext_User_Prm_Data_Ref(94)	= 5049
Ext_User_Prm_Data_Ref(96)	= 5050
Ext_User_Prm_Data_Ref(98)	= 5051
Ext_User_Prm_Data_Ref(100)	= 5052
Ext_User_Prm_Data_Ref(102)	= 5053
Ext_User_Prm_Data_Ref(104)	= 5054
Ext_User_Prm_Data_Ref(106)	= 5055
Ext_User_Prm_Data_Ref(108)	= 5056
Ext_User_Prm_Data_Ref(110)	= 5057
Ext_User_Prm_Data_Ref(112)	= 5058
Ext_User_Prm_Data_Ref(114)	= 5059
Ext_User_Prm_Data_Ref(116)	= 5060
Ext_User_Prm_Data_Ref(118)	= 5061
Ext_User_Prm_Data_Ref(120)	= 5062
Ext_User_Prm_Data_Ref(122)	= 5063
Ext_User_Prm_Data_Ref(124)	= 5064
Ext_User_Prm_Data_Ref(126)	= 5065
Ext_User_Prm_Data_Ref(128)	= 5066
Ext_User_Prm_Data_Ref(130)	= 5067
Ext_User_Prm_Data_Ref(132)	= 5068
Ext_User_Prm_Data_Ref(134)	= 5069
Ext_User_Prm_Data_Ref(136)	= 5070
Ext_User_Prm_Data_Ref(138)	= 5071
Ext_User_Prm_Data_Ref(140)	= 5072
Ext_User_Prm_Data_Ref(142)	= 5073
Ext_User_Prm_Data_Ref(144)	= 5074
Ext_User_Prm_Data_Ref(146)	= 5075
Ext_User_Prm_Data_Ref(148)	= 5079
Ext_User_Prm_Data_Ref(150)	= 5080
Ext_User_Prm_Data_Ref(152)	= 5081
Ext_User_Prm_Data_Ref(154)	= 5082
Ext_User_Prm_Data_Ref(156)	= 5083
Ext_User_Prm_Data_Ref(158)	= 5084
Ext_User_Prm_Data_Ref(160)	= 5097
Ext_User_Prm_Data_Ref(162)	= 5098
Ext_User_Prm_Data_Ref(164)	= 5106
Ext_User_Prm_Data_Ref(166)	= 5111
Ext_User_Prm_Data_Ref(168)	= 5112
Ext_User_Prm_Data_Ref(170)	= 5113
Ext_User_Prm_Data_Ref(172)	= 5114
Ext_User_Prm_Data_Ref(174)	= 5115
Ext_User_Prm_Data_Ref(176)	= 5116
Ext_User_Prm_Data_Ref(178)	= 5117
Ext_User_Prm_Data_Ref(180)	= 5123
Ext_User_Prm_Data_Ref(182)	= 5124
Ext_User_Prm_Data_Ref(184)	= 5125
Ext_User_Prm_Data_Ref(186)	= 5126
Ext_User_Prm_Data_Ref(188)	= 5127
Ext_User_Prm_Data_Ref(190)	= 5128
Ext_User_Prm_Data_Ref(192)	= 5129
Ext_User_Prm_Data_Ref(194)	= 5130
Ext_User_Prm_Data_Ref(196)	= 5131
Ext_User_Prm_Data_Ref(198)	= 5132
EndModule


Module="PST (CU 05.05.00)" 0x15, 0x21, 0x58, 0x65			;48 DI, 16 DO, 9 AI, 6 AO, Compatible with CU-version 05.05.00.
33
Ext_Module_Prm_Data_Len=202												;number of used data bytes
Ext_User_Prm_Data_Const(0)=\								 				;Initialising of Param data
	0x00,0x01,0x00,0x0A,0x00,0x00,0x00,0x1E,0x00,0x1E, \	;1-5, A:1-5, NA:-
	0x00,0x64,0x00,0x28,0x00,0x00,0x00,0x32,0x00,0x14, \	;6-10, A:6-10, NA:-
	0x00,0x00,0x00,0x00,0x00,0x01,0x00,0x01,0x00,0x01, \	;11-15, A:11-15, NA:-
	0x00,0x01,0x00,0x00,0x00,0x00,0x00,0x28,0x00,0x0A, \	;16-20, A:16-20 NA:-
	0x00,0x00,0x00,0x00,0x00,0x05,0x00,0x0A,0x00,0x00, \	;21-25, A:21-25, NA:-
	0x00,0x00,0x00,0x50,0x00,0x00,0x00,0x00,0x00,0x00, \	;26-30, A:26-30, NA:-
	0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \	;31-35, A:31-35, NA:-
					0x00,0x00,0x00,0x0C,0x00,0x00,0x00,0x08, \	;36-40, A:37-40, NA:36
	0x00,0x00,0x00,0x5A,0x00,0x00,0x00,0x00,0x00,0x00, \	;41-45, A:41-45, NA:-
	0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x01,0x00,0x01, \	;46-50, A:46-50, NA:-
	0x00,0x00,0x00,0x01,0x00,0x02,0x00,0x02,0x00,0x00, \	;51-55, A:51-55, NA:-
	0x00,0x00,0x00,0x07,0x00,0x07,0x00,0x00,0x00,0x01, \	;56-60, A:56-60, NA:-
	0x00,0x00,0x00,0x01,0x00,0x0A,0x00,0x1E,0x00,0x28, \	;61-65, A:61-65, NA:-
	0x00,0x01,0x00,0x0A,0x00,0x1E,0x00,0x28,0x00,0x01, \	;66-70, A:66-70, NA:-
	0x00,0x0A,0x00,0x1E,0x00,0x28,0x00,0x01,0x00,0x01, \	;71-75, A:71-75, NA:-
													 0x00,0x00,0x0F,0xD2, \	;76-80, A:79-80, NA:76-78
	0x00,0x06,0x00,0x0F,0x00,0x0C,0x00,0x1E,					\	;81-85, A:81-84, NA:85
																						\	;86-90, A:-, NA:86-90
																						\	;91-95, A:-, NA:91-95
				 	0x00,0x00,0x00,0x00,									\	;96-100, A:97-98, NA:96, 99-100
																						\	;101-105, A:-, NA:101-105
	0x00,0x64,																	\	;106-110, A:106, NA:107-110
	0x00,0x00,0x00,0x28,0x00,0x00,0x00,0x00,0x00,0x00,	\	;111-115, A:111-115, NA:-
	0x00,0x96,0x00,0x64,													\	;116-120, A:116-117, NA:118-120
							  0x00,0x00,0x00,0x01,0x00,0x00,		\	;121-125, A:123-125, NA:121-122
	0x2A,0xF8,0x02,0x58,0x3A,0x98,0x3A,0x98,0x3A,0x98,	\	;126-130, A:126-130, NA:-
	0x3A,0x98,0x00,0x08,0x00,0x00										;131-133, A:131-133, NA:-

Ext_User_Prm_Data_Ref(0)	= 5201
Ext_User_Prm_Data_Ref(2)	= 5202
Ext_User_Prm_Data_Ref(4)	= 5203
Ext_User_Prm_Data_Ref(6)	= 5204
Ext_User_Prm_Data_Ref(8)	= 5205
Ext_User_Prm_Data_Ref(10)	= 5206
Ext_User_Prm_Data_Ref(12)	= 5207
Ext_User_Prm_Data_Ref(14)	= 5208
Ext_User_Prm_Data_Ref(16)	= 5209
Ext_User_Prm_Data_Ref(18)	= 5210
Ext_User_Prm_Data_Ref(20)	= 5211
Ext_User_Prm_Data_Ref(22)	= 5212
Ext_User_Prm_Data_Ref(24)	= 5213
Ext_User_Prm_Data_Ref(26)	= 5214
Ext_User_Prm_Data_Ref(28)	= 5215
Ext_User_Prm_Data_Ref(30)	= 5216
Ext_User_Prm_Data_Ref(32)	= 5217
Ext_User_Prm_Data_Ref(34)	= 5218
Ext_User_Prm_Data_Ref(36)	= 5219
Ext_User_Prm_Data_Ref(38)	= 5220
Ext_User_Prm_Data_Ref(40)	= 5221
Ext_User_Prm_Data_Ref(42)	= 5222
Ext_User_Prm_Data_Ref(44)	= 5223
Ext_User_Prm_Data_Ref(46)	= 5224
Ext_User_Prm_Data_Ref(48)	= 5225
Ext_User_Prm_Data_Ref(50)	= 5226
Ext_User_Prm_Data_Ref(52)	= 5227
Ext_User_Prm_Data_Ref(54)	= 5228
Ext_User_Prm_Data_Ref(56)	= 5229
Ext_User_Prm_Data_Ref(58)	= 5230
Ext_User_Prm_Data_Ref(60)	= 5231
Ext_User_Prm_Data_Ref(62)	= 5232
Ext_User_Prm_Data_Ref(64)	= 5233
Ext_User_Prm_Data_Ref(66)	= 5234
Ext_User_Prm_Data_Ref(68)	= 5235
Ext_User_Prm_Data_Ref(70)	= 5237
Ext_User_Prm_Data_Ref(72)	= 5238
Ext_User_Prm_Data_Ref(74)	= 5239
Ext_User_Prm_Data_Ref(76)	= 5240
Ext_User_Prm_Data_Ref(78)	= 5241
Ext_User_Prm_Data_Ref(80)	= 5242
Ext_User_Prm_Data_Ref(82)	= 5243
Ext_User_Prm_Data_Ref(84)	= 5244
Ext_User_Prm_Data_Ref(86)	= 5245
Ext_User_Prm_Data_Ref(88)	= 5246
Ext_User_Prm_Data_Ref(90)	= 5247
Ext_User_Prm_Data_Ref(92)	= 5248
Ext_User_Prm_Data_Ref(94)	= 5249
Ext_User_Prm_Data_Ref(96)	= 5250
Ext_User_Prm_Data_Ref(98)	= 5251
Ext_User_Prm_Data_Ref(100)	= 5252
Ext_User_Prm_Data_Ref(102)	= 5253
Ext_User_Prm_Data_Ref(104)	= 5254
Ext_User_Prm_Data_Ref(106)	= 5255
Ext_User_Prm_Data_Ref(108)	= 5256
Ext_User_Prm_Data_Ref(110)	= 5257
Ext_User_Prm_Data_Ref(112)	= 5258
Ext_User_Prm_Data_Ref(114)	= 5259
Ext_User_Prm_Data_Ref(116)	= 5260
Ext_User_Prm_Data_Ref(118)	= 5261
Ext_User_Prm_Data_Ref(120)	= 5262
Ext_User_Prm_Data_Ref(122)	= 5263
Ext_User_Prm_Data_Ref(124)	= 5264
Ext_User_Prm_Data_Ref(126)	= 5265
Ext_User_Prm_Data_Ref(128)	= 5266
Ext_User_Prm_Data_Ref(130)	= 5267
Ext_User_Prm_Data_Ref(132)	= 5268
Ext_User_Prm_Data_Ref(134)	= 5269
Ext_User_Prm_Data_Ref(136)	= 5270
Ext_User_Prm_Data_Ref(138)	= 5271
Ext_User_Prm_Data_Ref(140)	= 5272
Ext_User_Prm_Data_Ref(142)	= 5273
Ext_User_Prm_Data_Ref(144)	= 5274
Ext_User_Prm_Data_Ref(146)	= 5275
Ext_User_Prm_Data_Ref(148)	= 5279
Ext_User_Prm_Data_Ref(150)	= 5280
Ext_User_Prm_Data_Ref(152)	= 5281
Ext_User_Prm_Data_Ref(154)	= 5282
Ext_User_Prm_Data_Ref(156)	= 5283
Ext_User_Prm_Data_Ref(158)	= 5284
Ext_User_Prm_Data_Ref(160)	= 5297
Ext_User_Prm_Data_Ref(162)	= 5298
Ext_User_Prm_Data_Ref(164)	= 5306
Ext_User_Prm_Data_Ref(166)	= 5311
Ext_User_Prm_Data_Ref(168)	= 5312
Ext_User_Prm_Data_Ref(170)	= 5313
Ext_User_Prm_Data_Ref(172)	= 5314
Ext_User_Prm_Data_Ref(174)	= 5315
Ext_User_Prm_Data_Ref(176)	= 5316
Ext_User_Prm_Data_Ref(178)	= 5317
Ext_User_Prm_Data_Ref(180)	= 5323
Ext_User_Prm_Data_Ref(182)	= 5324
Ext_User_Prm_Data_Ref(184)	= 5325
Ext_User_Prm_Data_Ref(186)	= 5326
Ext_User_Prm_Data_Ref(188)	= 5327
Ext_User_Prm_Data_Ref(190)	= 5328
Ext_User_Prm_Data_Ref(192)	= 5329
Ext_User_Prm_Data_Ref(194)	= 5330
Ext_User_Prm_Data_Ref(196)	= 5331
Ext_User_Prm_Data_Ref(198)	= 5332
Ext_User_Prm_Data_Ref(200)	= 5333
EndModule


Module="PST (CU 06.00.00)" 0x15, 0x21, 0x58, 0x65			;48 DI, 16 DO, 9 AI, 6 AO, Compatible with CU-version 06.00.00.
36
Ext_Module_Prm_Data_Len=202												;number of used data bytes
Ext_User_Prm_Data_Const(0)=\								 				;Initialising of Param data
	0x00,0x01,0x00,0x0A,0x00,0x00,0x00,0x1E,0x00,0x1E, \	;1-5, A:1-5, NA:-
	0x00,0x64,0x00,0x28,0x00,0x00,0x00,0x32,0x00,0x14, \	;6-10, A:6-10, NA:-
	0x00,0x00,0x00,0x00,0x00,0x01,0x00,0x01,0x00,0x01, \	;11-15, A:11-15, NA:-
	0x00,0x01,0x00,0x00,0x00,0x00,0x00,0x28,0x00,0x0A, \	;16-20, A:16-20 NA:-
	0x00,0x00,0x00,0x00,0x00,0x05,0x00,0x0A,0x00,0x00, \	;21-25, A:21-25, NA:-
	0x00,0x00,0x00,0x50,0x00,0x00,0x00,0x00,0x00,0x00, \	;26-30, A:26-30, NA:-
	0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \	;31-35, A:31-35, NA:-
					0x00,0x00,0x00,0x0C,0x00,0x00,0x00,0x08, \	;36-40, A:37-40, NA:36
	0x00,0x00,0x00,0x5A,0x00,0x00,0x00,0x00,0x00,0x00, \	;41-45, A:41-45, NA:-
	0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x01,0x00,0x01, \	;46-50, A:46-50, NA:-
	0x00,0x00,0x00,0x01,0x00,0x02,0x00,0x02,0x00,0x00, \	;51-55, A:51-55, NA:-
	0x00,0x00,0x00,0x07,0x00,0x07,0x00,0x00,0x00,0x01, \	;56-60, A:56-60, NA:-
	0x00,0x00,0x00,0x01,0x00,0x0A,0x00,0x1E,0x00,0x28, \	;61-65, A:61-65, NA:-
	0x00,0x01,0x00,0x0A,0x00,0x1E,0x00,0x28,0x00,0x01, \	;66-70, A:66-70, NA:-
	0x00,0x0A,0x00,0x1E,0x00,0x28,0x00,0x01,0x00,0x01, \	;71-75, A:71-75, NA:-
													 0x00,0x00,0x07,0xD0, \	;76-80, A:76-80, NA:76-78
	0x00,0x01,0x00,0x01,0x00,0x00,0x00,0x00,					\	;81-85, A:81-84, NA:85
																						\	;86-90, A:-, NA:86-90
																						\	;91-95, A:-, NA:91-95
				 	0x00,0x00,0x00,0x00,									\	;96-100, A:97-98, NA:96, 99-100
																						\	;101-105, A:-, NA:101-105
	0x00,0x64,																	\	;106-110, A:106, NA:107-110
	0x00,0x00,0x00,0x28,0x00,0x00,0x00,0x00,0x00,0x00,	\	;111-115, A:111-115, NA:-
	0x00,0x96,0x00,0x64,													\	;116-120, A:116-117, NA:118-120
							  0x00,0x00,0x00,0x01,0x00,0x00,		\	;121-125, A:123-125, NA:121-122
	0x2A,0xF8,0x02,0x58,0x3A,0x98,0x3A,0x98,0x3A,0x98,	\	;126-130, A:126-130, NA:-
	0x3A,0x98,0x00,0x0A,0x00,0x00										;131-133, A:131-133, NA:-

Ext_User_Prm_Data_Ref(0)	= 5501
Ext_User_Prm_Data_Ref(2)	= 5502
Ext_User_Prm_Data_Ref(4)	= 5503
Ext_User_Prm_Data_Ref(6)	= 5504
Ext_User_Prm_Data_Ref(8)	= 5505
Ext_User_Prm_Data_Ref(10)	= 5506
Ext_User_Prm_Data_Ref(12)	= 5507
Ext_User_Prm_Data_Ref(14)	= 5508
Ext_User_Prm_Data_Ref(16)	= 5509
Ext_User_Prm_Data_Ref(18)	= 5510
Ext_User_Prm_Data_Ref(20)	= 5511
Ext_User_Prm_Data_Ref(22)	= 5512
Ext_User_Prm_Data_Ref(24)	= 5513
Ext_User_Prm_Data_Ref(26)	= 5514
Ext_User_Prm_Data_Ref(28)	= 5515
Ext_User_Prm_Data_Ref(30)	= 5516
Ext_User_Prm_Data_Ref(32)	= 5517
Ext_User_Prm_Data_Ref(34)	= 5518
Ext_User_Prm_Data_Ref(36)	= 5519
Ext_User_Prm_Data_Ref(38)	= 5520
Ext_User_Prm_Data_Ref(40)	= 5521
Ext_User_Prm_Data_Ref(42)	= 5522
Ext_User_Prm_Data_Ref(44)	= 5523
Ext_User_Prm_Data_Ref(46)	= 5524
Ext_User_Prm_Data_Ref(48)	= 5525
Ext_User_Prm_Data_Ref(50)	= 5526
Ext_User_Prm_Data_Ref(52)	= 5527
Ext_User_Prm_Data_Ref(54)	= 5528
Ext_User_Prm_Data_Ref(56)	= 5529
Ext_User_Prm_Data_Ref(58)	= 5530
Ext_User_Prm_Data_Ref(60)	= 5531
Ext_User_Prm_Data_Ref(62)	= 5532
Ext_User_Prm_Data_Ref(64)	= 5533
Ext_User_Prm_Data_Ref(66)	= 5534
Ext_User_Prm_Data_Ref(68)	= 5535
Ext_User_Prm_Data_Ref(70)	= 5537
Ext_User_Prm_Data_Ref(72)	= 5538
Ext_User_Prm_Data_Ref(74)	= 5539
Ext_User_Prm_Data_Ref(76)	= 5540
Ext_User_Prm_Data_Ref(78)	= 5541
Ext_User_Prm_Data_Ref(80)	= 5542
Ext_User_Prm_Data_Ref(82)	= 5543
Ext_User_Prm_Data_Ref(84)	= 5544
Ext_User_Prm_Data_Ref(86)	= 5545
Ext_User_Prm_Data_Ref(88)	= 5546
Ext_User_Prm_Data_Ref(90)	= 5547
Ext_User_Prm_Data_Ref(92)	= 5548
Ext_User_Prm_Data_Ref(94)	= 5549
Ext_User_Prm_Data_Ref(96)	= 5550
Ext_User_Prm_Data_Ref(98)	= 5551
Ext_User_Prm_Data_Ref(100)	= 5552
Ext_User_Prm_Data_Ref(102)	= 5553
Ext_User_Prm_Data_Ref(104)	= 5554
Ext_User_Prm_Data_Ref(106)	= 5555
Ext_User_Prm_Data_Ref(108)	= 5556
Ext_User_Prm_Data_Ref(110)	= 5557
Ext_User_Prm_Data_Ref(112)	= 5558
Ext_User_Prm_Data_Ref(114)	= 5559
Ext_User_Prm_Data_Ref(116)	= 5560
Ext_User_Prm_Data_Ref(118)	= 5561
Ext_User_Prm_Data_Ref(120)	= 5562
Ext_User_Prm_Data_Ref(122)	= 5563
Ext_User_Prm_Data_Ref(124)	= 5564
Ext_User_Prm_Data_Ref(126)	= 5565
Ext_User_Prm_Data_Ref(128)	= 5566
Ext_User_Prm_Data_Ref(130)	= 5567
Ext_User_Prm_Data_Ref(132)	= 5568
Ext_User_Prm_Data_Ref(134)	= 5569
Ext_User_Prm_Data_Ref(136)	= 5570
Ext_User_Prm_Data_Ref(138)	= 5571
Ext_User_Prm_Data_Ref(140)	= 5572
Ext_User_Prm_Data_Ref(142)	= 5573
Ext_User_Prm_Data_Ref(144)	= 5574
Ext_User_Prm_Data_Ref(146)	= 5575
Ext_User_Prm_Data_Ref(148)	= 5579
Ext_User_Prm_Data_Ref(150)	= 5580
Ext_User_Prm_Data_Ref(152)	= 5581
Ext_User_Prm_Data_Ref(154)	= 5582
Ext_User_Prm_Data_Ref(156)	= 5583
Ext_User_Prm_Data_Ref(158)	= 5584
Ext_User_Prm_Data_Ref(160)	= 5597
Ext_User_Prm_Data_Ref(162)	= 5598
Ext_User_Prm_Data_Ref(164)	= 5606
Ext_User_Prm_Data_Ref(166)	= 5611
Ext_User_Prm_Data_Ref(168)	= 5612
Ext_User_Prm_Data_Ref(170)	= 5613
Ext_User_Prm_Data_Ref(172)	= 5614
Ext_User_Prm_Data_Ref(174)	= 5615
Ext_User_Prm_Data_Ref(176)	= 5616
Ext_User_Prm_Data_Ref(178)	= 5617
Ext_User_Prm_Data_Ref(180)	= 5623
Ext_User_Prm_Data_Ref(182)	= 5624
Ext_User_Prm_Data_Ref(184)	= 5625
Ext_User_Prm_Data_Ref(186)	= 5626
Ext_User_Prm_Data_Ref(188)	= 5627
Ext_User_Prm_Data_Ref(190)	= 5628
Ext_User_Prm_Data_Ref(192)	= 5629
Ext_User_Prm_Data_Ref(194)	= 5630
Ext_User_Prm_Data_Ref(196)	= 5631
Ext_User_Prm_Data_Ref(198)	= 5632
Ext_User_Prm_Data_Ref(200)	= 5633
EndModule


Module="PSE" 0x11, 0x23, 0x5A			;16 DI, 32 DO, 11 AI, Compatible with PSE.
35
Ext_Module_Prm_Data_Len=44												;number of used data bytes
Ext_User_Prm_Data_Const(0)=\								 				;Initialising of Param data
	0x00,0x01,0x00,0x0A,0x00,0x00,0x00,0x01,0x00,0x28, \	;1-5, A:1-5, NA:-
	0x00,0x1E,0x00,0x46,0x00,0x00,0x00,0x00,0x00,0x00, \	;6-10, A:6-10, NA:-
	0x00,0x02,0x00,0x32,0x00,0x01,0x00,0x01,0x00,0x00, \	;11-15, A:11-15, NA:-
	0x00,0x00,0x00,0x05,0x00,0x00,0x00,0x00,0x00,0x0c, \	;16-20, A:16-20 NA:-
	0x00,0x00,0x00,0x00                                	;21-22, A:21-22, NA:-

Ext_User_Prm_Data_Ref(0)	= 5401
Ext_User_Prm_Data_Ref(2)	= 5402
Ext_User_Prm_Data_Ref(4)	= 5403
Ext_User_Prm_Data_Ref(6)	= 5404
Ext_User_Prm_Data_Ref(8)	= 5405
Ext_User_Prm_Data_Ref(10)	= 5406
Ext_User_Prm_Data_Ref(12)	= 5407
Ext_User_Prm_Data_Ref(14)	= 5408
Ext_User_Prm_Data_Ref(16)	= 5409
Ext_User_Prm_Data_Ref(18)	= 5410
Ext_User_Prm_Data_Ref(20)	= 5411
Ext_User_Prm_Data_Ref(22)	= 5412
Ext_User_Prm_Data_Ref(24)	= 5413
Ext_User_Prm_Data_Ref(26)	= 5414
Ext_User_Prm_Data_Ref(28)	= 5415
Ext_User_Prm_Data_Ref(30)	= 5416
Ext_User_Prm_Data_Ref(32)	= 5417
Ext_User_Prm_Data_Ref(34)	= 5418
Ext_User_Prm_Data_Ref(36)	= 5419
Ext_User_Prm_Data_Ref(38)	= 5420
Ext_User_Prm_Data_Ref(40)	= 5421
Ext_User_Prm_Data_Ref(42)	= 5422

EndModule


Module="PSR" 0x10, 0x20								; 1DO, 2DI
24
EndModule


Module="WDI100-FBP" 0x5F							;16 AI
13
Ext_Module_Prm_Data_Len  = 18					;Number of used Data Bytes
Ext_User_Prm_Data_Const(0)=\						;Initialising of Param Data
								0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,\
								0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00

Ext_User_Prm_Data_Ref(0)  = 500
Ext_User_Prm_Data_Ref(2)  = 501
Ext_User_Prm_Data_Ref(4)  = 502
Ext_User_Prm_Data_Ref(6)  = 503
Ext_User_Prm_Data_Ref(8)  = 504
Ext_User_Prm_Data_Ref(10) = 505
Ext_User_Prm_Data_Ref(12) = 506
Ext_User_Prm_Data_Ref(14) = 507
Ext_User_Prm_Data_Ref(16) = 508
EndModule


; WDIO100-WDI
Module="WDIO100-WDI" 0x5F							;16 AI
14
Ext_Module_Prm_Data_Len  = 20				;Number of used Param Bytes
Ext_User_Prm_Data_Const(0)=\					;Initialising of Param Data
								0x01, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,\
								0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00 

Ext_User_Prm_Data_Ref(0)  = 604
Ext_User_Prm_Data_Ref(2)  = 605
Ext_User_Prm_Data_Ref(4)  = 606
Ext_User_Prm_Data_Ref(6)  = 607
Ext_User_Prm_Data_Ref(8)  = 608
Ext_User_Prm_Data_Ref(10) = 609
Ext_User_Prm_Data_Ref(12) = 610
Ext_User_Prm_Data_Ref(14) = 611
Ext_User_Prm_Data_Ref(16) = 612
Ext_User_Prm_Data_Ref(18) = 616
EndModule

; WDIO100-WDX
Module="WDIO100-WDX" 0x5F, 0x63							;16 AI, 4 AO 
15
Ext_Module_Prm_Data_Len  = 20					;Number of used Param Bytes
Ext_User_Prm_Data_Const(0)=\					;Initialising of Param Data
								0x01, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,\
								0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00 

Ext_User_Prm_Data_Ref(0)  = 604
Ext_User_Prm_Data_Ref(2)  = 605
Ext_User_Prm_Data_Ref(4)  = 606
Ext_User_Prm_Data_Ref(6)  = 607
Ext_User_Prm_Data_Ref(8)  = 613
Ext_User_Prm_Data_Ref(10) = 614
Ext_User_Prm_Data_Ref(12) = 616
Ext_User_Prm_Data_Ref(14) = 617
Ext_User_Prm_Data_Ref(16) = 618
Ext_User_Prm_Data_Ref(18) = 619
EndModule

; WDIO100-WDP
Module="WDIO100-WDP" 0x5F, 0x66							;16 AI, 7 AO 
16
Ext_Module_Prm_Data_Len  = 12					;Number of used Param Bytes
Ext_User_Prm_Data_Const(0)=\					;Initialising of Param Data
								0x01, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00
								
Ext_User_Prm_Data_Ref(0)	= 604
Ext_User_Prm_Data_Ref(2)	= 615
Ext_User_Prm_Data_Ref(4)	= 616
Ext_User_Prm_Data_Ref(6)	= 617
Ext_User_Prm_Data_Ref(8)	= 618
Ext_User_Prm_Data_Ref(10)	= 619
EndModule


Module="Sensopart" 0x51								; 2AI
17
EndModule

													 ; Vogel Firmwareversion 2, 16.11.2004
Module="UFD10" 0x11,0x21 			 ; 2 Eingangsbyte 2 Ausgangsbyte
18
Ext_Module_Prm_Data_Len=24                      ;number of used data bytes
Ext_User_Prm_Data_Const(0) =\ ;initialising of param data
0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,\
0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,\
0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00


Ext_User_Prm_Data_Ref(0)        = 4000
Ext_User_Prm_Data_Ref(1)        = 4001
Ext_User_Prm_Data_Ref(2)        = 4002
Ext_User_Prm_Data_Ref(3)        = 4003
Ext_User_Prm_Data_Ref(4)        = 4004
Ext_User_Prm_Data_Ref(5)        = 4005
Ext_User_Prm_Data_Ref(6)        = 4006
Ext_User_Prm_Data_Ref(7)        = 4007
Ext_User_Prm_Data_Ref(8)        = 4008
Ext_User_Prm_Data_Ref(9)        = 4009
Ext_User_Prm_Data_Ref(10)        = 4010
Ext_User_Prm_Data_Ref(11)        = 4011
Ext_User_Prm_Data_Ref(12)        = 4012
Ext_User_Prm_Data_Ref(13)        = 4013
Ext_User_Prm_Data_Ref(14)        = 4014
Ext_User_Prm_Data_Ref(15)        = 4015
Ext_User_Prm_Data_Ref(16)        = 4016
Ext_User_Prm_Data_Ref(17)        = 4017
Ext_User_Prm_Data_Ref(18)        = 4018
Ext_User_Prm_Data_Ref(19)        = 4019
Ext_User_Prm_Data_Ref(20)        = 4020
Ext_User_Prm_Data_Ref(21)        = 4021
Ext_User_Prm_Data_Ref(22)        = 4022
Ext_User_Prm_Data_Ref(23)        = 4023
EndModule

														 ; Vogel Firmwareversion 2, 16.11.2004
Module="UFD20" 0x13,0x23 			; 4 Ausgangsbyte, 4 Eingangsbyte		
19
Ext_Module_Prm_Data_Len=48                      ;number of used data bytes
Ext_User_Prm_Data_Const(0) =\ ;initialising of param data
0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,\
0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,\
0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,\
0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,\
0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,\
0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00

Ext_User_Prm_Data_Ref(0)        = 4024
Ext_User_Prm_Data_Ref(1)        = 4025
Ext_User_Prm_Data_Ref(2)        = 4026
Ext_User_Prm_Data_Ref(3)        = 4027

Ext_User_Prm_Data_Ref(4)        = 4028
Ext_User_Prm_Data_Ref(5)        = 4029
Ext_User_Prm_Data_Ref(6)        = 4030
Ext_User_Prm_Data_Ref(7)        = 4031

Ext_User_Prm_Data_Ref(8)        = 4032
Ext_User_Prm_Data_Ref(9)        = 4033
Ext_User_Prm_Data_Ref(10)        = 4034
Ext_User_Prm_Data_Ref(11)        = 4035

Ext_User_Prm_Data_Ref(12)        = 4036
Ext_User_Prm_Data_Ref(13)        = 4037
Ext_User_Prm_Data_Ref(14)        = 4038
Ext_User_Prm_Data_Ref(15)        = 4039

Ext_User_Prm_Data_Ref(16)        = 4040
Ext_User_Prm_Data_Ref(17)        = 4041
Ext_User_Prm_Data_Ref(18)        = 4042
Ext_User_Prm_Data_Ref(19)        = 4043

Ext_User_Prm_Data_Ref(20)        = 4044
Ext_User_Prm_Data_Ref(21)        = 4045
Ext_User_Prm_Data_Ref(22)        = 4046
Ext_User_Prm_Data_Ref(23)        = 4047

Ext_User_Prm_Data_Ref(24)        = 4048
Ext_User_Prm_Data_Ref(25)        = 4049
Ext_User_Prm_Data_Ref(26)        = 4050
Ext_User_Prm_Data_Ref(27)        = 4051

Ext_User_Prm_Data_Ref(28)        = 4052
Ext_User_Prm_Data_Ref(29)        = 4053
Ext_User_Prm_Data_Ref(30)        = 4054
Ext_User_Prm_Data_Ref(31)        = 4055

Ext_User_Prm_Data_Ref(32)        = 4056
Ext_User_Prm_Data_Ref(33)        = 4057
Ext_User_Prm_Data_Ref(34)        = 4058
Ext_User_Prm_Data_Ref(35)        = 4059

Ext_User_Prm_Data_Ref(36)        = 4060
Ext_User_Prm_Data_Ref(37)        = 4061
Ext_User_Prm_Data_Ref(38)        = 4062
Ext_User_Prm_Data_Ref(39)        = 4063

Ext_User_Prm_Data_Ref(40)        = 4064
Ext_User_Prm_Data_Ref(41)        = 4065
Ext_User_Prm_Data_Ref(42)        = 4066
Ext_User_Prm_Data_Ref(43)        = 4067

Ext_User_Prm_Data_Ref(44)        = 4068
Ext_User_Prm_Data_Ref(45)        = 4069
Ext_User_Prm_Data_Ref(46)        = 4070
Ext_User_Prm_Data_Ref(47)        = 4071
EndModule

;Firmwareversion 14, 22.2.2006
Module="UFD10A" 0x11,0x21,0x56 			 ; 2 Eingangsbyte 2 Ausgangsbyte, 7AI
27
Ext_Module_Prm_Data_Len=24                      ;number of used data bytes
Ext_User_Prm_Data_Const(0) =\ ;initialising of param data
0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,\
0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,\
0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00


Ext_User_Prm_Data_Ref(0)        = 4072
Ext_User_Prm_Data_Ref(1)        = 4073
Ext_User_Prm_Data_Ref(2)        = 4074
Ext_User_Prm_Data_Ref(3)        = 4075
Ext_User_Prm_Data_Ref(4)        = 4076
Ext_User_Prm_Data_Ref(5)        = 4077
Ext_User_Prm_Data_Ref(6)        = 4078
Ext_User_Prm_Data_Ref(7)        = 4079
Ext_User_Prm_Data_Ref(8)        = 4080
Ext_User_Prm_Data_Ref(9)        = 4081
Ext_User_Prm_Data_Ref(10)        = 4082
Ext_User_Prm_Data_Ref(11)        = 4083
Ext_User_Prm_Data_Ref(12)        = 4084
Ext_User_Prm_Data_Ref(13)        = 4085
Ext_User_Prm_Data_Ref(14)        = 4086
Ext_User_Prm_Data_Ref(15)        = 4087
Ext_User_Prm_Data_Ref(16)        = 4088
Ext_User_Prm_Data_Ref(17)        = 4089
Ext_User_Prm_Data_Ref(18)        = 4090
Ext_User_Prm_Data_Ref(19)        = 4091
Ext_User_Prm_Data_Ref(20)        = 4092
Ext_User_Prm_Data_Ref(21)        = 4093
Ext_User_Prm_Data_Ref(22)        = 4094
Ext_User_Prm_Data_Ref(23)        = 4095
EndModule



Module="UFD20A" 0x13,0x23,0x5D    ;  4 Ausgangsbyte, 4 Eingangsbyte, 14AI		
28
Ext_Module_Prm_Data_Len=48                      ;number of used data bytes
Ext_User_Prm_Data_Const(0) =\ ;initialising of param data
0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,\
0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,\
0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,\
0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,\
0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,\
0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00

Ext_User_Prm_Data_Ref(0)        = 4096
Ext_User_Prm_Data_Ref(1)        = 4097
Ext_User_Prm_Data_Ref(2)        = 4098
Ext_User_Prm_Data_Ref(3)        = 4099

Ext_User_Prm_Data_Ref(4)        = 4100
Ext_User_Prm_Data_Ref(5)        = 4101
Ext_User_Prm_Data_Ref(6)        = 4102
Ext_User_Prm_Data_Ref(7)        = 4103

Ext_User_Prm_Data_Ref(8)        = 4104
Ext_User_Prm_Data_Ref(9)        = 4105
Ext_User_Prm_Data_Ref(10)        = 4106
Ext_User_Prm_Data_Ref(11)        = 4107

Ext_User_Prm_Data_Ref(12)        = 4108
Ext_User_Prm_Data_Ref(13)        = 4109
Ext_User_Prm_Data_Ref(14)        = 4110
Ext_User_Prm_Data_Ref(15)        = 4111

Ext_User_Prm_Data_Ref(16)        = 4112
Ext_User_Prm_Data_Ref(17)        = 4113
Ext_User_Prm_Data_Ref(18)        = 4114
Ext_User_Prm_Data_Ref(19)        = 4115

Ext_User_Prm_Data_Ref(20)        = 4116
Ext_User_Prm_Data_Ref(21)        = 4117
Ext_User_Prm_Data_Ref(22)        = 4118
Ext_User_Prm_Data_Ref(23)        = 4119

Ext_User_Prm_Data_Ref(24)        = 4120
Ext_User_Prm_Data_Ref(25)        = 4121
Ext_User_Prm_Data_Ref(26)        = 4122
Ext_User_Prm_Data_Ref(27)        = 4123

Ext_User_Prm_Data_Ref(28)        = 4124
Ext_User_Prm_Data_Ref(29)        = 4125
Ext_User_Prm_Data_Ref(30)        = 4126
Ext_User_Prm_Data_Ref(31)        = 4127

Ext_User_Prm_Data_Ref(32)        = 4128
Ext_User_Prm_Data_Ref(33)        = 4129
Ext_User_Prm_Data_Ref(34)        = 4130
Ext_User_Prm_Data_Ref(35)        = 4131

Ext_User_Prm_Data_Ref(36)        = 4132
Ext_User_Prm_Data_Ref(37)        = 4133
Ext_User_Prm_Data_Ref(38)        = 4134
Ext_User_Prm_Data_Ref(39)        = 4135

Ext_User_Prm_Data_Ref(40)        = 4136
Ext_User_Prm_Data_Ref(41)        = 4137
Ext_User_Prm_Data_Ref(42)        = 4138
Ext_User_Prm_Data_Ref(43)        = 4139

Ext_User_Prm_Data_Ref(44)        = 4140
Ext_User_Prm_Data_Ref(45)        = 4141
Ext_User_Prm_Data_Ref(46)        = 4142
Ext_User_Prm_Data_Ref(47)        = 4143
EndModule



Module="PR222DS" 0x19, 0x5F, 0x61 ; DI 10 byte, AI 16 Word, AO 2 Word
20
EndModule


Module="PR122/PR123/PR332/PR333" 0x1E, 0x5F, 0x61 ; DI 15 byte, AI 16 Word, AO 2 Word
21
EndModule


Module="PR223EF" 0x1B, 0x5F, 0x61 ; DI 12 byte, AI 16 Word, AO 2 Word
30
EndModule


Module="SS91-FBP" 0x17, 0x27			; 8DO, 8DI
22
EndModule


Module="LMC1_GLAS" 0x17, 0x27, 0x53, 0x63		; 64 DI, 64 DO, 4 AI, 4 AO
32
Ext_Module_Prm_Data_Len=10								  ;number of used data bytes
Ext_User_Prm_Data_Const(0)=\								 ;Initialising of Param data
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00

Ext_User_Prm_Data_Ref(0)	= 4565
Ext_User_Prm_Data_Ref(2)	= 4566
Ext_User_Prm_Data_Ref(4)	= 4567
Ext_User_Prm_Data_Ref(6)	= 4568
Ext_User_Prm_Data_Ref(8)	= 4570
EndModule

Module="ABB XR ITS" 0x1E, 0x5F, 0x61 ; DI 15 byte, AI 16 Word, AO 2 Word
34
EndModule



; DPV1 Alarm
DPV1_Slave                          = 1
C1_Read_Write_supp                  = 1
C1_Max_Data_Len                     = 8         ;The parameter specifies the maximum length of user data excluding
                                                ;Function_Num, Slot_number, Index, Length, transferred on the
                                                ;MSAC_1 communication channel.
                                                ;Type: Unsigned8 (0 .. 240)
C1_Response_Timeout                 = 300
Diagnostic_Alarm_supp               = 0
Process_Alarm_supp                  = 0
Pull_Plug_Alarm_supp                = 0
Status_Alarm_supp                   = 0
Update_Alarm_supp                   = 0
Manufacturer_Specific_Alarm_supp    = 0
Alarm_Sequence_Mode_Count           = 0
Alarm_Type_Mode_supp                = 0
Diagnostic_Alarm_required           = 0

C2_Read_Write_supp                  = 1
C2_Max_Data_Len                     = 48        ;The parameter specifies the maximum length of user data excluding
                                                ;Function_Num, Slot_number, Index, Length, transferred on the
                                                ;MSAC_2 communication channel.
                                                ;Type: Unsigned8 (0,48 .. 240)
C2_Response_Timeout                 = 300
C2_Read_Write_required              = 1
C2_Max_Count_Channels               = 3
Max_Initiate_PDU_Length             = 52        ;The parameter specifies the maximum length of an Initiate Request
                                                ;PDU including the Function_Num to the Resource Manager.
                                                ;Type: Unsigned8 (0,52.. 244)
DPV1_Data_Types                     = 0				;

Module="PSTX (FB 1.1)" 0x11, 0x23, 0x5a, 0x62			;16 DI, 32 DO, 11 AI, 3 AO, Compatible with CB-version 1.11.0.
37
EndModule