;======================================================
;======================================================
#Profibus_DP
;
; HIGHEST Module_Index currently in use: 21
;
; Version: 1.12 for ePlug DPV1-modular (PDQ22) modified by Brigitte Dien
; ** new modules UMC100.3 (Rx100 Rx200) and UMC100.3 Profile2 created by GSD-Generator, Date 25.08.2014 13:15:58

; Version: 1.11 for ePlug DPV1-modular (PDQ22) modified by Rolf Oestreich
; ** new module for I/O-Data-Profil 2 "UMC100(R0101 R0201)Profil2" added Date 14.11.2013 
;
; Version: 1.10 for ePlug DPV1-modular (PDQ22) modified by Brigitte Dien
; ** correction in line 3401 Date 11.12.2012 
;
; Version: 1.09 for ePlug DPV1-modular (PDQ22) modified by Rolf Oestreich
; ** new module UMC100 (R0101 R0201) created by GSD-Generator, Date 08.06.2011 07:28:52 
;
; Version: 1.08 for ePlug DPV1-modular (PDQ22) modified by Taji Kuruvilla/Brigitte Dien Date 2010-10-06
; ** new PSE added (module_index = 17)
;
; Version: 1.07 for ePlug DPV1-modular (PDQ22) modified by Brigitte Dien
; ** new module UMC100 created by GSD-Generator, Date 27.04.2010 11:24:33 
;
; Version: 1.07 for ePlug DPV1-modular (PDQ22) modified by Rolf Oestreich  
; ** Max_User_Prm_Data_Len changed from 237 -> 228, Date 15.03.2010 07:11:00 
;
; Version: 1.06 for ePlug DPV1-modular (PDQ22) modified by Brigitte Dien  
; ** new module UMC100 created by GSD-Generator, Date 28.10.2009 10:30:10 
;
; Version: 1.05 for ePlug DPV1-modular (PDQ22) modified by Brigitte Dien  Date 2007-06-21
; ** new UMC22 V4.00 1SAJ 510000 R0600 added (module_index = 15)
; ** current factor limit from 100 --> 2 changed
; ** local control boundary expanded from 5 --> 9       
;
; Version: 1.04 for ePlug DPV1-modular (PDQ22) modified by Brigitte Dien  Date 2007-02-15
; ** new modules: WDIO100-WDI,-WDP,-WDX
; ** WDI100: Cell ID from 1..59, default 1
;
; Version: 1.03 for ePlug DPV1-modular (PDQ22) modified by Brigitte Dien  Date 2006-11-22
; ** corrected: Set Current 1/2 for UMC22 V3.30 6300 -> 320000
;
; Version: 1.02 for ePlug DPV1-modular (PDQ22) modified by Brigitte Dien  Date 2006-07-31
; ** Comment for DPV1-Parameter-Bytes added
;
; Version: 1.01 for ePlug DPV1 (PDQ22) modified by Brigitte Dien  Date 2006-07-05
; ** modifictions in Diag-Area: for DTM-integration each bit has to be descibed
; ** Softstarter PSR inserted
;
; Version: 1.00  for FieldBusPlug DPV1 (PDQ22) created by Rolf Oestreich  Date 2005-10-25 
;
; History:
; 
;
; GSD file for the Plug PDQ22 valid for:
;
;	DEVICE / ID / firmware-version / device index
;-----------------------------------------------------
;	Sensor (direct)	  / -                 / -          / all
; 	MSD11             / 1SAJ 310000 Rxxxx / -          / all
;	MSR22             / 1SAJ 320000 Rxxxx / -          / all
;	MFI21             / 1SAJ 410000 R0100 / -          / all
;	UMC22 V3.0, 3.10  / 1SAJ 510000 R0100 / V3.0 V3.10 / a30  a31
; 	UMC22 V3.10, 3.20 / 1SAJ 510000 R0200 / V3.20      / b32
; 	UMC22 V3.30       / 1SAJ 510000 R0300 / V3.30      / b33
; 	UMC22 V3.40       / 1SAJ 510000 R0400 / V3.40      / c34
; 	UMC22 V3.50       / 1SAJ 510000 R0500 / V3.50      /

; 	UMC22 V4.00       / 1SAJ 510000 R0600 / V4.00      / c40

;	Wireless WDI100   / -                 / WDI100_Ver0_Rev9_5 / -
;	Wireless WDIO100  / WDX / WDP / WDI          / 
;	PSR						 /
; 	UMC100 V1.10          
; 
;	If additional "Ext_User_Prm_Data_Ref" numbers for new devices are defined,
;	they must fit into the following predefined ranges:
;	STO Heidelberg		range 0...999
;	Sweden 					range 1000...1999
;	Italy					range 2000...2999 
;
; 				
;=============================================================
; Text-definition for User Prm Data  "UMC22_FBP (V3.0)"
;=============================================================
;
PrmText = 2
Text(0)   = "Acknowledge"
Text(1)   = "Auto"
EndPrmText
;PrmText = 4
;Text(1)   = "Trip"
;EndPrmText
PrmText = 5
Text(0)   = "Relays Off"
Text(1)   = "Outputs Retain Status"
EndPrmText
PrmText = 6
Text(0)  = "Class  5"
Text(1)  = "Class 10"
Text(2)  = "Class 20"
Text(3)  = "Class 30"
EndPrmText
PrmText = 7
Text(1)  = "Transparent"
Text(2)  = "Overload Relay"
Text(3)  = "Direct Starter"
Text(4)  = "Reversing Starter"
Text(5)  = "Star-Delta Starter 1"
Text(6)  = "Pole-Changing Starter 1"
EndPrmText
PrmText = 16
Text(0)   = "Off"
Text(1)   = "On"
EndPrmText
PrmText = 17
Text(1)   = "Auxiliary Contacts"
Text(2)   = "Motor Current"
Text(3)   = "Simulation"
EndPrmText
PrmText = 18
Text(0)   = "Time"
Text(1)   = "Current"
EndPrmText
; do not delete this comment, req. by FB1131
;ExtUserPrmData =  1 "0301 Set Current 1=10mA*"
;Unsigned32 50 24-6300
;EndExtUserPrmData
ExtUserPrmData =  1 "0301 Set Current 1=10mA*"
Unsigned32 50 24-6300
EndExtUserPrmData
;ExtUserPrmData =  2 "Factor for Current Transformer"
;Unsigned16 1 0-200
;EndExtUserPrmData
ExtUserPrmData =  3 "0401 Trip Class"
Unsigned8 1 0-3
Prm_Text_Ref = 6
EndExtUserPrmData
;ExtUserPrmData =  4 "Overload Behaviour"
;Unsigned8 1 1-1
;Prm_Text_Ref = 4
;EndExtUserPrmData
ExtUserPrmData =  5 "0402 Phase Loss Protection"
Unsigned8 1 0-1
Prm_Text_Ref = 16
EndExtUserPrmData
ExtUserPrmData =  6 "0407 Low Current Threshold=5%*"
Unsigned8 10 6-20
EndExtUserPrmData
ExtUserPrmData =  7 "0408 High Current Threshold=5%*"
Unsigned8 30 20-160
EndExtUserPrmData
ExtUserPrmData =  8 "0403 Cooling Time=0.1s*"
Unsigned16 1200 300-36000
EndExtUserPrmData
ExtUserPrmData =  9 "0404 Automatic fault reset"
Unsigned8 0 0-1
Prm_Text_Ref = 2
EndExtUserPrmData
ExtUserPrmData = 10 "0101 Control Function"
Unsigned8 1 1-6
Prm_Text_Ref = 7
EndExtUserPrmData
ExtUserPrmData = 11 "0202 Check Back"
Unsigned8 2 1-3
Prm_Text_Ref = 17
EndExtUserPrmData
ExtUserPrmData = 12 "0207 Star-Delta Start.Time=0.1s*"
Unsigned16 600 10-36000
EndExtUserPrmData
ExtUserPrmData = 13 "0205 Revers. Lockout Time=0.1s*"
Unsigned16 20 2-36000
EndExtUserPrmData
;ExtUserPrmData = 14 "0601 Operating Hours of Motor"
;Unsigned32 0 0-15000000
;EndExtUserPrmData
;ExtUserPrmData = 15 "0602 Number of Starts"
;Unsigned32 0 0-15000000
;EndExtUserPrmData
ExtUserPrmData = 16 "0501 Commun. fault reaction"
Unsigned8 0 0-1
Prm_Text_Ref = 5
EndExtUserPrmData
ExtUserPrmData = 17 "0405 Start Up Time=0.1s*"
Unsigned16 1200 0-6000
EndExtUserPrmData
ExtUserPrmData = 18 "0201 Local Control via DIs"
Unsigned8 0 0-1
Prm_Text_Ref = 16
EndExtUserPrmData
ExtUserPrmData = 19 "0406 Block.Current Threshold=5%*"
Unsigned8 160 0-160
EndExtUserPrmData
ExtUserPrmData = 20 "0204 Fault Output"
Unsigned8 0 0-1
Prm_Text_Ref = 16
EndExtUserPrmData
ExtUserPrmData = 21 "0206 Star-Delta Changeover Mode"
Unsigned8 1 0-1
Prm_Text_Ref = 18
EndExtUserPrmData
ExtUserPrmData = 23 "0302 Set Current 2=10mA*"
Unsigned32 50 24-6300
EndExtUserPrmData
ExtUserPrmData = 24 "0203 Fault Input"
Unsigned8 0 0-1
Prm_Text_Ref = 16
EndExtUserPrmData
ExtUserPrmData = 25 "0502 Address Check"
Unsigned8 0 0-1
Prm_Text_Ref = 16
EndExtUserPrmData
;
;=============================================================
; Text-definition for User Prm Data  "UMC22_FBP (V3.10, V3.20)"
;=============================================================
;
PrmText = 102
Text(0)   = "Disabled"
Text(1)   = "Autoreset"
EndPrmText
;PrmText = 104
;Text(1)   = "Trip"
;EndPrmText
PrmText = 105
Text(0)   = "Relays Off"
Text(1)   = "Outputs Retain Status"
EndPrmText
PrmText = 106
Text(0)  = "Class  5"
Text(1)  = "Class 10"
Text(2)  = "Class 20"
Text(3)  = "Class 30"
EndPrmText
PrmText = 107
Text(1)  = "Transparent"
Text(2)  = "Overload Relay"
Text(3)  = "Direct Starter"
Text(4)  = "Reversing Starter"
Text(5)  = "Star-Delta Starter 1"
Text(6)  = "Pole-Changing Starter 1"
EndPrmText
PrmText = 116
Text(0)   = "Off"
Text(1)   = "On"
EndPrmText
PrmText = 117
Text(1)   = "Auxiliary Contacts"
Text(2)   = "Motor Current"
Text(3)   = "Simulation"
EndPrmText
PrmText = 118
Text(0)   = "Time"
Text(1)   = "Current"
EndPrmText
; do not delete this comment, req. by FB1131
;ExtUserPrmData = 101 "01 Set Current 1=10mA*"
;Unsigned32 50 24-320000
;EndExtUserPrmData
ExtUserPrmData = 101 "01 Set Current 1=10mA*"
Unsigned32 50 24-320000
EndExtUserPrmData
ExtUserPrmData = 102 "02 Current Factor"
Unsigned16 100 100-64000
EndExtUserPrmData
ExtUserPrmData = 103 "04 Trip Class"
Unsigned8 1 0-3
Prm_Text_Ref = 106
EndExtUserPrmData
;ExtUserPrmData =  104 "05 Overload Behaviour"
;Unsigned8 1 1-1
;Prm_Text_Ref = 4
;EndExtUserPrmData
ExtUserPrmData =  105 "06 Phase Loss Protection"
Unsigned8 1 0-1
Prm_Text_Ref = 116
EndExtUserPrmData
ExtUserPrmData =  106 "08 Low Current Threshold=5%*"
Unsigned8 10 6-20
EndExtUserPrmData
ExtUserPrmData =  107 "09 High Current Threshold=5%*"
Unsigned8 30 20-160
EndExtUserPrmData
ExtUserPrmData =  108 "10 Cooling Time=0.1s*"
Unsigned16 1200 300-36000
EndExtUserPrmData
ExtUserPrmData =  109 "11 Automatic fault reset"
Unsigned8 0 0-1
Prm_Text_Ref = 102
EndExtUserPrmData
ExtUserPrmData = 110 "12 Control Function"
Unsigned8 1 1-6
Prm_Text_Ref = 107
EndExtUserPrmData
ExtUserPrmData = 111 "13 Check-Back"
Unsigned8 2 1-3
Prm_Text_Ref = 117
EndExtUserPrmData
ExtUserPrmData = 112 "16 Star-Delta Start.Time=0.1s*"
Unsigned16 600 10-36000
EndExtUserPrmData
ExtUserPrmData = 113 "17 Reverse Lockout Time=0.1s*"
Unsigned16 20 2-36000
EndExtUserPrmData
ExtUserPrmData = 114 "18 Operating Hours of Motor"
Unsigned16 0 0-65535
EndExtUserPrmData
ExtUserPrmData = 115 "19 Number of Starts"
Unsigned32 0 0-1000000
EndExtUserPrmData
ExtUserPrmData = 116 "20 Bus fault reaction"
Unsigned8 0 0-1
Prm_Text_Ref = 105
EndExtUserPrmData
ExtUserPrmData = 117 "14 Start-Up Time=0.1s*"
Unsigned16 1200 0-6000
EndExtUserPrmData
ExtUserPrmData = 118 "22 Local Control via DIs"
Unsigned8 0 0-1
Prm_Text_Ref = 116
EndExtUserPrmData
ExtUserPrmData = 119 "23 Block.Current Threshold=5%*"
Unsigned8 160 0-160
EndExtUserPrmData
ExtUserPrmData = 120 "24 Fault Output"
Unsigned8 0 0-1
Prm_Text_Ref = 116
EndExtUserPrmData
ExtUserPrmData = 121 "15 Star-Delta Changeover Mode"
Unsigned8 1 0-1
Prm_Text_Ref = 118
EndExtUserPrmData
ExtUserPrmData = 123 "03 Set Current 2=10mA*"
Unsigned32 50 24-320000
EndExtUserPrmData
ExtUserPrmData = 124 "21 Fault Input"
Unsigned8 0 0-1
Prm_Text_Ref = 116
EndExtUserPrmData
ExtUserPrmData = 125 "26 Address Check"
Unsigned8 0 0-1
Prm_Text_Ref = 116
EndExtUserPrmData
ExtUserPrmData = 126 "25 Number of Trips"
Unsigned8 0 0-255
EndExtUserPrmData
;ExtUserPrmData = 127 "07 Load type"
;Unsigned8 1 1-1
;EndExtUserPrmData
;
;
;=============================================================
; Text-definition for User Prm Data  "UMC22_FBP (V3.30)"
;=============================================================
;
PrmText = 152
Text(0)   = "Disabled"
Text(1)   = "Autoreset"
EndPrmText
;PrmText = 154
;Text(1)   = "Trip"
;EndPrmText
PrmText = 155
Text(0)   = "Relays Off"
Text(1)   = "Outputs Retain Status"
EndPrmText
PrmText = 156
Text(0)  = "Class  5"
Text(1)  = "Class 10"
Text(2)  = "Class 20"
Text(3)  = "Class 30"
EndPrmText
PrmText = 157
Text(1)  = "Transparent"
Text(2)  = "Overload Relay"
Text(3)  = "Direct Starter"
Text(4)  = "Reversing Starter"
Text(5)  = "Star-Delta Starter 1"
Text(6)  = "Pole-Changing Starter 1"
Text(7)  = "Actuator 1"
Text(8)  = "Actuator 2"
Text(9)  = "Actuator 3"
Text(10) = "Actuator 4"
EndPrmText
PrmText = 166
Text(0)   = "Off"
Text(1)   = "On"
EndPrmText
PrmText = 167
Text(1)   = "Auxiliary Contacts"
Text(2)   = "Motor Current"
Text(3)   = "Simulation"
EndPrmText
PrmText = 168
Text(0)   = "Time"
Text(1)   = "Current"
EndPrmText
PrmText = 169
Text(0)   = "Off"
Text(1)   = "On"
Text(2)   = "002"
Text(3)   = "003"
Text(4)   = "004"
Text(5)   = "005"
EndPrmText
; do not delete this comment, req. by FB1131
;ExtUserPrmData = 151 "01 Set Current 1=10mA*"
;Unsigned32 50 24-6300
;EndExtUserPrmData
ExtUserPrmData = 151 "01 Set Current 1=10mA*"
Unsigned32 50 24-32000
EndExtUserPrmData
ExtUserPrmData = 152 "02 Current Factor (%)" 
Unsigned16 100 100-64000
EndExtUserPrmData
ExtUserPrmData = 153 "04 Trip Class"
Unsigned8 1 0-3
Prm_Text_Ref = 156
EndExtUserPrmData
ExtUserPrmData =  154 "05 DI0 Multi Function Input" 
Unsigned8 0 0-255
EndExtUserPrmData
ExtUserPrmData =  155 "06 Phase Loss Protection"
Unsigned8 1 0-1
Prm_Text_Ref = 166
EndExtUserPrmData
ExtUserPrmData =  156 "08 Low Current Threshold=5%*"
Unsigned8 10 1-20				   
EndExtUserPrmData
ExtUserPrmData =  157 "09 High Current Threshold=5%*"
Unsigned8 30 20-160
EndExtUserPrmData
ExtUserPrmData =  158 "10 Cooling Time=0.1s*"
Unsigned16 1200 300-36000
EndExtUserPrmData
ExtUserPrmData =  159 "11 Automatic fault reset"
Unsigned8 0 0-1
Prm_Text_Ref = 152
EndExtUserPrmData
ExtUserPrmData = 160 "12 Control Function"
Unsigned8 1 1-10
Prm_Text_Ref = 157
EndExtUserPrmData
ExtUserPrmData = 161 "13 Check-Back"
Unsigned8 2 1-3
Prm_Text_Ref = 167
EndExtUserPrmData
ExtUserPrmData = 162 "16 Star-Delta Start.Time=0.1s*"
Unsigned16 600 10-36000
EndExtUserPrmData
ExtUserPrmData = 163 "17 Reverse Lockout Time=0.1s*"
Unsigned16 20 2-36000
EndExtUserPrmData
ExtUserPrmData = 164 "18 Operating Hours of Motor"
Unsigned16 0 0-65535
EndExtUserPrmData
ExtUserPrmData = 165 "19 Number of Starts"
Unsigned32 0 0-1000000
EndExtUserPrmData
ExtUserPrmData = 166 "20 Bus fault reaction"
Unsigned8 0 0-1
Prm_Text_Ref = 155
EndExtUserPrmData
ExtUserPrmData = 167 "14 Start-Up Time=0.1s*"
Unsigned16 1200 0-6000
EndExtUserPrmData
ExtUserPrmData = 168 "22 Local Control" 
Unsigned8 0 0-5
Prm_Text_Ref = 169
EndExtUserPrmData
ExtUserPrmData = 169 "23 Block.Current Threshold=5%*"
Unsigned8 160 0-160
EndExtUserPrmData
ExtUserPrmData = 170 "24 Fault Output"
Unsigned8 0 0-1
Prm_Text_Ref = 166
EndExtUserPrmData
ExtUserPrmData = 171 "15 Star-Delta Changeover Mode"
Unsigned8 1 0-1
Prm_Text_Ref = 168
EndExtUserPrmData
ExtUserPrmData = 173 "03 Set Current 2=10mA*"
Unsigned32 50 24-320000
EndExtUserPrmData
ExtUserPrmData = 174 "21 DI2 Multi Function Input"
Unsigned8 0 0-255
EndExtUserPrmData
ExtUserPrmData = 175 "26 Address Check"
Unsigned8 0 0-1
Prm_Text_Ref = 166
EndExtUserPrmData
ExtUserPrmData = 176 "25 Number of Trips"
Unsigned8 0 0-255
EndExtUserPrmData
ExtUserPrmData = 177 "07 DI1 Multi Function Input"
Unsigned8 0 0-255
EndExtUserPrmData
ExtUserPrmData = 178 "27 Emergency by PLC"
Unsigned8 0 0-1
Prm_Text_Ref = 166
EndExtUserPrmData
;
;==============================================================
; Text-definition for User Prm Data  "UMC22_FBP (V3.40, V3.50)"
;==============================================================
;
PrmText = 170
Text(0)   = "Off"
Text(1)   = "On"
Text(2)   = "Off+PTC Warn"
Text(3)   = "On+PTC Warn"
;Text(4)   = "004"
;Text(5)   = "005"
Text(6)   = "Off+PTC Trip"
Text(7)   = "On+PTC Trip"
EndPrmText

PrmText = 171
Text(1)  = "Transparent"
Text(2)  = "Overload Relay"
Text(3)  = "Direct Starter"
Text(4)  = "Reversing Starter"
Text(5)  = "Star-Delta Starter 1"
Text(6)  = "Pole-Changing Starter 1"
Text(7)  = "Actuator 1"
Text(8)  = "Actuator 2"
Text(9)  = "Actuator 3"
Text(10) = "Actuator 4"
Text(11) = "Star-Delta Starter 2"
EndPrmText

PrmText = 172
Text(0)   = "Off"
Text(1)   = "On"
Text(3)   = "blink"
EndPrmText



ExtUserPrmData = 181 "01 Set Current 1=10mA*"
Unsigned32 50 24-320000
EndExtUserPrmData
ExtUserPrmData = 182 "02 Current Factor (%)" 
Unsigned16 100 100-64000
EndExtUserPrmData
ExtUserPrmData = 183 "04 Trip Class"
Unsigned8 1 0-3
Prm_Text_Ref = 156
EndExtUserPrmData
ExtUserPrmData =  184 "05 DI0 Multi Function Input" 
Unsigned8 0 0-255
EndExtUserPrmData
ExtUserPrmData =  185 "06 Phase Loss Protection"
Unsigned8 1 0-7
Prm_Text_Ref = 170
EndExtUserPrmData

ExtUserPrmData =  186 "08 Low Current Threshold=5%*"
Unsigned8 10 1-20				   
EndExtUserPrmData
ExtUserPrmData =  187 "09 High Current Threshold=5%*"
Unsigned8 30 20-160
EndExtUserPrmData
ExtUserPrmData =  188 "10 Cooling Time=0.1s*"
Unsigned16 1200 300-36000
EndExtUserPrmData
ExtUserPrmData =  189 "11 Automatic fault reset"
Unsigned8 0 0-1
Prm_Text_Ref = 152
EndExtUserPrmData

ExtUserPrmData = 190 "12 Control Function"
Unsigned8 1 1-11
Prm_Text_Ref = 171
EndExtUserPrmData

ExtUserPrmData = 191 "13 Check-Back"
Unsigned8 2 1-3
Prm_Text_Ref = 167
EndExtUserPrmData
ExtUserPrmData = 192 "16 Star-Delta Start.Time=0.1s*"
Unsigned16 600 10-36000
EndExtUserPrmData
ExtUserPrmData = 193 "17 Reverse Lockout Time=0.1s*"
Unsigned16 20 2-36000
EndExtUserPrmData
ExtUserPrmData = 194 "18 Operating Hours of Motor"
Unsigned16 0 0-65535
EndExtUserPrmData
ExtUserPrmData = 195 "19 Number of Starts"
Unsigned32 0 0-1000000
EndExtUserPrmData
ExtUserPrmData = 196 "20 Bus fault reaction"
Unsigned8 0 0-1
Prm_Text_Ref = 155
EndExtUserPrmData
ExtUserPrmData = 197 "14 Start-Up Time=0.1s*"
Unsigned16 1200 0-6000
EndExtUserPrmData
ExtUserPrmData = 198 "22 Local Control" 
Unsigned8 0 0-5
Prm_Text_Ref = 169
EndExtUserPrmData
ExtUserPrmData = 199 "23 Block.Current Threshold=5%*"
Unsigned8 160 0-160
EndExtUserPrmData

ExtUserPrmData = 200 "24 Fault Output"
Unsigned8 0 0-3
Prm_Text_Ref = 172
EndExtUserPrmData

ExtUserPrmData = 201 "15 Star-Delta Changeover Mode"
Unsigned8 1 0-1
Prm_Text_Ref = 168
EndExtUserPrmData
ExtUserPrmData = 203 "03 Set Current 2=10mA*"
Unsigned32 50 24-320000
EndExtUserPrmData
ExtUserPrmData = 204 "21 DI2 Multi Function Input"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData = 205 "26 Address Check"
Unsigned8 0 0-1
Prm_Text_Ref = 166
EndExtUserPrmData
ExtUserPrmData = 206 "25 Number of Trips"
Unsigned8 0 0-255
EndExtUserPrmData
ExtUserPrmData = 207 "07 DI1 Multi Function Input"
Unsigned8 0 0-255
EndExtUserPrmData
ExtUserPrmData = 208 "27 Emergency by PLC"
Unsigned8 0 0-1
Prm_Text_Ref = 166
EndExtUserPrmData

;
;=============================================================
; Text-definition for User Prm Data  "UMC22_FBP (V4.00)"
; only changes compared to "UMC22_FBP (V3.40)"
;=============================================================
;
PrmText = 173
Text(0)   = "Off"
Text(1)   = "On"
Text(2)   = "002"
Text(3)   = "003"
Text(4)   = "004"
Text(5)   = "005"
Text(6)   = "006"
Text(7)   = "007"
Text(8)   = "008"
Text(9)   = "009"
EndPrmText
;
ExtUserPrmData = 210 "22 Local Control" 
Unsigned8 0 0-9
Prm_Text_Ref = 173
EndExtUserPrmData
;
ExtUserPrmData = 211 "02 Current Factor (%)" 
Unsigned16 100 2-64000
EndExtUserPrmData

;
;=============================================================
; Text-definition for User Prm Data "MFI21-FBP"
;=============================================================
;
PrmText=50
Text(0)= "No Configuration"
Text(1)= "Direct, FB=Off"
Text(2)= "Direct, FB=On"
Text(3)= "Reverse, FB=Off"
Text(4)= "Reverse, FB=On"
Text(5)= "Star-Delta, FB=Off"
Text(6)= "Star-Delta, FB=On"
Text(7)= "MFI Transparent"
EndPrmText
; do not delete this comment, req. by FB1131
;ExtUserPrmData=50	"MFI Mode"
;Unsigned8 0 0-7	
;Prm_Text_Ref=50
;EndExtUserPrmData
ExtUserPrmData=50	"MFI Mode"			; MFI application mode
Unsigned8 0 0-7								; Default 0, range 0..7
Prm_Text_Ref=50								; Reference to PrmText 50
EndExtUserPrmData

ExtUserPrmData=51   "Start-Delta Time = 1ms*"	; MFI delay time in ms
Unsigned32 50 50-260100		   	; Default 50 ms, range 50..260100 ms
EndExtUserPrmData


;=============================================================
; Text-definition for User Prm Data  UMC100_FBP (V1.13)
;=============================================================
;
ExtUserPrmData =  401  "Setting Ie 1 [0.01A]"
Unsigned32 50 24-320000
EndExtUserPrmData

ExtUserPrmData =  402  "Setting Ie 2 [0.01A]"
Unsigned32 50 24-320000
EndExtUserPrmData

ExtUserPrmData =  403  "YD Starting Time [0.1s]"
Unsigned16 600 10-36000
EndExtUserPrmData

ExtUserPrmData =  404  "Current Factor [%]"
Unsigned16 100 2-64000
EndExtUserPrmData

ExtUserPrmData =  405  "Cooling Time [s]"
Unsigned16 120 30-64000
EndExtUserPrmData

PrmText = 406 
Text(0) = "English"
Text(1) = "Deutsch"
Text(2) = "Francais"
Text(3) = "Espanol"
Text(4) = "Italiano"
Text(5) = "Portugues"
EndPrmText
ExtUserPrmData =  406  "Language"
Unsigned8 0 0-5
Prm_Text_Ref = 406 
EndExtUserPrmData

ExtUserPrmData =  407  "Rev Lock-Out Time [s]"
Unsigned8 1 1-255
EndExtUserPrmData

PrmText = 408 
Text(0) = "Off"
Text(1) = "Flash DO2"
Text(2) = "On DO2"
Text(3) = "Invert DO2"
Text(4) = "Flash DO3"
Text(5) = "On DO3"
Text(6) = "Invert DO3"
EndPrmText
ExtUserPrmData =  408  "Fault Output"
Unsigned8 0 0-6
Prm_Text_Ref = 408 
EndExtUserPrmData

PrmText = 409 
Text(0) = "Class 5"
Text(1) = "Class 10"
Text(2) = "Class 20"
Text(3) = "Class 30"
Text(4) = "Class 40"
EndPrmText
ExtUserPrmData =  409  "Trip Class"
Unsigned8 1 0-4
Prm_Text_Ref = 409 
EndExtUserPrmData

ExtUserPrmData =  410  "Low Curr Warn Level [5%]"
Unsigned8 10 0-20
EndExtUserPrmData

ExtUserPrmData =  411  "Low Curr Trip Level [5%]"
Unsigned8 0 0-20
EndExtUserPrmData

ExtUserPrmData =  412  "High Curr Warn Level [5%]"
Unsigned8 30 20-160
EndExtUserPrmData

ExtUserPrmData =  413  "High Curr Trip Level [5%]"
Unsigned8 160 20-160
EndExtUserPrmData

ExtUserPrmData =  414  "Locked Rotor Level [5%]"
Unsigned8 160 20-160
EndExtUserPrmData

ExtUserPrmData =  415  "Locked Rotor Delay [0.1s]"
Unsigned8 5 0-255
EndExtUserPrmData

ExtUserPrmData =  416  "Custom App Parameter"
Unsigned8 0 0-255
EndExtUserPrmData

PrmText = 417 
Text(0) = "Off"
Text(1) = "Stop (NC)"
Text(2) = "Stop (NO)"
Text(3) = "Ext. Flt (NC) always"
Text(4) = "Ext. Flt (NO) always"
Text(5) = "Ext. Flt (NC) Motor on"
Text(6) = "Ext. Flt (NO) Motor on"
Text(7) = "Prep. emerg. Start (NC)"
Text(8) = "Prep. emerg. Start (NO)"
Text(9) = "Testposition (NC)"
Text(10) = "Testposition (NO)"
Text(11) = "Force local (NC)"
Text(12) = "Force local (NO)"
Text(13) = "Fault reset (NC)"
Text(14) = "Fault reset (NO)"
Text(15) = "Voltage DIP (NC)"
Text(16) = "Voltage DIP (NO)"
Text(17) = "CEM11 always (Warning)"
Text(18) = "CEM11 after startup (Warning)"
Text(19) = "CEM11 always (Fault)"
Text(20) = "CEM11 after startup time (Fault)"
EndPrmText
ExtUserPrmData =  417  "Multif In 0"
Unsigned8 0 0-20
Prm_Text_Ref = 417 
EndExtUserPrmData

PrmText = 418 
Text(0) = "Off"
Text(1) = "Stop (NC)"
Text(2) = "Stop (NO)"
Text(3) = "Ext. Flt (NC) always"
Text(4) = "Ext. Flt (NO) always"
Text(5) = "Ext. Flt (NC) Motor on"
Text(6) = "Ext. Flt (NO) Motor on"
Text(7) = "Prep. emerg. Start (NC)"
Text(8) = "Prep. emerg. Start (NO)"
Text(9) = "Testposition (NC)"
Text(10) = "Testposition (NO)"
Text(11) = "Force local (NC)"
Text(12) = "Force local (NO)"
Text(13) = "Fault reset (NC)"
Text(14) = "Fault reset (NO)"
Text(15) = "Voltage DIP (NC)"
Text(16) = "Voltage DIP (NO)"
Text(17) = "CEM11 always (Warning)"
Text(18) = "CEM11 after startup (Warning)"
Text(19) = "CEM11 always (Fault)"
Text(20) = "CEM11 after startup time (Fault)"
EndPrmText
ExtUserPrmData =  418  "Multif In 1"
Unsigned8 0 0-20
Prm_Text_Ref = 418 
EndExtUserPrmData

PrmText = 419 
Text(0) = "Off"
Text(1) = "Stop (NC)"
Text(2) = "Stop (NO)"
Text(3) = "Ext. Flt (NC) always"
Text(4) = "Ext. Flt (NO) always"
Text(5) = "Ext. Flt (NC) Motor on"
Text(6) = "Ext. Flt (NO) Motor on"
Text(7) = "Prep. emerg. Start (NC)"
Text(8) = "Prep. emerg. Start (NO)"
Text(9) = "Testposition (NC)"
Text(10) = "Testposition (NO)"
Text(11) = "Force local (NC)"
Text(12) = "Force local (NO)"
Text(13) = "Fault reset (NC)"
Text(14) = "Fault reset (NO)"
Text(15) = "Voltage DIP (NC)"
Text(16) = "Voltage DIP (NO)"
Text(17) = "CEM11 always (Warning)"
Text(18) = "CEM11 after startup (Warning)"
Text(19) = "CEM11 always (Fault)"
Text(20) = "CEM11 after startup time (Fault)"
EndPrmText
ExtUserPrmData =  419  "Multif In 2"
Unsigned8 0 0-20
Prm_Text_Ref = 419 
EndExtUserPrmData

ExtUserPrmData =  420  "Multif In 0 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  421  "Multif In 1 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  422  "Multif In 2 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

PrmText = 423 
Text(1) = "Transparent"
Text(2) = "Overload Relay"
Text(3) = "Direct Starter"
Text(4) = "Reverse Starter"
Text(5) = "Star-delta Starter"
Text(7) = "Pole-Changing Starter"
Text(9) = "Actuator 1"
Text(10) = "Actuator 2"
Text(11) = "Actuator 3"
Text(12) = "Actuator 4"
EndPrmText
ExtUserPrmData =  423  "Control Function"
Unsigned8 3 1-12
Prm_Text_Ref = 423 
EndExtUserPrmData

PrmText = 424 
Text(0) = "Motor Off"
Text(1) = "Retain"
Text(2) = "Start Forward"
Text(3) = "Start Reverse"
EndPrmText
ExtUserPrmData =  424  "Busfault Reaction"
BitArea(0-3) 0 0-3
Prm_Text_Ref = 424 
EndExtUserPrmData

PrmText = 425 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  425  "Aux Inp 1 Reaction"
BitArea(0-3) 0 0-8
Prm_Text_Ref = 425 
EndExtUserPrmData

PrmText = 426 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  426  "Aux Inp 2 Reaction"
BitArea(4-7) 0 0-8
Prm_Text_Ref = 426 
EndExtUserPrmData

PrmText = 427 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  427  "Aux Inp 3 Reaction"
BitArea(0-3) 0 0-8
Prm_Text_Ref = 427 
EndExtUserPrmData

PrmText = 428 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  428  "Aux Inp 4 Reaction"
BitArea(4-7) 0 0-8
Prm_Text_Ref = 428 
EndExtUserPrmData

PrmText = 429 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  429  "Aux Inp 5 Reaction"
BitArea(0-3) 0 0-8
Prm_Text_Ref = 429 
EndExtUserPrmData

PrmText = 430 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  430  "Aux Inp 6 Reaction"
BitArea(4-7) 0 0-8
Prm_Text_Ref = 430 
EndExtUserPrmData

PrmText = 431 
Text(0) = "Disabled"
Text(1) = "Trip"
Text(2) = "Warning"
EndPrmText
ExtUserPrmData =  431  "PTC, Thermistor"
BitArea(0-1) 0 0-2
Prm_Text_Ref = 431 
EndExtUserPrmData

PrmText = 432 
Text(1) = "Contact DI0"
Text(2) = "Current"
Text(3) = "Simulation"
EndPrmText
ExtUserPrmData =  432  "Check-Back"
BitArea(2-3) 2 1-3
Prm_Text_Ref = 432 
EndExtUserPrmData

PrmText = 433 
Text(0) = "Disabled"
Text(1) = "Trip"
Text(2) = "Warning"
EndPrmText
ExtUserPrmData =  433  "Check Phase Sequence"
BitArea(4-5) 0 0-2
Prm_Text_Ref = 433 
EndExtUserPrmData

PrmText = 434 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  434  "Fault Auto Reset"
Bit(0) 0 0-1
Prm_Text_Ref = 434 
EndExtUserPrmData

PrmText = 435 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  435  "Emergency Start"
Bit(1) 0 0-1
Prm_Text_Ref = 435 
EndExtUserPrmData

PrmText = 436 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  436  "Address Check"
Bit(3) 0 0-1
Prm_Text_Ref = 436 
EndExtUserPrmData

PrmText = 437 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  437  "Enable Custom Logic"
Bit(4) 0 0-1
Prm_Text_Ref = 437 
EndExtUserPrmData

PrmText = 438 
Text(0) = "Time"
Text(1) = "Current"
EndPrmText
ExtUserPrmData =  438  "YD Change-Over Mode"
Bit(5) 1 0-1
Prm_Text_Ref = 438 
EndExtUserPrmData

PrmText = 439 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  439  "Phase Loss Prot."
Bit(6) 1 0-1
Prm_Text_Ref = 439 
EndExtUserPrmData

PrmText = 440 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  440  "DX1xx Enabled"
Bit(0) 0 0-1
Prm_Text_Ref = 440 
EndExtUserPrmData

PrmText = 441 
Text(0) = "Error"
Text(1) = "Warning"
EndPrmText
ExtUserPrmData =  441  "Missing Module React."
Bit(7) 0 0-1
Prm_Text_Ref = 441 
EndExtUserPrmData

PrmText = 442 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  442  "Aux Inp 1 Ack Mode"
Bit(0) 0 0-1
Prm_Text_Ref = 442 
EndExtUserPrmData

PrmText = 443 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  443  "Aux Inp 2 Ack Mode"
Bit(1) 0 0-1
Prm_Text_Ref = 443 
EndExtUserPrmData

PrmText = 444 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  444  "Aux Inp 3 Ack Mode"
Bit(2) 0 0-1
Prm_Text_Ref = 444 
EndExtUserPrmData

PrmText = 445 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  445  "Aux Inp 4 Ack Mode"
Bit(3) 0 0-1
Prm_Text_Ref = 445 
EndExtUserPrmData

PrmText = 446 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  446  "Aux Inp 5 Ack Mode"
Bit(4) 0 0-1
Prm_Text_Ref = 446 
EndExtUserPrmData

PrmText = 447 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  447  "Aux Inp 6 Ack Mode"
Bit(5) 0 0-1
Prm_Text_Ref = 447 
EndExtUserPrmData

PrmText = 448 
Text(0) = "Time"
Text(1) = "x% Therm. Load"
EndPrmText
ExtUserPrmData =  448  "Cooling Mode"
Bit(7) 0 0-1
Prm_Text_Ref = 448 
EndExtUserPrmData

PrmText = 449 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  449  "Invert DI Start Inp."
Bit(0) 0 0-1
Prm_Text_Ref = 449 
EndExtUserPrmData

PrmText = 450 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  450  "Invert DI Stop Inp."
Bit(1) 1 0-1
Prm_Text_Ref = 450 
EndExtUserPrmData

PrmText = 451 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  451  "Inching DI Start Inp"
Bit(4) 0 0-1
Prm_Text_Ref = 451 
EndExtUserPrmData

PrmText = 452 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  452  "Loc 1 Start Bus Cyc"
Bit(0) 0 0-1
Prm_Text_Ref = 452 
EndExtUserPrmData

PrmText = 453 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  453  "Loc 1 Stop Bus Cyc"
Bit(1) 1 0-1
Prm_Text_Ref = 453 
EndExtUserPrmData

PrmText = 454 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  454  "Loc 1 Start DI"
Bit(2) 1 0-1
Prm_Text_Ref = 454 
EndExtUserPrmData

PrmText = 455 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  455  "Loc 1 Stop DI"
Bit(3) 1 0-1
Prm_Text_Ref = 455 
EndExtUserPrmData

PrmText = 456 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  456  "Loc 1 Start LCD"
Bit(4) 1 0-1
Prm_Text_Ref = 456 
EndExtUserPrmData

PrmText = 457 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  457  "Loc 1 Stop LCD"
Bit(5) 1 0-1
Prm_Text_Ref = 457 
EndExtUserPrmData

PrmText = 458 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  458  "Loc 1 Start Bus Acyc"
Bit(6) 0 0-1
Prm_Text_Ref = 458 
EndExtUserPrmData

PrmText = 459 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  459  "Loc 1 Stop Bus Acyc"
Bit(7) 1 0-1
Prm_Text_Ref = 459 
EndExtUserPrmData

PrmText = 460 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  460  "Auto Start Bus Cyc"
Bit(0) 1 0-1
Prm_Text_Ref = 460 
EndExtUserPrmData

PrmText = 461 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  461  "Auto Stop Bus Cyc"
Bit(1) 1 0-1
Prm_Text_Ref = 461 
EndExtUserPrmData

PrmText = 462 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  462  "Auto Start DI"
Bit(2) 0 0-1
Prm_Text_Ref = 462 
EndExtUserPrmData

PrmText = 463 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  463  "Auto Stop DI"
Bit(3) 1 0-1
Prm_Text_Ref = 463 
EndExtUserPrmData

PrmText = 464 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  464  "Auto Start LCD"
Bit(4) 0 0-1
Prm_Text_Ref = 464 
EndExtUserPrmData

PrmText = 465 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  465  "Auto Stop LCD"
Bit(5) 1 0-1
Prm_Text_Ref = 465 
EndExtUserPrmData

PrmText = 466 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  466  "Auto Start Bus Acyc"
Bit(6) 1 0-1
Prm_Text_Ref = 466 
EndExtUserPrmData

PrmText = 467 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  467  "Auto Stop Bus Acyc"
Bit(7) 1 0-1
Prm_Text_Ref = 467 
EndExtUserPrmData

PrmText = 468 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  468  "Loc 2 Start Bus Cyc"
Bit(0) 0 0-1
Prm_Text_Ref = 468 
EndExtUserPrmData

PrmText = 469 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  469  "Loc 2 Stop Bus Cyc"
Bit(1) 1 0-1
Prm_Text_Ref = 469 
EndExtUserPrmData

PrmText = 470 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  470  "Loc 2 Start DI"
Bit(2) 1 0-1
Prm_Text_Ref = 470 
EndExtUserPrmData

PrmText = 471 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  471  "Loc 2 Stop DI"
Bit(3) 1 0-1
Prm_Text_Ref = 471 
EndExtUserPrmData

PrmText = 472 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  472  "Loc 2 Start LCD"
Bit(4) 1 0-1
Prm_Text_Ref = 472 
EndExtUserPrmData

PrmText = 473 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  473  "Loc 2 Stop LCD"
Bit(5) 1 0-1
Prm_Text_Ref = 473 
EndExtUserPrmData

PrmText = 474 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  474  "Loc 2 Start Bus Acyc"
Bit(6) 0 0-1
Prm_Text_Ref = 474 
EndExtUserPrmData

PrmText = 475 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  475  "Loc 2 Stop Bus Acyc"
Bit(7) 1 0-1
Prm_Text_Ref = 475 
EndExtUserPrmData

PrmText = 476 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  476  "Multif In 0 Autoreset"
Bit(4) 0 0-1
Prm_Text_Ref = 476 
EndExtUserPrmData

PrmText = 477 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  477  "Multif In 1 Autoreset"
Bit(5) 0 0-1
Prm_Text_Ref = 477 
EndExtUserPrmData

PrmText = 478 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  478  "Multif In 2 Autoreset"
Bit(6) 0 0-1
Prm_Text_Ref = 478 
EndExtUserPrmData


;=============================================================
; Definition for Ext User Prm Data "Wireless WDI100"
;=============================================================
;
; do not delete this comment, req. by FB1131
;ExtUserPrmData= 204 "Cell ID"					; Cell ID WDI100
;Unsigned16 0 0-60									; Default 0, Bereich 0..60
;EndExtUserPrmData
ExtUserPrmData= 500 "Cell ID"					; Cell ID WDI100
Unsigned16 1 1-59									; Default 0, Bereich 0..60
EndExtUserPrmData

ExtUserPrmData= 501 "Sensors   1-16"	; 
Unsigned16 0 0-65535								; 
EndExtUserPrmData

ExtUserPrmData= 502 "Sensors  17-32"	; 
Unsigned16 0 0-65535								; 
EndExtUserPrmData

ExtUserPrmData= 503 "Sensors  33-48"	; 
Unsigned16 0 0-65535								; 
EndExtUserPrmData

ExtUserPrmData= 504 "Sensors  49-64"	; 
Unsigned16 0 0-65535								; 
EndExtUserPrmData

ExtUserPrmData= 505 "Sensors  65-80"	; 
Unsigned16 0 0-65535								; 
EndExtUserPrmData

ExtUserPrmData= 506 "Sensors  81-96"	; 
Unsigned16 0 0-65535								; 
EndExtUserPrmData

ExtUserPrmData= 507 "Sensors  97-112"	; 
Unsigned16 0 0-65535								; 
EndExtUserPrmData

ExtUserPrmData= 508 "Sensors 113-120"	; 
Unsigned16 0 0-255  								; 
EndExtUserPrmData


;==================================================================
; Definition for Ext User Prm Data "Wireless WDIO100 - WDI/WDX/WDP"
;==================================================================
;
PrmText = 600
Text(0)   = "On"
Text(1)   = "Off"
EndPrmText

PrmText = 601
Text(0)   = "AUTO ACK"
Text(1)   = "WDIO100 ACK"
EndPrmText

PrmText = 602
Text(0)   = "Zero"
Text(1)   = "Keep"
EndPrmText

PrmText = 603
Text(0)   = "1ms"
Text(1)   = "5ms"
Text(2)   = "25ms"
EndPrmText



; Cell ID WDI100
; Default 1, Bereich 1__59
ExtUserPrmData = 604 "Cell-ID"
Unsigned16 1 1-59		
EndExtUserPrmData

ExtUserPrmData = 605 "WSIX  15-0"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 606 "WSIX  31-16" 
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 607 "WSIX  47-32"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 608 "WSIX  63-48"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 609 "WSIX  79-64"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 610 "WSIX  95-80"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 611 "WSIX 111-96"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData = 612 "WSIX 119-112"
Unsigned16 0 0-255
EndExtUserPrmData

ExtUserPrmData = 616 "ANTENNA SWITCH"
Unsigned16 0 0-1
Prm_Text_Ref=600
EndExtUserPrmData


;=============================================================
; Definition for Ext User Prm Data "Wireless WDIO100-WDX"
;=============================================================
;
; WDIO100 max 7 I/O Pads

ExtUserPrmData = 613 "WSIX  55-48"
Unsigned16 0 0-255
EndExtUserPrmData

ExtUserPrmData = 614 "WDP  6-0"
Unsigned16 0 0-127
EndExtUserPrmData

;=============================================================
; Definition for Ext User Prm Data "Wireless WDIO100-WDP"
;=============================================================
;
; WDIOP100 max 13 I/O Pads

ExtUserPrmData = 615 "WDP  12-0"
Unsigned16 0 0-8191
EndExtUserPrmData

;=============================================================
; Definition for Ext User Prm Data "Wireless WDIO100-WDX/WDP"
;=============================================================
;
ExtUserPrmData = 617 "WDP ERROR ACK"
Unsigned16 0 0-1
Prm_Text_Ref=601
EndExtUserPrmData

ExtUserPrmData = 618 "FAILSAFE MODE"
Unsigned16 0 0-1
Prm_Text_Ref=602
EndExtUserPrmData

ExtUserPrmData = 619 "FILTER TIME"
Unsigned16 0 0-2
Prm_Text_Ref=603
EndExtUserPrmData

;=============================================================
; Text-definition for User Prm Data  UMC100_FBP (R0101 R0201)
;=============================================================
;
ExtUserPrmData =  701  "Setting Ie 1 [0.01A]"
Unsigned32 50 24-320000
EndExtUserPrmData

ExtUserPrmData =  702  "Setting Ie 2 [0.01A]"
Unsigned32 50 24-320000
EndExtUserPrmData

ExtUserPrmData =  703  "YD Starting Time [0.1s]"
Unsigned16 600 10-36000
EndExtUserPrmData

ExtUserPrmData =  704  "Current Factor [%]"
Unsigned16 100 2-64000
EndExtUserPrmData

ExtUserPrmData =  705  "Cooling Time [s]"
Unsigned16 120 30-64000
EndExtUserPrmData

ExtUserPrmData =  706  "Earth Flt Trip Level [%]"
Unsigned8 255 20-255
EndExtUserPrmData

ExtUserPrmData =  707  "Earth Flt Trip Delay [0.1s]"
Unsigned8 5 0-255
EndExtUserPrmData

PrmText = 708 
Text(0) = "English"
Text(1) = "Deutsch"
Text(2) = "Francais"
Text(3) = "Espanol"
Text(4) = "Italiano"
Text(5) = "Portugues"
Text(6) = "Russian"
EndPrmText
ExtUserPrmData =  708  "Language"
Unsigned8 0 0-6
Prm_Text_Ref = 708 
EndExtUserPrmData

ExtUserPrmData =  709  "Rev Lock-Out Time [s]"
Unsigned8 1 1-255
EndExtUserPrmData

PrmText = 710 
Text(0) = "Off"
Text(1) = "Flash DO2"
Text(2) = "On DO2"
Text(3) = "Invert DO2"
Text(4) = "Flash DO3"
Text(5) = "On DO3"
Text(6) = "Invert DO3"
EndPrmText
ExtUserPrmData =  710  "Fault Output"
Unsigned8 0 0-6
Prm_Text_Ref = 710 
EndExtUserPrmData

PrmText = 711 
Text(0) = "Class 5"
Text(1) = "Class 10"
Text(2) = "Class 20"
Text(3) = "Class 30"
Text(4) = "Class 40"
EndPrmText
ExtUserPrmData =  711  "Trip Class"
Unsigned8 1 0-4
Prm_Text_Ref = 711 
EndExtUserPrmData

ExtUserPrmData =  712  "Low Curr Warn Level [5%]"
Unsigned8 10 0-20
EndExtUserPrmData

ExtUserPrmData =  713  "Low Curr Trip Level [5%]"
Unsigned8 0 0-20
EndExtUserPrmData

ExtUserPrmData =  714  "High Curr Warn Level [5%]"
Unsigned8 30 20-160
EndExtUserPrmData

ExtUserPrmData =  715  "High Curr Trip Level [5%]"
Unsigned8 160 20-160
EndExtUserPrmData

ExtUserPrmData =  716  "Locked Rotor Level [5%]"
Unsigned8 160 20-160
EndExtUserPrmData

ExtUserPrmData =  717  "Locked Rotor Delay [0.1s]"
Unsigned8 5 0-255
EndExtUserPrmData

ExtUserPrmData =  718  "Custom App Parameter"
Unsigned8 0 0-255
EndExtUserPrmData

PrmText = 719 
Text(0) = "Off"
Text(1) = "Stop (NC)"
Text(2) = "Stop (NO)"
Text(3) = "Ext. Flt (NC) always"
Text(4) = "Ext. Flt (NO) always"
Text(5) = "Ext. Flt (NC) Motor on"
Text(6) = "Ext. Flt (NO) Motor on"
Text(7) = "Prep. emerg. Start (NC)"
Text(8) = "Prep. emerg. Start (NO)"
Text(9) = "Testposition (NC)"
Text(10) = "Testposition (NO)"
Text(11) = "Force local (NC)"
Text(12) = "Force local (NO)"
Text(13) = "Fault reset (NC)"
Text(14) = "Fault reset (NO)"
Text(15) = "Voltage DIP (NC)"
Text(16) = "Voltage DIP (NO)"
Text(17) = "CEM11 always (Warning)"
Text(18) = "CEM11 after startup (Warning)"
Text(19) = "CEM11 always (Fault)"
Text(20) = "CEM11 after startup time (Fault)"
EndPrmText
ExtUserPrmData =  719  "Multif In 0"
Unsigned8 0 0-20
Prm_Text_Ref = 719 
EndExtUserPrmData

PrmText = 720 
Text(0) = "Off"
Text(1) = "Stop (NC)"
Text(2) = "Stop (NO)"
Text(3) = "Ext. Flt (NC) always"
Text(4) = "Ext. Flt (NO) always"
Text(5) = "Ext. Flt (NC) Motor on"
Text(6) = "Ext. Flt (NO) Motor on"
Text(7) = "Prep. emerg. Start (NC)"
Text(8) = "Prep. emerg. Start (NO)"
Text(9) = "Testposition (NC)"
Text(10) = "Testposition (NO)"
Text(11) = "Force local (NC)"
Text(12) = "Force local (NO)"
Text(13) = "Fault reset (NC)"
Text(14) = "Fault reset (NO)"
Text(15) = "Voltage DIP (NC)"
Text(16) = "Voltage DIP (NO)"
Text(17) = "CEM11 always (Warning)"
Text(18) = "CEM11 after startup (Warning)"
Text(19) = "CEM11 always (Fault)"
Text(20) = "CEM11 after startup time (Fault)"
EndPrmText
ExtUserPrmData =  720  "Multif In 1"
Unsigned8 0 0-20
Prm_Text_Ref = 720 
EndExtUserPrmData

PrmText = 721 
Text(0) = "Off"
Text(1) = "Stop (NC)"
Text(2) = "Stop (NO)"
Text(3) = "Ext. Flt (NC) always"
Text(4) = "Ext. Flt (NO) always"
Text(5) = "Ext. Flt (NC) Motor on"
Text(6) = "Ext. Flt (NO) Motor on"
Text(7) = "Prep. emerg. Start (NC)"
Text(8) = "Prep. emerg. Start (NO)"
Text(9) = "Testposition (NC)"
Text(10) = "Testposition (NO)"
Text(11) = "Force local (NC)"
Text(12) = "Force local (NO)"
Text(13) = "Fault reset (NC)"
Text(14) = "Fault reset (NO)"
Text(15) = "Voltage DIP (NC)"
Text(16) = "Voltage DIP (NO)"
Text(17) = "CEM11 always (Warning)"
Text(18) = "CEM11 after startup (Warning)"
Text(19) = "CEM11 always (Fault)"
Text(20) = "CEM11 after startup time (Fault)"
EndPrmText
ExtUserPrmData =  721  "Multif In 2"
Unsigned8 0 0-20
Prm_Text_Ref = 721 
EndExtUserPrmData

ExtUserPrmData =  722  "Multif In 0 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  723  "Multif In 1 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  724  "Multif In 2 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

PrmText = 725 
Text(1) = "Transparent"
Text(2) = "Overload Relay"
Text(3) = "Direct Starter"
Text(4) = "Reverse Starter"
Text(5) = "Star-delta Starter"
Text(7) = "Pole-Changing Starter"
Text(9) = "Actuator 1"
Text(10) = "Actuator 2"
Text(11) = "Actuator 3"
Text(12) = "Actuator 4"
EndPrmText
ExtUserPrmData =  725  "Control Function"
Unsigned8 3 1-12
Prm_Text_Ref = 725 
EndExtUserPrmData

PrmText = 726 
Text(0) = "Motor Off"
Text(1) = "Retain"
Text(2) = "Start Forward"
Text(3) = "Start Reverse"
EndPrmText
ExtUserPrmData =  726  "Busfault Reaction"
BitArea(0-3) 0 0-3
Prm_Text_Ref = 726 
EndExtUserPrmData

PrmText = 727 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  727  "Aux Inp 1 Reaction"
BitArea(0-3) 0 0-8
Prm_Text_Ref = 727 
EndExtUserPrmData

PrmText = 728 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  728  "Aux Inp 2 Reaction"
BitArea(4-7) 0 0-8
Prm_Text_Ref = 728 
EndExtUserPrmData

PrmText = 729 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  729  "Aux Inp 3 Reaction"
BitArea(0-3) 0 0-8
Prm_Text_Ref = 729 
EndExtUserPrmData

PrmText = 730 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  730  "Aux Inp 4 Reaction"
BitArea(4-7) 0 0-8
Prm_Text_Ref = 730 
EndExtUserPrmData

PrmText = 731 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  731  "Aux Inp 5 Reaction"
BitArea(0-3) 0 0-8
Prm_Text_Ref = 731 
EndExtUserPrmData

PrmText = 732 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  732  "Aux Inp 6 Reaction"
BitArea(4-7) 0 0-8
Prm_Text_Ref = 732 
EndExtUserPrmData

PrmText = 733 
Text(0) = "Disabled"
Text(1) = "Trip"
Text(2) = "Warning"
EndPrmText
ExtUserPrmData =  733  "PTC, Thermistor"
BitArea(0-1) 0 0-2
Prm_Text_Ref = 733 
EndExtUserPrmData

PrmText = 734 
Text(1) = "Contact DI0"
Text(2) = "Current"
Text(3) = "Simulation"
EndPrmText
ExtUserPrmData =  734  "Check-Back"
BitArea(2-3) 2 1-3
Prm_Text_Ref = 734 
EndExtUserPrmData

PrmText = 735 
Text(0) = "Disabled"
Text(1) = "Trip"
Text(2) = "Warning"
EndPrmText
ExtUserPrmData =  735  "Check Phase Sequence"
BitArea(4-5) 0 0-2
Prm_Text_Ref = 735 
EndExtUserPrmData

PrmText = 736 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  736  "Fault Auto Reset"
Bit(0) 0 0-1
Prm_Text_Ref = 736 
EndExtUserPrmData

PrmText = 737 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  737  "Emergency Start"
Bit(1) 0 0-1
Prm_Text_Ref = 737 
EndExtUserPrmData

PrmText = 738 
Text(0) = "Always"
Text(1) = "After Startup"
EndPrmText
ExtUserPrmData =  738  "Earth Flt Detection"
Bit(2) 1 0-1
Prm_Text_Ref = 738 
EndExtUserPrmData

PrmText = 739 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  739  "Address Check"
Bit(3) 0 0-1
Prm_Text_Ref = 739 
EndExtUserPrmData

PrmText = 740 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  740  "Enable Custom Logic"
Bit(4) 0 0-1
Prm_Text_Ref = 740 
EndExtUserPrmData

PrmText = 741 
Text(0) = "Time"
Text(1) = "Current"
EndPrmText
ExtUserPrmData =  741  "YD Change-Over Mode"
Bit(5) 1 0-1
Prm_Text_Ref = 741 
EndExtUserPrmData

PrmText = 742 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  742  "Phase Loss Prot."
Bit(6) 1 0-1
Prm_Text_Ref = 742 
EndExtUserPrmData

PrmText = 743 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  743  "DX1xx Enabled"
Bit(0) 0 0-1
Prm_Text_Ref = 743 
EndExtUserPrmData

PrmText = 744 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  744  "VI15x Enabled"
Bit(3) 0 0-1
Prm_Text_Ref = 744 
EndExtUserPrmData

PrmText = 745 
Text(0) = "Error"
Text(1) = "Warning"
EndPrmText
ExtUserPrmData =  745  "Missing Module React."
Bit(7) 0 0-1
Prm_Text_Ref = 745 
EndExtUserPrmData

PrmText = 746 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  746  "Aux Inp 1 Ack Mode"
Bit(0) 0 0-1
Prm_Text_Ref = 746 
EndExtUserPrmData

PrmText = 747 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  747  "Aux Inp 2 Ack Mode"
Bit(1) 0 0-1
Prm_Text_Ref = 747 
EndExtUserPrmData

PrmText = 748 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  748  "Aux Inp 3 Ack Mode"
Bit(2) 0 0-1
Prm_Text_Ref = 748 
EndExtUserPrmData

PrmText = 749 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  749  "Aux Inp 4 Ack Mode"
Bit(3) 0 0-1
Prm_Text_Ref = 749 
EndExtUserPrmData

PrmText = 750 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  750  "Aux Inp 5 Ack Mode"
Bit(4) 0 0-1
Prm_Text_Ref = 750 
EndExtUserPrmData

PrmText = 751 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  751  "Aux Inp 6 Ack Mode"
Bit(5) 0 0-1
Prm_Text_Ref = 751 
EndExtUserPrmData

PrmText = 752 
Text(0) = "Time"
Text(1) = "x% Therm. Load"
EndPrmText
ExtUserPrmData =  752  "Cooling Mode"
Bit(7) 0 0-1
Prm_Text_Ref = 752 
EndExtUserPrmData

PrmText = 753 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  753  "Invert DI Start Inp."
Bit(0) 0 0-1
Prm_Text_Ref = 753 
EndExtUserPrmData

PrmText = 754 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  754  "Invert DI Stop Inp."
Bit(1) 1 0-1
Prm_Text_Ref = 754 
EndExtUserPrmData

PrmText = 755 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  755  "Inching DI Start Inp"
Bit(4) 0 0-1
Prm_Text_Ref = 755 
EndExtUserPrmData

PrmText = 756 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  756  "Loc 1 Start Bus Cyc"
Bit(0) 0 0-1
Prm_Text_Ref = 756 
EndExtUserPrmData

PrmText = 757 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  757  "Loc 1 Stop Bus Cyc"
Bit(1) 1 0-1
Prm_Text_Ref = 757 
EndExtUserPrmData

PrmText = 758 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  758  "Loc 1 Start DI"
Bit(2) 1 0-1
Prm_Text_Ref = 758 
EndExtUserPrmData

PrmText = 759 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  759  "Loc 1 Stop DI"
Bit(3) 1 0-1
Prm_Text_Ref = 759 
EndExtUserPrmData

PrmText = 760 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  760  "Loc 1 Start LCD"
Bit(4) 1 0-1
Prm_Text_Ref = 760 
EndExtUserPrmData

PrmText = 761 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  761  "Loc 1 Stop LCD"
Bit(5) 1 0-1
Prm_Text_Ref = 761 
EndExtUserPrmData

PrmText = 762 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  762  "Loc 1 Start Bus Acyc"
Bit(6) 0 0-1
Prm_Text_Ref = 762 
EndExtUserPrmData

PrmText = 763 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  763  "Loc 1 Stop Bus Acyc"
Bit(7) 1 0-1
Prm_Text_Ref = 763 
EndExtUserPrmData

PrmText = 764 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  764  "Auto Start Bus Cyc"
Bit(0) 1 0-1
Prm_Text_Ref = 764 
EndExtUserPrmData

PrmText = 765 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  765  "Auto Stop Bus Cyc"
Bit(1) 1 0-1
Prm_Text_Ref = 765 
EndExtUserPrmData

PrmText = 766 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  766  "Auto Start DI"
Bit(2) 0 0-1
Prm_Text_Ref = 766 
EndExtUserPrmData

PrmText = 767 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  767  "Auto Stop DI"
Bit(3) 1 0-1
Prm_Text_Ref = 767 
EndExtUserPrmData

PrmText = 768 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  768  "Auto Start LCD"
Bit(4) 0 0-1
Prm_Text_Ref = 768 
EndExtUserPrmData

PrmText = 769 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  769  "Auto Stop LCD"
Bit(5) 1 0-1
Prm_Text_Ref = 769 
EndExtUserPrmData

PrmText = 770 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  770  "Auto Start Bus Acyc"
Bit(6) 1 0-1
Prm_Text_Ref = 770 
EndExtUserPrmData

PrmText = 771 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  771  "Auto Stop Bus Acyc"
Bit(7) 1 0-1
Prm_Text_Ref = 771 
EndExtUserPrmData

PrmText = 772 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  772  "Loc 2 Start Bus Cyc"
Bit(0) 0 0-1
Prm_Text_Ref = 772 
EndExtUserPrmData

PrmText = 773 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  773  "Loc 2 Stop Bus Cyc"
Bit(1) 1 0-1
Prm_Text_Ref = 773 
EndExtUserPrmData

PrmText = 774 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  774  "Loc 2 Start DI"
Bit(2) 1 0-1
Prm_Text_Ref = 774 
EndExtUserPrmData

PrmText = 775 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  775  "Loc 2 Stop DI"
Bit(3) 1 0-1
Prm_Text_Ref = 775 
EndExtUserPrmData

PrmText = 776 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  776  "Loc 2 Start LCD"
Bit(4) 1 0-1
Prm_Text_Ref = 776 
EndExtUserPrmData

PrmText = 777 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  777  "Loc 2 Stop LCD"
Bit(5) 1 0-1
Prm_Text_Ref = 777 
EndExtUserPrmData

PrmText = 778 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  778  "Loc 2 Start Bus Acyc"
Bit(6) 0 0-1
Prm_Text_Ref = 778 
EndExtUserPrmData

PrmText = 779 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  779  "Loc 2 Stop Bus Acyc"
Bit(7) 1 0-1
Prm_Text_Ref = 779 
EndExtUserPrmData

PrmText = 780 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  780  "Multif In 0 Autoreset"
Bit(4) 0 0-1
Prm_Text_Ref = 780 
EndExtUserPrmData

PrmText = 781 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  781  "Multif In 1 Autoreset"
Bit(5) 0 0-1
Prm_Text_Ref = 781 
EndExtUserPrmData

PrmText = 782 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  782  "Multif In 2 Autoreset"
Bit(6) 0 0-1
Prm_Text_Ref = 782 
EndExtUserPrmData

;=============================================================
; Text-definition for User Prm Data  UMC100.3 (R0100 R0200)
;=============================================================
;
ExtUserPrmData =  801  "Setting Ie 1 [0.01A]"
Unsigned32 50 24-320000
EndExtUserPrmData

ExtUserPrmData =  802  "Setting Ie 2 [0.01A]"
Unsigned32 50 24-320000
EndExtUserPrmData

ExtUserPrmData =  803  "YD Starting Time [0.1s]"
Unsigned16 600 10-36000
EndExtUserPrmData

ExtUserPrmData =  804  "Current Factor [%]"
Unsigned16 100 2-64000
EndExtUserPrmData

ExtUserPrmData =  805  "Cooling Time [s]"
Unsigned16 120 30-64000
EndExtUserPrmData

ExtUserPrmData =  806  "Earth Flt Trip Level [%]"
Unsigned8 255 20-255
EndExtUserPrmData

ExtUserPrmData =  807  "Earth Flt Trip Delay [0.1s]"
Unsigned8 5 0-255
EndExtUserPrmData

PrmText = 808 
Text(0) = "English"
Text(1) = "Deutsch"
Text(2) = "Francais"
Text(3) = "Espanol"
Text(4) = "Italiano"
Text(5) = "Portugues"
Text(6) = "Russian"
Text(7) = "Polski"
EndPrmText
ExtUserPrmData =  808  "Language"
Unsigned8 0 0-7
Prm_Text_Ref = 808 
EndExtUserPrmData

ExtUserPrmData =  809  "Rev Lock-Out Time [s]"
Unsigned8 1 1-255
EndExtUserPrmData

PrmText = 810 
Text(0) = "Off"
Text(1) = "Flash DO2"
Text(2) = "On DO2"
Text(3) = "Invert DO2"
Text(4) = "Flash DO3"
Text(5) = "On DO3"
Text(6) = "Invert DO3"
EndPrmText
ExtUserPrmData =  810  "Fault Output"
Unsigned8 0 0-6
Prm_Text_Ref = 810 
EndExtUserPrmData

PrmText = 811 
Text(0) = "Class 5"
Text(1) = "Class 10"
Text(2) = "Class 20"
Text(3) = "Class 30"
Text(4) = "Class 40"
EndPrmText
ExtUserPrmData =  811  "Trip Class"
Unsigned8 1 0-4
Prm_Text_Ref = 811 
EndExtUserPrmData

ExtUserPrmData =  812  "Low Curr Warn Level [5%]"
Unsigned8 10 0-20
EndExtUserPrmData

ExtUserPrmData =  813  "Low Curr Trip Level [5%]"
Unsigned8 0 0-20
EndExtUserPrmData

ExtUserPrmData =  814  "High Curr Warn Level [5%]"
Unsigned8 30 20-160
EndExtUserPrmData

ExtUserPrmData =  815  "High Curr Trip Level [5%]"
Unsigned8 160 20-160
EndExtUserPrmData

ExtUserPrmData =  816  "Locked Rotor Level [5%]"
Unsigned8 160 20-160
EndExtUserPrmData

ExtUserPrmData =  817  "Locked Rotor Delay [0.1s]"
Unsigned8 5 0-255
EndExtUserPrmData

ExtUserPrmData =  818  "Custom App Parameter"
Unsigned8 0 0-255
EndExtUserPrmData

PrmText = 819 
Text(0) = "Off"
Text(1) = "Stop (NC)"
Text(2) = "Stop (NO)"
Text(3) = "Ext. Flt (NC) always"
Text(4) = "Ext. Flt (NO) always"
Text(5) = "Ext. Flt (NC) Motor on"
Text(6) = "Ext. Flt (NO) Motor on"
Text(7) = "Prep. emerg. Start (NC)"
Text(8) = "Prep. emerg. Start (NO)"
Text(9) = "Testposition (NC)"
Text(10) = "Testposition (NO)"
Text(11) = "Force local (NC)"
Text(12) = "Force local (NO)"
Text(13) = "Fault reset (NC)"
Text(14) = "Fault reset (NO)"
Text(15) = "Voltage DIP (NC)"
Text(16) = "Voltage DIP (NO)"
Text(17) = "CEM11 always (Warning)"
Text(18) = "CEM11 after startup (Warning)"
Text(19) = "CEM11 always (Fault)"
Text(20) = "CEM11 after startup time (Fault)"
EndPrmText
ExtUserPrmData =  819  "Multif In 0"
Unsigned8 0 0-20
Prm_Text_Ref = 819 
EndExtUserPrmData

PrmText = 820 
Text(0) = "Off"
Text(1) = "Stop (NC)"
Text(2) = "Stop (NO)"
Text(3) = "Ext. Flt (NC) always"
Text(4) = "Ext. Flt (NO) always"
Text(5) = "Ext. Flt (NC) Motor on"
Text(6) = "Ext. Flt (NO) Motor on"
Text(7) = "Prep. emerg. Start (NC)"
Text(8) = "Prep. emerg. Start (NO)"
Text(9) = "Testposition (NC)"
Text(10) = "Testposition (NO)"
Text(11) = "Force local (NC)"
Text(12) = "Force local (NO)"
Text(13) = "Fault reset (NC)"
Text(14) = "Fault reset (NO)"
Text(15) = "Voltage DIP (NC)"
Text(16) = "Voltage DIP (NO)"
Text(17) = "CEM11 always (Warning)"
Text(18) = "CEM11 after startup (Warning)"
Text(19) = "CEM11 always (Fault)"
Text(20) = "CEM11 after startup time (Fault)"
EndPrmText
ExtUserPrmData =  820  "Multif In 1"
Unsigned8 0 0-20
Prm_Text_Ref = 820 
EndExtUserPrmData

PrmText = 821 
Text(0) = "Off"
Text(1) = "Stop (NC)"
Text(2) = "Stop (NO)"
Text(3) = "Ext. Flt (NC) always"
Text(4) = "Ext. Flt (NO) always"
Text(5) = "Ext. Flt (NC) Motor on"
Text(6) = "Ext. Flt (NO) Motor on"
Text(7) = "Prep. emerg. Start (NC)"
Text(8) = "Prep. emerg. Start (NO)"
Text(9) = "Testposition (NC)"
Text(10) = "Testposition (NO)"
Text(11) = "Force local (NC)"
Text(12) = "Force local (NO)"
Text(13) = "Fault reset (NC)"
Text(14) = "Fault reset (NO)"
Text(15) = "Voltage DIP (NC)"
Text(16) = "Voltage DIP (NO)"
Text(17) = "CEM11 always (Warning)"
Text(18) = "CEM11 after startup (Warning)"
Text(19) = "CEM11 always (Fault)"
Text(20) = "CEM11 after startup time (Fault)"
EndPrmText
ExtUserPrmData =  821  "Multif In 2"
Unsigned8 0 0-20
Prm_Text_Ref = 821 
EndExtUserPrmData

ExtUserPrmData =  822  "Multif In 0 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  823  "Multif In 1 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  824  "Multif In 2 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

PrmText = 825 
Text(1) = "Transparent"
Text(2) = "Overload Relay"
Text(3) = "Direct Starter"
Text(4) = "Reverse Starter"
Text(5) = "Star-delta Starter"
Text(7) = "Pole-Changing Starter"
Text(9) = "Actuator 1"
Text(10) = "Actuator 2"
Text(11) = "Actuator 3"
Text(12) = "Actuator 4"
Text(13) = "Softstarter"
EndPrmText
ExtUserPrmData =  825  "Control Function"
Unsigned8 3 1-13
Prm_Text_Ref = 825 
EndExtUserPrmData

PrmText = 826 
Text(0) = "Motor Off"
Text(1) = "Retain"
Text(2) = "Start Forward"
Text(3) = "Start Reverse"
EndPrmText
ExtUserPrmData =  826  "Busfault Reaction"
BitArea(0-3) 0 0-3
Prm_Text_Ref = 826 
EndExtUserPrmData

PrmText = 827 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  827  "Aux Inp 1 Reaction"
BitArea(0-3) 0 0-8
Prm_Text_Ref = 827 
EndExtUserPrmData

PrmText = 828 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  828  "Aux Inp 2 Reaction"
BitArea(4-7) 0 0-8
Prm_Text_Ref = 828 
EndExtUserPrmData

PrmText = 829 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  829  "Aux Inp 3 Reaction"
BitArea(0-3) 0 0-8
Prm_Text_Ref = 829 
EndExtUserPrmData

PrmText = 830 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  830  "Aux Inp 4 Reaction"
BitArea(4-7) 0 0-8
Prm_Text_Ref = 830 
EndExtUserPrmData

PrmText = 831 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  831  "Aux Inp 5 Reaction"
BitArea(0-3) 0 0-8
Prm_Text_Ref = 831 
EndExtUserPrmData

PrmText = 832 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  832  "Aux Inp 6 Reaction"
BitArea(4-7) 0 0-8
Prm_Text_Ref = 832 
EndExtUserPrmData

PrmText = 833 
Text(0) = "Disabled"
Text(1) = "Trip"
Text(2) = "Warning"
EndPrmText
ExtUserPrmData =  833  "PTC, Thermistor"
BitArea(0-1) 0 0-2
Prm_Text_Ref = 833 
EndExtUserPrmData

PrmText = 834 
Text(1) = "Contact DI0"
Text(2) = "Current"
Text(3) = "Simulation"
EndPrmText
ExtUserPrmData =  834  "Check-Back"
BitArea(2-3) 2 1-3
Prm_Text_Ref = 834 
EndExtUserPrmData

PrmText = 835 
Text(0) = "Disabled"
Text(1) = "Trip"
Text(2) = "Warning"
EndPrmText
ExtUserPrmData =  835  "Check Phase Sequence"
BitArea(4-5) 0 0-2
Prm_Text_Ref = 835 
EndExtUserPrmData

PrmText = 836 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  836  "Fault Auto Reset"
Bit(0) 0 0-1
Prm_Text_Ref = 836 
EndExtUserPrmData

PrmText = 837 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  837  "Emergency Start"
Bit(1) 0 0-1
Prm_Text_Ref = 837 
EndExtUserPrmData

PrmText = 838 
Text(0) = "Always"
Text(1) = "After Startup"
EndPrmText
ExtUserPrmData =  838  "Earth Flt Detection"
Bit(2) 1 0-1
Prm_Text_Ref = 838 
EndExtUserPrmData

PrmText = 839 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  839  "Address Check"
Bit(3) 0 0-1
Prm_Text_Ref = 839 
EndExtUserPrmData

PrmText = 840 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  840  "Enable Custom Logic"
Bit(4) 0 0-1
Prm_Text_Ref = 840 
EndExtUserPrmData

PrmText = 841 
Text(0) = "Time"
Text(1) = "Current"
EndPrmText
ExtUserPrmData =  841  "YD Change-Over Mode"
Bit(5) 1 0-1
Prm_Text_Ref = 841 
EndExtUserPrmData

PrmText = 842 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  842  "Phase Loss Prot."
Bit(6) 1 0-1
Prm_Text_Ref = 842 
EndExtUserPrmData

PrmText = 843 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  843  "Resistive Load"
Bit(7) 0 0-1
Prm_Text_Ref = 843 
EndExtUserPrmData

PrmText = 844 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  844  "DX1xx Enabled"
Bit(0) 0 0-1
Prm_Text_Ref = 844 
EndExtUserPrmData

PrmText = 845 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  845  "AI1xx AM1 Enabled"
Bit(1) 0 0-1
Prm_Text_Ref = 845 
EndExtUserPrmData

PrmText = 846 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  846  "AI1xx AM2 Enabled"
Bit(2) 0 0-1
Prm_Text_Ref = 846 
EndExtUserPrmData

PrmText = 847 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  847  "VI15x Enabled"
Bit(3) 0 0-1
Prm_Text_Ref = 847 
EndExtUserPrmData

PrmText = 848 
Text(0) = "Error"
Text(1) = "Warning"
EndPrmText
ExtUserPrmData =  848  "Missing Module React."
Bit(7) 0 0-1
Prm_Text_Ref = 848 
EndExtUserPrmData

PrmText = 849 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  849  "Aux Inp 1 Ack Mode"
Bit(0) 0 0-1
Prm_Text_Ref = 849 
EndExtUserPrmData

PrmText = 850 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  850  "Aux Inp 2 Ack Mode"
Bit(1) 0 0-1
Prm_Text_Ref = 850 
EndExtUserPrmData

PrmText = 851 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  851  "Aux Inp 3 Ack Mode"
Bit(2) 0 0-1
Prm_Text_Ref = 851 
EndExtUserPrmData

PrmText = 852 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  852  "Aux Inp 4 Ack Mode"
Bit(3) 0 0-1
Prm_Text_Ref = 852 
EndExtUserPrmData

PrmText = 853 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  853  "Aux Inp 5 Ack Mode"
Bit(4) 0 0-1
Prm_Text_Ref = 853 
EndExtUserPrmData

PrmText = 854 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  854  "Aux Inp 6 Ack Mode"
Bit(5) 0 0-1
Prm_Text_Ref = 854 
EndExtUserPrmData

PrmText = 855 
Text(0) = "3 Phases"
Text(1) = "1 Phase"
EndPrmText
ExtUserPrmData =  855  "Number Of Phases"
Bit(6) 0 0-1
Prm_Text_Ref = 855 
EndExtUserPrmData

PrmText = 856 
Text(0) = "Time"
Text(1) = "x% Therm. Load"
EndPrmText
ExtUserPrmData =  856  "Cooling Mode"
Bit(7) 0 0-1
Prm_Text_Ref = 856 
EndExtUserPrmData

PrmText = 857 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  857  "Invert DI Start Inp."
Bit(0) 0 0-1
Prm_Text_Ref = 857 
EndExtUserPrmData

PrmText = 858 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  858  "Invert DI Stop Inp."
Bit(1) 1 0-1
Prm_Text_Ref = 858 
EndExtUserPrmData

PrmText = 859 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  859  "Inching DI Start Inp"
Bit(4) 0 0-1
Prm_Text_Ref = 859 
EndExtUserPrmData

PrmText = 860 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  860  "Loc 1 Start Bus Cyc"
Bit(0) 0 0-1
Prm_Text_Ref = 860 
EndExtUserPrmData

PrmText = 861 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  861  "Loc 1 Stop Bus Cyc"
Bit(1) 1 0-1
Prm_Text_Ref = 861 
EndExtUserPrmData

PrmText = 862 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  862  "Loc 1 Start DI"
Bit(2) 1 0-1
Prm_Text_Ref = 862 
EndExtUserPrmData

PrmText = 863 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  863  "Loc 1 Stop DI"
Bit(3) 1 0-1
Prm_Text_Ref = 863 
EndExtUserPrmData

PrmText = 864 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  864  "Loc 1 Start LCD"
Bit(4) 1 0-1
Prm_Text_Ref = 864 
EndExtUserPrmData

PrmText = 865 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  865  "Loc 1 Stop LCD"
Bit(5) 1 0-1
Prm_Text_Ref = 865 
EndExtUserPrmData

PrmText = 866 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  866  "Loc 1 Start Bus Acyc"
Bit(6) 0 0-1
Prm_Text_Ref = 866 
EndExtUserPrmData

PrmText = 867 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  867  "Loc 1 Stop Bus Acyc"
Bit(7) 1 0-1
Prm_Text_Ref = 867 
EndExtUserPrmData

PrmText = 868 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  868  "Auto Start Bus Cyc"
Bit(0) 1 0-1
Prm_Text_Ref = 868 
EndExtUserPrmData

PrmText = 869 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  869  "Auto Stop Bus Cyc"
Bit(1) 1 0-1
Prm_Text_Ref = 869 
EndExtUserPrmData

PrmText = 870 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  870  "Auto Start DI"
Bit(2) 0 0-1
Prm_Text_Ref = 870 
EndExtUserPrmData

PrmText = 871 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  871  "Auto Stop DI"
Bit(3) 1 0-1
Prm_Text_Ref = 871 
EndExtUserPrmData

PrmText = 872 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  872  "Auto Start LCD"
Bit(4) 0 0-1
Prm_Text_Ref = 872 
EndExtUserPrmData

PrmText = 873 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  873  "Auto Stop LCD"
Bit(5) 1 0-1
Prm_Text_Ref = 873 
EndExtUserPrmData

PrmText = 874 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  874  "Auto Start Bus Acyc"
Bit(6) 1 0-1
Prm_Text_Ref = 874 
EndExtUserPrmData

PrmText = 875 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  875  "Auto Stop Bus Acyc"
Bit(7) 1 0-1
Prm_Text_Ref = 875 
EndExtUserPrmData

PrmText = 876 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  876  "Loc 2 Start Bus Cyc"
Bit(0) 0 0-1
Prm_Text_Ref = 876 
EndExtUserPrmData

PrmText = 877 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  877  "Loc 2 Stop Bus Cyc"
Bit(1) 1 0-1
Prm_Text_Ref = 877 
EndExtUserPrmData

PrmText = 878 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  878  "Loc 2 Start DI"
Bit(2) 1 0-1
Prm_Text_Ref = 878 
EndExtUserPrmData

PrmText = 879 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  879  "Loc 2 Stop DI"
Bit(3) 1 0-1
Prm_Text_Ref = 879 
EndExtUserPrmData

PrmText = 880 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  880  "Loc 2 Start LCD"
Bit(4) 1 0-1
Prm_Text_Ref = 880 
EndExtUserPrmData

PrmText = 881 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  881  "Loc 2 Stop LCD"
Bit(5) 1 0-1
Prm_Text_Ref = 881 
EndExtUserPrmData

PrmText = 882 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  882  "Loc 2 Start Bus Acyc"
Bit(6) 0 0-1
Prm_Text_Ref = 882 
EndExtUserPrmData

PrmText = 883 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  883  "Loc 2 Stop Bus Acyc"
Bit(7) 1 0-1
Prm_Text_Ref = 883 
EndExtUserPrmData

PrmText = 884 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  884  "Multif In 0 Autoreset"
Bit(4) 0 0-1
Prm_Text_Ref = 884 
EndExtUserPrmData

PrmText = 885 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  885  "Multif In 1 Autoreset"
Bit(5) 0 0-1
Prm_Text_Ref = 885 
EndExtUserPrmData

PrmText = 886 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  886  "Multif In 2 Autoreset"
Bit(6) 0 0-1
Prm_Text_Ref = 886 
EndExtUserPrmData

;=============================================================
; Text-definition for User Prm Data "Softstarter PSE"
;=============================================================
;<
PrmText = 5403
Text(0)   = "Off"
Text(1)   = "On"
EndPrmText
PrmText = 5414
Text(0)  = "Class 10A"
Text(1)  = "Class 10"
Text(2)  = "Class 20"
Text(3)  = "Class 30"
EndPrmText
PrmText = 5415
Text(0)   = "Hand"
Text(1)   = "Auto"
EndPrmText


ExtUserPrmData = 5401 "Setting Ie [0.1A]"
Unsigned16 1 0-3700
EndExtUserPrmData

ExtUserPrmData = 5402 "Start Ramp [s]"
Unsigned16 10 1-30
EndExtUserPrmData

ExtUserPrmData = 5403 "Stop R On"
Unsigned16 0 0-1
Prm_Text_Ref=5403
EndExtUserPrmData

ExtUserPrmData = 5404 "Stop Ramp [s]"
Unsigned16 1 0-30
EndExtUserPrmData

ExtUserPrmData = 5405 "Init Volt [%]"
Unsigned16 40 30-70
EndExtUserPrmData

ExtUserPrmData = 5406 "End Volt [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 5407 "Curr Lim [0.1*Ie]"
Unsigned16 70 15-70
EndExtUserPrmData

ExtUserPrmData = 5408 "Trq Start"
Unsigned16 0 0-1
Prm_Text_Ref=5403
EndExtUserPrmData

ExtUserPrmData = 5409 "Trq Stop"
Unsigned16 0 0-1
Prm_Text_Ref=5403
EndExtUserPrmData

ExtUserPrmData = 5410 "Kick Start"
Unsigned16 0 0-1
Prm_Text_Ref=5403
EndExtUserPrmData

ExtUserPrmData = 5411 "Kick Time [0.1s]"
Unsigned16 2 1-10
EndExtUserPrmData

ExtUserPrmData = 5412 "Kick Volt [%]"
Unsigned16 50 30-100
EndExtUserPrmData

ExtUserPrmData = 5413 "EOL On"
Unsigned16 1 0-1
Prm_Text_Ref=5403
EndExtUserPrmData

ExtUserPrmData = 5414 "EOL Class"
Unsigned16 1 0-3
Prm_Text_Ref=5414
EndExtUserPrmData

ExtUserPrmData = 5415 "EOL Op"
Unsigned16 0 0-1
Prm_Text_Ref=5415
EndExtUserPrmData

ExtUserPrmData = 5416 "Underload"
Unsigned16 0 0-1
Prm_Text_Ref=5403
EndExtUserPrmData

ExtUserPrmData = 5417 "Underl Lev [0.1*Ie]"
Unsigned16 5 2-10
EndExtUserPrmData

ExtUserPrmData =5418 "Underl Op"
Unsigned16 0 0-1
Prm_Text_Ref=5415
EndExtUserPrmData

ExtUserPrmData = 5419 "Locked R"
Unsigned16 0 0-1
Prm_Text_Ref=5403
EndExtUserPrmData

ExtUserPrmData = 5420 "Lock R Lev [0.1*Ie]"
Unsigned16 12 5-70
EndExtUserPrmData

ExtUserPrmData = 5421 "Lock Op"
Unsigned16 0 0-1
Prm_Text_Ref=5415
EndExtUserPrmData

ExtUserPrmData = 5422 "Bad Net Op"
Unsigned16 0 0-1
Prm_Text_Ref=5415
EndExtUserPrmData




;
;=====================================================================
;=====================================================================

;=====================================================================
; special Parameter-Definitions for DPV1-Plug PDQ22
;=====================================================================
PrmText = 10000
Text(0)   = "Use Block-Parameters Port 1"
Text(1)   = "Ignore Block-Parameters Port 1"
EndPrmText
PrmText = 10001
Text(0)   = "Use Block-Parameters Port 2"
Text(1)   = "Ignore Block-Parameters Port 2"
EndPrmText
PrmText = 10002
Text(0)   = "Use Block-Parameters Port 3"
Text(1)   = "Ignore Block-Parameters Port 3"
EndPrmText
PrmText = 10003
Text(0)   = "Use Block-Parameters Port 4"
Text(1)   = "Ignore Block-Parameters Port 4"
EndPrmText

ExtUserPrmData=10000	"Block-Parameter port 1"	; 
Unsigned8 0 0-1   					; 
Prm_Text_Ref=10000
EndExtUserPrmData
ExtUserPrmData=10001	"Block-Parameter port 2"	; 
Unsigned8 0 0-1
Prm_Text_Ref=10001
EndExtUserPrmData
ExtUserPrmData=10002	"Block-Parameter port 3"	; 
Unsigned8 0 0-1
Prm_Text_Ref=10002
EndExtUserPrmData
ExtUserPrmData=10003	"Block-Parameter port 4"	; 
Unsigned8 0 0-1
Prm_Text_Ref=10003
EndExtUserPrmData

;
;===========================================================
;General parameters
;===========================================================
;
GSD_Revision   =5
Vendor_Name    ="ABB"
Model_Name     ="PDQ22-FBP.0"
Revision       ="V 1.12"
Ident_Number   =0x0A09
Protocol_Ident =0
Station_Type   =0
FMS_supp       =0
Hardware_Release= "V 1.0"
Software_Release= "V 1.0"
9.6_supp       =1
19.2_supp      =1
31.25_supp     =0
45.45_supp     =1
93.75_supp     =1
187.5_supp     =1
500_supp       =1
1.5M_supp      =1
3M_supp        =1
6M_supp        =1
12M_supp       =1
MaxTsdr_9.6    =15
MaxTsdr_19.2   =15
MaxTsdr_31.25  =15
MaxTsdr_45.45  =15
MaxTsdr_93.75  =15
MaxTsdr_187.5  =15
MaxTsdr_500    =15
MaxTsdr_1.5M   =20
MaxTsdr_3M     =35
MaxTsdr_6M     =50
MaxTsdr_12M    =95
Redundancy     =0
Repeater_Ctrl_Sig=0
24V_Pins       =1
Implementation_Type ="VPC3 solution"
Bitmap_Device       ="FBP_N"
Bitmap_Diag         ="FBP_DIAG"
Bitmap_SF           ="FBP_RUN"
;
;================================
; Slave-Specification:
;================================
;
Freeze_Mode_supp    =1
Sync_Mode_supp      =1
Set_Slave_Add_Supp  =0
Auto_Baud_supp      =1
Min_Slave_Intervall =1
Fail_Safe           =1
Max_Diag_Data_Len   =50	; 1 byte length + 6 bytes systemdiag. + 3 DPV1 + 5*8 bytes
Modul_Offset        =0
Slave_Family=9@FieldBusPlug@ProfibusDP
Modular_Station		 =1
Max_Module          =4
Max_Input_len       =192	; 4 * (16BI + 16AI)
Max_Output_len      =192	; 4 * (16BO + 16AO)
Max_Data_len        =384

;=================================
; Device specific diagnostic data
;=================================
;
;---------------------------------
; first 3 bytes DPV1 diag. (Bits 0..23)
;
; Diag bytes 0...7 for Quattro
Unit_Diag_Area = 24-31
Value(0) = "Port 1 OK"
Value(1) = "Port 1: Wrong device address"
Value(2) = "Port 1: Wrong device type" 
Value(3) = "Port 1: Wrong device & address" 
Value(4) = "Port 1: Device missing"
Value(8) = "Port 1: No device specified"
Unit_Diag_Area_End

Unit_Diag_Area = 32-39
Value(0) = "Port 2 OK"
Value(1) = "Port 2: Wrong device address"
Value(2) = "Port 2: Wrong device type" 
Value(3) = "Port 2: Wrong device & address" 
Value(4) = "Port 2: Device missing"
Value(8) = "Port 2: No device specified"
Unit_Diag_Area_End

Unit_Diag_Area = 40-47
Value(0) = "Port 3 OK"
Value(1) = "Port 3: Wrong device address"
Value(2) = "Port 3: Wrong device type" 
Value(3) = "Port 3: Wrong device & address" 
Value(4) = "Port 3: Device missing"
Value(8) = "Port 3: No device specified"
Unit_Diag_Area_End

Unit_Diag_Area = 48-55
Value(0) = "Port 4 OK"
Value(1) = "Port 4: Wrong device address"
Value(2) = "Port 4: Wrong device type" 
Value(3) = "Port 4: Wrong device & address" 
Value(4) = "Port 4: Device missing"
Value(8) = "Port 4: No device specified"
Unit_Diag_Area_End

; Bits 56-63 not specified
; Bits 64-71 not specified
; Bits 72-79 not specified
; Bits 80-87 not specified
;
;---------------------------------
; Diag bytes 0...7 for Device on port 1
Unit_Diag_bit(88) = "Device Diag Port1, Byte 0, Bit 0"
Unit_Diag_bit(89) = "Device Diag Port1, Byte 0, Bit 1"
Unit_Diag_bit(90) = "Device Diag Port1, Byte 0, Bit 2"
Unit_Diag_bit(91) = "Device Diag Port1, Byte 0, Bit 3"
Unit_Diag_bit(92) = "Device Diag Port1, Byte 0, Bit 4"
Unit_Diag_bit(93) = "Device Diag Port1, Byte 0, Bit 5"
Unit_Diag_bit(94) = "Device Diag Port1, Byte 0, Bit 6"
Unit_Diag_bit(95) = "Device Diag Port1, Byte 0, Bit 7"

Unit_Diag_bit(96) = "Device Diag Port1, Byte 1, Bit 0"
Unit_Diag_bit(97) = "Device Diag Port1, Byte 1, Bit 1"
Unit_Diag_bit(98) = "Device Diag Port1, Byte 1, Bit 2"
Unit_Diag_bit(99) = "Device Diag Port1, Byte 1, Bit 3"
Unit_Diag_bit(100) = "Device Diag Port1, Byte 1, Bit 4"
Unit_Diag_bit(101) = "Device Diag Port1, Byte 1, Bit 5"
Unit_Diag_bit(102) = "Device Diag Port1, Byte 1, Bit 6"
Unit_Diag_bit(103) = "Device Diag Port1, Byte 1, Bit 7"

Unit_Diag_bit(104) = "Device Diag Port1, Byte 2, Bit 0"
Unit_Diag_bit(105) = "Device Diag Port1, Byte 2, Bit 1"
Unit_Diag_bit(106) = "Device Diag Port1, Byte 2, Bit 2"
Unit_Diag_bit(107) = "Device Diag Port1, Byte 2, Bit 3"
Unit_Diag_bit(108) = "Device Diag Port1, Byte 2, Bit 4"
Unit_Diag_bit(109) = "Device Diag Port1, Byte 2, Bit 5"
Unit_Diag_bit(110) = "Device Diag Port1, Byte 2, Bit 6"
Unit_Diag_bit(111) = "Device Diag Port1, Byte 2, Bit 7"

Unit_Diag_bit(112) = "Device Diag Port1, Byte 3, Bit 0"
Unit_Diag_bit(113) = "Device Diag Port1, Byte 3, Bit 1"
Unit_Diag_bit(114) = "Device Diag Port1, Byte 3, Bit 2"
Unit_Diag_bit(115) = "Device Diag Port1, Byte 3, Bit 3"
Unit_Diag_bit(116) = "Device Diag Port1, Byte 3, Bit 4"
Unit_Diag_bit(117) = "Device Diag Port1, Byte 3, Bit 5"
Unit_Diag_bit(118) = "Device Diag Port1, Byte 3, Bit 6"
Unit_Diag_bit(119) = "Device Diag Port1, Byte 3, Bit 7"

Unit_Diag_bit(120) = "Device Diag Port1, Byte 4, Bit 0"
Unit_Diag_bit(121) = "Device Diag Port1, Byte 4, Bit 1"
Unit_Diag_bit(122) = "Device Diag Port1, Byte 4, Bit 2"
Unit_Diag_bit(123) = "Device Diag Port1, Byte 4, Bit 3"
Unit_Diag_bit(124) = "Device Diag Port1, Byte 4, Bit 4"
Unit_Diag_bit(125) = "Device Diag Port1, Byte 4, Bit 5"
Unit_Diag_bit(126) = "Device Diag Port1, Byte 4, Bit 6"
Unit_Diag_bit(127) = "Device Diag Port1, Byte 4, Bit 7"

Unit_Diag_bit(128) = "Device Diag Port1, Byte 5, Bit 0"
Unit_Diag_bit(129) = "Device Diag Port1, Byte 5, Bit 1"
Unit_Diag_bit(130) = "Device Diag Port1, Byte 5, Bit 2"
Unit_Diag_bit(131) = "Device Diag Port1, Byte 5, Bit 3"
Unit_Diag_bit(132) = "Device Diag Port1, Byte 5, Bit 4"
Unit_Diag_bit(133) = "Device Diag Port1, Byte 5, Bit 5"
Unit_Diag_bit(134) = "Device Diag Port1, Byte 5, Bit 6"
Unit_Diag_bit(135) = "Device Diag Port1, Byte 5, Bit 7"

Unit_Diag_bit(136) = "Device Diag Port1, Byte 6, Bit 0"
Unit_Diag_bit(137) = "Device Diag Port1, Byte 6, Bit 1"
Unit_Diag_bit(138) = "Device Diag Port1, Byte 6, Bit 2"
Unit_Diag_bit(139) = "Device Diag Port1, Byte 6, Bit 3"
Unit_Diag_bit(140) = "Device Diag Port1, Byte 6, Bit 4"
Unit_Diag_bit(141) = "Device Diag Port1, Byte 6, Bit 5"
Unit_Diag_bit(142) = "Device Diag Port1, Byte 6, Bit 6"
Unit_Diag_bit(143) = "Device Diag Port1, Byte 6, Bit 7"

Unit_Diag_bit(144) = "Device Diag Port1, Byte 7, Bit 0"
Unit_Diag_bit(145) = "Device Diag Port1, Byte 7, Bit 1"
Unit_Diag_bit(146) = "Device Diag Port1, Byte 7, Bit 2"
Unit_Diag_bit(147) = "Device Diag Port1, Byte 7, Bit 3"
Unit_Diag_bit(148) = "Device Diag Port1, Byte 7, Bit 4"
Unit_Diag_bit(149) = "Device Diag Port1, Byte 7, Bit 5"
Unit_Diag_bit(150) = "Device Diag Port1, Byte 7, Bit 6"
Unit_Diag_bit(151) = "Device Diag Port1, Byte 7, Bit 7"

;---------------------------------
; Diag bytes 0...7 for Device on port 2
Unit_Diag_bit(152) = "Device Diag Port2, Byte 0, Bit 0"
Unit_Diag_bit(153) = "Device Diag Port2, Byte 0, Bit 1"
Unit_Diag_bit(154) = "Device Diag Port2, Byte 0, Bit 2"
Unit_Diag_bit(155) = "Device Diag Port2, Byte 0, Bit 3"
Unit_Diag_bit(156) = "Device Diag Port2, Byte 0, Bit 4"
Unit_Diag_bit(157) = "Device Diag Port2, Byte 0, Bit 5"
Unit_Diag_bit(158) = "Device Diag Port2, Byte 0, Bit 6"
Unit_Diag_bit(159) = "Device Diag Port2, Byte 0, Bit 7"

Unit_Diag_bit(160) = "Device Diag Port2, Byte 1, Bit 0"
Unit_Diag_bit(161) = "Device Diag Port2, Byte 1, Bit 1"
Unit_Diag_bit(162) = "Device Diag Port2, Byte 1, Bit 2"
Unit_Diag_bit(163) = "Device Diag Port2, Byte 1, Bit 3"
Unit_Diag_bit(164) = "Device Diag Port2, Byte 1, Bit 4"
Unit_Diag_bit(165) = "Device Diag Port2, Byte 1, Bit 5"
Unit_Diag_bit(166) = "Device Diag Port2, Byte 1, Bit 6"
Unit_Diag_bit(167) = "Device Diag Port2, Byte 1, Bit 7"

Unit_Diag_bit(168) = "Device Diag Port2, Byte 2, Bit 0"
Unit_Diag_bit(169) = "Device Diag Port2, Byte 2, Bit 1"
Unit_Diag_bit(170) = "Device Diag Port2, Byte 2, Bit 2"
Unit_Diag_bit(171) = "Device Diag Port2, Byte 2, Bit 3"
Unit_Diag_bit(172) = "Device Diag Port2, Byte 2, Bit 4"
Unit_Diag_bit(173) = "Device Diag Port2, Byte 2, Bit 5"
Unit_Diag_bit(174) = "Device Diag Port2, Byte 2, Bit 6"
Unit_Diag_bit(175) = "Device Diag Port2, Byte 2, Bit 7"

Unit_Diag_bit(176) = "Device Diag Port2, Byte 3, Bit 0"
Unit_Diag_bit(177) = "Device Diag Port2, Byte 3, Bit 1"
Unit_Diag_bit(178) = "Device Diag Port2, Byte 3, Bit 2"
Unit_Diag_bit(179) = "Device Diag Port2, Byte 3, Bit 3"
Unit_Diag_bit(180) = "Device Diag Port2, Byte 3, Bit 4"
Unit_Diag_bit(181) = "Device Diag Port2, Byte 3, Bit 5"
Unit_Diag_bit(182) = "Device Diag Port2, Byte 3, Bit 6"
Unit_Diag_bit(183) = "Device Diag Port2, Byte 3, Bit 7"

Unit_Diag_bit(184) = "Device Diag Port2, Byte 4, Bit 0"
Unit_Diag_bit(185) = "Device Diag Port2, Byte 4, Bit 1"
Unit_Diag_bit(186) = "Device Diag Port2, Byte 4, Bit 2"
Unit_Diag_bit(187) = "Device Diag Port2, Byte 4, Bit 3"
Unit_Diag_bit(188) = "Device Diag Port2, Byte 4, Bit 4"
Unit_Diag_bit(189) = "Device Diag Port2, Byte 4, Bit 5"
Unit_Diag_bit(190) = "Device Diag Port2, Byte 4, Bit 6"
Unit_Diag_bit(191) = "Device Diag Port2, Byte 4, Bit 7"

Unit_Diag_bit(192) = "Device Diag Port2, Byte 5, Bit 0"
Unit_Diag_bit(193) = "Device Diag Port2, Byte 5, Bit 1"
Unit_Diag_bit(194) = "Device Diag Port2, Byte 5, Bit 2"
Unit_Diag_bit(195) = "Device Diag Port2, Byte 5, Bit 3"
Unit_Diag_bit(196) = "Device Diag Port2, Byte 5, Bit 4"
Unit_Diag_bit(197) = "Device Diag Port2, Byte 5, Bit 5"
Unit_Diag_bit(198) = "Device Diag Port2, Byte 5, Bit 6"
Unit_Diag_bit(199) = "Device Diag Port2, Byte 5, Bit 7"

Unit_Diag_bit(200) = "Device Diag Port2, Byte 6, Bit 0"
Unit_Diag_bit(201) = "Device Diag Port2, Byte 6, Bit 1"
Unit_Diag_bit(202) = "Device Diag Port2, Byte 6, Bit 2"
Unit_Diag_bit(203) = "Device Diag Port2, Byte 6, Bit 3"
Unit_Diag_bit(204) = "Device Diag Port2, Byte 6, Bit 4"
Unit_Diag_bit(205) = "Device Diag Port2, Byte 6, Bit 5"
Unit_Diag_bit(206) = "Device Diag Port2, Byte 6, Bit 6"
Unit_Diag_bit(207) = "Device Diag Port2, Byte 6, Bit 7"

Unit_Diag_bit(208) = "Device Diag Port2, Byte 7, Bit 0"
Unit_Diag_bit(209) = "Device Diag Port2, Byte 7, Bit 1"
Unit_Diag_bit(210) = "Device Diag Port2, Byte 7, Bit 2"
Unit_Diag_bit(211) = "Device Diag Port2, Byte 7, Bit 3"
Unit_Diag_bit(212) = "Device Diag Port2, Byte 7, Bit 4"
Unit_Diag_bit(213) = "Device Diag Port2, Byte 7, Bit 5"
Unit_Diag_bit(214) = "Device Diag Port2, Byte 7, Bit 6"
Unit_Diag_bit(215) = "Device Diag Port2, Byte 7, Bit 7"

;
;---------------------------------
; Diag bytes 0...7 for Device on port 3
Unit_Diag_bit(216) = "Device Diag Port3, Byte 0, Bit 0"
Unit_Diag_bit(217) = "Device Diag Port3, Byte 0, Bit 1"
Unit_Diag_bit(218) = "Device Diag Port3, Byte 0, Bit 2"
Unit_Diag_bit(219) = "Device Diag Port3, Byte 0, Bit 3"
Unit_Diag_bit(220) = "Device Diag Port3, Byte 0, Bit 4"
Unit_Diag_bit(221) = "Device Diag Port3, Byte 0, Bit 5"
Unit_Diag_bit(222) = "Device Diag Port3, Byte 0, Bit 6"
Unit_Diag_bit(223) = "Device Diag Port3, Byte 0, Bit 7"

Unit_Diag_bit(224) = "Device Diag Port3, Byte 1, Bit 0"
Unit_Diag_bit(225) = "Device Diag Port3, Byte 1, Bit 1"
Unit_Diag_bit(226) = "Device Diag Port3, Byte 1, Bit 2"
Unit_Diag_bit(227) = "Device Diag Port3, Byte 1, Bit 3"
Unit_Diag_bit(228) = "Device Diag Port3, Byte 1, Bit 4"
Unit_Diag_bit(229) = "Device Diag Port3, Byte 1, Bit 5"
Unit_Diag_bit(230) = "Device Diag Port3, Byte 1, Bit 6"
Unit_Diag_bit(231) = "Device Diag Port3, Byte 1, Bit 7"

Unit_Diag_bit(232) = "Device Diag Port3, Byte 2, Bit 0"
Unit_Diag_bit(233) = "Device Diag Port3, Byte 2, Bit 1"
Unit_Diag_bit(234) = "Device Diag Port3, Byte 2, Bit 2"
Unit_Diag_bit(235) = "Device Diag Port3, Byte 2, Bit 3"
Unit_Diag_bit(236) = "Device Diag Port3, Byte 2, Bit 4"
Unit_Diag_bit(237) = "Device Diag Port3, Byte 2, Bit 5"
Unit_Diag_bit(238) = "Device Diag Port3, Byte 2, Bit 6"
Unit_Diag_bit(239) = "Device Diag Port3, Byte 2, Bit 7"

Unit_Diag_bit(240) = "Device Diag Port3, Byte 3, Bit 0"
Unit_Diag_bit(241) = "Device Diag Port3, Byte 3, Bit 1"
Unit_Diag_bit(242) = "Device Diag Port3, Byte 3, Bit 2"
Unit_Diag_bit(243) = "Device Diag Port3, Byte 3, Bit 3"
Unit_Diag_bit(244) = "Device Diag Port3, Byte 3, Bit 4"
Unit_Diag_bit(245) = "Device Diag Port3, Byte 3, Bit 5"
Unit_Diag_bit(246) = "Device Diag Port3, Byte 3, Bit 6"
Unit_Diag_bit(247) = "Device Diag Port3, Byte 3, Bit 7"

Unit_Diag_bit(248) = "Device Diag Port3, Byte 4, Bit 0"
Unit_Diag_bit(249) = "Device Diag Port3, Byte 4, Bit 1"
Unit_Diag_bit(250) = "Device Diag Port3, Byte 4, Bit 2"
Unit_Diag_bit(251) = "Device Diag Port3, Byte 4, Bit 3"
Unit_Diag_bit(252) = "Device Diag Port3, Byte 4, Bit 4"
Unit_Diag_bit(253) = "Device Diag Port3, Byte 4, Bit 5"
Unit_Diag_bit(254) = "Device Diag Port3, Byte 4, Bit 6"
Unit_Diag_bit(255) = "Device Diag Port3, Byte 4, Bit 7"

Unit_Diag_bit(256) = "Device Diag Port3, Byte 5, Bit 0"
Unit_Diag_bit(257) = "Device Diag Port3, Byte 5, Bit 1"
Unit_Diag_bit(258) = "Device Diag Port3, Byte 5, Bit 2"
Unit_Diag_bit(259) = "Device Diag Port3, Byte 5, Bit 3"
Unit_Diag_bit(260) = "Device Diag Port3, Byte 5, Bit 4"
Unit_Diag_bit(261) = "Device Diag Port3, Byte 5, Bit 5"
Unit_Diag_bit(262) = "Device Diag Port3, Byte 5, Bit 6"
Unit_Diag_bit(263) = "Device Diag Port3, Byte 5, Bit 7"

Unit_Diag_bit(264) = "Device Diag Port3, Byte 6, Bit 0"
Unit_Diag_bit(265) = "Device Diag Port3, Byte 6, Bit 1"
Unit_Diag_bit(266) = "Device Diag Port3, Byte 6, Bit 2"
Unit_Diag_bit(267) = "Device Diag Port3, Byte 6, Bit 3"
Unit_Diag_bit(268) = "Device Diag Port3, Byte 6, Bit 4"
Unit_Diag_bit(269) = "Device Diag Port3, Byte 6, Bit 5"
Unit_Diag_bit(270) = "Device Diag Port3, Byte 6, Bit 6"
Unit_Diag_bit(271) = "Device Diag Port3, Byte 6, Bit 7"

Unit_Diag_bit(272) = "Device Diag Port3, Byte 7, Bit 0"
Unit_Diag_bit(273) = "Device Diag Port3, Byte 7, Bit 1"
Unit_Diag_bit(274) = "Device Diag Port3, Byte 7, Bit 2"
Unit_Diag_bit(275) = "Device Diag Port3, Byte 7, Bit 3"
Unit_Diag_bit(276) = "Device Diag Port3, Byte 7, Bit 4"
Unit_Diag_bit(277) = "Device Diag Port3, Byte 7, Bit 5"
Unit_Diag_bit(278) = "Device Diag Port3, Byte 7, Bit 6"
Unit_Diag_bit(279) = "Device Diag Port3, Byte 7, Bit 7"

;
;---------------------------------
; Diag bytes 0...7 for Device on port 4
Unit_Diag_bit(280) = "Device Diag Port4, Byte 0, Bit 0"
Unit_Diag_bit(281) = "Device Diag Port4, Byte 0, Bit 1"
Unit_Diag_bit(282) = "Device Diag Port4, Byte 0, Bit 2"
Unit_Diag_bit(283) = "Device Diag Port4, Byte 0, Bit 3"
Unit_Diag_bit(284) = "Device Diag Port4, Byte 0, Bit 4"
Unit_Diag_bit(285) = "Device Diag Port4, Byte 0, Bit 5"
Unit_Diag_bit(286) = "Device Diag Port4, Byte 0, Bit 6"
Unit_Diag_bit(287) = "Device Diag Port4, Byte 0, Bit 7"

Unit_Diag_bit(288) = "Device Diag Port4, Byte 1, Bit 0"
Unit_Diag_bit(289) = "Device Diag Port4, Byte 1, Bit 1"
Unit_Diag_bit(290) = "Device Diag Port4, Byte 1, Bit 2"
Unit_Diag_bit(291) = "Device Diag Port4, Byte 1, Bit 3"
Unit_Diag_bit(292) = "Device Diag Port4, Byte 1, Bit 4"
Unit_Diag_bit(293) = "Device Diag Port4, Byte 1, Bit 5"
Unit_Diag_bit(294) = "Device Diag Port4, Byte 1, Bit 6"
Unit_Diag_bit(295) = "Device Diag Port4, Byte 1, Bit 7"

Unit_Diag_bit(296) = "Device Diag Port4, Byte 2, Bit 0"
Unit_Diag_bit(297) = "Device Diag Port4, Byte 2, Bit 1"
Unit_Diag_bit(298) = "Device Diag Port4, Byte 2, Bit 2"
Unit_Diag_bit(299) = "Device Diag Port4, Byte 2, Bit 3"
Unit_Diag_bit(300) = "Device Diag Port4, Byte 2, Bit 4"
Unit_Diag_bit(301) = "Device Diag Port4, Byte 2, Bit 5"
Unit_Diag_bit(302) = "Device Diag Port4, Byte 2, Bit 6"
Unit_Diag_bit(303) = "Device Diag Port4, Byte 2, Bit 7"

Unit_Diag_bit(304) = "Device Diag Port4, Byte 3, Bit 0"
Unit_Diag_bit(305) = "Device Diag Port4, Byte 3, Bit 1"
Unit_Diag_bit(306) = "Device Diag Port4, Byte 3, Bit 2"
Unit_Diag_bit(307) = "Device Diag Port4, Byte 3, Bit 3"
Unit_Diag_bit(308) = "Device Diag Port4, Byte 3, Bit 4"
Unit_Diag_bit(309) = "Device Diag Port4, Byte 3, Bit 5"
Unit_Diag_bit(310) = "Device Diag Port4, Byte 3, Bit 6"
Unit_Diag_bit(311) = "Device Diag Port4, Byte 3, Bit 7"

Unit_Diag_bit(312) = "Device Diag Port4, Byte 4, Bit 0"
Unit_Diag_bit(313) = "Device Diag Port4, Byte 4, Bit 1"
Unit_Diag_bit(314) = "Device Diag Port4, Byte 4, Bit 2"
Unit_Diag_bit(315) = "Device Diag Port4, Byte 4, Bit 3"
Unit_Diag_bit(316) = "Device Diag Port4, Byte 4, Bit 4"
Unit_Diag_bit(317) = "Device Diag Port4, Byte 4, Bit 5"
Unit_Diag_bit(318) = "Device Diag Port4, Byte 4, Bit 6"
Unit_Diag_bit(319) = "Device Diag Port4, Byte 4, Bit 7"

Unit_Diag_bit(320) = "Device Diag Port4, Byte 5, Bit 0"
Unit_Diag_bit(321) = "Device Diag Port4, Byte 5, Bit 1"
Unit_Diag_bit(322) = "Device Diag Port4, Byte 5, Bit 2"
Unit_Diag_bit(323) = "Device Diag Port4, Byte 5, Bit 3"
Unit_Diag_bit(324) = "Device Diag Port4, Byte 5, Bit 4"
Unit_Diag_bit(325) = "Device Diag Port4, Byte 5, Bit 5"
Unit_Diag_bit(326) = "Device Diag Port4, Byte 5, Bit 6"
Unit_Diag_bit(327) = "Device Diag Port4, Byte 5, Bit 7"

Unit_Diag_bit(328) = "Device Diag Port4, Byte 6, Bit 0"
Unit_Diag_bit(329) = "Device Diag Port4, Byte 6, Bit 1"
Unit_Diag_bit(330) = "Device Diag Port4, Byte 6, Bit 2"
Unit_Diag_bit(331) = "Device Diag Port4, Byte 6, Bit 3"
Unit_Diag_bit(332) = "Device Diag Port4, Byte 6, Bit 4"
Unit_Diag_bit(333) = "Device Diag Port4, Byte 6, Bit 5"
Unit_Diag_bit(334) = "Device Diag Port4, Byte 6, Bit 6"
Unit_Diag_bit(335) = "Device Diag Port4, Byte 6, Bit 7"

Unit_Diag_bit(336) = "Device Diag Port4, Byte 7, Bit 0"
Unit_Diag_bit(337) = "Device Diag Port4, Byte 7, Bit 1"
Unit_Diag_bit(338) = "Device Diag Port4, Byte 7, Bit 2"
Unit_Diag_bit(339) = "Device Diag Port4, Byte 7, Bit 3"
Unit_Diag_bit(340) = "Device Diag Port4, Byte 7, Bit 4"
Unit_Diag_bit(341) = "Device Diag Port4, Byte 7, Bit 5"
Unit_Diag_bit(342) = "Device Diag Port4, Byte 7, Bit 6"
Unit_Diag_bit(343) = "Device Diag Port4, Byte 7, Bit 7"
;
;=============================================
; User Prm Data: Length and Preset:
;=============================================
;
Max_User_Prm_Data_Len	= 228					;   number of parameter of the longest module 
;                                        + number of parameter for the FBP itself
Ext_User_Prm_Data_Const(0) = 0x80,0x01,0x00,0x00,0x00,0x00,0x00,0x00 	; constant values for ASIC
;DPV1 status1 = 0x00 =>
;       Bit2 = 0 WD_Base=10ms (1ms=1)
;       Bit7 = 1 DPV1 Enable (Disable=0)
;DPV1 status2 = 0x00 =>
;       Bit0 = 0 ChkCfg nach EN50170(User specific=1)
;DPV1 status3 = 0x00 =>
;       alarm not implemented
Ext_User_Prm_Data_Ref(3) = 10000		; use/ignore Block-Parameters Port 1
Ext_User_Prm_Data_Ref(4) = 10001		; use/ignore Block-Parameters Port 2
Ext_User_Prm_Data_Ref(5) = 10002		; use/ignore Block-Parameters Port 3
Ext_User_Prm_Data_Ref(6) = 10003		; use/ignore Block-Parameters Port 4
;
;=============================================
; Module Definition List
;=============================================
;
Module="Empty Module" 0x00		; 
1
Ext_Module_Prm_Data_Len   = 7 							    ; length of module parameters
Ext_User_Prm_Data_Const(0)= 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00 ; ProductCode,BI,BO,AI,AO,Par
EndModule

Module="Sensor (static mode)" 0x10, 0x20				; 1DO, 2DI
2
Ext_Module_Prm_Data_Len   = 7 							    ; length of module parameters
Ext_User_Prm_Data_Const(0)= 0x00, 0x01, 0x01, 0x01, 0x00, 0x00, 0x00 ; ProductCode,BI,BO,AI,AO,Par
EndModule

Module="MSD11-FBP" 0x10, 0x20								; 1DO, 2DI
3
Ext_Module_Prm_Data_Len   = 7 							    ; length of module parameters
Ext_User_Prm_Data_Const(0)= 0x00, 0x01, 0x01, 0x01, 0x00, 0x00, 0x00 ; ProductCode,BI,BO,AI,AO,Par
EndModule

Module="MSR22-FBP" 0x10, 0x20								; 2DO, 3DI
4
Ext_Module_Prm_Data_Len   = 7 							    ; length of module parameters
Ext_User_Prm_Data_Const(0)= 0x2A, 0xFA, 0x01, 0x01, 0x00, 0x00, 0x00 ; ProductCode,BI,BO,AI,AO,Par
EndModule

Module="MFI21-FBP" 0x10, 0x20								; 3DO, 4DI
5
Ext_Module_Prm_Data_Len   = 12								; number of used data byte
; initialising of param data
; ProductCode,BI,BO,AI,AO,Par
Ext_User_Prm_Data_Const(0)= 0x2A, 0xF9, 0x01, 0x01, 0x00, 0x00, 0x05, \
                            0x00,0x00,0x00,0x00,0x32		
Ext_User_Prm_Data_Ref(7) = 50								; application mode
Ext_User_Prm_Data_Ref(8) = 51								; delay time
EndModule	

Module="UMC22-FBP (V3.0)" 0x11, 0x21, 0x50    	; 16DI, 16DO, 1AI
6
Ext_Module_Prm_Data_Len=49										; number of used data byte
; initialising of param data
; ProductCode,BI,BO,AI,AO,Par
Ext_User_Prm_Data_Const(0) =	 0x2A, 0xFB, 0x02, 0x02, 0x02, 0x00, 0x2A, \ 
							0x00,0x00,0x00,0x32,0x00,0x01,0x00,0x00,0x00,0x32, \
							0x01,0x01,0x01,0x00,0x0A,0x1E,0x04,0xB0,0x00,0x01, \
							0x02,0x04,0xB0,0x00,0x00,0xC8,0x00,0x14,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x0A,0x00
Ext_User_Prm_Data_Ref(7)	= 1
;Ext_User_Prm_Data_Ref(11)	= 2
Ext_User_Prm_Data_Ref(13)	= 23
Ext_User_Prm_Data_Ref(17)	= 3
;Ext_User_Prm_Data_Ref(18)	= 4
Ext_User_Prm_Data_Ref(19)	= 5

Ext_User_Prm_Data_Ref(21)	= 6
Ext_User_Prm_Data_Ref(22)	= 7
Ext_User_Prm_Data_Ref(23)	= 8
Ext_User_Prm_Data_Ref(25)	= 9
Ext_User_Prm_Data_Ref(26) = 10
Ext_User_Prm_Data_Ref(27)	= 11
Ext_User_Prm_Data_Ref(28)	= 17
Ext_User_Prm_Data_Ref(30)	= 21
Ext_User_Prm_Data_Ref(31)	= 12
Ext_User_Prm_Data_Ref(33)	= 13
;Ext_User_Prm_Data_Ref(35)	= 14
;Ext_User_Prm_Data_Ref(39)	= 15
Ext_User_Prm_Data_Ref(43) = 25  
Ext_User_Prm_Data_Ref(44)	= 16
Ext_User_Prm_Data_Ref(45)	= 24
Ext_User_Prm_Data_Ref(46)	= 18
Ext_User_Prm_Data_Ref(47)	= 19
Ext_User_Prm_Data_Ref(48)	= 20
EndModule

Module="UMC22-FBP (V3.10, V3.20)" 0x11, 0x21, 0x50   	; 16DI, 16DO, 1AI
7
Ext_Module_Prm_Data_Len=49										; number of used data byte
; initialising of param data
;ProductCode,BI,BO,AI,AO,Par
Ext_User_Prm_Data_Const(0) =	 0x2A, 0xFB, 0x02, 0x02, 0x02, 0x00, 0x2A, \ 
							0x00,0x00,0x00,0x32,0x00,0x01,0x00,0x00,0x00,0x32, \
							0x01,0x01,0x01,0x00,0x0A,0x1E,0x04,0xB0,0x00,0x01, \
							0x02,0x04,0xB0,0x00,0x00,0xC8,0x00,0x14,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x0A,0x00
Ext_User_Prm_Data_Ref(7)	= 101
Ext_User_Prm_Data_Ref(11)	= 102
Ext_User_Prm_Data_Ref(13)	= 123
Ext_User_Prm_Data_Ref(17)	= 103
;Ext_User_Prm_Data_Ref(18)	= 104
Ext_User_Prm_Data_Ref(19)	= 105

Ext_User_Prm_Data_Ref(21)	= 106
Ext_User_Prm_Data_Ref(22)	= 107
Ext_User_Prm_Data_Ref(23)	= 108
Ext_User_Prm_Data_Ref(25)	= 109
Ext_User_Prm_Data_Ref(26) = 110
Ext_User_Prm_Data_Ref(27)	= 111
Ext_User_Prm_Data_Ref(28)	= 117
Ext_User_Prm_Data_Ref(30)	= 121
Ext_User_Prm_Data_Ref(31)	= 112
Ext_User_Prm_Data_Ref(33)	= 113
Ext_User_Prm_Data_Ref(35)	= 114
Ext_User_Prm_Data_Ref(37)	= 126
Ext_User_Prm_Data_Ref(39)	= 115
Ext_User_Prm_Data_Ref(43) = 125  
Ext_User_Prm_Data_Ref(44)	= 116
Ext_User_Prm_Data_Ref(45)	= 124
Ext_User_Prm_Data_Ref(46)	= 118
Ext_User_Prm_Data_Ref(47)	= 119
Ext_User_Prm_Data_Ref(48)	= 120
EndModule

Module="UMC22-FBP (V3.30)" 0x11, 0x21, 0x50   	; 16DI, 16DO, 1AI
8
Ext_Module_Prm_Data_Len=49										; number of used data byte
; initialising of param data
; ProductCode,BI,BO,AI,AO,Par
Ext_User_Prm_Data_Const(0) = 0x2A, 0xFB, 0x02, 0x02, 0x02, 0x00, 0x2A, \
							0x00,0x00,0x00,0x32,0x00,0x64,0x00,0x00,0x00,0x32, \
							0x01,0x00,0x01,0x00,0x0A,0x1E,0x04,0xB0,0x00,0x01, \
							0x02,0x04,0xB0,0x00,0x00,0xC8,0x00,0x14,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x0A,0x00
Ext_User_Prm_Data_Ref(7)	= 151
Ext_User_Prm_Data_Ref(11)	= 152
Ext_User_Prm_Data_Ref(13)	= 173
Ext_User_Prm_Data_Ref(17)	= 153
Ext_User_Prm_Data_Ref(18)	= 154
Ext_User_Prm_Data_Ref(19)	= 155
Ext_User_Prm_Data_Ref(20)	= 177
Ext_User_Prm_Data_Ref(21)	= 156
Ext_User_Prm_Data_Ref(22)	= 157
Ext_User_Prm_Data_Ref(23)	= 158
Ext_User_Prm_Data_Ref(25)	= 159
Ext_User_Prm_Data_Ref(26) = 160
Ext_User_Prm_Data_Ref(27)	= 161
Ext_User_Prm_Data_Ref(28)	= 167
Ext_User_Prm_Data_Ref(30)	= 171
Ext_User_Prm_Data_Ref(31)	= 162
Ext_User_Prm_Data_Ref(33)	= 163
Ext_User_Prm_Data_Ref(35)	= 164
Ext_User_Prm_Data_Ref(37)	= 176
Ext_User_Prm_Data_Ref(38)	= 178
Ext_User_Prm_Data_Ref(39)	= 165
Ext_User_Prm_Data_Ref(43) = 175  
Ext_User_Prm_Data_Ref(44)	= 166
Ext_User_Prm_Data_Ref(45)	= 174
Ext_User_Prm_Data_Ref(46)	= 168
Ext_User_Prm_Data_Ref(47)	= 169
Ext_User_Prm_Data_Ref(48)	= 170
EndModule

Module="UMC22-FBP (V3.40, V3.50)" 0x11, 0x21, 0x50   	; 16DI, 16DO, 1AI
9
Ext_Module_Prm_Data_Len=49
; initialising of param data
; ProductCode,BI,BO,AI,AO,Par
Ext_User_Prm_Data_Const(0) = 0x2A, 0xFB, 0x02, 0x02, 0x02, 0x00, 0x2A, \
							0x00,0x00,0x00,0x32,0x00,0x64,0x00,0x00,0x00,0x32, \
							0x01,0x00,0x01,0x00,0x0A,0x1E,0x04,0xB0,0x00,0x01, \
							0x02,0x04,0xB0,0x00,0x00,0xC8,0x00,0x14,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x0A,0x00
Ext_User_Prm_Data_Ref(7)	= 181
Ext_User_Prm_Data_Ref(11)	= 182
Ext_User_Prm_Data_Ref(13)	= 203
Ext_User_Prm_Data_Ref(17)	= 183
Ext_User_Prm_Data_Ref(18)	= 184
Ext_User_Prm_Data_Ref(19)	= 185
Ext_User_Prm_Data_Ref(20)	= 207
Ext_User_Prm_Data_Ref(21)	= 186
Ext_User_Prm_Data_Ref(22)	= 187
Ext_User_Prm_Data_Ref(23)	= 188
Ext_User_Prm_Data_Ref(25)	= 189
Ext_User_Prm_Data_Ref(26)	= 190
Ext_User_Prm_Data_Ref(27)	= 191
Ext_User_Prm_Data_Ref(28)	= 197
Ext_User_Prm_Data_Ref(30)	= 201
Ext_User_Prm_Data_Ref(31)	= 192
Ext_User_Prm_Data_Ref(33)	= 193
Ext_User_Prm_Data_Ref(35)	= 194
Ext_User_Prm_Data_Ref(37)	= 206
Ext_User_Prm_Data_Ref(38)	= 208
Ext_User_Prm_Data_Ref(39)	= 195
Ext_User_Prm_Data_Ref(43)	= 205  
Ext_User_Prm_Data_Ref(44)	= 196
Ext_User_Prm_Data_Ref(45)	= 204
Ext_User_Prm_Data_Ref(46)	= 198
Ext_User_Prm_Data_Ref(47)	= 199
Ext_User_Prm_Data_Ref(48)	= 200
EndModule

Module="UMC22-FBP (V4.00)" 0x11, 0x21, 0x50   	; 16DI, 16DO, 1AI
15
Ext_Module_Prm_Data_Len=49
; initialising of param data
; ProductCode,BI,BO,AI,AO,Par
Ext_User_Prm_Data_Const(0) = 0x2A, 0xFB, 0x02, 0x02, 0x02, 0x00, 0x2A, \
							0x00,0x00,0x00,0x32,0x00,0x64,0x00,0x00,0x00,0x32, \
							0x01,0x00,0x01,0x00,0x0A,0x1E,0x04,0xB0,0x00,0x01, \
							0x02,0x04,0xB0,0x00,0x00,0xC8,0x00,0x14,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x0A,0x00
Ext_User_Prm_Data_Ref(7)	= 181	; Set Current 1
Ext_User_Prm_Data_Ref(11)	= 211	; Current Factor (%) --> changed
Ext_User_Prm_Data_Ref(13)	= 203	; Set Current 2
Ext_User_Prm_Data_Ref(17)	= 183	; Trip Class
Ext_User_Prm_Data_Ref(18)	= 184	; DI0 Multi Function Input
Ext_User_Prm_Data_Ref(19)	= 185	; Phase Loss Protection
Ext_User_Prm_Data_Ref(20)	= 207	; DI1 Multi Function Input
Ext_User_Prm_Data_Ref(21)	= 186	; Low Current Threshold
Ext_User_Prm_Data_Ref(22)	= 187	; High Current Threshold
Ext_User_Prm_Data_Ref(23)	= 188	; Cooling Time
Ext_User_Prm_Data_Ref(25)	= 189	; Automatic fault reset
Ext_User_Prm_Data_Ref(26)	= 190	; Control Function
Ext_User_Prm_Data_Ref(27)	= 191	; Check-Back
Ext_User_Prm_Data_Ref(28)	= 197	; Start-Up Time
Ext_User_Prm_Data_Ref(30)	= 201	; Star-Delta Changeover Mode
Ext_User_Prm_Data_Ref(31)	= 192	; Star-Delta Start Time
Ext_User_Prm_Data_Ref(33)	= 193	; Reverse Lockout Time
Ext_User_Prm_Data_Ref(35)	= 194	; Operating Hours of Motor
Ext_User_Prm_Data_Ref(37)	= 206	; Number of Trips
Ext_User_Prm_Data_Ref(38)	= 208	; Emergency by PLC
Ext_User_Prm_Data_Ref(39)	= 195	; Number of Starts
Ext_User_Prm_Data_Ref(43)	= 205   ; Address Check
Ext_User_Prm_Data_Ref(44)	= 196	; Bus fault reaction
Ext_User_Prm_Data_Ref(45)	= 204	; DI2 Multi Function Input
Ext_User_Prm_Data_Ref(46)	= 210	; Local Control --> changed
Ext_User_Prm_Data_Ref(47)	= 199	; Block Current Threshold
Ext_User_Prm_Data_Ref(48)	= 200	; Fault Output
EndModule

Module="WDI100-FBP" 0x5F							;16 AI
10
Ext_Module_Prm_Data_Len  = 25					;Number of used Data Bytes
;Initialising of Param Data
;ProductCode,BI,BO,AI,AO,Par
Ext_User_Prm_Data_Const(0)=\
								0x27, 0x11, 0x00, 0x00, 0x20, 0x00, 0x12, \
								0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,\
								0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00
Ext_User_Prm_Data_Ref(7)  = 500
Ext_User_Prm_Data_Ref(9)  = 501
Ext_User_Prm_Data_Ref(11) = 502
Ext_User_Prm_Data_Ref(13) = 503
Ext_User_Prm_Data_Ref(15) = 504
Ext_User_Prm_Data_Ref(17) = 505
Ext_User_Prm_Data_Ref(19) = 506
Ext_User_Prm_Data_Ref(21) = 507
Ext_User_Prm_Data_Ref(23) = 508
EndModule


; WDIO100-WDI
Module="WDIO100-WDI" 0x5F							;16 AI
12
Ext_Module_Prm_Data_Len  = 27				;Number of used Param Bytes
Ext_User_Prm_Data_Const(0)=\					;Initialising of Param Data
	0x27, 0x1A, 0x00, 0x00, 0x10, 0x00, 0x1B, \ ; ProductCode,BI,BO,AI,AO,Par
	0x01, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,\
	0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00 

Ext_User_Prm_Data_Ref(7)  = 604
Ext_User_Prm_Data_Ref(9)  = 605
Ext_User_Prm_Data_Ref(11) = 606
Ext_User_Prm_Data_Ref(13) = 607
Ext_User_Prm_Data_Ref(15) = 608
Ext_User_Prm_Data_Ref(17) = 609
Ext_User_Prm_Data_Ref(19) = 610
Ext_User_Prm_Data_Ref(21) = 611
Ext_User_Prm_Data_Ref(23) = 612
Ext_User_Prm_Data_Ref(25) = 616
EndModule

; WDIO100-WDX
Module="WDIO100-WDX" 0x5F, 0x63							;16 AI, 4 AO 
13
Ext_Module_Prm_Data_Len  = 27					;Number of used Param Bytes
Ext_User_Prm_Data_Const(0)=\					;Initialising of Param Data
	0x27, 0x1B, 0x00, 0x00, 0x10, 0x04, 0x1B, \ ; ProductCode,BI,BO,AI,AO,Par
	0x01, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, \
	0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00 

Ext_User_Prm_Data_Ref(7)  = 604
Ext_User_Prm_Data_Ref(9)  = 605
Ext_User_Prm_Data_Ref(11) = 606
Ext_User_Prm_Data_Ref(13) = 607
Ext_User_Prm_Data_Ref(15) = 613
Ext_User_Prm_Data_Ref(17) = 614
Ext_User_Prm_Data_Ref(19) = 616
Ext_User_Prm_Data_Ref(21) = 617
Ext_User_Prm_Data_Ref(23) = 618
Ext_User_Prm_Data_Ref(25) = 619
EndModule

; WDIO100-WDP
Module="WDIO100-WDP" 0x5F, 0x66							;16 AI, 7 AO 
14
Ext_Module_Prm_Data_Len  = 19					;Number of used Param Bytes
Ext_User_Prm_Data_Const(0)=\					;Initialising of Param Data
	0x27, 0x1C, 0x00, 0x00, 0x10, 0x07, 0x0C, \ ; ProductCode,BI,BO,AI,AO,Par
 	0x01, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, \
	0x00, 0x00
								
Ext_User_Prm_Data_Ref(7)	= 604
Ext_User_Prm_Data_Ref(9)	= 615
Ext_User_Prm_Data_Ref(11)	= 616
Ext_User_Prm_Data_Ref(13)	= 617
Ext_User_Prm_Data_Ref(15)	= 618
Ext_User_Prm_Data_Ref(17)	= 619
EndModule


Module="PSR" 0x10, 0x20								; 1DO, 2DI
11
Ext_Module_Prm_Data_Len   = 7 							    ; length of module parameters
Ext_User_Prm_Data_Const(0)= 0x00, 0x01, 0x01, 0x01, 0x00, 0x00, 0x00 ; ProductCode,BI,BO,AI,AO,Par
EndModule


;=============================================================
; Module description  UMC100_FBP (V1.13)
;=============================================================
;
Module="UMC100-FBP (V1.13)"0x11, 0x23, 0x56, 0x63      ; 16DI, 32DO, 7AI, 4AO
16
Ext_Module_Prm_Data_Len=55                     ; number of used data byte
Ext_User_Prm_Data_Const(0) =    \                 ; initialising of param data
    0x2B, 0xC0, 0x02, 0x04, 0x0E, 0x08, 0x30, \ ; ProductCode,BI,BO,AI,AO,Par
    0x00, 0x00, 0x00, 0x32, 0x00, 0x00, 0x00, 0x32, 0x02, 0x58,  \
    0x00, 0x64, 0x00, 0x78, 0x00, 0x05, 0x00, 0x01, 0x00, 0x01,  \
    0x0A, 0x00, 0x1E, 0xA0, 0xA0, 0x05, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x03, 0x00, 0x00, 0x00, 0x00, 0x08, 0x60,  \
    0x00, 0x00, 0x02, 0xBE, 0xEB, 0xBE, 0x00, 0x00
Ext_User_Prm_Data_Ref( 7 ) = 401 ;   Setting Ie 1
Ext_User_Prm_Data_Ref( 11 ) = 402 ;   Setting Ie 2
Ext_User_Prm_Data_Ref( 15 ) = 403 ;   YD Starting Time
Ext_User_Prm_Data_Ref( 17 ) = 404 ;   Current Factor
Ext_User_Prm_Data_Ref( 19 ) = 405 ;   Cooling Time
Ext_User_Prm_Data_Ref( 23 ) = 406 ;   Language
Ext_User_Prm_Data_Ref( 24 ) = 407 ;   Rev Lock-Out Time
Ext_User_Prm_Data_Ref( 25 ) = 408 ;   Fault Output
Ext_User_Prm_Data_Ref( 26 ) = 409 ;   Trip Class
Ext_User_Prm_Data_Ref( 27 ) = 410 ;   Low Curr Warn Level
Ext_User_Prm_Data_Ref( 28 ) = 411 ;   Low Curr Trip Level
Ext_User_Prm_Data_Ref( 29 ) = 412 ;   High Curr Warn Level
Ext_User_Prm_Data_Ref( 30 ) = 413 ;   High Curr Trip Level
Ext_User_Prm_Data_Ref( 31 ) = 414 ;   Locked Rotor Level
Ext_User_Prm_Data_Ref( 32 ) = 415 ;   Locked Rotor Delay
Ext_User_Prm_Data_Ref( 33 ) = 416 ;   Custom App Parameter
Ext_User_Prm_Data_Ref( 34 ) = 417 ;   Multif In 0
Ext_User_Prm_Data_Ref( 35 ) = 418 ;   Multif In 1
Ext_User_Prm_Data_Ref( 36 ) = 419 ;   Multif In 2
Ext_User_Prm_Data_Ref( 37 ) = 420 ;   Multif In 0 Delay
Ext_User_Prm_Data_Ref( 38 ) = 421 ;   Multif In 1 Delay
Ext_User_Prm_Data_Ref( 39 ) = 422 ;   Multif In 2 Delay
Ext_User_Prm_Data_Ref( 40 ) = 423 ;   Control Function
Ext_User_Prm_Data_Ref( 41 ) = 424 ;   Busfault Reaction
Ext_User_Prm_Data_Ref( 42 ) = 425 ;   Aux Inp 1 Reaction
Ext_User_Prm_Data_Ref( 42 ) = 426 ;   Aux Inp 2 Reaction
Ext_User_Prm_Data_Ref( 43 ) = 427 ;   Aux Inp 3 Reaction
Ext_User_Prm_Data_Ref( 43 ) = 428 ;   Aux Inp 4 Reaction
Ext_User_Prm_Data_Ref( 44 ) = 429 ;   Aux Inp 5 Reaction
Ext_User_Prm_Data_Ref( 44 ) = 430 ;   Aux Inp 6 Reaction
Ext_User_Prm_Data_Ref( 45 ) = 431 ;   PTC, Thermistor
Ext_User_Prm_Data_Ref( 45 ) = 432 ;   Check-Back
Ext_User_Prm_Data_Ref( 45 ) = 433 ;   Check Phase Sequence
Ext_User_Prm_Data_Ref( 46 ) = 434 ;   Fault Auto Reset
Ext_User_Prm_Data_Ref( 46 ) = 435 ;   Emergency Start
Ext_User_Prm_Data_Ref( 46 ) = 436 ;   Address Check
Ext_User_Prm_Data_Ref( 46 ) = 437 ;   Enable Custom Logic
Ext_User_Prm_Data_Ref( 46 ) = 438 ;   YD Change-Over Mode
Ext_User_Prm_Data_Ref( 46 ) = 439 ;   Phase Loss Prot.
Ext_User_Prm_Data_Ref( 47 ) = 440 ;   DX1xx Enabled
Ext_User_Prm_Data_Ref( 47 ) = 441 ;   Missing Module React.
Ext_User_Prm_Data_Ref( 48 ) = 442 ;   Aux Inp 1 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 443 ;   Aux Inp 2 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 444 ;   Aux Inp 3 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 445 ;   Aux Inp 4 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 446 ;   Aux Inp 5 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 447 ;   Aux Inp 6 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 448 ;   Cooling Mode
Ext_User_Prm_Data_Ref( 49 ) = 449 ;   Invert DI Start Inp.
Ext_User_Prm_Data_Ref( 49 ) = 450 ;   Invert DI Stop Inp.
Ext_User_Prm_Data_Ref( 49 ) = 451 ;   Inching DI Start Inp
Ext_User_Prm_Data_Ref( 50 ) = 452 ;   Loc 1 Start Bus Cyc
Ext_User_Prm_Data_Ref( 50 ) = 453 ;   Loc 1 Stop Bus Cyc
Ext_User_Prm_Data_Ref( 50 ) = 454 ;   Loc 1 Start DI
Ext_User_Prm_Data_Ref( 50 ) = 455 ;   Loc 1 Stop DI
Ext_User_Prm_Data_Ref( 50 ) = 456 ;   Loc 1 Start LCD
Ext_User_Prm_Data_Ref( 50 ) = 457 ;   Loc 1 Stop LCD
Ext_User_Prm_Data_Ref( 50 ) = 458 ;   Loc 1 Start Bus Acyc
Ext_User_Prm_Data_Ref( 50 ) = 459 ;   Loc 1 Stop Bus Acyc
Ext_User_Prm_Data_Ref( 51 ) = 460 ;   Auto Start Bus Cyc
Ext_User_Prm_Data_Ref( 51 ) = 461 ;   Auto Stop Bus Cyc
Ext_User_Prm_Data_Ref( 51 ) = 462 ;   Auto Start DI
Ext_User_Prm_Data_Ref( 51 ) = 463 ;   Auto Stop DI
Ext_User_Prm_Data_Ref( 51 ) = 464 ;   Auto Start LCD
Ext_User_Prm_Data_Ref( 51 ) = 465 ;   Auto Stop LCD
Ext_User_Prm_Data_Ref( 51 ) = 466 ;   Auto Start Bus Acyc
Ext_User_Prm_Data_Ref( 51 ) = 467 ;   Auto Stop Bus Acyc
Ext_User_Prm_Data_Ref( 52 ) = 468 ;   Loc 2 Start Bus Cyc
Ext_User_Prm_Data_Ref( 52 ) = 469 ;   Loc 2 Stop Bus Cyc
Ext_User_Prm_Data_Ref( 52 ) = 470 ;   Loc 2 Start DI
Ext_User_Prm_Data_Ref( 52 ) = 471 ;   Loc 2 Stop DI
Ext_User_Prm_Data_Ref( 52 ) = 472 ;   Loc 2 Start LCD
Ext_User_Prm_Data_Ref( 52 ) = 473 ;   Loc 2 Stop LCD
Ext_User_Prm_Data_Ref( 52 ) = 474 ;   Loc 2 Start Bus Acyc
Ext_User_Prm_Data_Ref( 52 ) = 475 ;   Loc 2 Stop Bus Acyc
Ext_User_Prm_Data_Ref( 53 ) = 476 ;   Multif In 0 Autoreset
Ext_User_Prm_Data_Ref( 53 ) = 477 ;   Multif In 1 Autoreset
Ext_User_Prm_Data_Ref( 53 ) = 478 ;   Multif In 2 Autoreset
EndModule


Module="PSE" 0x11, 0x23, 0x5A			;16 DI, 32 DO, 11 AI, Compatible with PSE.
17
Ext_Module_Prm_Data_Len=51												;number of used data bytes
Ext_User_Prm_Data_Const(0)=\								 				;Initialising of Param data
	0x2E,0xE2,0x02,0x04,0x16,0x00,0x2C, \ ; ProductCode,BI,BO,AI,AO,Par
	0x00,0x01,0x00,0x0A,0x00,0x00,0x00,0x01,0x00,0x28, \	;1-5, A:1-5, NA:-
	0x00,0x1E,0x00,0x46,0x00,0x00,0x00,0x00,0x00,0x00, \	;6-10, A:6-10, NA:-
	0x00,0x02,0x00,0x32,0x00,0x01,0x00,0x01,0x00,0x00, \	;11-15, A:11-15, NA:-
	0x00,0x00,0x00,0x05,0x00,0x00,0x00,0x00,0x00,0x0c, \	;16-20, A:16-20 NA:-
	0x00,0x00,0x00,0x00                                	;21-22, A:21-22, NA:-

Ext_User_Prm_Data_Ref(7)	= 5401
Ext_User_Prm_Data_Ref(9)	= 5402
Ext_User_Prm_Data_Ref(11)	= 5403
Ext_User_Prm_Data_Ref(13)	= 5404
Ext_User_Prm_Data_Ref(15)	= 5405
Ext_User_Prm_Data_Ref(17)	= 5406
Ext_User_Prm_Data_Ref(19)	= 5407
Ext_User_Prm_Data_Ref(21)	= 5408
Ext_User_Prm_Data_Ref(23)	= 5409
Ext_User_Prm_Data_Ref(25)	= 5410
Ext_User_Prm_Data_Ref(27)	= 5411
Ext_User_Prm_Data_Ref(29)	= 5412
Ext_User_Prm_Data_Ref(31)	= 5413
Ext_User_Prm_Data_Ref(33)	= 5414
Ext_User_Prm_Data_Ref(35)	= 5415
Ext_User_Prm_Data_Ref(37)	= 5416
Ext_User_Prm_Data_Ref(39)	= 5417
Ext_User_Prm_Data_Ref(41)	= 5418
Ext_User_Prm_Data_Ref(43)	= 5419
Ext_User_Prm_Data_Ref(45)	= 5420
Ext_User_Prm_Data_Ref(47)	= 5421
Ext_User_Prm_Data_Ref(49)	= 5422

EndModule

;=============================================================
; Module description  UMC100_FBP (R0101 R0201)
;=============================================================
;
Module="UMC100-FBP (R0101 R0201)"0x11, 0x23, 0x56, 0x63      ; 16DI, 32DO, 7AI, 4AO
18
Ext_Module_Prm_Data_Len=55                     ; number of used data byte
Ext_User_Prm_Data_Const(0) =    \                 ; initialising of param data
    0x2B, 0xC0, 0x02, 0x04, 0x0E, 0x08, 0x30, \ ; ProductCode,BI,BO,AI,AO,Par
    0x00, 0x00, 0x00, 0x32, 0x00, 0x00, 0x00, 0x32, 0x02, 0x58,  \
    0x00, 0x64, 0x00, 0x78, 0xFF, 0x05, 0x00, 0x01, 0x00, 0x01,  \
    0x0A, 0x00, 0x1E, 0xA0, 0xA0, 0x05, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x03, 0x00, 0x00, 0x00, 0x00, 0x08, 0x64,  \
    0x00, 0x00, 0x02, 0xBE, 0xEB, 0xBE, 0x00, 0x00
Ext_User_Prm_Data_Ref( 7 ) = 701 ;   Setting Ie 1
Ext_User_Prm_Data_Ref( 11 ) = 702 ;   Setting Ie 2
Ext_User_Prm_Data_Ref( 15 ) = 703 ;   YD Starting Time
Ext_User_Prm_Data_Ref( 17 ) = 704 ;   Current Factor
Ext_User_Prm_Data_Ref( 19 ) = 705 ;   Cooling Time
Ext_User_Prm_Data_Ref( 21 ) = 706 ;   Earth Flt Trip Level
Ext_User_Prm_Data_Ref( 22 ) = 707 ;   Earth Flt Trip Delay
Ext_User_Prm_Data_Ref( 23 ) = 708 ;   Language
Ext_User_Prm_Data_Ref( 24 ) = 709 ;   Rev Lock-Out Time
Ext_User_Prm_Data_Ref( 25 ) = 710 ;   Fault Output
Ext_User_Prm_Data_Ref( 26 ) = 711 ;   Trip Class
Ext_User_Prm_Data_Ref( 27 ) = 712 ;   Low Curr Warn Level
Ext_User_Prm_Data_Ref( 28 ) = 713 ;   Low Curr Trip Level
Ext_User_Prm_Data_Ref( 29 ) = 714 ;   High Curr Warn Level
Ext_User_Prm_Data_Ref( 30 ) = 715 ;   High Curr Trip Level
Ext_User_Prm_Data_Ref( 31 ) = 716 ;   Locked Rotor Level
Ext_User_Prm_Data_Ref( 32 ) = 717 ;   Locked Rotor Delay
Ext_User_Prm_Data_Ref( 33 ) = 718 ;   Custom App Parameter
Ext_User_Prm_Data_Ref( 34 ) = 719 ;   Multif In 0
Ext_User_Prm_Data_Ref( 35 ) = 720 ;   Multif In 1
Ext_User_Prm_Data_Ref( 36 ) = 721 ;   Multif In 2
Ext_User_Prm_Data_Ref( 37 ) = 722 ;   Multif In 0 Delay
Ext_User_Prm_Data_Ref( 38 ) = 723 ;   Multif In 1 Delay
Ext_User_Prm_Data_Ref( 39 ) = 724 ;   Multif In 2 Delay
Ext_User_Prm_Data_Ref( 40 ) = 725 ;   Control Function
Ext_User_Prm_Data_Ref( 41 ) = 726 ;   Busfault Reaction
Ext_User_Prm_Data_Ref( 42 ) = 727 ;   Aux Inp 1 Reaction
Ext_User_Prm_Data_Ref( 42 ) = 728 ;   Aux Inp 2 Reaction
Ext_User_Prm_Data_Ref( 43 ) = 729 ;   Aux Inp 3 Reaction
Ext_User_Prm_Data_Ref( 43 ) = 730 ;   Aux Inp 4 Reaction
Ext_User_Prm_Data_Ref( 44 ) = 731 ;   Aux Inp 5 Reaction
Ext_User_Prm_Data_Ref( 44 ) = 732 ;   Aux Inp 6 Reaction
Ext_User_Prm_Data_Ref( 45 ) = 733 ;   PTC, Thermistor
Ext_User_Prm_Data_Ref( 45 ) = 734 ;   Check-Back
Ext_User_Prm_Data_Ref( 45 ) = 735 ;   Check Phase Sequence
Ext_User_Prm_Data_Ref( 46 ) = 736 ;   Fault Auto Reset
Ext_User_Prm_Data_Ref( 46 ) = 737 ;   Emergency Start
Ext_User_Prm_Data_Ref( 46 ) = 738 ;   Earth Flt Detection
Ext_User_Prm_Data_Ref( 46 ) = 739 ;   Address Check
Ext_User_Prm_Data_Ref( 46 ) = 740 ;   Enable Custom Logic
Ext_User_Prm_Data_Ref( 46 ) = 741 ;   YD Change-Over Mode
Ext_User_Prm_Data_Ref( 46 ) = 742 ;   Phase Loss Prot.
Ext_User_Prm_Data_Ref( 47 ) = 743 ;   DX1xx Enabled
Ext_User_Prm_Data_Ref( 47 ) = 744 ;   VI15x Enabled
Ext_User_Prm_Data_Ref( 47 ) = 745 ;   Missing Module React.
Ext_User_Prm_Data_Ref( 48 ) = 746 ;   Aux Inp 1 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 747 ;   Aux Inp 2 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 748 ;   Aux Inp 3 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 749 ;   Aux Inp 4 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 750 ;   Aux Inp 5 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 751 ;   Aux Inp 6 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 752 ;   Cooling Mode
Ext_User_Prm_Data_Ref( 49 ) = 753 ;   Invert DI Start Inp.
Ext_User_Prm_Data_Ref( 49 ) = 754 ;   Invert DI Stop Inp.
Ext_User_Prm_Data_Ref( 49 ) = 755 ;   Inching DI Start Inp
Ext_User_Prm_Data_Ref( 50 ) = 756 ;   Loc 1 Start Bus Cyc
Ext_User_Prm_Data_Ref( 50 ) = 757 ;   Loc 1 Stop Bus Cyc
Ext_User_Prm_Data_Ref( 50 ) = 758 ;   Loc 1 Start DI
Ext_User_Prm_Data_Ref( 50 ) = 759 ;   Loc 1 Stop DI
Ext_User_Prm_Data_Ref( 50 ) = 760 ;   Loc 1 Start LCD
Ext_User_Prm_Data_Ref( 50 ) = 761 ;   Loc 1 Stop LCD
Ext_User_Prm_Data_Ref( 50 ) = 762 ;   Loc 1 Start Bus Acyc
Ext_User_Prm_Data_Ref( 50 ) = 763 ;   Loc 1 Stop Bus Acyc
Ext_User_Prm_Data_Ref( 51 ) = 764 ;   Auto Start Bus Cyc
Ext_User_Prm_Data_Ref( 51 ) = 765 ;   Auto Stop Bus Cyc
Ext_User_Prm_Data_Ref( 51 ) = 766 ;   Auto Start DI
Ext_User_Prm_Data_Ref( 51 ) = 767 ;   Auto Stop DI
Ext_User_Prm_Data_Ref( 51 ) = 768 ;   Auto Start LCD
Ext_User_Prm_Data_Ref( 51 ) = 769 ;   Auto Stop LCD
Ext_User_Prm_Data_Ref( 51 ) = 770 ;   Auto Start Bus Acyc
Ext_User_Prm_Data_Ref( 51 ) = 771 ;   Auto Stop Bus Acyc
Ext_User_Prm_Data_Ref( 52 ) = 772 ;   Loc 2 Start Bus Cyc
Ext_User_Prm_Data_Ref( 52 ) = 773 ;   Loc 2 Stop Bus Cyc
Ext_User_Prm_Data_Ref( 52 ) = 774 ;   Loc 2 Start DI
Ext_User_Prm_Data_Ref( 52 ) = 775 ;   Loc 2 Stop DI
Ext_User_Prm_Data_Ref( 52 ) = 776 ;   Loc 2 Start LCD
Ext_User_Prm_Data_Ref( 52 ) = 777 ;   Loc 2 Stop LCD
Ext_User_Prm_Data_Ref( 52 ) = 778 ;   Loc 2 Start Bus Acyc
Ext_User_Prm_Data_Ref( 52 ) = 779 ;   Loc 2 Stop Bus Acyc
Ext_User_Prm_Data_Ref( 53 ) = 780 ;   Multif In 0 Autoreset
Ext_User_Prm_Data_Ref( 53 ) = 781 ;   Multif In 1 Autoreset
Ext_User_Prm_Data_Ref( 53 ) = 782 ;   Multif In 2 Autoreset
EndModule

;=============================================================
; Module description  UMC100_FBP (R0101 R0201) Profil 2
;=============================================================
;
Module="UMC100-FBP (R0101 R0201)Profil2" 0x11, 0x21, 0x50      ; 16DI, 16DO, 1AI, I/O-Data-Profil 2
19
Ext_Module_Prm_Data_Len=55                     ; number of used data byte
Ext_User_Prm_Data_Const(0) =    \                 ; initialising of param data
    0x2B, 0xC0, 0x02, 0x02, 0x02, 0x00, 0x30, \ ; ProductCode,BI,BO,AI,AO,Par
    0x00, 0x00, 0x00, 0x32, 0x00, 0x00, 0x00, 0x32, 0x02, 0x58,  \
    0x00, 0x64, 0x00, 0x78, 0xFF, 0x05, 0x00, 0x01, 0x00, 0x01,  \
    0x0A, 0x00, 0x1E, 0xA0, 0xA0, 0x05, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x03, 0x00, 0x00, 0x00, 0x00, 0x08, 0x64,  \
    0x00, 0x00, 0x02, 0xBE, 0xEB, 0xBE, 0x00, 0x00
Ext_User_Prm_Data_Ref( 7 ) = 701 ;   Setting Ie 1
Ext_User_Prm_Data_Ref( 11 ) = 702 ;   Setting Ie 2
Ext_User_Prm_Data_Ref( 15 ) = 703 ;   YD Starting Time
Ext_User_Prm_Data_Ref( 17 ) = 704 ;   Current Factor
Ext_User_Prm_Data_Ref( 19 ) = 705 ;   Cooling Time
Ext_User_Prm_Data_Ref( 21 ) = 706 ;   Earth Flt Trip Level
Ext_User_Prm_Data_Ref( 22 ) = 707 ;   Earth Flt Trip Delay
Ext_User_Prm_Data_Ref( 23 ) = 708 ;   Language
Ext_User_Prm_Data_Ref( 24 ) = 709 ;   Rev Lock-Out Time
Ext_User_Prm_Data_Ref( 25 ) = 710 ;   Fault Output
Ext_User_Prm_Data_Ref( 26 ) = 711 ;   Trip Class
Ext_User_Prm_Data_Ref( 27 ) = 712 ;   Low Curr Warn Level
Ext_User_Prm_Data_Ref( 28 ) = 713 ;   Low Curr Trip Level
Ext_User_Prm_Data_Ref( 29 ) = 714 ;   High Curr Warn Level
Ext_User_Prm_Data_Ref( 30 ) = 715 ;   High Curr Trip Level
Ext_User_Prm_Data_Ref( 31 ) = 716 ;   Locked Rotor Level
Ext_User_Prm_Data_Ref( 32 ) = 717 ;   Locked Rotor Delay
Ext_User_Prm_Data_Ref( 33 ) = 718 ;   Custom App Parameter
Ext_User_Prm_Data_Ref( 34 ) = 719 ;   Multif In 0
Ext_User_Prm_Data_Ref( 35 ) = 720 ;   Multif In 1
Ext_User_Prm_Data_Ref( 36 ) = 721 ;   Multif In 2
Ext_User_Prm_Data_Ref( 37 ) = 722 ;   Multif In 0 Delay
Ext_User_Prm_Data_Ref( 38 ) = 723 ;   Multif In 1 Delay
Ext_User_Prm_Data_Ref( 39 ) = 724 ;   Multif In 2 Delay
Ext_User_Prm_Data_Ref( 40 ) = 725 ;   Control Function
Ext_User_Prm_Data_Ref( 41 ) = 726 ;   Busfault Reaction
Ext_User_Prm_Data_Ref( 42 ) = 727 ;   Aux Inp 1 Reaction
Ext_User_Prm_Data_Ref( 42 ) = 728 ;   Aux Inp 2 Reaction
Ext_User_Prm_Data_Ref( 43 ) = 729 ;   Aux Inp 3 Reaction
Ext_User_Prm_Data_Ref( 43 ) = 730 ;   Aux Inp 4 Reaction
Ext_User_Prm_Data_Ref( 44 ) = 731 ;   Aux Inp 5 Reaction
Ext_User_Prm_Data_Ref( 44 ) = 732 ;   Aux Inp 6 Reaction
Ext_User_Prm_Data_Ref( 45 ) = 733 ;   PTC, Thermistor
Ext_User_Prm_Data_Ref( 45 ) = 734 ;   Check-Back
Ext_User_Prm_Data_Ref( 45 ) = 735 ;   Check Phase Sequence
Ext_User_Prm_Data_Ref( 46 ) = 736 ;   Fault Auto Reset
Ext_User_Prm_Data_Ref( 46 ) = 737 ;   Emergency Start
Ext_User_Prm_Data_Ref( 46 ) = 738 ;   Earth Flt Detection
Ext_User_Prm_Data_Ref( 46 ) = 739 ;   Address Check
Ext_User_Prm_Data_Ref( 46 ) = 740 ;   Enable Custom Logic
Ext_User_Prm_Data_Ref( 46 ) = 741 ;   YD Change-Over Mode
Ext_User_Prm_Data_Ref( 46 ) = 742 ;   Phase Loss Prot.
Ext_User_Prm_Data_Ref( 47 ) = 743 ;   DX1xx Enabled
Ext_User_Prm_Data_Ref( 47 ) = 744 ;   VI15x Enabled
Ext_User_Prm_Data_Ref( 47 ) = 745 ;   Missing Module React.
Ext_User_Prm_Data_Ref( 48 ) = 746 ;   Aux Inp 1 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 747 ;   Aux Inp 2 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 748 ;   Aux Inp 3 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 749 ;   Aux Inp 4 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 750 ;   Aux Inp 5 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 751 ;   Aux Inp 6 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 752 ;   Cooling Mode
Ext_User_Prm_Data_Ref( 49 ) = 753 ;   Invert DI Start Inp.
Ext_User_Prm_Data_Ref( 49 ) = 754 ;   Invert DI Stop Inp.
Ext_User_Prm_Data_Ref( 49 ) = 755 ;   Inching DI Start Inp
Ext_User_Prm_Data_Ref( 50 ) = 756 ;   Loc 1 Start Bus Cyc
Ext_User_Prm_Data_Ref( 50 ) = 757 ;   Loc 1 Stop Bus Cyc
Ext_User_Prm_Data_Ref( 50 ) = 758 ;   Loc 1 Start DI
Ext_User_Prm_Data_Ref( 50 ) = 759 ;   Loc 1 Stop DI
Ext_User_Prm_Data_Ref( 50 ) = 760 ;   Loc 1 Start LCD
Ext_User_Prm_Data_Ref( 50 ) = 761 ;   Loc 1 Stop LCD
Ext_User_Prm_Data_Ref( 50 ) = 762 ;   Loc 1 Start Bus Acyc
Ext_User_Prm_Data_Ref( 50 ) = 763 ;   Loc 1 Stop Bus Acyc
Ext_User_Prm_Data_Ref( 51 ) = 764 ;   Auto Start Bus Cyc
Ext_User_Prm_Data_Ref( 51 ) = 765 ;   Auto Stop Bus Cyc
Ext_User_Prm_Data_Ref( 51 ) = 766 ;   Auto Start DI
Ext_User_Prm_Data_Ref( 51 ) = 767 ;   Auto Stop DI
Ext_User_Prm_Data_Ref( 51 ) = 768 ;   Auto Start LCD
Ext_User_Prm_Data_Ref( 51 ) = 769 ;   Auto Stop LCD
Ext_User_Prm_Data_Ref( 51 ) = 770 ;   Auto Start Bus Acyc
Ext_User_Prm_Data_Ref( 51 ) = 771 ;   Auto Stop Bus Acyc
Ext_User_Prm_Data_Ref( 52 ) = 772 ;   Loc 2 Start Bus Cyc
Ext_User_Prm_Data_Ref( 52 ) = 773 ;   Loc 2 Stop Bus Cyc
Ext_User_Prm_Data_Ref( 52 ) = 774 ;   Loc 2 Start DI
Ext_User_Prm_Data_Ref( 52 ) = 775 ;   Loc 2 Stop DI
Ext_User_Prm_Data_Ref( 52 ) = 776 ;   Loc 2 Start LCD
Ext_User_Prm_Data_Ref( 52 ) = 777 ;   Loc 2 Stop LCD
Ext_User_Prm_Data_Ref( 52 ) = 778 ;   Loc 2 Start Bus Acyc
Ext_User_Prm_Data_Ref( 52 ) = 779 ;   Loc 2 Stop Bus Acyc
Ext_User_Prm_Data_Ref( 53 ) = 780 ;   Multif In 0 Autoreset
Ext_User_Prm_Data_Ref( 53 ) = 781 ;   Multif In 1 Autoreset
Ext_User_Prm_Data_Ref( 53 ) = 782 ;   Multif In 2 Autoreset
EndModule

;=============================================================
; Module description  UMC100.3 (Rx100 Rx200)
;=============================================================
;
Module="UMC100.3 (Rx100 Rx200)"0x11, 0x23, 0x56, 0x63      ; 16DI, 32DO, 7AI, 4AO
20
Ext_Module_Prm_Data_Len=55                     ; number of used data byte
Ext_User_Prm_Data_Const(0) =    \                 ; initialising of param data
    0x2B, 0xC1, 0x02, 0x04, 0x0E, 0x08, 0x30, \ ; ProductCode,BI,BO,AI,AO,Par
    0x00, 0x00, 0x00, 0x32, 0x00, 0x00, 0x00, 0x32, 0x02, 0x58,  \
    0x00, 0x64, 0x00, 0x78, 0xFF, 0x05, 0x00, 0x01, 0x00, 0x01,  \
    0x0A, 0x00, 0x1E, 0xA0, 0xA0, 0x05, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x03, 0x00, 0x00, 0x00, 0x00, 0x08, 0x64,  \
    0x00, 0x00, 0x02, 0xBE, 0xEB, 0xBE, 0x00, 0x00
Ext_User_Prm_Data_Ref( 7 ) = 801 ;   Setting Ie 1
Ext_User_Prm_Data_Ref( 11 ) = 802 ;   Setting Ie 2
Ext_User_Prm_Data_Ref( 15 ) = 803 ;   YD Starting Time
Ext_User_Prm_Data_Ref( 17 ) = 804 ;   Current Factor
Ext_User_Prm_Data_Ref( 19 ) = 805 ;   Cooling Time
Ext_User_Prm_Data_Ref( 21 ) = 806 ;   Earth Flt Trip Level
Ext_User_Prm_Data_Ref( 22 ) = 807 ;   Earth Flt Trip Delay
Ext_User_Prm_Data_Ref( 23 ) = 808 ;   Language
Ext_User_Prm_Data_Ref( 24 ) = 809 ;   Rev Lock-Out Time
Ext_User_Prm_Data_Ref( 25 ) = 810 ;   Fault Output
Ext_User_Prm_Data_Ref( 26 ) = 811 ;   Trip Class
Ext_User_Prm_Data_Ref( 27 ) = 812 ;   Low Curr Warn Level
Ext_User_Prm_Data_Ref( 28 ) = 813 ;   Low Curr Trip Level
Ext_User_Prm_Data_Ref( 29 ) = 814 ;   High Curr Warn Level
Ext_User_Prm_Data_Ref( 30 ) = 815 ;   High Curr Trip Level
Ext_User_Prm_Data_Ref( 31 ) = 816 ;   Locked Rotor Level
Ext_User_Prm_Data_Ref( 32 ) = 817 ;   Locked Rotor Delay
Ext_User_Prm_Data_Ref( 33 ) = 818 ;   Custom App Parameter
Ext_User_Prm_Data_Ref( 34 ) = 819 ;   Multif In 0
Ext_User_Prm_Data_Ref( 35 ) = 820 ;   Multif In 1
Ext_User_Prm_Data_Ref( 36 ) = 821 ;   Multif In 2
Ext_User_Prm_Data_Ref( 37 ) = 822 ;   Multif In 0 Delay
Ext_User_Prm_Data_Ref( 38 ) = 823 ;   Multif In 1 Delay
Ext_User_Prm_Data_Ref( 39 ) = 824 ;   Multif In 2 Delay
Ext_User_Prm_Data_Ref( 40 ) = 825 ;   Control Function
Ext_User_Prm_Data_Ref( 41 ) = 826 ;   Busfault Reaction
Ext_User_Prm_Data_Ref( 42 ) = 827 ;   Aux Inp 1 Reaction
Ext_User_Prm_Data_Ref( 42 ) = 828 ;   Aux Inp 2 Reaction
Ext_User_Prm_Data_Ref( 43 ) = 829 ;   Aux Inp 3 Reaction
Ext_User_Prm_Data_Ref( 43 ) = 830 ;   Aux Inp 4 Reaction
Ext_User_Prm_Data_Ref( 44 ) = 831 ;   Aux Inp 5 Reaction
Ext_User_Prm_Data_Ref( 44 ) = 832 ;   Aux Inp 6 Reaction
Ext_User_Prm_Data_Ref( 45 ) = 833 ;   PTC, Thermistor
Ext_User_Prm_Data_Ref( 45 ) = 834 ;   Check-Back
Ext_User_Prm_Data_Ref( 45 ) = 835 ;   Check Phase Sequence
Ext_User_Prm_Data_Ref( 46 ) = 836 ;   Fault Auto Reset
Ext_User_Prm_Data_Ref( 46 ) = 837 ;   Emergency Start
Ext_User_Prm_Data_Ref( 46 ) = 838 ;   Earth Flt Detection
Ext_User_Prm_Data_Ref( 46 ) = 839 ;   Address Check
Ext_User_Prm_Data_Ref( 46 ) = 840 ;   Enable Custom Logic
Ext_User_Prm_Data_Ref( 46 ) = 841 ;   YD Change-Over Mode
Ext_User_Prm_Data_Ref( 46 ) = 842 ;   Phase Loss Prot.
Ext_User_Prm_Data_Ref( 46 ) = 843 ;   Resistive Load
Ext_User_Prm_Data_Ref( 47 ) = 844 ;   DX1xx Enabled
Ext_User_Prm_Data_Ref( 47 ) = 845 ;   AI1xx AM1 Enabled
Ext_User_Prm_Data_Ref( 47 ) = 846 ;   AI1xx AM2 Enabled
Ext_User_Prm_Data_Ref( 47 ) = 847 ;   VI15x Enabled
Ext_User_Prm_Data_Ref( 47 ) = 848 ;   Missing Module React.
Ext_User_Prm_Data_Ref( 48 ) = 849 ;   Aux Inp 1 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 850 ;   Aux Inp 2 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 851 ;   Aux Inp 3 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 852 ;   Aux Inp 4 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 853 ;   Aux Inp 5 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 854 ;   Aux Inp 6 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 855 ;   Number Of Phases
Ext_User_Prm_Data_Ref( 48 ) = 856 ;   Cooling Mode
Ext_User_Prm_Data_Ref( 49 ) = 857 ;   Invert DI Start Inp.
Ext_User_Prm_Data_Ref( 49 ) = 858 ;   Invert DI Stop Inp.
Ext_User_Prm_Data_Ref( 49 ) = 859 ;   Inching DI Start Inp
Ext_User_Prm_Data_Ref( 50 ) = 860 ;   Loc 1 Start Bus Cyc
Ext_User_Prm_Data_Ref( 50 ) = 861 ;   Loc 1 Stop Bus Cyc
Ext_User_Prm_Data_Ref( 50 ) = 862 ;   Loc 1 Start DI
Ext_User_Prm_Data_Ref( 50 ) = 863 ;   Loc 1 Stop DI
Ext_User_Prm_Data_Ref( 50 ) = 864 ;   Loc 1 Start LCD
Ext_User_Prm_Data_Ref( 50 ) = 865 ;   Loc 1 Stop LCD
Ext_User_Prm_Data_Ref( 50 ) = 866 ;   Loc 1 Start Bus Acyc
Ext_User_Prm_Data_Ref( 50 ) = 867 ;   Loc 1 Stop Bus Acyc
Ext_User_Prm_Data_Ref( 51 ) = 868 ;   Auto Start Bus Cyc
Ext_User_Prm_Data_Ref( 51 ) = 869 ;   Auto Stop Bus Cyc
Ext_User_Prm_Data_Ref( 51 ) = 870 ;   Auto Start DI
Ext_User_Prm_Data_Ref( 51 ) = 871 ;   Auto Stop DI
Ext_User_Prm_Data_Ref( 51 ) = 872 ;   Auto Start LCD
Ext_User_Prm_Data_Ref( 51 ) = 873 ;   Auto Stop LCD
Ext_User_Prm_Data_Ref( 51 ) = 874 ;   Auto Start Bus Acyc
Ext_User_Prm_Data_Ref( 51 ) = 875 ;   Auto Stop Bus Acyc
Ext_User_Prm_Data_Ref( 52 ) = 876 ;   Loc 2 Start Bus Cyc
Ext_User_Prm_Data_Ref( 52 ) = 877 ;   Loc 2 Stop Bus Cyc
Ext_User_Prm_Data_Ref( 52 ) = 878 ;   Loc 2 Start DI
Ext_User_Prm_Data_Ref( 52 ) = 879 ;   Loc 2 Stop DI
Ext_User_Prm_Data_Ref( 52 ) = 880 ;   Loc 2 Start LCD
Ext_User_Prm_Data_Ref( 52 ) = 881 ;   Loc 2 Stop LCD
Ext_User_Prm_Data_Ref( 52 ) = 882 ;   Loc 2 Start Bus Acyc
Ext_User_Prm_Data_Ref( 52 ) = 883 ;   Loc 2 Stop Bus Acyc
Ext_User_Prm_Data_Ref( 53 ) = 884 ;   Multif In 0 Autoreset
Ext_User_Prm_Data_Ref( 53 ) = 885 ;   Multif In 1 Autoreset
Ext_User_Prm_Data_Ref( 53 ) = 886 ;   Multif In 2 Autoreset
EndModule

;=============================================================
; Module description  UMC100.3 (Rx100 Rx200) Profil 2
;=============================================================
;
Module="UMC100.3 (Rx100 Rx200)Profil2"0x11, 0x21, 0x50      ; 16DI, 16DO, 1AI
21
Ext_Module_Prm_Data_Len=55                     ; number of used data byte
Ext_User_Prm_Data_Const(0) =    \                 ; initialising of param data
    0x2B, 0xC1, 0x02, 0x02, 0x02, 0x00, 0x30, \ ; ProductCode,BI,BO,AI,AO,Par
    0x00, 0x00, 0x00, 0x32, 0x00, 0x00, 0x00, 0x32, 0x02, 0x58,  \
    0x00, 0x64, 0x00, 0x78, 0xFF, 0x05, 0x00, 0x01, 0x00, 0x01,  \
    0x0A, 0x00, 0x1E, 0xA0, 0xA0, 0x05, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x03, 0x00, 0x00, 0x00, 0x00, 0x08, 0x64,  \
    0x00, 0x00, 0x02, 0xBE, 0xEB, 0xBE, 0x00, 0x00
Ext_User_Prm_Data_Ref( 7 ) = 801 ;   Setting Ie 1
Ext_User_Prm_Data_Ref( 11 ) = 802 ;   Setting Ie 2
Ext_User_Prm_Data_Ref( 15 ) = 803 ;   YD Starting Time
Ext_User_Prm_Data_Ref( 17 ) = 804 ;   Current Factor
Ext_User_Prm_Data_Ref( 19 ) = 805 ;   Cooling Time
Ext_User_Prm_Data_Ref( 21 ) = 806 ;   Earth Flt Trip Level
Ext_User_Prm_Data_Ref( 22 ) = 807 ;   Earth Flt Trip Delay
Ext_User_Prm_Data_Ref( 23 ) = 808 ;   Language
Ext_User_Prm_Data_Ref( 24 ) = 809 ;   Rev Lock-Out Time
Ext_User_Prm_Data_Ref( 25 ) = 810 ;   Fault Output
Ext_User_Prm_Data_Ref( 26 ) = 811 ;   Trip Class
Ext_User_Prm_Data_Ref( 27 ) = 812 ;   Low Curr Warn Level
Ext_User_Prm_Data_Ref( 28 ) = 813 ;   Low Curr Trip Level
Ext_User_Prm_Data_Ref( 29 ) = 814 ;   High Curr Warn Level
Ext_User_Prm_Data_Ref( 30 ) = 815 ;   High Curr Trip Level
Ext_User_Prm_Data_Ref( 31 ) = 816 ;   Locked Rotor Level
Ext_User_Prm_Data_Ref( 32 ) = 817 ;   Locked Rotor Delay
Ext_User_Prm_Data_Ref( 33 ) = 818 ;   Custom App Parameter
Ext_User_Prm_Data_Ref( 34 ) = 819 ;   Multif In 0
Ext_User_Prm_Data_Ref( 35 ) = 820 ;   Multif In 1
Ext_User_Prm_Data_Ref( 36 ) = 821 ;   Multif In 2
Ext_User_Prm_Data_Ref( 37 ) = 822 ;   Multif In 0 Delay
Ext_User_Prm_Data_Ref( 38 ) = 823 ;   Multif In 1 Delay
Ext_User_Prm_Data_Ref( 39 ) = 824 ;   Multif In 2 Delay
Ext_User_Prm_Data_Ref( 40 ) = 825 ;   Control Function
Ext_User_Prm_Data_Ref( 41 ) = 826 ;   Busfault Reaction
Ext_User_Prm_Data_Ref( 42 ) = 827 ;   Aux Inp 1 Reaction
Ext_User_Prm_Data_Ref( 42 ) = 828 ;   Aux Inp 2 Reaction
Ext_User_Prm_Data_Ref( 43 ) = 829 ;   Aux Inp 3 Reaction
Ext_User_Prm_Data_Ref( 43 ) = 830 ;   Aux Inp 4 Reaction
Ext_User_Prm_Data_Ref( 44 ) = 831 ;   Aux Inp 5 Reaction
Ext_User_Prm_Data_Ref( 44 ) = 832 ;   Aux Inp 6 Reaction
Ext_User_Prm_Data_Ref( 45 ) = 833 ;   PTC, Thermistor
Ext_User_Prm_Data_Ref( 45 ) = 834 ;   Check-Back
Ext_User_Prm_Data_Ref( 45 ) = 835 ;   Check Phase Sequence
Ext_User_Prm_Data_Ref( 46 ) = 836 ;   Fault Auto Reset
Ext_User_Prm_Data_Ref( 46 ) = 837 ;   Emergency Start
Ext_User_Prm_Data_Ref( 46 ) = 838 ;   Earth Flt Detection
Ext_User_Prm_Data_Ref( 46 ) = 839 ;   Address Check
Ext_User_Prm_Data_Ref( 46 ) = 840 ;   Enable Custom Logic
Ext_User_Prm_Data_Ref( 46 ) = 841 ;   YD Change-Over Mode
Ext_User_Prm_Data_Ref( 46 ) = 842 ;   Phase Loss Prot.
Ext_User_Prm_Data_Ref( 46 ) = 843 ;   Resistive Load
Ext_User_Prm_Data_Ref( 47 ) = 844 ;   DX1xx Enabled
Ext_User_Prm_Data_Ref( 47 ) = 845 ;   AI1xx AM1 Enabled
Ext_User_Prm_Data_Ref( 47 ) = 846 ;   AI1xx AM2 Enabled
Ext_User_Prm_Data_Ref( 47 ) = 847 ;   VI15x Enabled
Ext_User_Prm_Data_Ref( 47 ) = 848 ;   Missing Module React.
Ext_User_Prm_Data_Ref( 48 ) = 849 ;   Aux Inp 1 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 850 ;   Aux Inp 2 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 851 ;   Aux Inp 3 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 852 ;   Aux Inp 4 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 853 ;   Aux Inp 5 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 854 ;   Aux Inp 6 Ack Mode
Ext_User_Prm_Data_Ref( 48 ) = 855 ;   Number Of Phases
Ext_User_Prm_Data_Ref( 48 ) = 856 ;   Cooling Mode
Ext_User_Prm_Data_Ref( 49 ) = 857 ;   Invert DI Start Inp.
Ext_User_Prm_Data_Ref( 49 ) = 858 ;   Invert DI Stop Inp.
Ext_User_Prm_Data_Ref( 49 ) = 859 ;   Inching DI Start Inp
Ext_User_Prm_Data_Ref( 50 ) = 860 ;   Loc 1 Start Bus Cyc
Ext_User_Prm_Data_Ref( 50 ) = 861 ;   Loc 1 Stop Bus Cyc
Ext_User_Prm_Data_Ref( 50 ) = 862 ;   Loc 1 Start DI
Ext_User_Prm_Data_Ref( 50 ) = 863 ;   Loc 1 Stop DI
Ext_User_Prm_Data_Ref( 50 ) = 864 ;   Loc 1 Start LCD
Ext_User_Prm_Data_Ref( 50 ) = 865 ;   Loc 1 Stop LCD
Ext_User_Prm_Data_Ref( 50 ) = 866 ;   Loc 1 Start Bus Acyc
Ext_User_Prm_Data_Ref( 50 ) = 867 ;   Loc 1 Stop Bus Acyc
Ext_User_Prm_Data_Ref( 51 ) = 868 ;   Auto Start Bus Cyc
Ext_User_Prm_Data_Ref( 51 ) = 869 ;   Auto Stop Bus Cyc
Ext_User_Prm_Data_Ref( 51 ) = 870 ;   Auto Start DI
Ext_User_Prm_Data_Ref( 51 ) = 871 ;   Auto Stop DI
Ext_User_Prm_Data_Ref( 51 ) = 872 ;   Auto Start LCD
Ext_User_Prm_Data_Ref( 51 ) = 873 ;   Auto Stop LCD
Ext_User_Prm_Data_Ref( 51 ) = 874 ;   Auto Start Bus Acyc
Ext_User_Prm_Data_Ref( 51 ) = 875 ;   Auto Stop Bus Acyc
Ext_User_Prm_Data_Ref( 52 ) = 876 ;   Loc 2 Start Bus Cyc
Ext_User_Prm_Data_Ref( 52 ) = 877 ;   Loc 2 Stop Bus Cyc
Ext_User_Prm_Data_Ref( 52 ) = 878 ;   Loc 2 Start DI
Ext_User_Prm_Data_Ref( 52 ) = 879 ;   Loc 2 Stop DI
Ext_User_Prm_Data_Ref( 52 ) = 880 ;   Loc 2 Start LCD
Ext_User_Prm_Data_Ref( 52 ) = 881 ;   Loc 2 Stop LCD
Ext_User_Prm_Data_Ref( 52 ) = 882 ;   Loc 2 Start Bus Acyc
Ext_User_Prm_Data_Ref( 52 ) = 883 ;   Loc 2 Stop Bus Acyc
Ext_User_Prm_Data_Ref( 53 ) = 884 ;   Multif In 0 Autoreset
Ext_User_Prm_Data_Ref( 53 ) = 885 ;   Multif In 1 Autoreset
Ext_User_Prm_Data_Ref( 53 ) = 886 ;   Multif In 2 Autoreset
EndModule



;=============================================
; Other Definitions:
;=============================================
; DPV1 Alarm
DPV1_Slave                          = 1
C1_Read_Write_supp                  = 1
C1_Max_Data_Len                     = 68         ;The parameter specifies the maximum length of user data excluding
                                                ;Function_Num, Slot_number, Index, Length, transferred on the
                                                ;MSAC_1 communication channel.
                                                ;Type: Unsigned8 (0 .. 240)
C1_Response_Timeout                 = 300
Diagnostic_Alarm_supp               = 0
Process_Alarm_supp                  = 0
Pull_Plug_Alarm_supp                = 0
Status_Alarm_supp                   = 0
Update_Alarm_supp                   = 0
Manufacturer_Specific_Alarm_supp    = 0
Alarm_Sequence_Mode_Count           = 0
Alarm_Type_Mode_supp                = 0
Diagnostic_Alarm_required           = 0

C2_Read_Write_supp                  = 1
C2_Max_Data_Len                     = 68        ;The parameter specifies the maximum length of user data excluding
                                                ;Function_Num, Slot_number, Index, Length, transferred on the
                                                ;MSAC_2 communication channel.
                                                ;Type: Unsigned8 (0,48 .. 240)
C2_Response_Timeout                 = 300
C2_Read_Write_required              = 1
C2_Max_Count_Channels               = 3
Max_Initiate_PDU_Length             = 52        ;The parameter specifies the maximum length of an Initiate Request
                                                ;PDU including the Function_Num to the Resource Manager.
                                                ;Type: Unsigned8 (0,52.. 244)
DPV1_Data_Types                     = 0				;
Ident_Maintenance_supp		= 1			;supports I&M functions





















































