;======================================================
;======================================================
#Profibus_DP
; HIGHEST Module_Index currently in use: 5  (starting at 4)
;
; File Version: 3.01
;    Language "suomi" added, date 13.01.2016
;
; File Version: 3.00
; dedicated for use with ePlug DPV1 (PDP32):
;    Rx100 Rx200 of UMC100.3 created by GSD-Generator, Date 27.05.2014 10:09:29 
;    Rx100 Rx200 of UMC100.3 with I/O-Data-Profil2
;
;
;=============================================================
; Text-definition for User Prm Data  UMC100.3 (Rx100 Rx200)
;=============================================================
;
ExtUserPrmData =  401  "Setting Ie 1 [0.01A]"
Unsigned32 50 24-320000
EndExtUserPrmData

ExtUserPrmData =  402  "Setting Ie 2 [0.01A]"
Unsigned32 50 24-320000
EndExtUserPrmData

ExtUserPrmData =  403  "YD Starting Time [0.1s]"
Unsigned16 600 10-36000
EndExtUserPrmData

ExtUserPrmData =  404  "Current Factor [%]"
Unsigned16 100 2-64000
EndExtUserPrmData

ExtUserPrmData =  405  "Cooling Time [s]"
Unsigned16 120 30-64000
EndExtUserPrmData

ExtUserPrmData =  406  "Earth Flt Trip Level [%]"
Unsigned8 255 20-255
EndExtUserPrmData

ExtUserPrmData =  407  "Earth Flt Trip Delay [0.1s]"
Unsigned8 5 0-255
EndExtUserPrmData

PrmText = 408 
Text(0) = "English"
Text(1) = "Deutsch"
Text(2) = "Francais"
Text(3) = "Espanol"
Text(4) = "Italiano"
Text(5) = "Portugues"
Text(6) = "Russian"
Text(7) = "Polski"
Text(8) = "Suomi"
EndPrmText
ExtUserPrmData =  408  "Language"
Unsigned8 0 0-8
Prm_Text_Ref = 408 
EndExtUserPrmData

ExtUserPrmData =  409  "Rev Lock-Out Time [s]"
Unsigned8 1 1-255
EndExtUserPrmData

PrmText = 410 
Text(0) = "Off"
Text(1) = "Flash DO2"
Text(2) = "On DO2"
Text(3) = "Invert DO2"
Text(4) = "Flash DO3"
Text(5) = "On DO3"
Text(6) = "Invert DO3"
EndPrmText
ExtUserPrmData =  410  "Fault Output"
Unsigned8 0 0-6
Prm_Text_Ref = 410 
EndExtUserPrmData

PrmText = 411 
Text(0) = "Class 5"
Text(1) = "Class 10"
Text(2) = "Class 20"
Text(3) = "Class 30"
Text(4) = "Class 40"
EndPrmText
ExtUserPrmData =  411  "Trip Class"
Unsigned8 1 0-4
Prm_Text_Ref = 411 
EndExtUserPrmData

ExtUserPrmData =  412  "Low Curr Warn Level [5%]"
Unsigned8 10 0-20
EndExtUserPrmData

ExtUserPrmData =  413  "Low Curr Trip Level [5%]"
Unsigned8 0 0-20
EndExtUserPrmData

ExtUserPrmData =  414  "High Curr Warn Level [5%]"
Unsigned8 30 20-160
EndExtUserPrmData

ExtUserPrmData =  415  "High Curr Trip Level [5%]"
Unsigned8 160 20-160
EndExtUserPrmData

ExtUserPrmData =  416  "Locked Rotor Level [5%]"
Unsigned8 160 20-160
EndExtUserPrmData

ExtUserPrmData =  417  "Locked Rotor Delay [0.1s]"
Unsigned8 5 0-255
EndExtUserPrmData

ExtUserPrmData =  418  "Custom App Parameter"
Unsigned8 0 0-255
EndExtUserPrmData

PrmText = 419 
Text(0) = "Off"
Text(1) = "Stop (NC)"
Text(2) = "Stop (NO)"
Text(3) = "Ext. Flt (NC) always"
Text(4) = "Ext. Flt (NO) always"
Text(5) = "Ext. Flt (NC) Motor on"
Text(6) = "Ext. Flt (NO) Motor on"
Text(7) = "Prep. emerg. Start (NC)"
Text(8) = "Prep. emerg. Start (NO)"
Text(9) = "Testposition (NC)"
Text(10) = "Testposition (NO)"
Text(11) = "Force local (NC)"
Text(12) = "Force local (NO)"
Text(13) = "Fault reset (NC)"
Text(14) = "Fault reset (NO)"
Text(15) = "Voltage DIP (NC)"
Text(16) = "Voltage DIP (NO)"
Text(17) = "CEM11 always (Warning)"
Text(18) = "CEM11 after startup (Warning)"
Text(19) = "CEM11 always (Fault)"
Text(20) = "CEM11 after startup time (Fault)"
EndPrmText
ExtUserPrmData =  419  "Multif In 0"
Unsigned8 0 0-20
Prm_Text_Ref = 419 
EndExtUserPrmData

PrmText = 420 
Text(0) = "Off"
Text(1) = "Stop (NC)"
Text(2) = "Stop (NO)"
Text(3) = "Ext. Flt (NC) always"
Text(4) = "Ext. Flt (NO) always"
Text(5) = "Ext. Flt (NC) Motor on"
Text(6) = "Ext. Flt (NO) Motor on"
Text(7) = "Prep. emerg. Start (NC)"
Text(8) = "Prep. emerg. Start (NO)"
Text(9) = "Testposition (NC)"
Text(10) = "Testposition (NO)"
Text(11) = "Force local (NC)"
Text(12) = "Force local (NO)"
Text(13) = "Fault reset (NC)"
Text(14) = "Fault reset (NO)"
Text(15) = "Voltage DIP (NC)"
Text(16) = "Voltage DIP (NO)"
Text(17) = "CEM11 always (Warning)"
Text(18) = "CEM11 after startup (Warning)"
Text(19) = "CEM11 always (Fault)"
Text(20) = "CEM11 after startup time (Fault)"
EndPrmText
ExtUserPrmData =  420  "Multif In 1"
Unsigned8 0 0-20
Prm_Text_Ref = 420 
EndExtUserPrmData

PrmText = 421 
Text(0) = "Off"
Text(1) = "Stop (NC)"
Text(2) = "Stop (NO)"
Text(3) = "Ext. Flt (NC) always"
Text(4) = "Ext. Flt (NO) always"
Text(5) = "Ext. Flt (NC) Motor on"
Text(6) = "Ext. Flt (NO) Motor on"
Text(7) = "Prep. emerg. Start (NC)"
Text(8) = "Prep. emerg. Start (NO)"
Text(9) = "Testposition (NC)"
Text(10) = "Testposition (NO)"
Text(11) = "Force local (NC)"
Text(12) = "Force local (NO)"
Text(13) = "Fault reset (NC)"
Text(14) = "Fault reset (NO)"
Text(15) = "Voltage DIP (NC)"
Text(16) = "Voltage DIP (NO)"
Text(17) = "CEM11 always (Warning)"
Text(18) = "CEM11 after startup (Warning)"
Text(19) = "CEM11 always (Fault)"
Text(20) = "CEM11 after startup time (Fault)"
EndPrmText
ExtUserPrmData =  421  "Multif In 2"
Unsigned8 0 0-20
Prm_Text_Ref = 421 
EndExtUserPrmData

ExtUserPrmData =  422  "Multif In 0 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  423  "Multif In 1 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  424  "Multif In 2 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

PrmText = 425 
Text(1) = "Transparent"
Text(2) = "Overload Relay"
Text(3) = "Direct Starter"
Text(4) = "Reverse Starter"
Text(5) = "Star-delta Starter"
Text(7) = "Pole-Changing Starter"
Text(9) = "Actuator 1"
Text(10) = "Actuator 2"
Text(11) = "Actuator 3"
Text(12) = "Actuator 4"
Text(13) = "Softstarter"
EndPrmText
ExtUserPrmData =  425  "Control Function"
Unsigned8 3 1-13
Prm_Text_Ref = 425 
EndExtUserPrmData

PrmText = 426 
Text(0) = "Motor Off"
Text(1) = "Retain"
Text(2) = "Start Forward"
Text(3) = "Start Reverse"
EndPrmText
ExtUserPrmData =  426  "Busfault Reaction"
BitArea(0-3) 0 0-3
Prm_Text_Ref = 426 
EndExtUserPrmData                    

PrmText = 427 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  427  "Aux Inp 1 Reaction"
BitArea(0-3) 0 0-8
Prm_Text_Ref = 427 
EndExtUserPrmData

PrmText = 428 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  428  "Aux Inp 2 Reaction"
BitArea(4-7) 0 0-8
Prm_Text_Ref = 428 
EndExtUserPrmData

PrmText = 429 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  429  "Aux Inp 3 Reaction"
BitArea(0-3) 0 0-8
Prm_Text_Ref = 429 
EndExtUserPrmData

PrmText = 430 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  430  "Aux Inp 4 Reaction"
BitArea(4-7) 0 0-8
Prm_Text_Ref = 430 
EndExtUserPrmData

PrmText = 431 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  431  "Aux Inp 5 Reaction"
BitArea(0-3) 0 0-8
Prm_Text_Ref = 431 
EndExtUserPrmData

PrmText = 432 
Text(0) = "Disabled"
Text(1) = "Fault (NC) Motor in On/Off"
Text(2) = "Fault (NO) Motor in On/Off"
Text(3) = "Fault (NC) Motor in On"
Text(4) = "Fault (NO) Motor in On"
Text(5) = "Warning (NC) Motor in On/Off"
Text(6) = "Warning (NO) Motor in On/Off"
Text(7) = "Warning (NC) Motor in On"
Text(8) = "Warning (NO) Motor in On"
EndPrmText
ExtUserPrmData =  432  "Aux Inp 6 Reaction"
BitArea(4-7) 0 0-8
Prm_Text_Ref = 432 
EndExtUserPrmData

PrmText = 433 
Text(0) = "Disabled"
Text(1) = "Trip"
Text(2) = "Warning"
EndPrmText
ExtUserPrmData =  433  "PTC, Thermistor"
BitArea(0-1) 0 0-2
Prm_Text_Ref = 433 
EndExtUserPrmData

PrmText = 434 
Text(1) = "Contact DI0"
Text(2) = "Current"
Text(3) = "Simulation"
EndPrmText
ExtUserPrmData =  434  "Check-Back"
BitArea(2-3) 2 1-3
Prm_Text_Ref = 434 
EndExtUserPrmData

PrmText = 435 
Text(0) = "Disabled"
Text(1) = "Trip"
Text(2) = "Warning"
EndPrmText
ExtUserPrmData =  435  "Check Phase Sequence"
BitArea(4-5) 0 0-2
Prm_Text_Ref = 435 
EndExtUserPrmData

PrmText = 436 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  436  "Fault Auto Reset"
Bit(0) 0 0-1
Prm_Text_Ref = 436 
EndExtUserPrmData

PrmText = 437 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  437  "Emergency Start"
Bit(1) 0 0-1
Prm_Text_Ref = 437 
EndExtUserPrmData

PrmText = 438 
Text(0) = "Always"
Text(1) = "After Startup"
EndPrmText
ExtUserPrmData =  438  "Earth Flt Detection"
Bit(2) 1 0-1
Prm_Text_Ref = 438 
EndExtUserPrmData

PrmText = 439 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  439  "Address Check"
Bit(3) 0 0-1
Prm_Text_Ref = 439 
EndExtUserPrmData

PrmText = 440 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  440  "Enable Custom Logic"
Bit(4) 0 0-1
Prm_Text_Ref = 440 
EndExtUserPrmData

PrmText = 441 
Text(0) = "Time"
Text(1) = "Current"
EndPrmText
ExtUserPrmData =  441  "YD Change-Over Mode"
Bit(5) 1 0-1
Prm_Text_Ref = 441 
EndExtUserPrmData

PrmText = 442 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  442  "Phase Loss Prot."
Bit(6) 1 0-1
Prm_Text_Ref = 442 
EndExtUserPrmData

PrmText = 443 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  443  "Resistive Load"
Bit(7) 0 0-1
Prm_Text_Ref = 443 
EndExtUserPrmData

PrmText = 444 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  444  "DX1xx Enabled"
Bit(0) 0 0-1
Prm_Text_Ref = 444 
EndExtUserPrmData

PrmText = 445 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  445  "AI1xx AM1 Enabled"
Bit(1) 0 0-1
Prm_Text_Ref = 445 
EndExtUserPrmData

PrmText = 446 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  446  "AI1xx AM2 Enabled"
Bit(2) 0 0-1
Prm_Text_Ref = 446 
EndExtUserPrmData

PrmText = 447 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  447  "VI15x Enabled"
Bit(3) 0 0-1
Prm_Text_Ref = 447 
EndExtUserPrmData

PrmText = 448 
Text(0) = "Error"
Text(1) = "Warning"
EndPrmText
ExtUserPrmData =  448  "Missing Module React."
Bit(7) 0 0-1
Prm_Text_Ref = 448 
EndExtUserPrmData

PrmText = 449 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  449  "Aux Inp 1 Ack Mode"
Bit(0) 0 0-1
Prm_Text_Ref = 449 
EndExtUserPrmData

PrmText = 450 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  450  "Aux Inp 2 Ack Mode"
Bit(1) 0 0-1
Prm_Text_Ref = 450 
EndExtUserPrmData

PrmText = 451 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  451  "Aux Inp 3 Ack Mode"
Bit(2) 0 0-1
Prm_Text_Ref = 451 
EndExtUserPrmData

PrmText = 452 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  452  "Aux Inp 4 Ack Mode"
Bit(3) 0 0-1
Prm_Text_Ref = 452 
EndExtUserPrmData

PrmText = 453 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  453  "Aux Inp 5 Ack Mode"
Bit(4) 0 0-1
Prm_Text_Ref = 453 
EndExtUserPrmData

PrmText = 454 
Text(0) = "Manual Reset"
Text(1) = "Auto Reset"
EndPrmText
ExtUserPrmData =  454  "Aux Inp 6 Ack Mode"
Bit(5) 0 0-1
Prm_Text_Ref = 454 
EndExtUserPrmData

PrmText = 455 
Text(0) = "3 Phases"
Text(1) = "1 Phase"
EndPrmText
ExtUserPrmData =  455  "Number Of Phases"
Bit(6) 0 0-1
Prm_Text_Ref = 455 
EndExtUserPrmData

PrmText = 456 
Text(0) = "Time"
Text(1) = "x% Therm. Load"
EndPrmText
ExtUserPrmData =  456  "Cooling Mode"
Bit(7) 0 0-1
Prm_Text_Ref = 456 
EndExtUserPrmData

PrmText = 457 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  457  "Invert DI Start Inp."
Bit(0) 0 0-1
Prm_Text_Ref = 457 
EndExtUserPrmData

PrmText = 458 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  458  "Invert DI Stop Inp."
Bit(1) 1 0-1
Prm_Text_Ref = 458 
EndExtUserPrmData

PrmText = 459 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  459  "Inching DI Start Inp"
Bit(4) 0 0-1
Prm_Text_Ref = 459 
EndExtUserPrmData

PrmText = 460 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  460  "Loc 1 Start Bus Cyc"
Bit(0) 0 0-1
Prm_Text_Ref = 460 
EndExtUserPrmData

PrmText = 461 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  461  "Loc 1 Stop Bus Cyc"
Bit(1) 1 0-1
Prm_Text_Ref = 461 
EndExtUserPrmData

PrmText = 462 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  462  "Loc 1 Start DI"
Bit(2) 1 0-1
Prm_Text_Ref = 462 
EndExtUserPrmData

PrmText = 463 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  463  "Loc 1 Stop DI"
Bit(3) 1 0-1
Prm_Text_Ref = 463 
EndExtUserPrmData

PrmText = 464 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  464  "Loc 1 Start LCD"
Bit(4) 1 0-1
Prm_Text_Ref = 464 
EndExtUserPrmData

PrmText = 465 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  465  "Loc 1 Stop LCD"
Bit(5) 1 0-1
Prm_Text_Ref = 465 
EndExtUserPrmData

PrmText = 466 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  466  "Loc 1 Start Bus Acyc"
Bit(6) 0 0-1
Prm_Text_Ref = 466 
EndExtUserPrmData

PrmText = 467 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  467  "Loc 1 Stop Bus Acyc"
Bit(7) 1 0-1
Prm_Text_Ref = 467 
EndExtUserPrmData

PrmText = 468 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  468  "Auto Start Bus Cyc"
Bit(0) 1 0-1
Prm_Text_Ref = 468 
EndExtUserPrmData

PrmText = 469 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  469  "Auto Stop Bus Cyc"
Bit(1) 1 0-1
Prm_Text_Ref = 469 
EndExtUserPrmData

PrmText = 470 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  470  "Auto Start DI"
Bit(2) 0 0-1
Prm_Text_Ref = 470 
EndExtUserPrmData

PrmText = 471 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  471  "Auto Stop DI"
Bit(3) 1 0-1
Prm_Text_Ref = 471 
EndExtUserPrmData

PrmText = 472 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  472  "Auto Start LCD"
Bit(4) 0 0-1
Prm_Text_Ref = 472 
EndExtUserPrmData

PrmText = 473 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  473  "Auto Stop LCD"
Bit(5) 1 0-1
Prm_Text_Ref = 473 
EndExtUserPrmData

PrmText = 474 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  474  "Auto Start Bus Acyc"
Bit(6) 1 0-1
Prm_Text_Ref = 474 
EndExtUserPrmData

PrmText = 475 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  475  "Auto Stop Bus Acyc"
Bit(7) 1 0-1
Prm_Text_Ref = 475 
EndExtUserPrmData

PrmText = 476 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  476  "Loc 2 Start Bus Cyc"
Bit(0) 0 0-1
Prm_Text_Ref = 476 
EndExtUserPrmData

PrmText = 477 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  477  "Loc 2 Stop Bus Cyc"
Bit(1) 1 0-1
Prm_Text_Ref = 477 
EndExtUserPrmData

PrmText = 478 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  478  "Loc 2 Start DI"
Bit(2) 1 0-1
Prm_Text_Ref = 478 
EndExtUserPrmData

PrmText = 479 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  479  "Loc 2 Stop DI"
Bit(3) 1 0-1
Prm_Text_Ref = 479 
EndExtUserPrmData

PrmText = 480 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  480  "Loc 2 Start LCD"
Bit(4) 1 0-1
Prm_Text_Ref = 480 
EndExtUserPrmData

PrmText = 481 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  481  "Loc 2 Stop LCD"
Bit(5) 1 0-1
Prm_Text_Ref = 481 
EndExtUserPrmData

PrmText = 482 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  482  "Loc 2 Start Bus Acyc"
Bit(6) 0 0-1
Prm_Text_Ref = 482 
EndExtUserPrmData

PrmText = 483 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  483  "Loc 2 Stop Bus Acyc"
Bit(7) 1 0-1
Prm_Text_Ref = 483 
EndExtUserPrmData

PrmText = 484 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  484  "Multif In 0 Autoreset"
Bit(4) 0 0-1
Prm_Text_Ref = 484 
EndExtUserPrmData

PrmText = 485 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  485  "Multif In 1 Autoreset"
Bit(5) 0 0-1
Prm_Text_Ref = 485 
EndExtUserPrmData

PrmText = 486 
Text(0) = "No"
Text(1) = "Yes"
EndPrmText
ExtUserPrmData =  486  "Multif In 2 Autoreset"
Bit(6) 0 0-1
Prm_Text_Ref = 486 
EndExtUserPrmData

ExtUserPrmData =  487  "Aux Inp 1 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  488  "Aux Inp 2 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  489  "Aux Inp 3 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  490  "Aux Inp 4 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  491  "Aux Inp 5 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  492  "Aux Inp 6 Delay [0.1s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  493  "Check-Back Time [0.1s]"
Unsigned8 5 1-255
EndExtUserPrmData

ExtUserPrmData =  494  "Low Curr Warn Delay [0.1s]"
Unsigned8 5 0-255
EndExtUserPrmData

ExtUserPrmData =  495  "Low Curr Trip Delay [0.1s]"
Unsigned8 5 0-255
EndExtUserPrmData

ExtUserPrmData =  496  "High Curr Warn Delay [0.1s]"
Unsigned8 5 0-255
EndExtUserPrmData

ExtUserPrmData =  497  "High Curr Trip Delay [0.1s]"
Unsigned8 5 0-255
EndExtUserPrmData

ExtUserPrmData =  498  "Curr Imb Trip Level [%]"
Unsigned8 50 0-100
EndExtUserPrmData

ExtUserPrmData =  499  "Curr Imb Warn Level [%]"
Unsigned8 100 0-100
EndExtUserPrmData

PrmText = 500 
Text(0) = "Phase Sequence L1 L2 L3"
Text(1) = "Phase Sequence L3 L2 L1"
EndPrmText
ExtUserPrmData =  500  "Phase Reversal"
Bit(0) 0 0-1
Prm_Text_Ref = 500 
EndExtUserPrmData

ExtUserPrmData =  501  "Restart Level [%]"
Unsigned8 30 10-100
EndExtUserPrmData

PrmText = 502 
Text(0) = "Thermal Load"
Text(1) = "DX1xx DI"
Text(2) = "DX1xx DO"
Text(3) = "Operating Hours"
Text(4) = "Number of Trips"
Text(5) = "Number of Starts"
Text(6) = "max. Startup Current"
Text(7) = "Real Startup Time"
EndPrmText
ExtUserPrmData =  502  "User Display 1"
Unsigned8 0 0-7
Prm_Text_Ref = 502 
EndExtUserPrmData

PrmText = 503 
Text(0) = "Thermal Load"
Text(1) = "DX1xx DI"
Text(2) = "DX1xx DO"
Text(3) = "Operating Hours"
Text(4) = "Number of Trips"
Text(5) = "Number of Starts"
Text(6) = "max. Startup Current"
Text(7) = "Real Startup Time"
EndPrmText
ExtUserPrmData =  503  "User Display 2"
Unsigned8 6 0-7
Prm_Text_Ref = 503 
EndExtUserPrmData

PrmText = 504 
Text(0) = "Thermal Load"
Text(1) = "DX1xx DI"
Text(2) = "DX1xx DO"
Text(3) = "Operating Hours"
Text(4) = "Number of Trips"
Text(5) = "Number of Starts"
Text(6) = "max. Startup Current"
Text(7) = "Real Startup Time"
EndPrmText
ExtUserPrmData =  504  "User Display 3"
Unsigned8 7 0-7
Prm_Text_Ref = 504 
EndExtUserPrmData

PrmText = 505 
Text(0) = "Binary 0"
Text(1) = "Binary 1"
Text(2) = "Analog 0"
Text(3) = "Analog 1"
Text(4) = "Time to Trip"
Text(5) = "Time to Cool"
Text(6) = "Current to earth"
EndPrmText
ExtUserPrmData =  505  "User Display 4"
Unsigned8 4 0-6
Prm_Text_Ref = 505 
EndExtUserPrmData

PrmText = 506 
Text(0) = "Binary 0"
Text(1) = "Binary 1"
Text(2) = "Analog 0"
Text(3) = "Analog 1"
Text(4) = "Time to Trip"
Text(5) = "Time to Cool"
Text(6) = "Current to earth"
EndPrmText
ExtUserPrmData =  506  "User Display 5"
Unsigned8 5 0-6
Prm_Text_Ref = 506 
EndExtUserPrmData

ExtUserPrmData =  507  "Dip Duration [0.1s]"
Unsigned8 5 1-255
EndExtUserPrmData

ExtUserPrmData =  508  "Dip Autorestart Window [0.1s]"
Unsigned8 1 1-10
EndExtUserPrmData

ExtUserPrmData =  509  "Dip Autorestart Delay [s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  510  "Thermal Load Warnlev [%]"
Unsigned8 100 20-100
EndExtUserPrmData

ExtUserPrmData =  511  "Num Starts Allowed"
Unsigned8 0 0-32
EndExtUserPrmData

ExtUserPrmData =  512  "Num Starts Window [1 min.]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  513  "Num Starts Pause [1 min.]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  514  "Earth Flt Warn Level [%]"
Unsigned8 255 20-255
EndExtUserPrmData

ExtUserPrmData =  515  "Earth Flt Warn Delay [0.1s]"
Unsigned8 5 0-255
EndExtUserPrmData

ExtUserPrmData =  516  "Dip Restart Level [%]"
Unsigned8 90 50-115
EndExtUserPrmData

ExtUserPrmData =  517  "Dip Level [%]"
Unsigned8 70 50-115
EndExtUserPrmData

ExtUserPrmData =  518  "DX1xx DI Delay [ms]"
Unsigned8 20 3-200
EndExtUserPrmData

ExtUserPrmData =  519  "AM1 Tmax Delay [s]"
Unsigned8 6 0-255
EndExtUserPrmData

ExtUserPrmData =  520  "AM2 Tmax Delay [s]"
Unsigned8 6 0-255
EndExtUserPrmData

PrmText = 521 
Text(0) = "Disabled"
Text(1) = "Trip"
Text(2) = "Warning"
EndPrmText
ExtUserPrmData =  521  "AM2 CH2 Err Reac"
BitArea(0-1) 0 0-2
Prm_Text_Ref = 521 
EndExtUserPrmData

PrmText = 522 
Text(0) = "Disabled"
Text(1) = "Trip"
Text(2) = "Warning"
EndPrmText
ExtUserPrmData =  522  "AM2 CH3 Err Reac"
BitArea(2-3) 0 0-2
Prm_Text_Ref = 522 
EndExtUserPrmData

PrmText = 523 
Text(0) = "Temperature"
Text(1) = "Universal"
EndPrmText
ExtUserPrmData =  523  "AM1 Mode"
Bit(4) 0 0-1
Prm_Text_Ref = 523 
EndExtUserPrmData

PrmText = 524 
Text(0) = "Temperature"
Text(1) = "Universal"
EndPrmText
ExtUserPrmData =  524  "AM2 Mode"
Bit(5) 0 0-1
Prm_Text_Ref = 524 
EndExtUserPrmData

ExtUserPrmData =  525  "U Low Trip Level [%]"
Unsigned8 70 70-100
EndExtUserPrmData

ExtUserPrmData =  526  "U Low Trip Delay [0.1s]"
Unsigned8 30 0-255
EndExtUserPrmData

ExtUserPrmData =  527  "U Low Warn Level [%]"
Unsigned8 70 70-100
EndExtUserPrmData

ExtUserPrmData =  528  "U Low Warn Delay [0.1s]"
Unsigned8 30 0-255
EndExtUserPrmData

ExtUserPrmData =  529  "U High Trip Level [%]"
Unsigned8 116 100-116
EndExtUserPrmData

ExtUserPrmData =  530  "U High Trip Delay [0.1s]"
Unsigned8 30 0-255
EndExtUserPrmData

ExtUserPrmData =  531  "U High Warn Level [%]"
Unsigned8 116 100-116
EndExtUserPrmData

ExtUserPrmData =  532  "U High Warn Delay [0.1s]"
Unsigned8 30 0-255
EndExtUserPrmData

ExtUserPrmData =  533  "AM1 Tmax Trip Level [1K]"
Unsigned16 65535 0-65535
EndExtUserPrmData

ExtUserPrmData =  534  "AM1 Tmax Warn Level [1K]"
Unsigned16 65535 0-65535
EndExtUserPrmData

ExtUserPrmData =  535  "AM2 Tmax Trip Level [1K]"
Unsigned16 65535 0-65535
EndExtUserPrmData

ExtUserPrmData =  536  "AM2 Tmax Warn Level [1K]"
Unsigned16 65535 0-65535
EndExtUserPrmData

PrmText = 537 
Text(0) = "Disabled"
Text(1) = "PT100 -50 C...+400 C (2-wire)"
Text(2) = "PT100 -50 C...+400 C (3-wire)"
Text(3) = "PT100 -50 C...+70 C (2-wire)"
Text(4) = "PT100 -50 C...+70 C (3-wire)"
Text(5) = "PT1000 -50 C...+400 C (2-wire)"
Text(6) = "PT1000 -50 C...+400 C (3-wire)"
Text(7) = "KTY83 -50 C...+175 C"
Text(8) = "KTY84 -40 C...+300 C"
Text(9) = "NTC +80 C...+160 C"
Text(10) = "0...10V"
Text(11) = "0...20mA"
Text(12) = "4...20mA"
EndPrmText
ExtUserPrmData =  537  "AM1 CH1 Type"
BitArea(0-3) 0 0-12
Prm_Text_Ref = 537 
EndExtUserPrmData

PrmText = 538 
Text(0) = "Disabled"
Text(1) = "PT100 -50 C...+400 C (2-wire)"
Text(2) = "PT100 -50 C...+400 C (3-wire)"
Text(3) = "PT100 -50 C...+70 C (2-wire)"
Text(4) = "PT100 -50 C...+70 C (3-wire)"
Text(5) = "PT1000 -50 C...+400 C (2-wire)"
Text(6) = "PT1000 -50 C...+400 C (3-wire)"
Text(7) = "KTY83 -50 C...+175 C"
Text(8) = "KTY84 -40 C...+300 C"
Text(9) = "NTC +80 C...+160 C"
Text(10) = "0...10V"
Text(11) = "0...20mA"
Text(12) = "4...20mA"
EndPrmText
ExtUserPrmData =  538  "AM1 CH2 Type"
BitArea(4-7) 0 0-12
Prm_Text_Ref = 538 
EndExtUserPrmData

PrmText = 539 
Text(0) = "Disabled"
Text(1) = "PT100 -50 C...+400 C (2-wire)"
Text(2) = "PT100 -50 C...+400 C (3-wire)"
Text(3) = "PT100 -50 C...+70 C (2-wire)"
Text(4) = "PT100 -50 C...+70 C (3-wire)"
Text(5) = "PT1000 -50 C...+400 C (2-wire)"
Text(6) = "PT1000 -50 C...+400 C (3-wire)"
Text(7) = "KTY83 -50 C...+175 C"
Text(8) = "KTY84 -40 C...+300 C"
Text(9) = "NTC +80 C...+160 C"
Text(10) = "0...10V"
Text(11) = "0...20mA"
Text(12) = "4...20mA"
EndPrmText
ExtUserPrmData =  539  "AM1 CH3 Type"
BitArea(0-3) 0 0-12
Prm_Text_Ref = 539 
EndExtUserPrmData

PrmText = 540 
Text(0) = "Disabled"
Text(1) = "PT100 -50 C...+400 C (2-wire)"
Text(2) = "PT100 -50 C...+400 C (3-wire)"
Text(3) = "PT100 -50 C...+70 C (2-wire)"
Text(4) = "PT100 -50 C...+70 C (3-wire)"
Text(5) = "PT1000 -50 C...+400 C (2-wire)"
Text(6) = "PT1000 -50 C...+400 C (3-wire)"
Text(7) = "KTY83 -50 C...+175 C"
Text(8) = "KTY84 -40 C...+300 C"
Text(9) = "NTC +80 C...+160 C"
Text(10) = "0...10V"
Text(11) = "0...20mA"
Text(12) = "4...20mA"
EndPrmText
ExtUserPrmData =  540  "AM2 CH1 Type"
BitArea(4-7) 0 0-12
Prm_Text_Ref = 540 
EndExtUserPrmData

PrmText = 541 
Text(0) = "Disabled"
Text(1) = "PT100 -50 C...+400 C (2-wire)"
Text(2) = "PT100 -50 C...+400 C (3-wire)"
Text(3) = "PT100 -50 C...+70 C (2-wire)"
Text(4) = "PT100 -50 C...+70 C (3-wire)"
Text(5) = "PT1000 -50 C...+400 C (2-wire)"
Text(6) = "PT1000 -50 C...+400 C (3-wire)"
Text(7) = "KTY83 -50 C...+175 C"
Text(8) = "KTY84 -40 C...+300 C"
Text(9) = "NTC +80 C...+160 C"
Text(10) = "0...10V"
Text(11) = "0...20mA"
Text(12) = "4...20mA"
EndPrmText
ExtUserPrmData =  541  "AM2 CH2 Type"
BitArea(0-3) 0 0-12
Prm_Text_Ref = 541 
EndExtUserPrmData

PrmText = 542 
Text(0) = "Disabled"
Text(1) = "PT100 -50 C...+400 C (2-wire)"
Text(2) = "PT100 -50 C...+400 C (3-wire)"
Text(3) = "PT100 -50 C...+70 C (2-wire)"
Text(4) = "PT100 -50 C...+70 C (3-wire)"
Text(5) = "PT1000 -50 C...+400 C (2-wire)"
Text(6) = "PT1000 -50 C...+400 C (3-wire)"
Text(7) = "KTY83 -50 C...+175 C"
Text(8) = "KTY84 -40 C...+300 C"
Text(9) = "NTC +80 C...+160 C"
Text(10) = "0...10V"
Text(11) = "0...20mA"
Text(12) = "4...20mA"
EndPrmText
ExtUserPrmData =  542  "AM2 CH3 Type"
BitArea(4-7) 0 0-12
Prm_Text_Ref = 542 
EndExtUserPrmData

PrmText = 543 
Text(0) = "Disabled"
Text(1) = "Trip"
Text(2) = "Warning"
EndPrmText
ExtUserPrmData =  543  "AM1 CH1 Err Reac"
BitArea(0-1) 0 0-2
Prm_Text_Ref = 543 
EndExtUserPrmData

PrmText = 544 
Text(0) = "Disabled"
Text(1) = "Trip"
Text(2) = "Warning"
EndPrmText
ExtUserPrmData =  544  "AM1 CH2 Err Reac"
BitArea(2-3) 0 0-2
Prm_Text_Ref = 544 
EndExtUserPrmData

PrmText = 545 
Text(0) = "Disabled"
Text(1) = "Trip"
Text(2) = "Warning"
EndPrmText
ExtUserPrmData =  545  "AM1 CH3 Err Reac"
BitArea(4-5) 0 0-2
Prm_Text_Ref = 545 
EndExtUserPrmData

PrmText = 546 
Text(0) = "Disabled"
Text(1) = "Trip"
Text(2) = "Warning"
EndPrmText
ExtUserPrmData =  546  "AM2 CH1 Err Reac"
BitArea(6-7) 0 0-2
Prm_Text_Ref = 546 
EndExtUserPrmData

ExtUserPrmData =  547  "Param To PV 1"
Unsigned8 1 0-255
EndExtUserPrmData

ExtUserPrmData =  548  "Param To PV 2"
Unsigned8 2 0-255
EndExtUserPrmData

ExtUserPrmData =  549  "Param To PV 3"
Unsigned8 3 0-255
EndExtUserPrmData

ExtUserPrmData =  550  "Param To PV 4"
Unsigned8 4 0-255
EndExtUserPrmData

PrmText = 551 
Text(0) = "0-20mA"
Text(1) = "4-20mA"
Text(2) = "0-10mA"
Text(3) = "0-10V"
EndPrmText
ExtUserPrmData =  551  "DX1xx AO Type"
BitArea(0-1) 0 0-3
Prm_Text_Ref = 551 
EndExtUserPrmData

PrmText = 552 
Text(0) = "Disabled"
Text(1) = "Trip"
Text(2) = "Warning"
EndPrmText
ExtUserPrmData =  552  "DX1xx AO Err Reac"
BitArea(2-3) 0 0-2
Prm_Text_Ref = 552 
EndExtUserPrmData

ExtUserPrmData =  553  "Param To PV 5"
Unsigned8 5 0-255
EndExtUserPrmData

ExtUserPrmData =  554  "Mot. op. hours level"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  555  "Mot. stand still lev"
Unsigned8 0 0-255
EndExtUserPrmData

PrmText = 556 
Text(0) = "Disabled"
Text(1) = "Trip"
Text(2) = "Warning"
EndPrmText
ExtUserPrmData =  556  "Num Starts Overrun"
BitArea(2-3) 0 0-2
Prm_Text_Ref = 556 
EndExtUserPrmData

PrmText = 557 
Text(0) = "Disabled"
Text(1) = "Trip"
Text(2) = "Warning"
EndPrmText
ExtUserPrmData =  557  "Num Starts Prewarn"
BitArea(4-5) 0 0-2
Prm_Text_Ref = 557 
EndExtUserPrmData

PrmText = 558 
Text(0) = "Power Scale Factor 1"
Text(1) = "Power Scale Factor 10"
Text(2) = "Power Scale Factor 100"
Text(3) = "Power Scale Factor 1000"
EndPrmText
ExtUserPrmData =  558  "Power Scale Factor"
BitArea(6-7) 1 0-3
Prm_Text_Ref = 558 
EndExtUserPrmData

PrmText = 559 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  559  "Backlight"
Bit(0) 1 0-1
Prm_Text_Ref = 559 
EndExtUserPrmData

PrmText = 560 
Text(0) = "Off"
Text(1) = "On for Parameters"
Text(2) = "On for Param. + Motor Control"
EndPrmText
ExtUserPrmData =  560  "Password Protection"
BitArea(1-2) 0 0-2
Prm_Text_Ref = 560 
EndExtUserPrmData

PrmText = 561 
Text(0) = "Off"
Text(1) = "On"
Text(2) = "On + Rapid Cycle Lockout"
EndPrmText
ExtUserPrmData =  561  "Dip Enable"
BitArea(3-4) 0 0-2
Prm_Text_Ref = 561 
EndExtUserPrmData

PrmText = 562 
Text(0) = "Off"
Text(1) = "On"
EndPrmText
ExtUserPrmData =  562  "Dip Autorestart Enable"
Bit(5) 0 0-1
Prm_Text_Ref = 562 
EndExtUserPrmData

PrmText = 563 
Text(0) = "Celcius"
Text(1) = "Fahrenheit"
EndPrmText
ExtUserPrmData =  563  "LCD Panel T Unit"
Bit(6) 0 0-1
Prm_Text_Ref = 563 
EndExtUserPrmData

ExtUserPrmData =  564  "Nominal Voltage [V]"
Unsigned16 400 90-690
EndExtUserPrmData

ExtUserPrmData =  565  "PwrFactor Trip Level"
Unsigned8 30 30-100
EndExtUserPrmData

ExtUserPrmData =  566  "PwrFactor Trip Delay [0.1s]"
Unsigned8 30 0-255
EndExtUserPrmData

ExtUserPrmData =  567  "PwrFactor Warn Level"
Unsigned8 30 30-100
EndExtUserPrmData

ExtUserPrmData =  568  "PwrFactor Warn Delay [0.1s]"
Unsigned8 30 0-255
EndExtUserPrmData

ExtUserPrmData =  569  "U Imb. Trip Level [0.1%]"
Unsigned8 200 2-200
EndExtUserPrmData

ExtUserPrmData =  570  "U Imb. Trip Delay [0.1s]"
Unsigned8 10 0-255
EndExtUserPrmData

ExtUserPrmData =  571  "U Imb. Warn Level [0.1%]"
Unsigned8 200 2-200
EndExtUserPrmData

ExtUserPrmData =  572  "U Imb. Warn Delay [0.1s]"
Unsigned8 10 0-255
EndExtUserPrmData

ExtUserPrmData =  573  "P Low Trip Level [%]"
Unsigned8 20 20-100
EndExtUserPrmData

ExtUserPrmData =  574  "P Low Trip Delay [s]"
Unsigned8 5 0-255
EndExtUserPrmData

ExtUserPrmData =  575  "P Low Warn Level [%]"
Unsigned8 20 20-100
EndExtUserPrmData

ExtUserPrmData =  576  "P Low Warn Delay [s]"
Unsigned8 5 0-255
EndExtUserPrmData

ExtUserPrmData =  577  "P High Trip Level [5%]"
Unsigned8 200 20-200
EndExtUserPrmData

ExtUserPrmData =  578  "P High Trip Delay [s]"
Unsigned8 10 0-255
EndExtUserPrmData

ExtUserPrmData =  579  "P High Warn Level [5%]"
Unsigned8 200 20-200
EndExtUserPrmData

ExtUserPrmData =  580  "P High Warn Delay [s]"
Unsigned8 10 0-255
EndExtUserPrmData

ExtUserPrmData =  581  "Nominal Power Factor"
Unsigned8 100 1-100
EndExtUserPrmData

ExtUserPrmData =  582  "THD Warning Level [%]"
Unsigned8 10 3-10
EndExtUserPrmData

ExtUserPrmData =  583  "Load Startup Delay [s]"
Unsigned8 0 0-255
EndExtUserPrmData

ExtUserPrmData =  584  "THD Warning Delay [s]"
Unsigned8 5 0-255
EndExtUserPrmData

;
;=====================================================================
; special Parameter-Definitions for DPV1-Plug PDP22/PDP32
;=====================================================================
PrmText = 10000
Text(0) ="Use Block-Parameters"
Text(1) ="Ignore Block-Parameters"
EndPrmText

PrmText = 10001
Text(0) ="DPV0 Diagnosis Format"
Text(1) ="DPV1 Diagnosis Format"
EndPrmText

ExtUserPrmData = 10000 "Block - Parameter"
Unsigned8 0 0-1
Prm_Text_Ref = 10000
EndExtUserPrmData

ExtUserPrmData = 10001 "Diagnosis Format"
Unsigned8 0 0-1
Prm_Text_Ref = 10001
EndExtUserPrmData

;
;===========================================================
;General parameters
;===========================================================
;
GSD_Revision = 3
Vendor_Name ="ABB"
Model_Name ="UMC100"
Revision ="3.01"
Ident_Number   =0x34E0
Protocol_Ident = 0
Station_Type = 0
FMS_supp = 0
Hardware_Release ="V 1.0"
Software_Release ="V 3.xx"
9.6_supp       =1
19.2_supp      =1
31.25_supp     =0
45.45_supp     =1
93.75_supp     =1
187.5_supp     =1
500_supp       =1
1.5M_supp      =1
3M_supp = 1
6M_supp = 1
12M_supp = 1
MaxTsdr_9.6 = 15
MaxTsdr_19.2 = 15
MaxTsdr_31.25 = 15
MaxTsdr_45.45 = 15
MaxTsdr_93.75 = 15
MaxTsdr_187.5 = 15
MaxTsdr_500 = 15
MaxTsdr_1.5M   =20
MaxTsdr_3M = 35
MaxTsdr_6M = 50
MaxTsdr_12M = 95
Redundancy = 0
Repeater_Ctrl_Sig = 0
24V_Pins = 1
Implementation_Type ="VPC3 solution"
Bitmap_Device ="FBP_N"
Bitmap_Diag ="FBP_DIAG"
Bitmap_SF ="FBP_RUN"
;
;================================
; Slave-Specification:
;================================
;
Freeze_Mode_supp = 1
Sync_Mode_supp = 1
Set_Slave_Add_Supp = 0
Auto_Baud_supp = 1
Min_Slave_Intervall = 1
Fail_Safe = 1
Max_Diag_Data_Len = 19
Modul_Offset = 0
Slave_Family=9@FieldBusPlug@ProfibusDP
Modular_Station = 1
Max_Module = 1
Max_Input_len = 48
Max_Output_len = 48
Max_Data_len = 96

;=======================================
; Device specific diagnostic data (DPV1)
;=======================================
;

Unit_Diag_Area = 0 - 7
; Diag Status available
Value(129) ="UMC100 Diag status available"
Unit_Diag_Area_End

Unit_Diag_Area = 24 - 31
; Comm-State-Info
Value(0) ="Communication OK"
Value(1) ="Lost Communication to UMC100"
Unit_Diag_Area_End

Unit_Diag_bit(32) = "Thermal Overload Trip"
Unit_Diag_bit(33) = "Phase Loss"
Unit_Diag_bit(34) = "Phase Imbalance"
Unit_Diag_bit(35) = "Locked Rotor"
Unit_Diag_bit(36) = "Thermal Load Prewarn."
Unit_Diag_bit(37) = "PTC Temperature High"
Unit_Diag_bit(38) = "PTC Wiring Problem"
Unit_Diag_bit(39) = "Check-Back Error"

Unit_Diag_bit(40) = "I below Trip Level"
Unit_Diag_bit(41) = "I below Warn Level"
Unit_Diag_bit(42) = "I above Trip Level"
Unit_Diag_bit(43) = "I above Warn Level"
Unit_Diag_bit(44) = "Earthfault Trip"
Unit_Diag_bit(45) = "Earthfault Warning"
Unit_Diag_bit(46) = "UMC Selftest Error"
Unit_Diag_bit(47) = "Actuator"

Unit_Diag_bit(48) = "IO-Module Missing"
Unit_Diag_bit(49) = "Application Error"
Unit_Diag_bit(50) = "IO-Module Warning/Error"
Unit_Diag_bit(51) = "Auxiliary Input 1"
Unit_Diag_bit(52) = "Auxiliary Input 2"
Unit_Diag_bit(53) = "Auxiliary Input 3"
Unit_Diag_bit(54) = "Auxiliary Input 4"
Unit_Diag_bit(55) = "Auxiliary Input 5"

Unit_Diag_bit(56) = "Auxiliary Input 6"
Unit_Diag_bit(57) = "Ext. Fault Multif. DI0"
Unit_Diag_bit(58) = "Ext. Fault Multif. DI1"
Unit_Diag_bit(59) = "Ext. Fault Multif. DI2"
Unit_Diag_bit(60) = "AM1 >/< Trip Level"
Unit_Diag_bit(61) = "AM1 >/< Warn Level"
Unit_Diag_bit(62) = "AM2 >/< Trip Level"
Unit_Diag_bit(63) = "AM2 >/< Warn Level"

Unit_Diag_bit(64) = "reserved"
Unit_Diag_bit(65) = "reserved"
Unit_Diag_bit(66) = "Underload Power"
Unit_Diag_bit(67) = "Overload Power"
Unit_Diag_bit(68) = "Voltage out of spec."
Unit_Diag_bit(69) = "THD Warning"
Unit_Diag_bit(70) = "reserved"
Unit_Diag_bit(71) = "reserved"

Unit_Diag_bit(72) = "reserved"
Unit_Diag_bit(73) = "reserved"
Unit_Diag_bit(74) = "reserved"
Unit_Diag_bit(75) = "Num Starts Overrun"
Unit_Diag_bit(76) = "Just one start left"
Unit_Diag_bit(77) = "Cooling Time Running"
Unit_Diag_bit(78) = "reserved"
Unit_Diag_bit(79) = "reserved"

Unit_Diag_bit(80) = "reserved"
Unit_Diag_bit(81) = "reserved"
Unit_Diag_bit(82) = "reserved"
Unit_Diag_bit(83) = "reserved"
Unit_Diag_bit(84) = "reserved"
Unit_Diag_bit(85) = "reserved"
Unit_Diag_bit(86) = "Parameter out of range"
Unit_Diag_bit(87) = "Ext. Diag. Available"

Unit_Diag_bit(88) = "Bit0 ext. UMC-Diagnosis"
Unit_Diag_bit(89) = "Bit1 ext. UMC-Diagnosis"
Unit_Diag_bit(90) = "Bit2 ext. UMC-Diagnosis"
Unit_Diag_bit(91) = "Bit3 ext. UMC-Diagnosis"
Unit_Diag_bit(92) = "Bit4 ext. UMC-Diagnosis"
Unit_Diag_bit(93) = "Bit5 ext. UMC-Diagnosis"
Unit_Diag_bit(94) = "Bit6 ext. UMC-Diagnosis"
Unit_Diag_bit(95) = "Bit7 ext. UMC-Diagnosis"

;=============================================
; User Prm Data: Length and Preset:
;=============================================
;
Max_User_Prm_Data_Len   = 232             ;   number of parameter of UMC100 (max 224)
;                                        + number of parameter for the FBP itself (8)
Ext_User_Prm_Data_Const(0) = 0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00    ; constant values for ASIC
;DPV1 status1 = 0x00 =>
;       Bit2 = 0 WD_Base=10ms (1ms=1)
;       Bit7 = 1 DPV1 Enable (Disable=0)
;DPV1 status2 = 0x00 =>
;       Bit0 = 0 ChkCfg nach EN50170(User specific=1)
;DPV1 status3 = 0x00 =>
;       alarm not implemented

Ext_User_Prm_Data_Ref(3) = 10000        ; use/ignore Block-Parameters
Ext_User_Prm_Data_Ref(4) = 10001        ; Diag-Format DPV0/V1
;
;=============================================
; Module Definition List
;=============================================
;
Module="UMC 100.3 (Rx100 Rx200)"0x11, 0x23, 0x56, 0x63      ; 16DI, 32DO, 7AI, 4AO
4
Ext_Module_Prm_Data_Len= 224                        ; number of used data byte
Ext_User_Prm_Data_Const(0) =    \                 ; initialising of param data
    0x00, 0x00, 0x00, 0x32, 0x00, 0x00, 0x00, 0x32, 0x02, 0x58,  \
    0x00, 0x64, 0x00, 0x78, 0xFF, 0x05, 0x00, 0x01, 0x00, 0x01,  \
    0x0A, 0x00, 0x1E, 0xA0, 0xA0, 0x05, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x03, 0x00, 0x00, 0x00, 0x00, 0x08, 0x64,  \
    0x00, 0x00, 0x02, 0xBE, 0xEB, 0xBE, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x05, 0x05, 0x05, 0x05,  \
    0x05, 0x32, 0x64, 0x00, 0x1E, 0x00, 0x06, 0x07, 0x04, 0x05,  \
    0x00, 0x05, 0x01, 0x00, 0x64, 0x00, 0x00, 0x00, 0xFF, 0x05,  \
    0x5A, 0x46, 0x00, 0x14, 0x06, 0x06, 0x00, 0x46, 0x1E, 0x46,  \
    0x1E, 0x74, 0x1E, 0x74, 0x1E, 0xFF, 0xFF, 0xFF, 0xFF, 0xFF,  \
    0xFF, 0xFF, 0xFF, 0x00, 0x00, 0x00, 0x00, 0x01, 0x02, 0x03,  \
    0x04, 0x00, 0x05, 0x00, 0x00, 0x40, 0x01, 0x01, 0x90, 0x1E,  \
    0x1E, 0x1E, 0x1E, 0xC8, 0x0A, 0xC8, 0x0A, 0x14, 0x05, 0x14,  \
    0x05, 0xC8, 0x0A, 0xC8, 0x0A, 0x64, 0x00, 0x00, 0x0A, 0x00,  \
    0x05, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00
Ext_User_Prm_Data_Ref( 0 ) = 401 ;   Setting Ie 1
Ext_User_Prm_Data_Ref( 4 ) = 402 ;   Setting Ie 2
Ext_User_Prm_Data_Ref( 8 ) = 403 ;   YD Starting Time
Ext_User_Prm_Data_Ref( 10 ) = 404 ;   Current Factor
Ext_User_Prm_Data_Ref( 12 ) = 405 ;   Cooling Time
Ext_User_Prm_Data_Ref( 14 ) = 406 ;   Earth Flt Trip Level
Ext_User_Prm_Data_Ref( 15 ) = 407 ;   Earth Flt Trip Delay
Ext_User_Prm_Data_Ref( 16 ) = 408 ;   Language
Ext_User_Prm_Data_Ref( 17 ) = 409 ;   Rev Lock-Out Time
Ext_User_Prm_Data_Ref( 18 ) = 410 ;   Fault Output
Ext_User_Prm_Data_Ref( 19 ) = 411 ;   Trip Class
Ext_User_Prm_Data_Ref( 20 ) = 412 ;   Low Curr Warn Level
Ext_User_Prm_Data_Ref( 21 ) = 413 ;   Low Curr Trip Level
Ext_User_Prm_Data_Ref( 22 ) = 414 ;   High Curr Warn Level
Ext_User_Prm_Data_Ref( 23 ) = 415 ;   High Curr Trip Level
Ext_User_Prm_Data_Ref( 24 ) = 416 ;   Locked Rotor Level
Ext_User_Prm_Data_Ref( 25 ) = 417 ;   Locked Rotor Delay
Ext_User_Prm_Data_Ref( 26 ) = 418 ;   Custom App Parameter
Ext_User_Prm_Data_Ref( 27 ) = 419 ;   Multif In 0
Ext_User_Prm_Data_Ref( 28 ) = 420 ;   Multif In 1
Ext_User_Prm_Data_Ref( 29 ) = 421 ;   Multif In 2
Ext_User_Prm_Data_Ref( 30 ) = 422 ;   Multif In 0 Delay
Ext_User_Prm_Data_Ref( 31 ) = 423 ;   Multif In 1 Delay
Ext_User_Prm_Data_Ref( 32 ) = 424 ;   Multif In 2 Delay
Ext_User_Prm_Data_Ref( 33 ) = 425 ;   Control Function
Ext_User_Prm_Data_Ref( 34 ) = 426 ;   Busfault Reaction
Ext_User_Prm_Data_Ref( 35 ) = 427 ;   Aux Inp 1 Reaction
Ext_User_Prm_Data_Ref( 35 ) = 428 ;   Aux Inp 2 Reaction
Ext_User_Prm_Data_Ref( 36 ) = 429 ;   Aux Inp 3 Reaction
Ext_User_Prm_Data_Ref( 36 ) = 430 ;   Aux Inp 4 Reaction
Ext_User_Prm_Data_Ref( 37 ) = 431 ;   Aux Inp 5 Reaction
Ext_User_Prm_Data_Ref( 37 ) = 432 ;   Aux Inp 6 Reaction
Ext_User_Prm_Data_Ref( 38 ) = 433 ;   PTC, Thermistor
Ext_User_Prm_Data_Ref( 38 ) = 434 ;   Check-Back
Ext_User_Prm_Data_Ref( 38 ) = 435 ;   Check Phase Sequence
Ext_User_Prm_Data_Ref( 39 ) = 436 ;   Fault Auto Reset
Ext_User_Prm_Data_Ref( 39 ) = 437 ;   Emergency Start
Ext_User_Prm_Data_Ref( 39 ) = 438 ;   Earth Flt Detection
Ext_User_Prm_Data_Ref( 39 ) = 439 ;   Address Check
Ext_User_Prm_Data_Ref( 39 ) = 440 ;   Enable Custom Logic
Ext_User_Prm_Data_Ref( 39 ) = 441 ;   YD Change-Over Mode
Ext_User_Prm_Data_Ref( 39 ) = 442 ;   Phase Loss Prot.
Ext_User_Prm_Data_Ref( 39 ) = 443 ;   Resistive Load
Ext_User_Prm_Data_Ref( 40 ) = 444 ;   DX1xx Enabled
Ext_User_Prm_Data_Ref( 40 ) = 445 ;   AI1xx AM1 Enabled
Ext_User_Prm_Data_Ref( 40 ) = 446 ;   AI1xx AM2 Enabled
Ext_User_Prm_Data_Ref( 40 ) = 447 ;   VI15x Enabled
Ext_User_Prm_Data_Ref( 40 ) = 448 ;   Missing Module React.
Ext_User_Prm_Data_Ref( 41 ) = 449 ;   Aux Inp 1 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 450 ;   Aux Inp 2 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 451 ;   Aux Inp 3 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 452 ;   Aux Inp 4 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 453 ;   Aux Inp 5 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 454 ;   Aux Inp 6 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 455 ;   Number Of Phases
Ext_User_Prm_Data_Ref( 41 ) = 456 ;   Cooling Mode
Ext_User_Prm_Data_Ref( 42 ) = 457 ;   Invert DI Start Inp.
Ext_User_Prm_Data_Ref( 42 ) = 458 ;   Invert DI Stop Inp.
Ext_User_Prm_Data_Ref( 42 ) = 459 ;   Inching DI Start Inp
Ext_User_Prm_Data_Ref( 43 ) = 460 ;   Loc 1 Start Bus Cyc
Ext_User_Prm_Data_Ref( 43 ) = 461 ;   Loc 1 Stop Bus Cyc
Ext_User_Prm_Data_Ref( 43 ) = 462 ;   Loc 1 Start DI
Ext_User_Prm_Data_Ref( 43 ) = 463 ;   Loc 1 Stop DI
Ext_User_Prm_Data_Ref( 43 ) = 464 ;   Loc 1 Start LCD
Ext_User_Prm_Data_Ref( 43 ) = 465 ;   Loc 1 Stop LCD
Ext_User_Prm_Data_Ref( 43 ) = 466 ;   Loc 1 Start Bus Acyc
Ext_User_Prm_Data_Ref( 43 ) = 467 ;   Loc 1 Stop Bus Acyc
Ext_User_Prm_Data_Ref( 44 ) = 468 ;   Auto Start Bus Cyc
Ext_User_Prm_Data_Ref( 44 ) = 469 ;   Auto Stop Bus Cyc
Ext_User_Prm_Data_Ref( 44 ) = 470 ;   Auto Start DI
Ext_User_Prm_Data_Ref( 44 ) = 471 ;   Auto Stop DI
Ext_User_Prm_Data_Ref( 44 ) = 472 ;   Auto Start LCD
Ext_User_Prm_Data_Ref( 44 ) = 473 ;   Auto Stop LCD
Ext_User_Prm_Data_Ref( 44 ) = 474 ;   Auto Start Bus Acyc
Ext_User_Prm_Data_Ref( 44 ) = 475 ;   Auto Stop Bus Acyc
Ext_User_Prm_Data_Ref( 45 ) = 476 ;   Loc 2 Start Bus Cyc
Ext_User_Prm_Data_Ref( 45 ) = 477 ;   Loc 2 Stop Bus Cyc
Ext_User_Prm_Data_Ref( 45 ) = 478 ;   Loc 2 Start DI
Ext_User_Prm_Data_Ref( 45 ) = 479 ;   Loc 2 Stop DI
Ext_User_Prm_Data_Ref( 45 ) = 480 ;   Loc 2 Start LCD
Ext_User_Prm_Data_Ref( 45 ) = 481 ;   Loc 2 Stop LCD
Ext_User_Prm_Data_Ref( 45 ) = 482 ;   Loc 2 Start Bus Acyc
Ext_User_Prm_Data_Ref( 45 ) = 483 ;   Loc 2 Stop Bus Acyc
Ext_User_Prm_Data_Ref( 46 ) = 484 ;   Multif In 0 Autoreset
Ext_User_Prm_Data_Ref( 46 ) = 485 ;   Multif In 1 Autoreset
Ext_User_Prm_Data_Ref( 46 ) = 486 ;   Multif In 2 Autoreset
Ext_User_Prm_Data_Ref( 50 ) = 487 ;   Aux Inp 1 Delay
Ext_User_Prm_Data_Ref( 51 ) = 488 ;   Aux Inp 2 Delay
Ext_User_Prm_Data_Ref( 52 ) = 489 ;   Aux Inp 3 Delay
Ext_User_Prm_Data_Ref( 53 ) = 490 ;   Aux Inp 4 Delay
Ext_User_Prm_Data_Ref( 54 ) = 491 ;   Aux Inp 5 Delay
Ext_User_Prm_Data_Ref( 55 ) = 492 ;   Aux Inp 6 Delay
Ext_User_Prm_Data_Ref( 56 ) = 493 ;   Check-Back Time
Ext_User_Prm_Data_Ref( 57 ) = 494 ;   Low Curr Warn Delay
Ext_User_Prm_Data_Ref( 58 ) = 495 ;   Low Curr Trip Delay
Ext_User_Prm_Data_Ref( 59 ) = 496 ;   High Curr Warn Delay
Ext_User_Prm_Data_Ref( 60 ) = 497 ;   High Curr Trip Delay
Ext_User_Prm_Data_Ref( 61 ) = 498 ;   Curr Imb Trip Level
Ext_User_Prm_Data_Ref( 62 ) = 499 ;   Curr Imb Warn Level
Ext_User_Prm_Data_Ref( 63 ) = 500 ;   Phase Reversal
Ext_User_Prm_Data_Ref( 64 ) = 501 ;   Restart Level
Ext_User_Prm_Data_Ref( 65 ) = 502 ;   User Display 1
Ext_User_Prm_Data_Ref( 66 ) = 503 ;   User Display 2
Ext_User_Prm_Data_Ref( 67 ) = 504 ;   User Display 3
Ext_User_Prm_Data_Ref( 68 ) = 505 ;   User Display 4
Ext_User_Prm_Data_Ref( 69 ) = 506 ;   User Display 5
Ext_User_Prm_Data_Ref( 71 ) = 507 ;   Dip Duration
Ext_User_Prm_Data_Ref( 72 ) = 508 ;   Dip Autorestart Window
Ext_User_Prm_Data_Ref( 73 ) = 509 ;   Dip Autorestart Delay
Ext_User_Prm_Data_Ref( 74 ) = 510 ;   Thermal Load Warnlev
Ext_User_Prm_Data_Ref( 75 ) = 511 ;   Num Starts Allowed
Ext_User_Prm_Data_Ref( 76 ) = 512 ;   Num Starts Window
Ext_User_Prm_Data_Ref( 77 ) = 513 ;   Num Starts Pause
Ext_User_Prm_Data_Ref( 78 ) = 514 ;   Earth Flt Warn Level
Ext_User_Prm_Data_Ref( 79 ) = 515 ;   Earth Flt Warn Delay
Ext_User_Prm_Data_Ref( 80 ) = 516 ;   Dip Restart Level
Ext_User_Prm_Data_Ref( 81 ) = 517 ;   Dip Level
Ext_User_Prm_Data_Ref( 83 ) = 518 ;   DX1xx DI Delay
Ext_User_Prm_Data_Ref( 84 ) = 519 ;   AM1 Tmax Delay
Ext_User_Prm_Data_Ref( 85 ) = 520 ;   AM2 Tmax Delay
Ext_User_Prm_Data_Ref( 86 ) = 521 ;   AM2 CH2 Err Reac
Ext_User_Prm_Data_Ref( 86 ) = 522 ;   AM2 CH3 Err Reac
Ext_User_Prm_Data_Ref( 86 ) = 523 ;   AM1 Mode
Ext_User_Prm_Data_Ref( 86 ) = 524 ;   AM2 Mode
Ext_User_Prm_Data_Ref( 88 ) = 525 ;   U Low Trip Level
Ext_User_Prm_Data_Ref( 89 ) = 526 ;   U Low Trip Delay
Ext_User_Prm_Data_Ref( 90 ) = 527 ;   U Low Warn Level
Ext_User_Prm_Data_Ref( 91 ) = 528 ;   U Low Warn Delay
Ext_User_Prm_Data_Ref( 92 ) = 529 ;   U High Trip Level
Ext_User_Prm_Data_Ref( 93 ) = 530 ;   U High Trip Delay
Ext_User_Prm_Data_Ref( 94 ) = 531 ;   U High Warn Level
Ext_User_Prm_Data_Ref( 95 ) = 532 ;   U High Warn Delay
Ext_User_Prm_Data_Ref( 96 ) = 533 ;   AM1 Tmax Trip Level
Ext_User_Prm_Data_Ref( 98 ) = 534 ;   AM1 Tmax Warn Level
Ext_User_Prm_Data_Ref( 100 ) = 535 ;   AM2 Tmax Trip Level
Ext_User_Prm_Data_Ref( 102 ) = 536 ;   AM2 Tmax Warn Level
Ext_User_Prm_Data_Ref( 104 ) = 537 ;   AM1 CH1 Type
Ext_User_Prm_Data_Ref( 104 ) = 538 ;   AM1 CH2 Type
Ext_User_Prm_Data_Ref( 105 ) = 539 ;   AM1 CH3 Type
Ext_User_Prm_Data_Ref( 105 ) = 540 ;   AM2 CH1 Type
Ext_User_Prm_Data_Ref( 106 ) = 541 ;   AM2 CH2 Type
Ext_User_Prm_Data_Ref( 106 ) = 542 ;   AM2 CH3 Type
Ext_User_Prm_Data_Ref( 107 ) = 543 ;   AM1 CH1 Err Reac
Ext_User_Prm_Data_Ref( 107 ) = 544 ;   AM1 CH2 Err Reac
Ext_User_Prm_Data_Ref( 107 ) = 545 ;   AM1 CH3 Err Reac
Ext_User_Prm_Data_Ref( 107 ) = 546 ;   AM2 CH1 Err Reac
Ext_User_Prm_Data_Ref( 108 ) = 547 ;   Param To PV 1
Ext_User_Prm_Data_Ref( 109 ) = 548 ;   Param To PV 2
Ext_User_Prm_Data_Ref( 110 ) = 549 ;   Param To PV 3
Ext_User_Prm_Data_Ref( 111 ) = 550 ;   Param To PV 4
Ext_User_Prm_Data_Ref( 112 ) = 551 ;   DX1xx AO Type
Ext_User_Prm_Data_Ref( 112 ) = 552 ;   DX1xx AO Err Reac
Ext_User_Prm_Data_Ref( 113 ) = 553 ;   Param To PV 5
Ext_User_Prm_Data_Ref( 114 ) = 554 ;   Mot. op. hours level
Ext_User_Prm_Data_Ref( 115 ) = 555 ;   Mot. stand still lev
Ext_User_Prm_Data_Ref( 116 ) = 556 ;   Num Starts Overrun
Ext_User_Prm_Data_Ref( 116 ) = 557 ;   Num Starts Prewarn
Ext_User_Prm_Data_Ref( 116 ) = 558 ;   Power Scale Factor
Ext_User_Prm_Data_Ref( 117 ) = 559 ;   Backlight
Ext_User_Prm_Data_Ref( 117 ) = 560 ;   Password Protection
Ext_User_Prm_Data_Ref( 117 ) = 561 ;   Dip Enable
Ext_User_Prm_Data_Ref( 117 ) = 562 ;   Dip Autorestart Enable
Ext_User_Prm_Data_Ref( 117 ) = 563 ;   LCD Panel T Unit
Ext_User_Prm_Data_Ref( 118 ) = 564 ;   Nominal Line Voltage
Ext_User_Prm_Data_Ref( 120 ) = 565 ;   PwrFactor Trip Level
Ext_User_Prm_Data_Ref( 121 ) = 566 ;   PwrFactor Trip Delay
Ext_User_Prm_Data_Ref( 122 ) = 567 ;   PwrFactor Warn Level
Ext_User_Prm_Data_Ref( 123 ) = 568 ;   PwrFactor Warn Delay
Ext_User_Prm_Data_Ref( 124 ) = 569 ;   U Imb. Trip Level
Ext_User_Prm_Data_Ref( 125 ) = 570 ;   U Imb. Trip Delay
Ext_User_Prm_Data_Ref( 126 ) = 571 ;   U Imb. Warn Level
Ext_User_Prm_Data_Ref( 127 ) = 572 ;   U Imb. Warn Delay
Ext_User_Prm_Data_Ref( 128 ) = 573 ;   P Low Trip Level
Ext_User_Prm_Data_Ref( 129 ) = 574 ;   P Low Trip Delay
Ext_User_Prm_Data_Ref( 130 ) = 575 ;   P Low Warn Level
Ext_User_Prm_Data_Ref( 131 ) = 576 ;   P Low Warn Delay
Ext_User_Prm_Data_Ref( 132 ) = 577 ;   P High Trip Level
Ext_User_Prm_Data_Ref( 133 ) = 578 ;   P High Trip Delay
Ext_User_Prm_Data_Ref( 134 ) = 579 ;   P High Warn Level
Ext_User_Prm_Data_Ref( 135 ) = 580 ;   P High Warn Delay
Ext_User_Prm_Data_Ref( 136 ) = 581 ;   Nominal Power Factor
Ext_User_Prm_Data_Ref( 139 ) = 582 ;   THD Warning Level
Ext_User_Prm_Data_Ref( 140 ) = 583 ;   Load Startup Delay
Ext_User_Prm_Data_Ref( 141 ) = 584 ;   THD Warning Delay
EndModule


Module="UMC 100.3 (Rx100 Rx200)Profil2" 0x11, 0x21, 0x50   	; 16DI, 16DO, 1AI, I/O-Data-Profil 2
5
Ext_Module_Prm_Data_Len= 224                        ; number of used data byte
Ext_User_Prm_Data_Const(0) =    \                 ; initialising of param data
    0x00, 0x00, 0x00, 0x32, 0x00, 0x00, 0x00, 0x32, 0x02, 0x58,  \
    0x00, 0x64, 0x00, 0x78, 0xFF, 0x05, 0x00, 0x01, 0x00, 0x01,  \
    0x0A, 0x00, 0x1E, 0xA0, 0xA0, 0x05, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x03, 0x00, 0x00, 0x00, 0x00, 0x08, 0x64,  \
    0x00, 0x00, 0x02, 0xBE, 0xEB, 0xBE, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x05, 0x05, 0x05, 0x05,  \
    0x05, 0x32, 0x64, 0x00, 0x1E, 0x00, 0x06, 0x07, 0x04, 0x05,  \
    0x00, 0x05, 0x01, 0x00, 0x64, 0x00, 0x00, 0x00, 0xFF, 0x05,  \
    0x5A, 0x46, 0x00, 0x14, 0x06, 0x06, 0x00, 0x46, 0x1E, 0x46,  \
    0x1E, 0x74, 0x1E, 0x74, 0x1E, 0xFF, 0xFF, 0xFF, 0xFF, 0xFF,  \
    0xFF, 0xFF, 0xFF, 0x00, 0x00, 0x00, 0x00, 0x01, 0x02, 0x03,  \
    0x04, 0x00, 0x05, 0x00, 0x00, 0x40, 0x01, 0x01, 0x90, 0x1E,  \
    0x1E, 0x1E, 0x1E, 0xC8, 0x0A, 0xC8, 0x0A, 0x14, 0x05, 0x14,  \
    0x05, 0xC8, 0x0A, 0xC8, 0x0A, 0x64, 0x00, 0x00, 0x0A, 0x00,  \
    0x05, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,  \
    0x00, 0x00, 0x00, 0x00
Ext_User_Prm_Data_Ref( 0 ) = 401 ;   Setting Ie 1
Ext_User_Prm_Data_Ref( 4 ) = 402 ;   Setting Ie 2
Ext_User_Prm_Data_Ref( 8 ) = 403 ;   YD Starting Time
Ext_User_Prm_Data_Ref( 10 ) = 404 ;   Current Factor
Ext_User_Prm_Data_Ref( 12 ) = 405 ;   Cooling Time
Ext_User_Prm_Data_Ref( 14 ) = 406 ;   Earth Flt Trip Level
Ext_User_Prm_Data_Ref( 15 ) = 407 ;   Earth Flt Trip Delay
Ext_User_Prm_Data_Ref( 16 ) = 408 ;   Language
Ext_User_Prm_Data_Ref( 17 ) = 409 ;   Rev Lock-Out Time
Ext_User_Prm_Data_Ref( 18 ) = 410 ;   Fault Output
Ext_User_Prm_Data_Ref( 19 ) = 411 ;   Trip Class
Ext_User_Prm_Data_Ref( 20 ) = 412 ;   Low Curr Warn Level
Ext_User_Prm_Data_Ref( 21 ) = 413 ;   Low Curr Trip Level
Ext_User_Prm_Data_Ref( 22 ) = 414 ;   High Curr Warn Level
Ext_User_Prm_Data_Ref( 23 ) = 415 ;   High Curr Trip Level
Ext_User_Prm_Data_Ref( 24 ) = 416 ;   Locked Rotor Level
Ext_User_Prm_Data_Ref( 25 ) = 417 ;   Locked Rotor Delay
Ext_User_Prm_Data_Ref( 26 ) = 418 ;   Custom App Parameter
Ext_User_Prm_Data_Ref( 27 ) = 419 ;   Multif In 0
Ext_User_Prm_Data_Ref( 28 ) = 420 ;   Multif In 1
Ext_User_Prm_Data_Ref( 29 ) = 421 ;   Multif In 2
Ext_User_Prm_Data_Ref( 30 ) = 422 ;   Multif In 0 Delay
Ext_User_Prm_Data_Ref( 31 ) = 423 ;   Multif In 1 Delay
Ext_User_Prm_Data_Ref( 32 ) = 424 ;   Multif In 2 Delay
Ext_User_Prm_Data_Ref( 33 ) = 425 ;   Control Function
Ext_User_Prm_Data_Ref( 34 ) = 426 ;   Busfault Reaction
Ext_User_Prm_Data_Ref( 35 ) = 427 ;   Aux Inp 1 Reaction
Ext_User_Prm_Data_Ref( 35 ) = 428 ;   Aux Inp 2 Reaction
Ext_User_Prm_Data_Ref( 36 ) = 429 ;   Aux Inp 3 Reaction
Ext_User_Prm_Data_Ref( 36 ) = 430 ;   Aux Inp 4 Reaction
Ext_User_Prm_Data_Ref( 37 ) = 431 ;   Aux Inp 5 Reaction
Ext_User_Prm_Data_Ref( 37 ) = 432 ;   Aux Inp 6 Reaction
Ext_User_Prm_Data_Ref( 38 ) = 433 ;   PTC, Thermistor
Ext_User_Prm_Data_Ref( 38 ) = 434 ;   Check-Back
Ext_User_Prm_Data_Ref( 38 ) = 435 ;   Check Phase Sequence
Ext_User_Prm_Data_Ref( 39 ) = 436 ;   Fault Auto Reset
Ext_User_Prm_Data_Ref( 39 ) = 437 ;   Emergency Start
Ext_User_Prm_Data_Ref( 39 ) = 438 ;   Earth Flt Detection
Ext_User_Prm_Data_Ref( 39 ) = 439 ;   Address Check
Ext_User_Prm_Data_Ref( 39 ) = 440 ;   Enable Custom Logic
Ext_User_Prm_Data_Ref( 39 ) = 441 ;   YD Change-Over Mode
Ext_User_Prm_Data_Ref( 39 ) = 442 ;   Phase Loss Prot.
Ext_User_Prm_Data_Ref( 39 ) = 443 ;   Resistive Load
Ext_User_Prm_Data_Ref( 40 ) = 444 ;   DX1xx Enabled
Ext_User_Prm_Data_Ref( 40 ) = 445 ;   AI1xx AM1 Enabled
Ext_User_Prm_Data_Ref( 40 ) = 446 ;   AI1xx AM2 Enabled
Ext_User_Prm_Data_Ref( 40 ) = 447 ;   VI15x Enabled
Ext_User_Prm_Data_Ref( 40 ) = 448 ;   Missing Module React.
Ext_User_Prm_Data_Ref( 41 ) = 449 ;   Aux Inp 1 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 450 ;   Aux Inp 2 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 451 ;   Aux Inp 3 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 452 ;   Aux Inp 4 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 453 ;   Aux Inp 5 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 454 ;   Aux Inp 6 Ack Mode
Ext_User_Prm_Data_Ref( 41 ) = 455 ;   Number Of Phases
Ext_User_Prm_Data_Ref( 41 ) = 456 ;   Cooling Mode
Ext_User_Prm_Data_Ref( 42 ) = 457 ;   Invert DI Start Inp.
Ext_User_Prm_Data_Ref( 42 ) = 458 ;   Invert DI Stop Inp.
Ext_User_Prm_Data_Ref( 42 ) = 459 ;   Inching DI Start Inp
Ext_User_Prm_Data_Ref( 43 ) = 460 ;   Loc 1 Start Bus Cyc
Ext_User_Prm_Data_Ref( 43 ) = 461 ;   Loc 1 Stop Bus Cyc
Ext_User_Prm_Data_Ref( 43 ) = 462 ;   Loc 1 Start DI
Ext_User_Prm_Data_Ref( 43 ) = 463 ;   Loc 1 Stop DI
Ext_User_Prm_Data_Ref( 43 ) = 464 ;   Loc 1 Start LCD
Ext_User_Prm_Data_Ref( 43 ) = 465 ;   Loc 1 Stop LCD
Ext_User_Prm_Data_Ref( 43 ) = 466 ;   Loc 1 Start Bus Acyc
Ext_User_Prm_Data_Ref( 43 ) = 467 ;   Loc 1 Stop Bus Acyc
Ext_User_Prm_Data_Ref( 44 ) = 468 ;   Auto Start Bus Cyc
Ext_User_Prm_Data_Ref( 44 ) = 469 ;   Auto Stop Bus Cyc
Ext_User_Prm_Data_Ref( 44 ) = 470 ;   Auto Start DI
Ext_User_Prm_Data_Ref( 44 ) = 471 ;   Auto Stop DI
Ext_User_Prm_Data_Ref( 44 ) = 472 ;   Auto Start LCD
Ext_User_Prm_Data_Ref( 44 ) = 473 ;   Auto Stop LCD
Ext_User_Prm_Data_Ref( 44 ) = 474 ;   Auto Start Bus Acyc
Ext_User_Prm_Data_Ref( 44 ) = 475 ;   Auto Stop Bus Acyc
Ext_User_Prm_Data_Ref( 45 ) = 476 ;   Loc 2 Start Bus Cyc
Ext_User_Prm_Data_Ref( 45 ) = 477 ;   Loc 2 Stop Bus Cyc
Ext_User_Prm_Data_Ref( 45 ) = 478 ;   Loc 2 Start DI
Ext_User_Prm_Data_Ref( 45 ) = 479 ;   Loc 2 Stop DI
Ext_User_Prm_Data_Ref( 45 ) = 480 ;   Loc 2 Start LCD
Ext_User_Prm_Data_Ref( 45 ) = 481 ;   Loc 2 Stop LCD
Ext_User_Prm_Data_Ref( 45 ) = 482 ;   Loc 2 Start Bus Acyc
Ext_User_Prm_Data_Ref( 45 ) = 483 ;   Loc 2 Stop Bus Acyc
Ext_User_Prm_Data_Ref( 46 ) = 484 ;   Multif In 0 Autoreset
Ext_User_Prm_Data_Ref( 46 ) = 485 ;   Multif In 1 Autoreset
Ext_User_Prm_Data_Ref( 46 ) = 486 ;   Multif In 2 Autoreset
Ext_User_Prm_Data_Ref( 50 ) = 487 ;   Aux Inp 1 Delay
Ext_User_Prm_Data_Ref( 51 ) = 488 ;   Aux Inp 2 Delay
Ext_User_Prm_Data_Ref( 52 ) = 489 ;   Aux Inp 3 Delay
Ext_User_Prm_Data_Ref( 53 ) = 490 ;   Aux Inp 4 Delay
Ext_User_Prm_Data_Ref( 54 ) = 491 ;   Aux Inp 5 Delay
Ext_User_Prm_Data_Ref( 55 ) = 492 ;   Aux Inp 6 Delay
Ext_User_Prm_Data_Ref( 56 ) = 493 ;   Check-Back Time
Ext_User_Prm_Data_Ref( 57 ) = 494 ;   Low Curr Warn Delay
Ext_User_Prm_Data_Ref( 58 ) = 495 ;   Low Curr Trip Delay
Ext_User_Prm_Data_Ref( 59 ) = 496 ;   High Curr Warn Delay
Ext_User_Prm_Data_Ref( 60 ) = 497 ;   High Curr Trip Delay
Ext_User_Prm_Data_Ref( 61 ) = 498 ;   Curr Imb Trip Level
Ext_User_Prm_Data_Ref( 62 ) = 499 ;   Curr Imb Warn Level
Ext_User_Prm_Data_Ref( 63 ) = 500 ;   Phase Reversal
Ext_User_Prm_Data_Ref( 64 ) = 501 ;   Restart Level
Ext_User_Prm_Data_Ref( 65 ) = 502 ;   User Display 1
Ext_User_Prm_Data_Ref( 66 ) = 503 ;   User Display 2
Ext_User_Prm_Data_Ref( 67 ) = 504 ;   User Display 3
Ext_User_Prm_Data_Ref( 68 ) = 505 ;   User Display 4
Ext_User_Prm_Data_Ref( 69 ) = 506 ;   User Display 5
Ext_User_Prm_Data_Ref( 71 ) = 507 ;   Dip Duration
Ext_User_Prm_Data_Ref( 72 ) = 508 ;   Dip Autorestart Window
Ext_User_Prm_Data_Ref( 73 ) = 509 ;   Dip Autorestart Delay
Ext_User_Prm_Data_Ref( 74 ) = 510 ;   Thermal Load Warnlev
Ext_User_Prm_Data_Ref( 75 ) = 511 ;   Num Starts Allowed
Ext_User_Prm_Data_Ref( 76 ) = 512 ;   Num Starts Window
Ext_User_Prm_Data_Ref( 77 ) = 513 ;   Num Starts Pause
Ext_User_Prm_Data_Ref( 78 ) = 514 ;   Earth Flt Warn Level
Ext_User_Prm_Data_Ref( 79 ) = 515 ;   Earth Flt Warn Delay
Ext_User_Prm_Data_Ref( 80 ) = 516 ;   Dip Restart Level
Ext_User_Prm_Data_Ref( 81 ) = 517 ;   Dip Level
Ext_User_Prm_Data_Ref( 83 ) = 518 ;   DX1xx DI Delay
Ext_User_Prm_Data_Ref( 84 ) = 519 ;   AM1 Tmax Delay
Ext_User_Prm_Data_Ref( 85 ) = 520 ;   AM2 Tmax Delay
Ext_User_Prm_Data_Ref( 86 ) = 521 ;   AM2 CH2 Err Reac
Ext_User_Prm_Data_Ref( 86 ) = 522 ;   AM2 CH3 Err Reac
Ext_User_Prm_Data_Ref( 86 ) = 523 ;   AM1 Mode
Ext_User_Prm_Data_Ref( 86 ) = 524 ;   AM2 Mode
Ext_User_Prm_Data_Ref( 88 ) = 525 ;   U Low Trip Level
Ext_User_Prm_Data_Ref( 89 ) = 526 ;   U Low Trip Delay
Ext_User_Prm_Data_Ref( 90 ) = 527 ;   U Low Warn Level
Ext_User_Prm_Data_Ref( 91 ) = 528 ;   U Low Warn Delay
Ext_User_Prm_Data_Ref( 92 ) = 529 ;   U High Trip Level
Ext_User_Prm_Data_Ref( 93 ) = 530 ;   U High Trip Delay
Ext_User_Prm_Data_Ref( 94 ) = 531 ;   U High Warn Level
Ext_User_Prm_Data_Ref( 95 ) = 532 ;   U High Warn Delay
Ext_User_Prm_Data_Ref( 96 ) = 533 ;   AM1 Tmax Trip Level
Ext_User_Prm_Data_Ref( 98 ) = 534 ;   AM1 Tmax Warn Level
Ext_User_Prm_Data_Ref( 100 ) = 535 ;   AM2 Tmax Trip Level
Ext_User_Prm_Data_Ref( 102 ) = 536 ;   AM2 Tmax Warn Level
Ext_User_Prm_Data_Ref( 104 ) = 537 ;   AM1 CH1 Type
Ext_User_Prm_Data_Ref( 104 ) = 538 ;   AM1 CH2 Type
Ext_User_Prm_Data_Ref( 105 ) = 539 ;   AM1 CH3 Type
Ext_User_Prm_Data_Ref( 105 ) = 540 ;   AM2 CH1 Type
Ext_User_Prm_Data_Ref( 106 ) = 541 ;   AM2 CH2 Type
Ext_User_Prm_Data_Ref( 106 ) = 542 ;   AM2 CH3 Type
Ext_User_Prm_Data_Ref( 107 ) = 543 ;   AM1 CH1 Err Reac
Ext_User_Prm_Data_Ref( 107 ) = 544 ;   AM1 CH2 Err Reac
Ext_User_Prm_Data_Ref( 107 ) = 545 ;   AM1 CH3 Err Reac
Ext_User_Prm_Data_Ref( 107 ) = 546 ;   AM2 CH1 Err Reac
Ext_User_Prm_Data_Ref( 108 ) = 547 ;   Param To PV 1
Ext_User_Prm_Data_Ref( 109 ) = 548 ;   Param To PV 2
Ext_User_Prm_Data_Ref( 110 ) = 549 ;   Param To PV 3
Ext_User_Prm_Data_Ref( 111 ) = 550 ;   Param To PV 4
Ext_User_Prm_Data_Ref( 112 ) = 551 ;   DX1xx AO Type
Ext_User_Prm_Data_Ref( 112 ) = 552 ;   DX1xx AO Err Reac
Ext_User_Prm_Data_Ref( 113 ) = 553 ;   Param To PV 5
Ext_User_Prm_Data_Ref( 114 ) = 554 ;   Mot. op. hours level
Ext_User_Prm_Data_Ref( 115 ) = 555 ;   Mot. stand still lev
Ext_User_Prm_Data_Ref( 116 ) = 556 ;   Num Starts Overrun
Ext_User_Prm_Data_Ref( 116 ) = 557 ;   Num Starts Prewarn
Ext_User_Prm_Data_Ref( 116 ) = 558 ;   Power Scale Factor
Ext_User_Prm_Data_Ref( 117 ) = 559 ;   Backlight
Ext_User_Prm_Data_Ref( 117 ) = 560 ;   Password Protection
Ext_User_Prm_Data_Ref( 117 ) = 561 ;   Dip Enable
Ext_User_Prm_Data_Ref( 117 ) = 562 ;   Dip Autorestart Enable
Ext_User_Prm_Data_Ref( 117 ) = 563 ;   LCD Panel T Unit
Ext_User_Prm_Data_Ref( 118 ) = 564 ;   Nominal Line Voltage
Ext_User_Prm_Data_Ref( 120 ) = 565 ;   PwrFactor Trip Level
Ext_User_Prm_Data_Ref( 121 ) = 566 ;   PwrFactor Trip Delay
Ext_User_Prm_Data_Ref( 122 ) = 567 ;   PwrFactor Warn Level
Ext_User_Prm_Data_Ref( 123 ) = 568 ;   PwrFactor Warn Delay
Ext_User_Prm_Data_Ref( 124 ) = 569 ;   U Imb. Trip Level
Ext_User_Prm_Data_Ref( 125 ) = 570 ;   U Imb. Trip Delay
Ext_User_Prm_Data_Ref( 126 ) = 571 ;   U Imb. Warn Level
Ext_User_Prm_Data_Ref( 127 ) = 572 ;   U Imb. Warn Delay
Ext_User_Prm_Data_Ref( 128 ) = 573 ;   P Low Trip Level
Ext_User_Prm_Data_Ref( 129 ) = 574 ;   P Low Trip Delay
Ext_User_Prm_Data_Ref( 130 ) = 575 ;   P Low Warn Level
Ext_User_Prm_Data_Ref( 131 ) = 576 ;   P Low Warn Delay
Ext_User_Prm_Data_Ref( 132 ) = 577 ;   P High Trip Level
Ext_User_Prm_Data_Ref( 133 ) = 578 ;   P High Trip Delay
Ext_User_Prm_Data_Ref( 134 ) = 579 ;   P High Warn Level
Ext_User_Prm_Data_Ref( 135 ) = 580 ;   P High Warn Delay
Ext_User_Prm_Data_Ref( 136 ) = 581 ;   Nominal Power Factor
Ext_User_Prm_Data_Ref( 139 ) = 582 ;   THD Warning Level
Ext_User_Prm_Data_Ref( 140 ) = 583 ;   Load Startup Delay
Ext_User_Prm_Data_Ref( 141 ) = 584 ;   THD Warning Delay
EndModule





; DPV1 Alarm
DPV1_Slave = 1
C1_Read_Write_supp = 1
C1_Max_Data_Len                     = 8         ;The parameter specifies the maximum length of user data excluding
                                                ;Function_Num, Slot_number, Index, Length, transferred on the
                                                ;MSAC_1 communication channel.
                                                ;Type: Unsigned8 (0 .. 240)
C1_Response_Timeout = 300
Diagnostic_Alarm_supp = 0
Process_Alarm_supp = 0
Pull_Plug_Alarm_supp = 0
Status_Alarm_supp = 0
Update_Alarm_supp = 0
Manufacturer_Specific_Alarm_supp = 0
Alarm_Sequence_Mode_Count = 0
Alarm_Type_Mode_supp = 0
Diagnostic_Alarm_required = 0

C2_Read_Write_supp = 1
C2_Max_Data_Len                     = 48        ;The parameter specifies the maximum length of user data excluding
                                                ;Function_Num, Slot_number, Index, Length, transferred on the
                                                ;MSAC_2 communication channel.
                                                ;Type: Unsigned8 (0,48 .. 240)
C2_Response_Timeout = 300
C2_Read_Write_required = 1
C2_Max_Count_Channels = 3
Max_Initiate_PDU_Length             = 52        ;The parameter specifies the maximum length of an Initiate Request
                                                ;PDU including the Function_Num to the Resource Manager.
                                                ;Type: Unsigned8 (0,52.. 244)
DPV1_Data_Types                     = 0             ;

