;======================================================
;======================================================
#Profibus_DP
;	Version:	1.51 for ePlug DPV1 (PDP22)
;	created by Brigitte Dien				Date 2004-07-19
;	(based on ABB_078F for PDP21, Version:	1.5 		Date 2004-07-05)
;       modified by Lothar Schollenberger (text only)		Date 2004-18-08
;
;GSD file for the Plug PDP22 valid for:
;
;	DEVICE / ID / firmware-version / device index
;-----------------------------------------------------
;	Sensor (direct)	/ - / - / all
; 	MSD11 / 1SAJ 310000 Rxxxx / - / all
;	MSR22 / 1SAJ 320000 Rxxxx / - / all
;	MFI21 / 1SAJ 410000 R0100 / - / all
;	UMC22 / 1SAJ 510000 R0100 / V3.0  V3.10 / a30  a31
; 	UMC22 / 1SAJ 510000 R0200 / V3.20 / b32
;	PST Softstarter / - / V01  V02 / -
;	Wireless WDI100 / - / WDI100_Ver0_Rev9_5 / -
;	Sensopart / - / Revision 1.50 / -
; 
;	If additional "Ext_User_Prm_Data_Ref" numbers for new devices are defined,
;	they must fit into the following predefined ranges:
;	STO Heidelberg				range 0...999
;	Sweden 					range 1000...1999
;	Italy					range 2000...2999 
;
; 				
;=============================================================
; Text-definition for User Prm Data  "UMC22_FBP (V3.0)"
;=============================================================
;
PrmText = 2
Text(0)   = "Acknowledge"
Text(1)   = "Auto"
EndPrmText
;PrmText = 4
;Text(1)   = "Trip"
;EndPrmText
PrmText = 5
Text(0)   = "Relays Off"
Text(1)   = "Outputs Retain Status"
EndPrmText
PrmText = 6
Text(0)  = "Class  5"
Text(1)  = "Class 10"
Text(2)  = "Class 20"
Text(3)  = "Class 30"
EndPrmText
PrmText = 7
Text(1)  = "Transparent"
Text(2)  = "Overload Relay"
Text(3)  = "Direct Starter"
Text(4)  = "Reversing Starter"
Text(5)  = "Star-Delta Starter 1"
Text(6)  = "Pole-Changing Starter 1"
EndPrmText
PrmText = 16
Text(0)   = "Off"
Text(1)   = "On"
EndPrmText
PrmText = 17
Text(1)   = "Auxiliary Contacts"
Text(2)   = "Motor Current"
Text(3)   = "Simulation"
EndPrmText
PrmText = 18
Text(0)   = "Time"
Text(1)   = "Current"
EndPrmText

ExtUserPrmData =  1 "0301 Set Current 1=10mA*"
Unsigned32 50 24-6300
EndExtUserPrmData
;ExtUserPrmData =  2 "Factor for Current Transformer"
;Unsigned16 1 0-200
;EndExtUserPrmData
ExtUserPrmData =  3 "0401 Trip Class"
Unsigned8 1 0-3
Prm_Text_Ref = 6
EndExtUserPrmData
;ExtUserPrmData =  4 "Overload Behaviour"
;Unsigned8 1 1-1
;Prm_Text_Ref = 4
;EndExtUserPrmData
ExtUserPrmData =  5 "0402 Phase Loss Protection"
Unsigned8 1 0-1
Prm_Text_Ref = 16
EndExtUserPrmData
ExtUserPrmData =  6 "0407 Low Current Threshold=5%*"
Unsigned8 10 6-20
EndExtUserPrmData
ExtUserPrmData =  7 "0408 High Current Threshold=5%*"
Unsigned8 30 20-160
EndExtUserPrmData
ExtUserPrmData =  8 "0403 Cooling Time=0.1s*"
Unsigned16 1200 300-36000
EndExtUserPrmData
ExtUserPrmData =  9 "0404 Automatic fault reset"
Unsigned8 0 0-1
Prm_Text_Ref = 2
EndExtUserPrmData
ExtUserPrmData = 10 "0101 Control Function"
Unsigned8 1 1-6
Prm_Text_Ref = 7
EndExtUserPrmData
ExtUserPrmData = 11 "0202 Check Back"
Unsigned8 2 1-3
Prm_Text_Ref = 17
EndExtUserPrmData
ExtUserPrmData = 12 "0207 Star-Delta Start.Time=0.1s*"
Unsigned16 600 10-36000
EndExtUserPrmData
ExtUserPrmData = 13 "0205 Revers. Lockout Time=0.1s*"
Unsigned16 20 2-36000
EndExtUserPrmData
;ExtUserPrmData = 14 "0601 Operating Hours of Motor"
;Unsigned32 0 0-15000000
;EndExtUserPrmData
;ExtUserPrmData = 15 "0602 Number of Starts"
;Unsigned32 0 0-15000000
;EndExtUserPrmData
ExtUserPrmData = 16 "0501 Commun. fault reaction"
Unsigned8 0 0-1
Prm_Text_Ref = 5
EndExtUserPrmData
ExtUserPrmData = 17 "0405 Start Up Time=0.1s*"
Unsigned16 1200 0-6000
EndExtUserPrmData
ExtUserPrmData = 18 "0201 Local Control via DIs"
Unsigned8 0 0-1
Prm_Text_Ref = 16
EndExtUserPrmData
ExtUserPrmData = 19 "0406 Block.Current Threshold=5%*"
Unsigned8 160 0-160
EndExtUserPrmData
ExtUserPrmData = 20 "0204 Fault Output"
Unsigned8 0 0-1
Prm_Text_Ref = 16
EndExtUserPrmData
ExtUserPrmData = 21 "0206 Star-Delta Changeover Mode"
Unsigned8 1 0-1
Prm_Text_Ref = 18
EndExtUserPrmData
ExtUserPrmData = 23 "0302 Set Current 2=10mA*"
Unsigned32 50 24-6300
EndExtUserPrmData
ExtUserPrmData = 24 "0203 Fault Input"
Unsigned8 0 0-1
Prm_Text_Ref = 16
EndExtUserPrmData
ExtUserPrmData = 25 "0502 Address Check"
Unsigned8 0 0-1
Prm_Text_Ref = 16
EndExtUserPrmData
;
;=============================================================
; Text-definition for User Prm Data  "UMC22_FBP (V3.10, V3.20)"
;=============================================================
;
PrmText = 102
Text(0)   = "Disabled"
Text(1)   = "Autoreset"
EndPrmText
;PrmText = 104
;Text(1)   = "Trip"
;EndPrmText
PrmText = 105
Text(0)   = "Relays Off"
Text(1)   = "Outputs Retain Status"
EndPrmText
PrmText = 106
Text(0)  = "Class  5"
Text(1)  = "Class 10"
Text(2)  = "Class 20"
Text(3)  = "Class 30"
EndPrmText
PrmText = 107
Text(1)  = "Transparent"
Text(2)  = "Overload Relay"
Text(3)  = "Direct Starter"
Text(4)  = "Reversing Starter"
Text(5)  = "Star-Delta Starter 1"
Text(6)  = "Pole-Changing Starter 1"
EndPrmText
PrmText = 116
Text(0)   = "Off"
Text(1)   = "On"
EndPrmText
PrmText = 117
Text(1)   = "Auxiliary Contacts"
Text(2)   = "Motor Current"
Text(3)   = "Simulation"
EndPrmText
PrmText = 118
Text(0)   = "Time"
Text(1)   = "Current"
EndPrmText

ExtUserPrmData = 101 "01 Set Current 1=10mA*"
Unsigned32 50 24-6300
EndExtUserPrmData
ExtUserPrmData = 102 "02 Current Factor"
Unsigned16 1 0-200
EndExtUserPrmData
ExtUserPrmData = 103 "04 Trip Class"
Unsigned8 1 0-3
Prm_Text_Ref = 106
EndExtUserPrmData
;ExtUserPrmData =  104 "05 Overload Behaviour"
;Unsigned8 1 1-1
;Prm_Text_Ref = 4
;EndExtUserPrmData
ExtUserPrmData =  105 "06 Phase Loss Protection"
Unsigned8 1 0-1
Prm_Text_Ref = 116
EndExtUserPrmData
ExtUserPrmData =  106 "08 Low Current Threshold=5%*"
Unsigned8 10 6-20
EndExtUserPrmData
ExtUserPrmData =  107 "09 High Current Threshold=5%*"
Unsigned8 30 20-160
EndExtUserPrmData
ExtUserPrmData =  108 "10 Cooling Time=0.1s*"
Unsigned16 1200 300-36000
EndExtUserPrmData
ExtUserPrmData =  109 "11 Automatic fault reset"
Unsigned8 0 0-1
Prm_Text_Ref = 102
EndExtUserPrmData
ExtUserPrmData = 110 "12 Control Function"
Unsigned8 1 1-6
Prm_Text_Ref = 107
EndExtUserPrmData
ExtUserPrmData = 111 "13 Check-Back"
Unsigned8 2 1-3
Prm_Text_Ref = 117
EndExtUserPrmData
ExtUserPrmData = 112 "16 Star-Delta Start.Time=0.1s*"
Unsigned16 600 10-36000
EndExtUserPrmData
ExtUserPrmData = 113 "17 Reverse Lockout Time=0.1s*"
Unsigned16 20 2-36000
EndExtUserPrmData
ExtUserPrmData = 114 "18 Operating Hours of Motor"
Unsigned16 0 0-65535
EndExtUserPrmData
ExtUserPrmData = 115 "19 Number of Starts"
Unsigned32 0 0-1000000
EndExtUserPrmData
ExtUserPrmData = 116 "20 Bus fault reaction"
Unsigned8 0 0-1
Prm_Text_Ref = 105
EndExtUserPrmData
ExtUserPrmData = 117 "14 Start-Up Time=0.1s*"
Unsigned16 1200 0-6000
EndExtUserPrmData
ExtUserPrmData = 118 "22 Local Control via DIs"
Unsigned8 0 0-1
Prm_Text_Ref = 116
EndExtUserPrmData
ExtUserPrmData = 119 "23 Block.Current Threshold=5%*"
Unsigned8 160 0-160
EndExtUserPrmData
ExtUserPrmData = 120 "24 Fault Output"
Unsigned8 0 0-1
Prm_Text_Ref = 116
EndExtUserPrmData
ExtUserPrmData = 121 "15 Star-Delta Changeover Mode"
Unsigned8 1 0-1
Prm_Text_Ref = 118
EndExtUserPrmData
ExtUserPrmData = 123 "03 Set Current 2=10mA*"
Unsigned32 50 24-6300
EndExtUserPrmData
ExtUserPrmData = 124 "21 Fault Input"
Unsigned8 0 0-1
Prm_Text_Ref = 116
EndExtUserPrmData
ExtUserPrmData = 125 "26 Address Check"
Unsigned8 0 0-1
Prm_Text_Ref = 116
EndExtUserPrmData
ExtUserPrmData = 126 "25 Number of Trips"
Unsigned8 0 0-255
EndExtUserPrmData
;ExtUserPrmData = 127 "07 Load type"
;Unsigned8 1 1-1
;EndExtUserPrmData
;
;=============================================================
; Text-definition for User Prm Data "MFI21-FBP"
;=============================================================
;
PrmText=50
Text(0)= "No Configuration"
Text(1)= "Direct, FB=Off"
Text(2)= "Direct, FB=On"
Text(3)= "Reverse, FB=Off"
Text(4)= "Reverse, FB=On"
Text(5)= "Star-Delta, FB=Off"
Text(6)= "Star-Delta, FB=On"
Text(7)= "MFI Transparent"
EndPrmText

ExtUserPrmData=50	"MFI Mode"			; MFI application mode
Unsigned8 0 0-7								; Default 0, range 0..7
Prm_Text_Ref=50								; Reference to PrmText 50
EndExtUserPrmData

ExtUserPrmData=51   "Start-Delta Time = 1ms*"	; MFI delay time in ms
Unsigned32 50 50-260100		   	; Default 50 ms, range 50..260100 ms
EndExtUserPrmData
;
;=============================================================
; Text-definition for User Prm Data "Softstarter PST(V01)"
;=============================================================
;
PrmText = 1008
Text(0)   = "Disable"
Text(1)   = "Enable"
EndPrmText
PrmText = 1011
Text(0)   = "1-30s"
Text(1)   = "1-120s"
EndPrmText
PrmText = 1012
Text(0)   = "0-30s"
Text(1)   = "0-120s"
EndPrmText
PrmText = 1013
Text(0)   = "No"
Text(1)   = "Normal"
Text(2)   = "Dual"
EndPrmText
PrmText = 1014
Text(0)   = "Class 5"
Text(1)  = "Class 10"
Text(2)  = "Class 20"
Text(3)  = "Class 30"
EndPrmText
PrmText = 1017
Text(0)   = "Stop-M"
Text(1)   = "Stop-A"
Text(2)   = "Ind"
EndPrmText
PrmText = 1036
Text(0)   = "Stop-M"
Text(1)   = "Stop-A"
EndPrmText
PrmText = 1049
Text(0)  = "None"
Text(1)  = "Reset"
Text(2)  = "Enable"
Text(3)  = "Jog"
Text(4)  = "DOL-On"
Text(5)  = "Start2"
EndPrmText
PrmText = 1050
Text(0)  = "None"
Text(1)  = "Reset"
Text(2)  = "Enable"
Text(3)  = "Jog"
Text(4)  = "DOL-On"
Text(5)  = "Start3"
EndPrmText
PrmText = 1051
Text(0)   = "Run"
Text(1)   = "TOR"
Text(2)   = "Event"
EndPrmText
PrmText = 1060
Text(0)   = "AS-I"
Text(1)   = "Other"
EndPrmText
PrmText = 1062
Text(0)   = "No"
Text(1)   = "2"
Text(2)   = "3"
EndPrmText
PrmText = 1075
Text(0)  = "US/UK"
Text(1)  = "FI"
Text(2)  = "SE"
Text(3)  = "PT"
Text(4)  = "NL"
Text(5)  = "IT"
Text(6)  = "FR"
Text(7)  = "ES"
Text(8)  = "DE"
Text(9)  = "CN"
EndPrmText
PrmText = 1079
Text(0)   = "ISO"
Text(1)   = "CE"
Text(2)   = "US"
EndPrmText

ExtUserPrmData = 1001 "Setting Ie = 0.1A *"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 1002 "Start Ramp [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 1003 "Stop Ramp  [s]"
Unsigned16 0 0-120
EndExtUserPrmData

ExtUserPrmData = 1004 "Init Volt  [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 1005 "End Volt   [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 1006 "Step Down  [%]"
Unsigned16 100 30-100
EndExtUserPrmData

ExtUserPrmData = 1007 "Current Lim = 0.1 * Ie *"
Unsigned16 40 20-50
EndExtUserPrmData

ExtUserPrmData = 1008 "Kick Start"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData = 1009 "Kick Level  [%]"
Unsigned16 50 50-100
EndExtUserPrmData

ExtUserPrmData = 1010 "Kick Time = 0.01s *"
Unsigned16 20 10-150
EndExtUserPrmData

ExtUserPrmData = 1011 "Start Range"
Unsigned16 0 0-1
Prm_Text_Ref=1011
EndExtUserPrmData

ExtUserPrmData = 1012 "Stop Range"
Unsigned16 0 0-1
Prm_Text_Ref=1012
EndExtUserPrmData

ExtUserPrmData = 1013 "Overload"
Unsigned16 1 0-2
Prm_Text_Ref=1013
EndExtUserPrmData

ExtUserPrmData = 1014 "OL Class"
Unsigned16 1 0-3
Prm_Text_Ref=1014
EndExtUserPrmData

ExtUserPrmData= 1015 "OL Class S"
Unsigned16 1 0-3
Prm_Text_Ref=1014
EndExtUserPrmData

ExtUserPrmData= 1016 "OL Class R"
Unsigned16 1 0-3
Prm_Text_Ref=1014
EndExtUserPrmData

ExtUserPrmData= 1017 "OL Op"
Unsigned16 0 0-2
Prm_Text_Ref=1017
EndExtUserPrmData

ExtUserPrmData= 1018 "Locked Rotor"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData= 1019 "Lock R Lev = 0.1 * Ie *"
Unsigned16 40 30-80
EndExtUserPrmData

ExtUserPrmData= 1020 "Lock R Time = 0.1s *"
Unsigned16 10 2-100
EndExtUserPrmData

ExtUserPrmData= 1021 "Lock R Op"
Unsigned16 0 0-2
Prm_Text_Ref=1017
EndExtUserPrmData

ExtUserPrmData= 1022 "Underload"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData= 1023 "Underl Lev = 0.1 * Ie *"
Unsigned16 8 4-8
EndExtUserPrmData

ExtUserPrmData= 1024 "Underl Time  [s]"
Unsigned16 10 1-30
EndExtUserPrmData

ExtUserPrmData=1025 "Underl Op"
Unsigned16 0 0-2
Prm_Text_Ref=1017
EndExtUserPrmData

ExtUserPrmData = 1026 "Phase Imb"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData= 1027 "Ph Imb Lev [%]"
Unsigned16 80 10-80
EndExtUserPrmData

ExtUserPrmData= 1028 "Ph Imb Op"
Unsigned16 0 0-2
Prm_Text_Ref=1017
EndExtUserPrmData

ExtUserPrmData = 1029 "High I"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData=1030 "High I Op"
Unsigned16 0 0-2
Prm_Text_Ref=1017
EndExtUserPrmData

ExtUserPrmData = 1031 "Phase Rev"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData=1032 "Ph Rev Op"
Unsigned16 0 0-2
Prm_Text_Ref=1017
EndExtUserPrmData

ExtUserPrmData = 1033 "PTC"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData=1034 "PTC Op"
Unsigned16 0 0-2
Prm_Text_Ref=1017
EndExtUserPrmData

ExtUserPrmData=1035 "Ext ByPass"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData
;36
ExtUserPrmData=1036 "BP Fault Op"
Unsigned16 0 0-2
Prm_Text_Ref=1036
EndExtUserPrmData

ExtUserPrmData = 1037 "Warn I=High"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData=1038 "Wa I=H Lev = 0.1* Ie *"
Unsigned16 12 5-50
EndExtUserPrmData

ExtUserPrmData = 1039 "Warn I=Low"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData= 1040 "Wa I=L Lev = 0.1 * Ie *"
Unsigned16 5 4-10
EndExtUserPrmData

ExtUserPrmData = 1041 "Warn OL"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData= 1042 "Wa OL Lev   [%]"
Unsigned16 90 40-99
EndExtUserPrmData

ExtUserPrmData = 1043 "Warn SCR OL"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData= 1044 "Ph Loss Op"
Unsigned16 0 0-1
Prm_Text_Ref=1036
EndExtUserPrmData

ExtUserPrmData= 1045 "FB Fault Op"
Unsigned16 0 0-1
Prm_Text_Ref=1036
EndExtUserPrmData

ExtUserPrmData= 1046 "Freq F Op"
Unsigned16 0 0-1
Prm_Text_Ref=1036
EndExtUserPrmData

ExtUserPrmData=1047 "Overtemp Op"
Unsigned16 0 0-1
Prm_Text_Ref=1036
EndExtUserPrmData

ExtUserPrmData=1048 "SCR SC Op"
Unsigned16 0 0-1
Prm_Text_Ref=1036
EndExtUserPrmData

ExtUserPrmData = 1049 "In0 - Read only"
Unsigned16 0 0-5
Prm_Text_Ref=1049
EndExtUserPrmData

ExtUserPrmData = 1050 "In1 - Read only"
Unsigned16 0 0-5
Prm_Text_Ref=1050
EndExtUserPrmData

ExtUserPrmData= 1051 "Relay K4"
Unsigned16 0 0-2
Prm_Text_Ref=1051
EndExtUserPrmData

ExtUserPrmData= 1052 "Relay K5"
Unsigned16 1 0-2
Prm_Text_Ref=1051
EndExtUserPrmData

ExtUserPrmData= 1053 "Relay K6"
Unsigned16 2 0-2
Prm_Text_Ref=1051
EndExtUserPrmData

ExtUserPrmData = 1054 "SW Outp V7"
Unsigned16 2 0-2
Prm_Text_Ref=1051
EndExtUserPrmData

ExtUserPrmData= 1055 "Event K4"
Unsigned16 0 0-65535
EndExtUserPrmData
;57
ExtUserPrmData= 1056 "Event K5"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData= 1057 "Event K6"
Unsigned16 7 0-65535
EndExtUserPrmData

ExtUserPrmData= 1058 "Event V7"
Unsigned16 7 0-65535
EndExtUserPrmData

ExtUserPrmData = 1059 "Fieldb Ctrl - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData = 1060 "Fieldb Type - Read only"
Unsigned16 1 0-1
Prm_Text_Ref=1060
EndExtUserPrmData

ExtUserPrmData = 1061 "Fieldb Addr - Read only"
Unsigned16 0 0-1000
EndExtUserPrmData

ExtUserPrmData = 1062 "No of Seq"
Unsigned16 0 0-2
Prm_Text_Ref=1062
EndExtUserPrmData

ExtUserPrmData= 1063 "StartRamp1 [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData= 1064 "Init Volt1 [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData= 1065 "Curr Lim1 = 0.1 * Ie *"
Unsigned16 40 20-50
EndExtUserPrmData

ExtUserPrmData= 1066 "1st Set Ie = 0.1A *"
Unsigned16 1000 0-10000
EndExtUserPrmData

ExtUserPrmData= 1067 "StartRamp2   [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData= 1068 "Init Volt2[%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData= 1069 "Curr Lim2 = 0.1 * Ie *"
Unsigned16 40 20-50
EndExtUserPrmData

ExtUserPrmData= 1070 "2nd Set Ie = 0.1A *"
Unsigned16 1000 0-10000
EndExtUserPrmData

ExtUserPrmData= 1071 "StartRamp3   [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData= 1072 "Init Volt3[%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData= 1073 "Curr Lim3 = 0.1 * Ie *"
Unsigned16 40 20-50
EndExtUserPrmData

ExtUserPrmData= 1074 "3rd Set Ie = 0.1A *"
Unsigned16 1000 0-10000
EndExtUserPrmData

ExtUserPrmData = 1075 "Language - Read only"
Unsigned16 0 0-9
Prm_Text_Ref=1075
EndExtUserPrmData

ExtUserPrmData = 1076 "Dummy76 - Read only"
Unsigned16 0 0-0
EndExtUserPrmData

ExtUserPrmData = 1077 "LCD Auto Off - Read only [min]"
Unsigned16 15 1-255
EndExtUserPrmData

ExtUserPrmData = 1078 "Password - Read only"
Unsigned16 0 0-255
EndExtUserPrmData

ExtUserPrmData = 1079 "Date Type - Read only"
Unsigned16 0 0-2
Prm_Text_Ref=1079
EndExtUserPrmData

ExtUserPrmData = 1080 "Date Year - Read only"
Unsigned16 2003 2001-2060
EndExtUserPrmData

ExtUserPrmData = 1081 "Date Month - Read only"
Unsigned16 6 1-12
EndExtUserPrmData

ExtUserPrmData = 1082 "Date Day - Read only"
Unsigned16 15 1-31
EndExtUserPrmData

ExtUserPrmData = 1083 "Time Hour - Read only"
Unsigned16 12 0-23
EndExtUserPrmData

ExtUserPrmData = 1084 "Time Min - Read only"
Unsigned16 30 0-59
EndExtUserPrmData

ExtUserPrmData = 1085 "S Port Ctrl - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData = 1086 "S Port Addr1 - Read only"
Unsigned16 123 0-255
EndExtUserPrmData

ExtUserPrmData = 1087 "S Port Addr2 - Read only"
Unsigned16 123 0-255
EndExtUserPrmData

ExtUserPrmData = 1088 "S Port Addr3 - Read only"
Unsigned16 123 0-255
EndExtUserPrmData

ExtUserPrmData = 1089 "S Port Addr4 - Read only"
Unsigned16 123 0-255
EndExtUserPrmData

ExtUserPrmData = 1090 "CT Ratio Ir [A] - Read only"
Unsigned16 0 0-2500
EndExtUserPrmData

ExtUserPrmData = 1091 "IntByPass - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1008
EndExtUserPrmData

ExtUserPrmData = 1092 "ByPass AC3 [A] - Read only"
Unsigned16 0 0-2500
EndExtUserPrmData

ExtUserPrmData = 1093 "SOP1= 0.01*  - Read only"
Unsigned16 100 70-120
EndExtUserPrmData

ExtUserPrmData = 1094 "SOP2= 0.01*  - Read only"
Unsigned16 100 5-2000
EndExtUserPrmData

ExtUserPrmData = 1095 "SOP3= 0.001*  - Read only"
Unsigned16 100 11-1200
EndExtUserPrmData

ExtUserPrmData = 1096 "SOP4= 0.1*  - Read only"
Unsigned16 100 10-200
EndExtUserPrmData
;
;=============================================================
; Text-definition for User Prm Data "Softstarter PST(V02)"
;=============================================================
;
PrmText = 1108
Text(0)   = "No"
Text(1)   = "Yes"
EndPrmText
PrmText = 1111
Text(0)   = "1-30s"
Text(1)   = "1-120s"
EndPrmText
PrmText = 1112
Text(0)   = "0-30s"
Text(1)   = "0-120s"
EndPrmText
PrmText = 1113
Text(0)   = "No"
Text(1)   = "Normal"
Text(2)   = "Dual"
EndPrmText
PrmText = 1114
Text(0)  = "Class 10A"
Text(1)  = "Class 10"
Text(2)  = "Class 20"
Text(3)  = "Class 30"
EndPrmText
PrmText = 1117
Text(0)   = "Stop-M"
Text(1)   = "Stop-A"
Text(2)   = "Ind"
EndPrmText
PrmText = 1136
Text(0)   = "Stop-M"
Text(1)   = "Stop-A"
EndPrmText
PrmText = 1149
Text(0)  = "None"
Text(1)  = "Reset"
Text(2)  = "Enable"
Text(3)  = "Jog"
Text(4)  = "DOL-On"
Text(5)  = "Start2"
Text(6)  = "FB-Dis"
EndPrmText
PrmText = 1150
Text(0)  = "None"
Text(1)  = "Reset"
Text(2)  = "Enable"
Text(3)  = "Jog"
Text(4)  = "DOL-On"
Text(5)  = "Start3"
Text(6)  = "FB-Dis"
EndPrmText
PrmText = 1151
Text(0)   = "Run"
Text(1)   = "TOR"
Text(2)   = "Event"
EndPrmText
PrmText = 1160
Text(0)   = "AS-Int"
Text(1)   = "Other"
EndPrmText
PrmText = 1162
Text(1)   = "No"
Text(2)   = "2"
Text(3)   = "3"
EndPrmText
PrmText = 1175
Text(1)  = "US/UK"
Text(2)  = "FI"
Text(3)  = "SE"
Text(4)  = "PT"
Text(5)  = "NL"
Text(6)  = "IT"
Text(7)  = "FR"
Text(8)  = "ES"
Text(9)  = "DE"
Text(10)  = "CN"
Text(11)  = "RU"
EndPrmText
PrmText = 1179
Text(0)   = "ISO"
Text(1)   = "CE"
Text(2)   = "US"
EndPrmText

ExtUserPrmData = 1101 "Setting Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 1102 "Start Ramp [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData = 1103 "Stop Ramp  [s]"
Unsigned16 0 0-120
EndExtUserPrmData

ExtUserPrmData = 1104 "Init Volt  [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 1105 "End Volt   [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData = 1106 "Step Down  [%]"
Unsigned16 100 30-100
EndExtUserPrmData

ExtUserPrmData = 1107 "Current Lim [0.1*Ie]"
Unsigned16 40 20-50
EndExtUserPrmData

ExtUserPrmData = 1108 "Kick Start"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData = 1109 "Kick Level  [%]"
Unsigned16 50 50-100
EndExtUserPrmData

ExtUserPrmData = 1110 "Kick Time [0.01s]"
Unsigned16 20 10-150
EndExtUserPrmData

ExtUserPrmData = 1111 "Start Range"
Unsigned16 0 0-1
Prm_Text_Ref=1111
EndExtUserPrmData

ExtUserPrmData = 1112 "Stop Range"
Unsigned16 0 0-1
Prm_Text_Ref=1112
EndExtUserPrmData

ExtUserPrmData = 1113 "Overload"
Unsigned16 1 0-2
Prm_Text_Ref=1113
EndExtUserPrmData

ExtUserPrmData = 1114 "OL Class"
Unsigned16 1 0-3
Prm_Text_Ref=1114
EndExtUserPrmData

ExtUserPrmData= 1115 "OL Class S"
Unsigned16 1 0-3
Prm_Text_Ref=1114
EndExtUserPrmData

ExtUserPrmData= 1116 "OL Class R"
Unsigned16 1 0-3
Prm_Text_Ref=1114
EndExtUserPrmData

ExtUserPrmData= 1117 "OL Op"
Unsigned16 0 0-2
Prm_Text_Ref=1117
EndExtUserPrmData

ExtUserPrmData= 1118 "Locked Rotor"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData= 1119 "Lock R Lev [0.1*Ie]"
Unsigned16 40 30-80
EndExtUserPrmData

ExtUserPrmData= 1120 "Lock R Time [0.1s]"
Unsigned16 10 2-100
EndExtUserPrmData

ExtUserPrmData= 1121 "Lock R Op"
Unsigned16 0 0-2
Prm_Text_Ref=1117
EndExtUserPrmData

ExtUserPrmData= 1122 "Underload"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData= 1123 "Underl Lev [0.1*Ie]"
Unsigned16 8 4-8
EndExtUserPrmData

ExtUserPrmData= 1124 "Underl Time [s]"
Unsigned16 10 1-30
EndExtUserPrmData

ExtUserPrmData=1125 "Underl Op"
Unsigned16 0 0-2
Prm_Text_Ref=1117
EndExtUserPrmData

ExtUserPrmData = 1126 "Phase Imb"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData= 1127 "Ph Imb Lev [%]"
Unsigned16 80 10-80
EndExtUserPrmData

ExtUserPrmData= 1128 "Ph Imb Op"
Unsigned16 0 0-2
Prm_Text_Ref=1117
EndExtUserPrmData

ExtUserPrmData = 1129 "High I"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData=1130 "High I Op"
Unsigned16 0 0-2
Prm_Text_Ref=1117
EndExtUserPrmData

ExtUserPrmData = 1131 "Phase Rev"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData=1132 "Ph Rev Op"
Unsigned16 0 0-2
Prm_Text_Ref=1117
EndExtUserPrmData

ExtUserPrmData = 1133 "PTC"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData=1134 "PTC Op"
Unsigned16 0 0-2
Prm_Text_Ref=1117
EndExtUserPrmData

ExtUserPrmData=1135 "Ext ByPass"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData
;36
ExtUserPrmData=1136 "BP Fault Op"
Unsigned16 0 0-1
Prm_Text_Ref=1136
EndExtUserPrmData

ExtUserPrmData = 1137 "Warn I=High"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData=1138 "Wa I=H Lev [0.1*Ie]"
Unsigned16 12 5-50
EndExtUserPrmData

ExtUserPrmData = 1139 "Warn I=Low"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData= 1140 "Wa I=L Lev [0.1*Ie]"
Unsigned16 5 4-10
EndExtUserPrmData

ExtUserPrmData = 1141 "Warn OL"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData= 1142 "Wa OL Lev  [%]"
Unsigned16 90 40-99
EndExtUserPrmData

ExtUserPrmData = 1143 "Warn SCR OL"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData= 1144 "Ph Loss Op"
Unsigned16 0 0-1
Prm_Text_Ref=1136
EndExtUserPrmData

ExtUserPrmData= 1145 "FB Fault Op"
Unsigned16 0 0-1
Prm_Text_Ref=1136
EndExtUserPrmData

ExtUserPrmData= 1146 "Freq F Op"
Unsigned16 0 0-1
Prm_Text_Ref=1136
EndExtUserPrmData

ExtUserPrmData=1147 "HC Temp Op"
Unsigned16 0 0-1
Prm_Text_Ref=1136
EndExtUserPrmData

ExtUserPrmData=1148 "SCR SC Op"
Unsigned16 0 0-1
Prm_Text_Ref=1136
EndExtUserPrmData

ExtUserPrmData = 1149 "In0 - Read only"
Unsigned16 1 0-6
Prm_Text_Ref=1149
EndExtUserPrmData

ExtUserPrmData = 1150 "In1 - Read only"
Unsigned16 1 0-6
Prm_Text_Ref=1150
EndExtUserPrmData

ExtUserPrmData= 1151 "Relay K4"
Unsigned16 0 0-2
Prm_Text_Ref=1151
EndExtUserPrmData

ExtUserPrmData= 1152 "Relay K5"
Unsigned16 1 0-2
Prm_Text_Ref=1151
EndExtUserPrmData

ExtUserPrmData= 1153 "Relay K6"
Unsigned16 2 0-2
Prm_Text_Ref=1151
EndExtUserPrmData

ExtUserPrmData = 1154 "SW Outp V7"
Unsigned16 2 0-2
Prm_Text_Ref=1151
EndExtUserPrmData

ExtUserPrmData= 1155 "Event K4"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData= 1156 "Event K5"
Unsigned16 0 0-65535
EndExtUserPrmData

ExtUserPrmData= 1157 "Event K6"
Unsigned16 7 0-65535
EndExtUserPrmData

ExtUserPrmData= 1158 "Event V7"
Unsigned16 7 0-65535
EndExtUserPrmData

ExtUserPrmData = 1159 "Fieldb Ctrl - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData = 1160 "Fieldb Type - Read only"
Unsigned16 1 0-1
Prm_Text_Ref=1160
EndExtUserPrmData

ExtUserPrmData = 1161 "Fieldb Addr - Read only"
Unsigned16 0 0-1000
EndExtUserPrmData

ExtUserPrmData = 1162 "No of Seq"
Unsigned16 1 1-3
Prm_Text_Ref=1162
EndExtUserPrmData

ExtUserPrmData= 1163 "StartRamp1 [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData= 1164 "Init Volt1 [%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData= 1165 "Curr Lim1 [0.1*Ie]"
Unsigned16 40 20-70
EndExtUserPrmData

ExtUserPrmData= 1166 "1st Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData= 1167 "StartRamp2  [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData= 1168 "Init Volt2 [%]"
Unsigned16 30 30-70
EndExtUserPrmData
;75
ExtUserPrmData= 1169 "Curr Lim2 [0.1*Ie]"
Unsigned16 40 20-70
EndExtUserPrmData

ExtUserPrmData= 1170 "2nd Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData= 1171 "StartRamp3  [s]"
Unsigned16 10 1-120
EndExtUserPrmData

ExtUserPrmData= 1172 "Init Volt3[%]"
Unsigned16 30 30-70
EndExtUserPrmData

ExtUserPrmData= 1173 "Curr Lim3 [0.1*Ie]"
Unsigned16 40 20-70
EndExtUserPrmData

ExtUserPrmData= 1174 "3rd Set Ie [0.1A]"
Unsigned16 1 0-30000
EndExtUserPrmData

ExtUserPrmData = 1175 "Language - Read only"
Unsigned16 1 1-11
Prm_Text_Ref=1175
EndExtUserPrmData

ExtUserPrmData = 1176 "Dummy76 - Read only"
Unsigned16 0 0-15
EndExtUserPrmData

ExtUserPrmData = 1177 "LCD Auto Off - Read only [min]"
Unsigned16 15 1-255
EndExtUserPrmData

ExtUserPrmData = 1178 "Password - Read only"
Unsigned16 0 0-255
EndExtUserPrmData

ExtUserPrmData = 1179 "Date Type - Read only"
Unsigned16 0 0-2
Prm_Text_Ref=1179
EndExtUserPrmData

ExtUserPrmData = 1180 "Date Year - Read only"
Unsigned16 2002 2001-2060
EndExtUserPrmData

ExtUserPrmData = 1181 "Date Month - Read only"
Unsigned16 6 1-12
EndExtUserPrmData

ExtUserPrmData = 1182 "Date Day - Read only"
Unsigned16 15 1-31
EndExtUserPrmData

ExtUserPrmData = 1183 "Time Hour - Read only"
Unsigned16 12 0-23
EndExtUserPrmData

ExtUserPrmData = 1184 "Time Min - Read only"
Unsigned16 30 0-59
EndExtUserPrmData

ExtUserPrmData = 1185 "S Port Ctrl - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData = 1186 "S Port Addr1 - Read only"
Unsigned16 192 0-255
EndExtUserPrmData

ExtUserPrmData = 1187 "S Port Addr2 - Read only"
Unsigned16 168 0-255
EndExtUserPrmData

ExtUserPrmData = 1188 "S Port Addr3 - Read only"
Unsigned16 0 0-255
EndExtUserPrmData

ExtUserPrmData = 1189 "S Port Addr4 - Read only"
Unsigned16 2 0-255
EndExtUserPrmData

ExtUserPrmData = 1190 "CT Ratio Ir [A] - Read only"
Unsigned16 100 1-2500
EndExtUserPrmData

ExtUserPrmData = 1191 "IntByPass - Read only"
Unsigned16 0 0-1
Prm_Text_Ref=1108
EndExtUserPrmData

ExtUserPrmData = 1192 "ByPass AC3 [A] - Read only"
Unsigned16 0 0-2500
EndExtUserPrmData

ExtUserPrmData = 1193 "SOP1 [0.01] - Read only"
Unsigned16 95 70-120
EndExtUserPrmData

ExtUserPrmData = 1194 "SOP2 [0.01] - Read only"
Unsigned16 1000 5-2000
EndExtUserPrmData

ExtUserPrmData = 1195 "SOP3 [0.001] - Read only"
Unsigned16 600 11-1200
EndExtUserPrmData

ExtUserPrmData = 1196 "SOP4 [0.1] - Read only"
Unsigned16 40 10-200
EndExtUserPrmData
;
;=============================================================
; Definition for Ext User Prm Data "Wireless WDI100"
;=============================================================
;
ExtUserPrmData= 204	"Cell ID"					; Cell ID WDI100
Unsigned16 0 0-60									; Default 0, Bereich 0..60
EndExtUserPrmData

ExtUserPrmData= 205	"Sensors   1...16"	; 
Unsigned16 0 0-65535								; 
EndExtUserPrmData

ExtUserPrmData= 206	"Sensors  17...32"	; 
Unsigned16 0 0-65535								; 
EndExtUserPrmData

ExtUserPrmData= 207	"Sensors  33...48"	; 
Unsigned16 0 0-65535								; 
EndExtUserPrmData

ExtUserPrmData= 208	"Sensors  49...64"	; 
Unsigned16 0 0-65535								; 
EndExtUserPrmData

ExtUserPrmData= 209	"Sensors  65...80"	; 
Unsigned16 0 0-65535								; 
EndExtUserPrmData

ExtUserPrmData=210	"Sensors  81...96"	; 
Unsigned16 0 0-65535								; 
EndExtUserPrmData

ExtUserPrmData=211	"Sensors  97..112"	; 
Unsigned16 0 0-65535								; 
EndExtUserPrmData

ExtUserPrmData=212	"Sensors 113..120"	; 
Unsigned16 0 0-255  								; 
EndExtUserPrmData


;=====================================================================
; special Parameter-Definitions for DPV1-Plug PDP22
;=====================================================================
PrmText = 10000
Text(0)   = "Use Block-Parameters"
Text(1)   = "Ignore Block-Parameters"
EndPrmText

ExtUserPrmData=10000	"Block-Parameter"	; 
Unsigned8 0 0-1    								; 
Prm_Text_Ref=10000
EndExtUserPrmData

;
;===========================================================
;General parameters
;===========================================================
;
GSD_Revision   =3
Vendor_Name    ="ABB"
Model_Name     ="PDP22-FBP ABB"
Revision       ="V 1.0"
Ident_Number   =0x082D
Protocol_Ident =0
Station_Type   =0
FMS_supp       =0
Hardware_Release= "V 1.0"
Software_Release= "V 1.0"
9.6_supp       =1
19.2_supp      =1
31.25_supp     =0
45.45_supp     =1
93.75_supp     =1
187.5_supp     =1
500_supp       =1
1.5M_supp      =1
3M_supp        =1
6M_supp        =1
12M_supp       =1
MaxTsdr_9.6    =15
MaxTsdr_19.2   =15
MaxTsdr_31.25  =15
MaxTsdr_45.45  =15
MaxTsdr_93.75  =15
MaxTsdr_187.5  =15
MaxTsdr_500    =15
MaxTsdr_1.5M   =20
MaxTsdr_3M     =35
MaxTsdr_6M     =50
MaxTsdr_12M    =95
Redundancy     =0
Repeater_Ctrl_Sig=0
24V_Pins       =0
Implementation_Type ="VPC3 solution"
Bitmap_Device       ="FBP_N"
Bitmap_Diag         ="FBP_DIAG"
Bitmap_SF           ="FBP_RUN"
;
;================================
; Slave-Specification:
;================================
;
Freeze_Mode_supp    =1
Sync_Mode_supp      =1
Set_Slave_Add_Supp  =1
Auto_Baud_supp      =1
Min_Slave_Intervall =1
Fail_Safe           =1
Max_Diag_Data_Len   =16
Modul_Offset        =0
Slave_Family=0
Modular_Station		 =1
Max_Module          =1
Max_Input_len       =48
Max_Output_len      =48
Max_Data_len        =96

;=================================
; Device specific diagnostic data
;=================================
;
Unit_Diag_Area = 0-7
; rest of device diagnosis
Value(0) = "FBP diag byte 0: 0"
Unit_Diag_Area_End

Unit_Diag_Area = 8-15
; rest of device diagnosis
Value(0) = "device diag byte 0: 0"
Unit_Diag_Area_End

Unit_Diag_Area = 16-23
; rest of device diagnosis
Value(0) = "device diag byte 1: 0"
Unit_Diag_Area_End

Unit_Diag_Area = 24-31
; rest of device diagnosis
Value(0) = "device diag byte 2: 0"
Unit_Diag_Area_End

Unit_Diag_Area = 32-39
; rest of device diagnosis
Value(0) = "device diag byte 3: 0"
Unit_Diag_Area_End

Unit_Diag_Area = 40-47
; rest of device diagnosis
Value(0) = "device diag byte 4: 0"
Unit_Diag_Area_End

Unit_Diag_Area = 48-55
; rest of device diagnosis
Value(0) = "device diag byte 5: 0"
Unit_Diag_Area_End

Unit_Diag_Area = 56-63
; rest of device diagnosis
Value(0) = "device diag byte 6: 0"
Unit_Diag_Area_End


;=============================================
; User Prm Data: Length and Preset:
;=============================================
;
Max_User_Prm_Data_Len	= 224									; number of parameter of the longest module
Ext_User_Prm_Data_Const(0) = 0x10,0x01,0x00,0x00,0x00,0x00,0x00,0x00 	; constant values for ASIC
Ext_User_Prm_Data_Ref(3) = 10000		; use/ignore Block-Parameters
;
;=============================================
; Module Definition List
;=============================================
;
Module="Sensor (static mode)" 0x10, 0x20				; 1DO, 2DI
1
EndModule

Module="MSD11-FBP" 0x10, 0x20								; 1DO, 2DI
2
EndModule

Module="MSR22-FBP" 0x10, 0x20								; 2DO, 3DI
3
EndModule

Module="MFI21-FBP" 0x10, 0x20								; 3DO, 4DI
4
Ext_Module_Prm_Data_Len   = 5								; number of used data byte
Ext_User_Prm_Data_Const(0)=0x00,0x00,0x00,0x00,0x32	; initialising of param data
Ext_User_Prm_Data_Ref(0) = 50								; application mode
Ext_User_Prm_Data_Ref(1) = 51								; delay time
EndModule	

Module="UMC22-FBP (V3.0)" 0x11, 0x21, 0x50    	; 16DI, 16DO, 1AI
5
Ext_Module_Prm_Data_Len=42										; number of used data byte
Ext_User_Prm_Data_Const(0) =	\								; initialising of param data
							0x00,0x00,0x00,0x32,0x00,0x01,0x00,0x00,0x00,0x32, \
							0x01,0x01,0x01,0x00,0x0A,0x1E,0x04,0xB0,0x00,0x01, \
							0x02,0x04,0xB0,0x00,0x00,0xC8,0x00,0x14,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x0A,0x00
Ext_User_Prm_Data_Ref(0)	= 1
;Ext_User_Prm_Data_Ref(4)	= 2
Ext_User_Prm_Data_Ref(6)	= 23
Ext_User_Prm_Data_Ref(10)	= 3
;Ext_User_Prm_Data_Ref(11)	= 4
Ext_User_Prm_Data_Ref(12)	= 5

Ext_User_Prm_Data_Ref(14)	= 6
Ext_User_Prm_Data_Ref(15)	= 7
Ext_User_Prm_Data_Ref(16)	= 8
Ext_User_Prm_Data_Ref(18)	= 9
Ext_User_Prm_Data_Ref(19) = 10
Ext_User_Prm_Data_Ref(20)	= 11
Ext_User_Prm_Data_Ref(21)	= 17
Ext_User_Prm_Data_Ref(23)	= 21
Ext_User_Prm_Data_Ref(24)	= 12
Ext_User_Prm_Data_Ref(26)	= 13
;Ext_User_Prm_Data_Ref(28)	= 14
;Ext_User_Prm_Data_Ref(32)	= 15
Ext_User_Prm_Data_Ref(36) = 25  
Ext_User_Prm_Data_Ref(37)	= 16
Ext_User_Prm_Data_Ref(38)	= 24
Ext_User_Prm_Data_Ref(39)	= 18
Ext_User_Prm_Data_Ref(40)	= 19
Ext_User_Prm_Data_Ref(41)	= 20
EndModule

Module="UMC22-FBP (V3.10, V3.20)" 0x11, 0x21, 0x50   	; 16DI, 16DO, 1AI
6
Ext_Module_Prm_Data_Len=42										; number of used data byte
Ext_User_Prm_Data_Const(0) =	\								; initialising of param data
							0x00,0x00,0x00,0x32,0x00,0x01,0x00,0x00,0x00,0x32, \
							0x01,0x01,0x01,0x00,0x0A,0x1E,0x04,0xB0,0x00,0x01, \
							0x02,0x04,0xB0,0x00,0x00,0xC8,0x00,0x14,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x0A,0x00
Ext_User_Prm_Data_Ref(0)	= 101
Ext_User_Prm_Data_Ref(4)	= 102
Ext_User_Prm_Data_Ref(6)	= 123
Ext_User_Prm_Data_Ref(10)	= 103
;Ext_User_Prm_Data_Ref(11)	= 104
Ext_User_Prm_Data_Ref(12)	= 105

Ext_User_Prm_Data_Ref(14)	= 106
Ext_User_Prm_Data_Ref(15)	= 107
Ext_User_Prm_Data_Ref(16)	= 108
Ext_User_Prm_Data_Ref(18)	= 109
Ext_User_Prm_Data_Ref(19) = 110
Ext_User_Prm_Data_Ref(20)	= 111
Ext_User_Prm_Data_Ref(21)	= 117
Ext_User_Prm_Data_Ref(23)	= 121
Ext_User_Prm_Data_Ref(24)	= 112
Ext_User_Prm_Data_Ref(26)	= 113
Ext_User_Prm_Data_Ref(28)	= 114
Ext_User_Prm_Data_Ref(30)	= 126
Ext_User_Prm_Data_Ref(32)	= 115
Ext_User_Prm_Data_Ref(36) = 125  
Ext_User_Prm_Data_Ref(37)	= 116
Ext_User_Prm_Data_Ref(38)	= 124
Ext_User_Prm_Data_Ref(39)	= 118
Ext_User_Prm_Data_Ref(40)	= 119
Ext_User_Prm_Data_Ref(41)	= 120
EndModule

Module="Softstarter (V01)" 0x15, 0x21, 0x58, 0x65			 ;48 DI, 16 DO, 12 AI, 6AO
7
Ext_Module_Prm_Data_Len=192								 ;number of used data bytes
Ext_User_Prm_Data_Const(0)=\								 ;Initialising of Param data
							0x00,0x01,0x00,0x0A,0x00,0x00,0x00,0x1E,0x00,0x1E, \
							0x00,0x64,0x00,0x28,0x00,0x00,0x00,0x32,0x00,0x14, \
							0x00,0x00,0x00,0x00,0x00,0x01,0x00,0x0A,0x00,0x0A, \
							0x00,0x0A,0x00,0x00,0x00,0x00,0x00,0x28,0x00,0x0A, \
							0x00,0x00,0x00,0x00,0x00,0x08,0x00,0x0A,0x00,0x00, \
							0x00,0x00,0x50,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x0C,0x00,0x00,0x00,0x05, \
							0x00,0x00,0x00,0x5A,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x01,0x00,0x02,0x00,0x02,0x00,0x00, \
							0x00,0x00,0x00,0x07,0x00,0x07,0x00,0x00,0x00,0x01, \
							0x00,0x00,0x00,0x00,0x00,0x0A,0x00,0x1E,0x00,0x28, \
							0x03,0xE8,0x00,0x0A,0x00,0x1E,0x00,0x28,0x03,0xE8, \
							0x00,0x0A,0x00,0x1E,0x00,0x28,0x03,0xE8,0x00,0x00, \
							0x00,0x00,0x00,0x0F,0x00,0x00,0x00,0x00,0x0F,0xD3, \
							0x00,0x06,0x00,0x0F,0x00,0x0C,0x00,0x1E,0x00,0x00, \
							0x00,0x7B,0x00,0x7B,0x00,0x7B,0x00,0x7B,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x64,0x00,0x64,0x00,0x64, \
							0x00,0x64

Ext_User_Prm_Data_Ref(0)	= 1001
Ext_User_Prm_Data_Ref(2)	= 1002
Ext_User_Prm_Data_Ref(4)	= 1003
Ext_User_Prm_Data_Ref(6)	= 1004
Ext_User_Prm_Data_Ref(8)	= 1005
Ext_User_Prm_Data_Ref(10)	= 1006
Ext_User_Prm_Data_Ref(12)	= 1007
Ext_User_Prm_Data_Ref(14)	= 1008
Ext_User_Prm_Data_Ref(16)	= 1009
Ext_User_Prm_Data_Ref(18)	= 1010
Ext_User_Prm_Data_Ref(20)	= 1011
Ext_User_Prm_Data_Ref(22)	= 1012
Ext_User_Prm_Data_Ref(24)	= 1013
Ext_User_Prm_Data_Ref(26)	= 1014
Ext_User_Prm_Data_Ref(28)	= 1015
Ext_User_Prm_Data_Ref(30)	= 1016
Ext_User_Prm_Data_Ref(32)	= 1017
Ext_User_Prm_Data_Ref(34)	= 1018
Ext_User_Prm_Data_Ref(36)	= 1019
Ext_User_Prm_Data_Ref(38)	= 1020
Ext_User_Prm_Data_Ref(40)	= 1021
Ext_User_Prm_Data_Ref(42)	= 1022
Ext_User_Prm_Data_Ref(44)	= 1023
Ext_User_Prm_Data_Ref(46)	= 1024
Ext_User_Prm_Data_Ref(48)	= 1025
Ext_User_Prm_Data_Ref(50)	= 1026
Ext_User_Prm_Data_Ref(52)	= 1027
Ext_User_Prm_Data_Ref(54)	= 1028
Ext_User_Prm_Data_Ref(56)	= 1029
Ext_User_Prm_Data_Ref(58)	= 1030
Ext_User_Prm_Data_Ref(60)	= 1031
Ext_User_Prm_Data_Ref(62)	= 1032
Ext_User_Prm_Data_Ref(64)	= 1033
Ext_User_Prm_Data_Ref(66)	= 1034
Ext_User_Prm_Data_Ref(68)	= 1035
Ext_User_Prm_Data_Ref(70)	= 1036
Ext_User_Prm_Data_Ref(72)	= 1037
Ext_User_Prm_Data_Ref(74)	= 1038
Ext_User_Prm_Data_Ref(76)	= 1039
Ext_User_Prm_Data_Ref(78)	= 1040
Ext_User_Prm_Data_Ref(80)	= 1041
Ext_User_Prm_Data_Ref(82)	= 1042
Ext_User_Prm_Data_Ref(84)	= 1043
Ext_User_Prm_Data_Ref(86)	= 1044
Ext_User_Prm_Data_Ref(88)	= 1045
Ext_User_Prm_Data_Ref(90)	= 1046
Ext_User_Prm_Data_Ref(92)	= 1047
Ext_User_Prm_Data_Ref(94)	= 1048
Ext_User_Prm_Data_Ref(96)	= 1049
Ext_User_Prm_Data_Ref(98)	= 1050
Ext_User_Prm_Data_Ref(100)	= 1051
Ext_User_Prm_Data_Ref(102)	= 1052
Ext_User_Prm_Data_Ref(104)	= 1053
Ext_User_Prm_Data_Ref(106)	= 1054
Ext_User_Prm_Data_Ref(108)	= 1055
Ext_User_Prm_Data_Ref(110)	= 1056
Ext_User_Prm_Data_Ref(112)	= 1057
Ext_User_Prm_Data_Ref(114)	= 1058
Ext_User_Prm_Data_Ref(116)	= 1059
Ext_User_Prm_Data_Ref(118)	= 1060
Ext_User_Prm_Data_Ref(120)	= 1061
Ext_User_Prm_Data_Ref(122)	= 1062
Ext_User_Prm_Data_Ref(124)	= 1063
Ext_User_Prm_Data_Ref(126)	= 1064
Ext_User_Prm_Data_Ref(128)	= 1065
Ext_User_Prm_Data_Ref(130)	= 1066
Ext_User_Prm_Data_Ref(132)	= 1067
Ext_User_Prm_Data_Ref(134)	= 1068
Ext_User_Prm_Data_Ref(136)	= 1069
Ext_User_Prm_Data_Ref(138)	= 1070
Ext_User_Prm_Data_Ref(140)	= 1071
Ext_User_Prm_Data_Ref(142)	= 1072
Ext_User_Prm_Data_Ref(144)	= 1073
Ext_User_Prm_Data_Ref(146)	= 1074
Ext_User_Prm_Data_Ref(148)	= 1075
Ext_User_Prm_Data_Ref(150)	= 1076
Ext_User_Prm_Data_Ref(152)	= 1077
Ext_User_Prm_Data_Ref(154)	= 1078
Ext_User_Prm_Data_Ref(156)	= 1079
Ext_User_Prm_Data_Ref(158)	= 1080
Ext_User_Prm_Data_Ref(160)	= 1081
Ext_User_Prm_Data_Ref(162)	= 1082
Ext_User_Prm_Data_Ref(164)	= 1083
Ext_User_Prm_Data_Ref(166)	= 1084
Ext_User_Prm_Data_Ref(168)	= 1085
Ext_User_Prm_Data_Ref(170)	= 1086
Ext_User_Prm_Data_Ref(172)	= 1087
Ext_User_Prm_Data_Ref(174)	= 1088
Ext_User_Prm_Data_Ref(176)	= 1089
Ext_User_Prm_Data_Ref(178)	= 1090
Ext_User_Prm_Data_Ref(180)	= 1091
Ext_User_Prm_Data_Ref(182)	= 1092
Ext_User_Prm_Data_Ref(184)	= 1093
Ext_User_Prm_Data_Ref(186)	= 1094
Ext_User_Prm_Data_Ref(188)	= 1095
Ext_User_Prm_Data_Ref(190)	= 1096						
EndModule

Module="Softstarter (V02)" 0x15, 0x21, 0x58, 0x65			 ;48 DI, 16 DO, 12 AI, 6AO
8
Ext_Module_Prm_Data_Len=192								 ;number of used data bytes
Ext_User_Prm_Data_Const(0)=\								 ;Initialising of Param data
							0x00,0x01,0x00,0x0A,0x00,0x00,0x00,0x1E,0x00,0x1E, \
							0x00,0x64,0x00,0x28,0x00,0x00,0x00,0x32,0x00,0x14, \
							0x00,0x00,0x00,0x00,0x00,0x01,0x00,0x01,0x00,0x01, \
							0x00,0x01,0x00,0x00,0x00,0x00,0x00,0x28,0x00,0x0A, \
							0x00,0x00,0x00,0x00,0x00,0x08,0x00,0x0A,0x00,0x00, \
							0x00,0x00,0x00,0x50,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x0C,0x00,0x00,0x00,0x05, \
							0x00,0x00,0x00,0x5A,0x00,0x00,0x00,0x00,0x00,0x00, \
							0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x01,0x00,0x01, \
							0x00,0x00,0x00,0x01,0x00,0x02,0x00,0x02,0x00,0x00, \
							0x00,0x00,0x00,0x07,0x00,0x07,0x00,0x00,0x00,0x01, \
							0x00,0x00,0x00,0x01,0x00,0x0A,0x00,0x1E,0x00,0x28, \
							0x00,0x01,0x00,0x0A,0x00,0x1E,0x00,0x28,0x00,0x01, \
							0x00,0x0A,0x00,0x1E,0x00,0x28,0x00,0x01,0x00,0x01, \
							0x00,0x00,0x00,0x0F,0x00,0x00,0x00,0x00,0x0F,0xD2, \
							0x00,0x06,0x00,0x0F,0x00,0x0C,0x00,0x1E,0x00,0x00, \
							0x00,0xC0,0x00,0xA8,0x00,0x00,0x00,0x02,0x00,0x64, \
							0x00,0x00,0x00,0x00,0x00,0x5F,0x03,0xE8,0x02,0x58, \
							0x00,0x28

Ext_User_Prm_Data_Ref(0)	= 1101
Ext_User_Prm_Data_Ref(2)	= 1102
Ext_User_Prm_Data_Ref(4)	= 1103
Ext_User_Prm_Data_Ref(6)	= 1104
Ext_User_Prm_Data_Ref(8)	= 1105
Ext_User_Prm_Data_Ref(10)	= 1106
Ext_User_Prm_Data_Ref(12)	= 1107
Ext_User_Prm_Data_Ref(14)	= 1108
Ext_User_Prm_Data_Ref(16)	= 1109
Ext_User_Prm_Data_Ref(18)	= 1110
Ext_User_Prm_Data_Ref(20)	= 1111
Ext_User_Prm_Data_Ref(22)	= 1112
Ext_User_Prm_Data_Ref(24)	= 1113
Ext_User_Prm_Data_Ref(26)	= 1114
Ext_User_Prm_Data_Ref(28)	= 1115
Ext_User_Prm_Data_Ref(30)	= 1116
Ext_User_Prm_Data_Ref(32)	= 1117
Ext_User_Prm_Data_Ref(34)	= 1118
Ext_User_Prm_Data_Ref(36)	= 1119
Ext_User_Prm_Data_Ref(38)	= 1120
Ext_User_Prm_Data_Ref(40)	= 1121
Ext_User_Prm_Data_Ref(42)	= 1122
Ext_User_Prm_Data_Ref(44)	= 1123
Ext_User_Prm_Data_Ref(46)	= 1124
Ext_User_Prm_Data_Ref(48)	= 1125
Ext_User_Prm_Data_Ref(50)	= 1126
Ext_User_Prm_Data_Ref(52)	= 1127
Ext_User_Prm_Data_Ref(54)	= 1128
Ext_User_Prm_Data_Ref(56)	= 1129
Ext_User_Prm_Data_Ref(58)	= 1130
Ext_User_Prm_Data_Ref(60)	= 1131
Ext_User_Prm_Data_Ref(62)	= 1132
Ext_User_Prm_Data_Ref(64)	= 1133
Ext_User_Prm_Data_Ref(66)	= 1134
Ext_User_Prm_Data_Ref(68)	= 1135
Ext_User_Prm_Data_Ref(70)	= 1136
Ext_User_Prm_Data_Ref(72)	= 1137
Ext_User_Prm_Data_Ref(74)	= 1138
Ext_User_Prm_Data_Ref(76)	= 1139
Ext_User_Prm_Data_Ref(78)	= 1140
Ext_User_Prm_Data_Ref(80)	= 1141
Ext_User_Prm_Data_Ref(82)	= 1142
Ext_User_Prm_Data_Ref(84)	= 1143
Ext_User_Prm_Data_Ref(86)	= 1144
Ext_User_Prm_Data_Ref(88)	= 1145
Ext_User_Prm_Data_Ref(90)	= 1146
Ext_User_Prm_Data_Ref(92)	= 1147
Ext_User_Prm_Data_Ref(94)	= 1148
Ext_User_Prm_Data_Ref(96)	= 1149
Ext_User_Prm_Data_Ref(98)	= 1150
Ext_User_Prm_Data_Ref(100)	= 1151
Ext_User_Prm_Data_Ref(102)	= 1152
Ext_User_Prm_Data_Ref(104)	= 1153
Ext_User_Prm_Data_Ref(106)	= 1154
Ext_User_Prm_Data_Ref(108)	= 1155
Ext_User_Prm_Data_Ref(110)	= 1156
Ext_User_Prm_Data_Ref(112)	= 1157
Ext_User_Prm_Data_Ref(114)	= 1158
Ext_User_Prm_Data_Ref(116)	= 1159
Ext_User_Prm_Data_Ref(118)	= 1160
Ext_User_Prm_Data_Ref(120)	= 1161
Ext_User_Prm_Data_Ref(122)	= 1162
Ext_User_Prm_Data_Ref(124)	= 1163
Ext_User_Prm_Data_Ref(126)	= 1164
Ext_User_Prm_Data_Ref(128)	= 1165
Ext_User_Prm_Data_Ref(130)	= 1166
Ext_User_Prm_Data_Ref(132)	= 1167
Ext_User_Prm_Data_Ref(134)	= 1168
Ext_User_Prm_Data_Ref(136)	= 1169
Ext_User_Prm_Data_Ref(138)	= 1170
Ext_User_Prm_Data_Ref(140)	= 1171
Ext_User_Prm_Data_Ref(142)	= 1172
Ext_User_Prm_Data_Ref(144)	= 1173
Ext_User_Prm_Data_Ref(146)	= 1174
Ext_User_Prm_Data_Ref(148)	= 1175
Ext_User_Prm_Data_Ref(150)	= 1176
Ext_User_Prm_Data_Ref(152)	= 1177
Ext_User_Prm_Data_Ref(154)	= 1178
Ext_User_Prm_Data_Ref(156)	= 1179
Ext_User_Prm_Data_Ref(158)	= 1180
Ext_User_Prm_Data_Ref(160)	= 1181
Ext_User_Prm_Data_Ref(162)	= 1182
Ext_User_Prm_Data_Ref(164)	= 1183
Ext_User_Prm_Data_Ref(166)	= 1184
Ext_User_Prm_Data_Ref(168)	= 1185
Ext_User_Prm_Data_Ref(170)	= 1186
Ext_User_Prm_Data_Ref(172)	= 1187
Ext_User_Prm_Data_Ref(174)	= 1188
Ext_User_Prm_Data_Ref(176)	= 1189
Ext_User_Prm_Data_Ref(178)	= 1190
Ext_User_Prm_Data_Ref(180)	= 1191
Ext_User_Prm_Data_Ref(182)	= 1192
Ext_User_Prm_Data_Ref(184)	= 1193
Ext_User_Prm_Data_Ref(186)	= 1194
Ext_User_Prm_Data_Ref(188)	= 1195
Ext_User_Prm_Data_Ref(190)	= 1196						
EndModule

Module="WDI100-FBP" 0x5F							;16 AI
9
Ext_Module_Prm_Data_Len  = 18					;Number of used Data Bytes
Ext_User_Prm_Data_Const(0)=\						;Initialising of Param Data
								0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00,\
								0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00, 0x00

Ext_User_Prm_Data_Ref(0)  = 204
Ext_User_Prm_Data_Ref(2)  = 205
Ext_User_Prm_Data_Ref(4)  = 206
Ext_User_Prm_Data_Ref(6)  = 207
Ext_User_Prm_Data_Ref(8)  = 208
Ext_User_Prm_Data_Ref(10) = 209
Ext_User_Prm_Data_Ref(12) = 210
Ext_User_Prm_Data_Ref(14) = 211
Ext_User_Prm_Data_Ref(16) = 212
EndModule

Module="Sensopart" 0x51								; 2AI
10
EndModule


; DPV1 Alarm
DPV1_Slave                          = 1
C1_Read_Write_supp                  = 1
C1_Max_Data_Len                     = 8         ;The parameter specifies the maximum length of user data excluding
                                                ;Function_Num, Slot_number, Index, Length, transferred on the
                                                ;MSAC_1 communication channel.
                                                ;Type: Unsigned8 (0 .. 240)
C1_Response_Timeout                 = 300
Diagnostic_Alarm_supp               = 0
Process_Alarm_supp                  = 0
Pull_Plug_Alarm_supp                = 0
Status_Alarm_supp                   = 0
Update_Alarm_supp                   = 0
Manufacturer_Specific_Alarm_supp    = 0
Alarm_Sequence_Mode_Count           = 0
Alarm_Type_Mode_supp                = 0
Diagnostic_Alarm_required           = 0

C2_Read_Write_supp                  = 1
C2_Max_Data_Len                     = 48        ;The parameter specifies the maximum length of user data excluding
                                                ;Function_Num, Slot_number, Index, Length, transferred on the
                                                ;MSAC_2 communication channel.
                                                ;Type: Unsigned8 (0,48 .. 240)
C2_Response_Timeout                 = 300
C2_Read_Write_required              = 1
C2_Max_Count_Channels               = 3
Max_Initiate_PDU_Length             = 52        ;The parameter specifies the maximum length of an Initiate Request
                                                ;PDU including the Function_Num to the Resource Manager.
                                                ;Type: Unsigned8 (0,52.. 244)
DPV1_Data_Types                     = 0				;






