;======================================================
;======================================================
#Profibus_DP
;	Version:	1.0001		date 13/02/07
;	GSD file for ABB AW600 Navigator
;
; 				
;=============================================================
; Text-definition for User Prm Data  - We don't have any at present
;=============================================================
;
;
;
;===========================================================
;General parameters
;===========================================================
;
GSD_Revision   =3
Vendor_Name    ="ABB Instrumentation"
Model_Name     ="AW600 V1.001"
Revision       ="V1.001"
Ident_Number   =0x0AD4
Protocol_Ident =0
Station_Type   =0
FMS_supp       =0
Hardware_Release= "V 1.0"
Software_Release= "V 1.0"
9.6_supp       =1
19.2_supp      =1
31.25_supp     =0
45.45_supp     =1
93.75_supp     =1
187.5_supp     =1
500_supp       =1
1.5M_supp      =1
3M_supp        =1
6M_supp        =0
12M_supp       =0
MaxTsdr_9.6    =15
MaxTsdr_19.2   =15
MaxTsdr_45.45  =15
MaxTsdr_31.25  =15
MaxTsdr_93.75  =15
MaxTsdr_187.5  =15
MaxTsdr_500    =15
MaxTsdr_1.5M   =20
MaxTsdr_3M     =35
MaxTsdr_6M     =60
MaxTsdr_12M    =95
Redundancy     =0
Repeater_Ctrl_Sig=0
24V_Pins       =1
Implementation_Type ="VPC3 Solution"
Bitmap_Device       ="FBP_N"
Bitmap_Diag         ="FBP_DIAG"
Bitmap_SF           ="FBP_RUN"
;
;
;================================
; Slave-Specification:
;================================
;
Freeze_Mode_supp    =1
Sync_Mode_supp      =1
Set_Slave_Add_Supp  =0
Auto_Baud_supp      =1
Min_Slave_Intervall =1
Fail_Safe           =1
Max_Diag_Data_Len   =19
Modul_Offset        =0
Slave_Family        =9
Modular_Station	    =1
Max_Module          =1
Max_Input_len       =48		; set to max value
Max_Output_len      =48		; set to max value
Max_Data_len        =96		; set to max value
;
;=============================================
; User Prm Data: Length and Preset:
;=============================================
;
Max_User_Prm_Data_Len	= 224	; number of parameter of the longest module
Ext_User_Prm_Data_Const(0) = 0x00,0x00,0x00,0x00,0x00,0x00,0x00,0x00	; constant values for ASIC
;
;=============================================
; Module Definition List
;=============================================
;

Module="AW600 15 words" 0x5E			; 15 words
24
EndModule

; DPV1 Alarm
DPV1_Slave                          = 1
C1_Read_Write_supp                  = 1
C1_Max_Data_Len                     = 32         ;The parameter specifies the maximum length of user data excluding
                                                ;Function_Num, Slot_number, Index, Length, transferred on the
                                                ;MSAC_1 communication channel.
                                                ;Type: Unsigned8 (0 .. 240)
C1_Read_Write_required              = 1
C1_Response_Timeout                 = 2000
Diagnostic_Alarm_supp               = 0
Process_Alarm_supp                  = 0
Pull_Plug_Alarm_supp                = 0
Status_Alarm_supp                   = 0
Update_Alarm_supp                   = 0
Manufacturer_Specific_Alarm_supp    = 0
Alarm_Sequence_Mode_Count           = 0
Alarm_Type_Mode_supp                = 0
Diagnostic_Alarm_required           = 0

C2_Read_Write_supp                  = 1
C2_Max_Data_Len                     = 48        ;The parameter specifies the maximum length of user data excluding
                                                ;Function_Num, Slot_number, Index, Length, transferred on the
                                                ;MSAC_2 communication channel.
                                                ;Type: Unsigned8 (0,48 .. 240)
C2_Response_Timeout                 = 2000
C2_Read_Write_required              = 1
C2_Max_Count_Channels               = 3
Max_Initiate_PDU_Length             = 52        ;The parameter specifies the maximum length of an Initiate Request
                                                ;PDU including the Function_Num to the Resource Manager.
                                                ;Type: Unsigned8 (0,52.. 244)
DPV1_Data_Types                     = 0				;

