#

##

##

    µVision Build Log
    Project:
    E:\MD880\code\HCAN_USER\HCAN_User_defined_Ex\4_Project\HCAN_User.uvproj
    Project File Date:  05/08/2018

    Output:
    Rebuild target 'Target 1'
    assembling startup_stm32f407.s...
    compiling system_stm32f4xx.c...
    compiling misc.c...
    compiling stm32f4xx_can.c...
    compiling stm32f4xx_dbgmcu.c...
    compiling stm32f4xx_dma.c...
    compiling stm32f4xx_exti.c...
    compiling stm32f4xx_flash.c...
    compiling stm32f4xx_gpio.c...
    compiling stm32f4xx_pwr.c...
    compiling stm32f4xx_rcc.c...
    compiling stm32f4xx_syscfg.c...
    compiling stm32f4xx_tim.c...
    compiling stm32f4xx_usart.c...
    compiling stm32f4xx_wwdg.c...
    compiling f_CAN_app.c...
    compiling f_CAN_drive.c...
    compiling f_user_main.c...
    linking...
    Program Size: Code=18984 RO-data=556 RW-data=164 ZI-data=7140
    FromELF: creating hex file...
    "..\5_Output\Objects\HCAN_User.axf" - 0 Error(s), 0 Warning(s).
    Load "..\\5_Output\\Objects\\HCAN_User.axf"
    Set JLink Project File to "E:\MD880\code\HCAN_USER\HCAN_User_defined_Ex\4_Project\JLinkSettings.ini"
    * JLink Info: Device "STM32F407VG" selected (1024 KB flash, 128 KB RAM).

    JLink info:
    ------------
    DLL: V4.80g, compiled Feb 13 2014 20:50:02
    Firmware: J-Link V9 compiled Aug  3 2016 18:50:44
    Hardware: V9.40
    S/N : 59425868
    Feature(s) : RDI, GDB, FlashDL, FlashBP, JFlash, RDDI

    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M4 r0p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F407VG
    VTarget = 3.308V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...