Static Call Graph - [..\5_Output\Objects\HCAN_User.axf]

# Static Call Graph for image ..\5_Output\Objects\HCAN_User.axf

#<CALLGRAPH># ARM Linker, 5.03 [Build 76]: Last Updated: Tue Aug 06 07:40:45 2019

### Maximum Stack Usage = 1168 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ ManufacMainLoop ⇒ C_InobusLoop ⇒ InobusMainLoop ⇒ Ino_RxDataProcess ⇒ InoProcessNormal ⇒ InoMsgRspCallbackFunc ⇒ C_Read_Func_Response

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - BusFault_Handler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - CAN1_RX0_IRQHandler from f_can_drive.o(.text) referenced from startup_stm32f407.o(RESET)
  - CAN1_RX1_IRQHandler from f_can_drive.o(.text) referenced from startup_stm32f407.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - CAN1_TX_IRQHandler from f_can_drive.o(.text) referenced from startup_stm32f407.o(RESET)
  - CAN2_RX0_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - CAN2_RX1_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - CAN2_SCE_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - CAN2_TX_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - CRYP_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - DCMI_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - DMA2_Stream1_IRQHandler from f_uart.o(.text) referenced from startup_stm32f407.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - DMA2_Stream6_IRQHandler from f_uart.o(.text) referenced from startup_stm32f407.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - DebugMon_Handler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - ETH_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - ETH_WKUP_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - FLASH_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - FPU_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - FSMC_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - HASH_RNG_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - HardFault_Handler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - MemManage_Handler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - NMI_Handler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - OTG_HS_EP1_IN_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - OTG_HS_EP1_OUT_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - OTG_HS_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - OTG_HS_WKUP_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - PVD_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - PendSV_Handler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - RCC_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - Reset_Handler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - SDIO_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - SPI1_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - SPI2_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - SPI3_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - SVC_Handler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - SysTick_Handler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - SystemInit from main.o(.text) referenced from startup_stm32f407.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from f_inobus.o(.text) referenced from startup_stm32f407.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - TIM2_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - TIM3_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - TIM4_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - TIM5_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - TIM7_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - TIM8_BRK_TIM12_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - TIM8_TRG_COM_TIM14_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - TIM8_UP_TIM13_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - UART4_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - UART5_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - USART1_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - USART2_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - USART3_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - USART6_IRQHandler from f_uart.o(.text) referenced from startup_stm32f407.o(RESET)
  - UsageFault_Handler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - WWDG_IRQHandler from startup_stm32f407.o(.text) referenced from startup_stm32f407.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f407.o(.text)
  - main from main.o(.text) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f407.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_stm32f407.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f407.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f407.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f407.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f407.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_stm32f407.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_stm32f407.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_stm32f407.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup_stm32f407.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f407.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  CAN2_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  CAN2_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  CAN2_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  CAN2_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  CRYP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  DCMI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  HASH_RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  OTG_HS_EP1_IN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  OTG_HS_EP1_OUT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  OTG_HS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  OTG_HS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  TIM8_BRK_TIM12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  TIM8_TRG_COM_TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  TIM8_UP_TIM13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f407.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f407.o(RESET)

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> NVIC_Configuration

  NVIC_Init (Thumb, 108 bytes, Stack size 16 bytes, misc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = NVIC_Init
  [Called By]
  - >> InitCanDrive
  - >> Uart6InitDma
  - >> Uart_Init
  - >> TIM9_Configuration

  NVIC_SetVectorTable (Thumb, 14 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> NVIC_Configuration

  NVIC_SystemLPConfig (Thumb, 34 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  SysTick_CLKSourceConfig (Thumb, 40 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  CAN_DeInit (Thumb, 50 bytes, Stack size 8 bytes, stm32f4xx_can.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = CAN_DeInit
  [Calls]
  - >> RCC_APB1PeriphResetCmd
  [Called By]
  - >> InitCanDrive

  CAN_Init (Thumb, 276 bytes, Stack size 12 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_FilterInit (Thumb, 258 bytes, Stack size 8 bytes, stm32f4xx_can.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = CAN_FilterInit
  [Called By]
  - >> InitRecMbox

  CAN_StructInit (Thumb, 32 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text))
  [Called By]

  - >> InitCanDrive

  CAN_SlaveStartBank (Thumb, 48 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_DBGFreeze (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_TTComModeCmd (Thumb, 118 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_Transmit (Thumb, 304 bytes, Stack size 8 bytes, stm32f4xx_can.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = CAN_Transmit
  [Called By]
  - >> CAN1_TX_IRQHandler
  - >> eCanDataTran

  CAN_TransmitStatus (Thumb, 138 bytes, Stack size 8 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_CancelTransmit (Thumb, 48 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_Receive (Thumb, 240 bytes, Stack size 8 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_FIFORelease (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_MessagePending (Thumb, 30 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_OperatingModeRequest (Thumb, 162 bytes, Stack size 8 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_Sleep (Thumb, 30 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_WakeUp (Thumb, 48 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_GetLastErrorCode (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_GetReceiveErrorCounter (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_GetLSBTransmitErrorCounter (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_ITConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text))
  [Called By]

  - >> CAN1_TX_IRQHandler
  - >> eCanDataTran
  - >> InitCanDrive

  CAN_GetFlagStatus (Thumb, 120 bytes, Stack size 8 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_ClearFlag (Thumb, 52 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)

  CAN_GetITStatus (Thumb, 308 bytes, Stack size 16 bytes, stm32f4xx_can.o(.text), UNUSED)
  [Calls]

  - >> CheckITStatus

  CAN_ClearITPendingBit (Thumb, 162 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)

  DBGMCU_GetREVID (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_dbgmcu.o(.text), UNUSED)

  DBGMCU_GetDEVID (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_dbgmcu.o(.text), UNUSED)

  DBGMCU_Config (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_dbgmcu.o(.text))
  [Called By]

  - >> SystemInit

  DBGMCU_APB1PeriphConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_dbgmcu.o(.text))
  [Called By]

  - >> SystemInit

  DBGMCU_APB2PeriphConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_dbgmcu.o(.text))
  [Called By]

  - >> SystemInit

  DMA_DeInit (Thumb, 324 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text))
  [Called By]

  - >> Uart6InitDma

  DMA_Init (Thumb, 82 bytes, Stack size 8 bytes, stm32f4xx_dma.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = DMA_Init
  [Called By]
  - >> Uart6InitDma

  DMA_StructInit (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_Cmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text))
  [Called By]

  - >> Uart6InitDma
  - >> USART6_IRQHandler
  - >> DMA2_Stream6_IRQHandler
  - >> Uart6DmaSend

  DMA_PeriphIncOffsetSizeConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_FlowControllerConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_SetCurrDataCounter (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text))
  [Called By]

  - >> USART6_IRQHandler
  - >> Uart6DmaSend

  DMA_GetCurrDataCounter (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text))
  [Called By]

  - >> USART6_IRQHandler

  DMA_DoubleBufferModeConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_DoubleBufferModeCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_MemoryTargetConfig (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text))
  [Called By]

  - >> Uart6DmaSend

  DMA_GetCurrentMemoryTarget (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_GetCmdStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_GetFIFOStatus (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_GetFlagStatus (Thumb, 54 bytes, Stack size 12 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_ClearFlag (Thumb, 40 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_ITConfig (Thumb, 58 bytes, Stack size 8 bytes, stm32f4xx_dma.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = DMA_ITConfig
  [Called By]
  - >> Uart6InitDma
  - >> USART6_IRQHandler
  - >> DMA2_Stream6_IRQHandler
  - >> Uart6DmaSend

  DMA_GetITStatus (Thumb, 82 bytes, Stack size 16 bytes, stm32f4xx_dma.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = DMA_GetITStatus
  [Called By]
  - >> DMA2_Stream6_IRQHandler
  - >> DMA2_Stream1_IRQHandler

  DMA_ClearITPendingBit (Thumb, 40 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text))
  [Called By]

  - >> USART6_IRQHandler
  - >> DMA2_Stream6_IRQHandler
  - >> DMA2_Stream1_IRQHandler

  GPIO_DeInit (Thumb, 220 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_AHB1PeriphResetCmd

  GPIO_Init (Thumb, 144 bytes, Stack size 20 bytes, stm32f4xx_gpio.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> InitCANIO
  - >> Uart_GPIO_Init
  - >> STM_LEDInit

  GPIO_StructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_PinLockConfig (Thumb, 34 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadInputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ToggleBits (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_PinAFConfig (Thumb, 70 bytes, Stack size 20 bytes, stm32f4xx_gpio.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_PinAFConfig
  [Called By]
  - >> InitCANIO
  - >> Uart_GPIO_Init

  RCC_DeInit (Thumb, 60 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HSEConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetFlagStatus (Thumb, 60 bytes, Stack size 8 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_WaitForHSEStartUp

  RCC_WaitForHSEStartUp (Thumb, 56 bytes, Stack size 16 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus

  RCC_AdjustHSICalibrationValue (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LSEConfig (Thumb, 46 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLConfig (Thumb, 32 bytes, Stack size 16 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLI2SConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLI2SCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_MCO1Config (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_MCO2Config (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SYSCLKConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetSYSCLKSource (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HCLKConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PCLK1Config (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PCLK2Config (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 222 bytes, Stack size 20 bytes, stm32f4xx_rcc.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> USART_Init

  RCC_RTCCLKConfig (Thumb, 54 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_RTCCLKCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_BackupResetCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_I2SCLKConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB1PeriphClockCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> InitCanDrive
  - >> Uart6InitDma
  - >> Uart_Init
  - >> STM_LEDInit

  RCC_AHB2PeriphClockCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB3PeriphClockCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphClockCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> InitCanDrive
  - >> TIM3_Configuration
  - >> TIM4_Configuration

  RCC_APB2PeriphClockCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> Uart_Init
  - >> TIM9_Configuration

  RCC_AHB1PeriphResetCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> GPIO_DeInit

  RCC_AHB2PeriphResetCmd (Thumb, 72 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB3PeriphResetCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphResetCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> USART_DeInit
  - >> TIM_DeInit
  - >> CAN_DeInit

  RCC_APB2PeriphResetCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> USART_DeInit
  - >> TIM_DeInit

  RCC_AHB1PeriphClockLPModeCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB2PeriphClockLPModeCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB3PeriphClockLPModeCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphClockLPModeCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB2PeriphClockLPModeCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ITConfig (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  TIM_DeInit (Thumb, 346 bytes, Stack size 8 bytes, stm32f4xx_tim.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_DeInit
  [Calls]
  - >> RCC_APB2PeriphResetCmd
  - >> RCC_APB1PeriphResetCmd
  [Called By]
  - >> TIM9_Configuration
  - >> TIM3_Configuration
  - >> TIM4_Configuration

  TIM_TimeBaseInit (Thumb, 104 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text))
  [Called By]

  - >> TIM9_Configuration
  - >> TIM3_Configuration
  - >> TIM4_Configuration

  TIM_TimeBaseStructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_PrescalerConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_CounterModeConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SetCounter (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text))
  [Called By]

  - >> Ino_SendSync

  TIM_SetAutoreload (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_GetCounter (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text))
  [Called By]

  - >> GetSyncPeriod
  - >> GetSysTime_1MHzClk

  TIM_GetPrescaler (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_UpdateDisableConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_UpdateRequestConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_ARRPreloadConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SelectOnePulseMode (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SetClockDivision (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text))
  [Called By]

  - >> TIM9_Configuration
  - >> Ino_SendSync
  - >> TIM1_BRK_TIM9_IRQHandler
  - >> TIM3_Configuration
  - >> TIM4_Configuration

  TIM_OC1Init (Thumb, 114 bytes, Stack size 16 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC2Init (Thumb, 154 bytes, Stack size 16 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC3Init (Thumb, 204 bytes, Stack size 16 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC4Init (Thumb, 112 bytes, Stack size 16 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OCStructInit (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SelectOCxM (Thumb, 86 bytes, Stack size 16 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SetCompare1 (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SetCompare2 (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SetCompare3 (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SetCompare4 (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_ForcedOC1Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_ForcedOC2Config (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_ForcedOC3Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_ForcedOC4Config (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC1PreloadConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC2PreloadConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC3PreloadConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC4PreloadConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC1FastConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC2FastConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC3FastConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC4FastConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_ClearOC1Ref (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_ClearOC2Ref (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_ClearOC3Ref (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_ClearOC4Ref (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC1PolarityConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC1NPolarityConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC2PolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC2NPolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC3PolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC3NPolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC4PolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_CCxCmd (Thumb, 30 bytes, Stack size 12 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_CCxNCmd (Thumb, 30 bytes, Stack size 12 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SetIC4Prescaler (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TIM_SetIC3Prescaler (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TIM_SetIC2Prescaler (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TIM_SetIC1Prescaler (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TIM_ICInit (Thumb, 110 bytes, Stack size 16 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SetIC1Prescaler
  - >> TIM_SetIC2Prescaler
  - >> TIM_SetIC3Prescaler
  - >> TIM_SetIC4Prescaler
  - >> TI1_Config
  - >> TI2_Config
  - >> TI3_Config
  - >> TI4_Config

  TIM_ICStructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_PWMIConfig (Thumb, 124 bytes, Stack size 24 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SetIC1Prescaler
  - >> TIM_SetIC2Prescaler
  - >> TI1_Config
  - >> TI2_Config

  TIM_GetCapture1 (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_GetCapture2 (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_GetCapture3 (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_GetCapture4 (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_BDTRConfig (Thumb, 32 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_BDTRStructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_CtrlPWMOutputs (Thumb, 30 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SelectCOM (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_CCPreloadControl (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_ITConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_GenerateEvent (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_GetFlagStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_GetITStatus (Thumb, 34 bytes, Stack size 12 bytes, stm32f4xx_tim.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_GetITStatus
  [Called By]
  - >> TIM1_BRK_TIM9_IRQHandler

  TIM_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text))
  [Called By]

  - >> TIM1_BRK_TIM9_IRQHandler

  TIM_DMAConfig (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_DMACmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SelectCCDMA (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_InternalClockConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SelectInputTrigger (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_ITRxExternalClockConfig

  TIM_ITRxExternalClockConfig (Thumb, 24 bytes, Stack size 12 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SelectInputTrigger

  TIM_TIxExternalClockConfig (Thumb, 62 bytes, Stack size 24 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SelectInputTrigger
  - >> TI1_Config
  - >> TI2_Config

  TIM_ETRConfig (Thumb, 28 bytes, Stack size 12 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ETRClockMode2Config
  - >> TIM_ETRClockMode1Config

  TIM_ETRClockMode1Config (Thumb, 54 bytes, Stack size 24 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_ETRConfig

  TIM_ETRClockMode2Config (Thumb, 32 bytes, Stack size 20 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_ETRConfig

  TIM_SelectOutputTrigger (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SelectSlaveMode (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SelectMasterSlaveMode (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_EncoderInterfaceConfig (Thumb, 66 bytes, Stack size 20 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SelectHallSensor (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_RemapConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  USART_DeInit (Thumb, 156 bytes, Stack size 8 bytes, stm32f4xx_usart.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd
  - >> RCC_APB1PeriphResetCmd

  USART_Init (Thumb, 204 bytes, Stack size 48 bytes, stm32f4xx_usart.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> Uart_Init

  USART_StructInit (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_ClockInit (Thumb, 32 bytes, Stack size 8 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_ClockStructInit (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text))
  [Called By]

  - >> Uart_Init

  USART_SetPrescaler (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_OverSampling8Cmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text))
  [Called By]

  - >> Uart_Init

  USART_OneBitMethodCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text))
  [Called By]

  - >> Ino_SendSync

  USART_ReceiveData (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text))
  [Called By]

  - >> USART6_IRQHandler

  USART_SetAddress (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_ReceiverWakeUpCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_WakeUpConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_LINBreakDetectLengthConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_LINCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_SendBreak (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_HalfDuplexCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_SetGuardTime (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_SmartCardCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_SmartCardNACKCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_IrDAConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_IrDACmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_DMACmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text))
  [Called By]

  - >> DMA2_Stream6_IRQHandler
  - >> Uart_Init
  - >> Uart6DmaSend

  USART_ITConfig (Thumb, 74 bytes, Stack size 20 bytes, stm32f4xx_usart.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = USART_ITConfig
  [Called By]
  - >> USART6_IRQHandler
  - >> Uart_Init
  - >> Ino_SendSync

  USART_GetFlagStatus (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_ClearFlag (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_GetITStatus (Thumb, 110 bytes, Stack size 16 bytes, stm32f4xx_usart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USART_GetITStatus
  [Called By]
  - >> USART6_IRQHandler

  USART_ClearITPendingBit (Thumb, 30 bytes, Stack size 8 bytes, stm32f4xx_usart.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USART_ClearITPendingBit
  [Called By]
  - >> USART6_IRQHandler

  STM_LEDInit (Thumb, 62 bytes, Stack size 16 bytes, f_led.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = STM_LEDInit ⇒ GPIO_Init
  [Calls]
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> LED_IO_Init

  STM_LEDOn (Thumb, 16 bytes, Stack size 0 bytes, f_led.o(.text))
  [Called By]

  - >> LED_Ctrl

  STM_LEDOff (Thumb, 16 bytes, Stack size 0 bytes, f_led.o(.text))
  [Called By]

  - >> LED_Ctrl

  STM_LEDToggle (Thumb, 26 bytes, Stack size 0 bytes, f_led.o(.text), UNUSED)

  LED_Ctrl (Thumb, 26 bytes, Stack size 8 bytes, f_led.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = LED_Ctrl
  [Calls]
  - >> STM_LEDOff
  - >> STM_LEDOn
  [Called By]
  - >> Host_Led_Proc
  - >> ModuleLedCtrl
  - >> LED_IO_Init

  LED_IO_Init (Thumb, 130 bytes, Stack size 8 bytes, f_led.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = LED_IO_Init ⇒ STM_LEDInit ⇒ GPIO_Init
  [Calls]
  - >> LED_Ctrl
  - >> STM_LEDInit
  [Called By]
  - >> main

  NVIC_Configuration (Thumb, 22 bytes, Stack size 8 bytes, f_main.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = NVIC_Configuration
  [Calls]
  - >> NVIC_SetVectorTable
  - >> NVIC_PriorityGroupConfig
  [Called By]
  - >> main

  TIM4_Configuration (Thumb, 58 bytes, Stack size 16 bytes, f_main.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = TIM4_Configuration ⇒ TIM_DeInit
  [Calls]
  - >> TIM_Cmd
  - >> TIM_TimeBaseInit
  - >> TIM_DeInit
  - >> RCC_APB1PeriphClockCmd
  [Called By]
  - >> main

  GetSysTime_1MHzClk (Thumb, 12 bytes, Stack size 8 bytes, f_main.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = GetSysTime_1MHzClk
  [Calls]
  - >> TIM_GetCounter
  [Called By]
  - >> main
  - >> UsersMainLoop
  - >> ManufacMainLoop

  ModuleLed2GreenDispSet (Thumb, 8 bytes, Stack size 0 bytes, f_main.o(.text))
  [Called By]

  - >> UpdateLedStatus

  ModuleLed2OrangeDispSet (Thumb, 8 bytes, Stack size 0 bytes, f_main.o(.text))
  [Called By]

  - >> UpdateLedStatus

  ModuleLed2RedDispSet (Thumb, 8 bytes, Stack size 0 bytes, f_main.o(.text))
  [Called By]

  - >> UpdateLedStatus

  ManufacMainLoop (Thumb, 44 bytes, Stack size 8 bytes, f_main.o(.text))
  [Stack]

  - Max Depth = 1168
  - Call Chain = ManufacMainLoop ⇒ C_InobusLoop ⇒ InobusMainLoop ⇒ Ino_RxDataProcess ⇒ InoProcessNormal ⇒ InoMsgRspCallbackFunc ⇒ C_Read_Func_Response
  [Calls]
  - >> SysInitDeal
  - >> HcuParaReadPeriod
  - >> C_InobusLoop
  - >> GetSysTime_1MHzClk
  - >> UpdateDataToUserApp
  - >> UpdateLedStatus
  - >> ModuleLedDeal
  [Called By]
  - >> main

  UsersMainLoop (Thumb, 24 bytes, Stack size 8 bytes, f_main.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = UsersMainLoop ⇒ userMainProc ⇒ CanMainProcess ⇒ InitCanConfig ⇒ CanFilterConfigDeal ⇒ InitRecMbox ⇒ CAN_FilterInit
  [Calls]
  - >> userMainProc
  - >> GetSysTime_1MHzClk
  [Called By]
  - >> main

  SysMonitorDeal (Thumb, 132 bytes, Stack size 0 bytes, f_main.o(.text))
  [Called By]

  - >> main

  GetSysLoadRealTime (Thumb, 6 bytes, Stack size 0 bytes, f_main.o(.text))
  [Called By]

  - >> userMainProc

  GetSysLoadMax (Thumb, 6 bytes, Stack size 0 bytes, f_main.o(.text))
  [Called By]

  - >> userMainProc

  InitModuleLedPara (Thumb, 64 bytes, Stack size 0 bytes, f_main.o(.text), UNUSED)

  ModuleLed1RedDispSet (Thumb, 8 bytes, Stack size 0 bytes, f_main.o(.text), UNUSED)

  ModuleLed1GreenDispSet (Thumb, 8 bytes, Stack size 0 bytes, f_main.o(.text), UNUSED)

  ModuleLed1OrangeDispSet (Thumb, 8 bytes, Stack size 0 bytes, f_main.o(.text), UNUSED)

  ModuleLed3RedDispSet (Thumb, 54 bytes, Stack size 0 bytes, f_main.o(.text), UNUSED)

  ModuleLed3GreenDispSet (Thumb, 12 bytes, Stack size 0 bytes, f_main.o(.text))
  [Called By]

  - >> UserLedCtrlTest

  ModuleLed3OrangeDispSet (Thumb, 12 bytes, Stack size 0 bytes, f_main.o(.text), UNUSED)

  ClolkInit (Thumb, 74 bytes, Stack size 8 bytes, f_rcc.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = ClolkInit ⇒ SetSysClock
  [Calls]
  - >> SetSysClock
  [Called By]
  - >> SystemInit

  PeripheralClockConfig (Thumb, 256 bytes, Stack size 0 bytes, f_rcc.o(.text))
  [Called By]

  - >> SystemInit

  SysInitVal (Thumb, 52 bytes, Stack size 8 bytes, f_tech_comm_interface.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = SysInitVal ⇒ C_SetPdLen ⇒ InoSetPdLen
  [Calls]
  - >> C_SetPdLen
  [Called By]
  - >> main

  FuncCodeRead (Thumb, 38 bytes, Stack size 24 bytes, f_tech_comm_interface.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = FuncCodeRead ⇒ C_Read_FunCode ⇒ MsgSendDeal
  [Calls]
  - >> C_Read_FunCode
  [Called By]
  - >> SysInitDeal
  - >> HcuParaReadPeriod

  SysInitDeal (Thumb, 258 bytes, Stack size 8 bytes, f_tech_comm_interface.o(.text))
  [Stack]

  - Max Depth = 76
  - Call Chain = SysInitDeal ⇒ FuncCodeRead ⇒ C_Read_FunCode ⇒ MsgSendDeal
  [Calls]
  - >> C_GetInobusOnline
  - >> FuncCodeRead
  [Called By]
  - >> ManufacMainLoop

  HcuParaReadPeriod (Thumb, 94 bytes, Stack size 8 bytes, f_tech_comm_interface.o(.text))
  [Stack]

  - Max Depth = 76
  - Call Chain = HcuParaReadPeriod ⇒ FuncCodeRead ⇒ C_Read_FunCode ⇒ MsgSendDeal
  [Calls]
  - >> FuncCodeRead
  [Called By]
  - >> ManufacMainLoop

  InobusAddrToFuncAddr (Thumb, 38 bytes, Stack size 8 bytes, f_tech_comm_interface.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = InobusAddrToFuncAddr
  [Called By]
  - >> InoMsgRspCallbackFunc

  C_Read_Func_Response (Thumb, 200 bytes, Stack size 24 bytes, f_tech_comm_interface.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = C_Read_Func_Response
  [Called By]
  - >> InoMsgRspCallbackFunc

  WatchDogInit (Thumb, 92 bytes, Stack size 0 bytes, f_wwdg.o(.text))
  [Called By]

  - >> main

  ServiceDog (Thumb, 20 bytes, Stack size 0 bytes, f_wwdg.o(.text))
  [Called By]

  - >> main

  DisableWDog (Thumb, 18 bytes, Stack size 0 bytes, f_wwdg.o(.text), UNUSED)

  SystemInit (Thumb, 44 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = SystemInit ⇒ ClolkInit ⇒ SetSysClock
  [Calls]
  - >> DBGMCU_APB2PeriphConfig
  - >> DBGMCU_APB1PeriphConfig
  - >> DBGMCU_Config
  - >> PeripheralClockConfig
  - >> ClolkInit
  [Address Reference Count : 1]
  - startup_stm32f407.o(.text)

  main (Thumb, 132 bytes, Stack size 0 bytes, main.o(.text))
  [Stack]

  - Max Depth = 1168
  - Call Chain = main ⇒ ManufacMainLoop ⇒ C_InobusLoop ⇒ InobusMainLoop ⇒ Ino_RxDataProcess ⇒ InoProcessNormal ⇒ InoMsgRspCallbackFunc ⇒ C_Read_Func_Response
  [Calls]
  - >> userInitProc
  - >> ServiceDog
  - >> WatchDogInit
  - >> SysInitVal
  - >> C_InobusLoop
  - >> SysMonitorDeal
  - >> UsersMainLoop
  - >> ManufacMainLoop
  - >> GetSysTime_1MHzClk
  - >> TIM4_Configuration
  - >> NVIC_Configuration
  - >> LED_IO_Init
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 34 bytes, Stack size 8 bytes, f_inobus.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = TIM1_BRK_TIM9_IRQHandler ⇒ Ino_SendNormalData ⇒ Uart6DmaSend ⇒ DMA_ITConfig
  [Calls]
  - >> TIM_ClearITPendingBit
  - >> TIM_GetITStatus
  - >> TIM_Cmd
  - >> Ino_SendNormalData
  [Address Reference Count : 1]
  - startup_stm32f407.o(RESET)

  Set_PdMappingAddr (Thumb, 2 bytes, Stack size 0 bytes, f_inobus.o(.text), UNUSED)

  Ino_SendSync (Thumb, 78 bytes, Stack size 8 bytes, f_inobus.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = Ino_SendSync ⇒ USART_ITConfig
  [Calls]
  - >> USART_ITConfig
  - >> USART_SendData
  - >> TIM_Cmd
  - >> TIM_SetCounter
  - >> GetSyncPeriod
  [Called By]
  - >> C_AppSyncRecv
  - >> InobusMainLoop

  InobusMainLoop (Thumb, 138 bytes, Stack size 8 bytes, f_inobus.o(.text))
  [Stack]

  - Max Depth = 1152
  - Call Chain = InobusMainLoop ⇒ Ino_RxDataProcess ⇒ InoProcessNormal ⇒ InoMsgRspCallbackFunc ⇒ C_Read_Func_Response
  [Calls]
  - >> Host_Led_Proc
  - >> Ino_SendSync
  - >> Ino_RxDataProcess
  - >> Ino_MsgWatchDog
  - >> Ino_SendHandshake
  - >> InobusInitDsp
  [Called By]
  - >> C_InobusLoop

  MsgSendDeal (Thumb, 102 bytes, Stack size 12 bytes, f_inobus.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = MsgSendDeal
  [Called By]
  - >> C_Read_FunCode

  InoSetPdLen (Thumb, 40 bytes, Stack size 16 bytes, f_inobus.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = InoSetPdLen
  [Calls]
  - >> Ino_GetPdAddr
  [Called By]
  - >> C_SetPdLen

  Ino_GetDevStatus (Thumb, 6 bytes, Stack size 0 bytes, f_inobus.o(.text), UNUSED)
  [Called By]

  - >> C_DeviceAppState

  Ino_SetCardStatus (Thumb, 6 bytes, Stack size 0 bytes, f_inobus.o(.text), UNUSED)
  [Called By]

  - >> CommStateSet

  Ino_GetBusOnline (Thumb, 14 bytes, Stack size 0 bytes, f_inobus.o(.text))
  [Called By]

  - >> C_GetInobusOnline

  TIM9_Configuration (Thumb, 86 bytes, Stack size 24 bytes, f_inobus.o(.text), UNUSED)
  [Calls]

  - >> TIM_Cmd
  - >> TIM_TimeBaseInit
  - >> TIM_DeInit
  - >> RCC_APB2PeriphClockCmd
  - >> NVIC_Init

  UartTranOverCallback (Thumb, 8 bytes, Stack size 8 bytes, f_inobus.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = UartTranOverCallback ⇒ Ino_SendNormalData ⇒ Uart6DmaSend ⇒ DMA_ITConfig
  [Calls]
  - >> Ino_SendNormalData
  [Called By]
  - >> USART6_IRQHandler

  UartRecvRdyCallback (Thumb, 12 bytes, Stack size 0 bytes, f_inobus.o(.text))
  [Called By]

  - >> USART6_IRQHandler

  C_InobusLoop (Thumb, 8 bytes, Stack size 8 bytes, f_inobusif.o(.text))
  [Stack]

  - Max Depth = 1160
  - Call Chain = C_InobusLoop ⇒ InobusMainLoop ⇒ Ino_RxDataProcess ⇒ InoProcessNormal ⇒ InoMsgRspCallbackFunc ⇒ C_Read_Func_Response
  [Calls]
  - >> InobusMainLoop
  [Called By]
  - >> main
  - >> ManufacMainLoop

  C_Read_FunCode (Thumb, 82 bytes, Stack size 32 bytes, f_inobusif.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = C_Read_FunCode ⇒ MsgSendDeal
  [Calls]
  - >> MsgSendDeal
  [Called By]
  - >> FuncCodeRead

  Ino_GetPdAddr (Thumb, 16 bytes, Stack size 0 bytes, f_inobusif.o(.text))
  [Called By]

  - >> InoSetPdLen

  C_SetPdLen (Thumb, 16 bytes, Stack size 16 bytes, f_inobusif.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = C_SetPdLen ⇒ InoSetPdLen
  [Calls]
  - >> InoSetPdLen
  [Called By]
  - >> SysInitVal

  C_DeviceAppState (Thumb, 8 bytes, Stack size 8 bytes, f_inobusif.o(.text), UNUSED)
  [Calls]

  - >> Ino_GetDevStatus

  C_GetInobusOnline (Thumb, 8 bytes, Stack size 8 bytes, f_inobusif.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = C_GetInobusOnline
  [Calls]
  - >> Ino_GetBusOnline
  [Called By]
  - >> SysInitDeal

  CommStateSet (Thumb, 12 bytes, Stack size 8 bytes, f_inobusif.o(.text), UNUSED)
  [Calls]

  - >> Ino_SetCardStatus

  C_AppSyncRecv (Thumb, 8 bytes, Stack size 8 bytes, f_inobusif.o(.text), UNUSED)
  [Calls]

  - >> Ino_SendSync

  InoMsgRspCallbackFunc (Thumb, 104 bytes, Stack size 32 bytes, f_inobusif.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = InoMsgRspCallbackFunc ⇒ C_Read_Func_Response
  [Calls]
  - >> C_Read_Func_Response
  - >> InobusAddrToFuncAddr
  [Called By]
  - >> InoProcessNormal

  GetCardType (Thumb, 4 bytes, Stack size 0 bytes, f_inobusif.o(.text))
  [Called By]

  - >> Ino_SendHandshake

  GetCardVesion (Thumb, 4 bytes, Stack size 0 bytes, f_inobusif.o(.text))
  [Called By]

  - >> Ino_SendHandshake

  Host_Led_Proc (Thumb, 168 bytes, Stack size 8 bytes, f_inobusif.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = Host_Led_Proc ⇒ LED_Ctrl
  [Calls]
  - >> LED_Ctrl
  [Called By]
  - >> InobusMainLoop

  DMA2_Stream1_IRQHandler (Thumb, 32 bytes, Stack size 8 bytes, f_uart.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA2_Stream1_IRQHandler ⇒ DMA_GetITStatus
  [Calls]
  - >> DMA_ClearITPendingBit
  - >> DMA_GetITStatus
  [Address Reference Count : 1]
  - startup_stm32f407.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 58 bytes, Stack size 8 bytes, f_uart.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA2_Stream6_IRQHandler ⇒ DMA_GetITStatus
  [Calls]
  - >> USART_DMACmd
  - >> DMA_ClearITPendingBit
  - >> DMA_GetITStatus
  - >> DMA_ITConfig
  - >> DMA_Cmd
  [Address Reference Count : 1]
  - startup_stm32f407.o(RESET)

  USART6_IRQHandler (Thumb, 170 bytes, Stack size 16 bytes, f_uart.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = USART6_IRQHandler ⇒ UartTranOverCallback ⇒ Ino_SendNormalData ⇒ Uart6DmaSend ⇒ DMA_ITConfig
  [Calls]
  - >> USART_ClearITPendingBit
  - >> USART_GetITStatus
  - >> USART_ITConfig
  - >> USART_ReceiveData
  - >> DMA_ClearITPendingBit
  - >> DMA_ITConfig
  - >> DMA_GetCurrDataCounter
  - >> DMA_SetCurrDataCounter
  - >> DMA_Cmd
  - >> UartRecvRdyCallback
  - >> UartTranOverCallback
  [Address Reference Count : 1]
  - startup_stm32f407.o(RESET)

  Uart6InitDma (Thumb, 204 bytes, Stack size 72 bytes, f_uart.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = Uart6InitDma ⇒ NVIC_Init
  [Calls]
  - >> RCC_AHB1PeriphClockCmd
  - >> DMA_ITConfig
  - >> DMA_Cmd
  - >> DMA_Init
  - >> DMA_DeInit
  - >> NVIC_Init
  [Called By]
  - >> Uart_Init

  Uart_GPIO_Init (Thumb, 54 bytes, Stack size 16 bytes, f_uart.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = Uart_GPIO_Init ⇒ GPIO_PinAFConfig
  [Calls]
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  [Called By]
  - >> Uart_Init

  Uart_Init (Thumb, 136 bytes, Stack size 24 bytes, f_uart.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = Uart_Init ⇒ Uart6InitDma ⇒ NVIC_Init
  [Calls]
  - >> USART_ITConfig
  - >> USART_DMACmd
  - >> USART_OverSampling8Cmd
  - >> USART_Cmd
  - >> USART_Init
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  - >> NVIC_Init
  - >> Uart_GPIO_Init
  - >> Uart6InitDma
  [Called By]
  - >> InobusInitDsp

  Uart6DmaSend (Thumb, 78 bytes, Stack size 16 bytes, f_uart.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = Uart6DmaSend ⇒ DMA_ITConfig
  [Calls]
  - >> USART_DMACmd
  - >> DMA_ITConfig
  - >> DMA_MemoryTargetConfig
  - >> DMA_SetCurrDataCounter
  - >> DMA_Cmd
  [Called By]
  - >> Ino_SendHandshake
  - >> Ino_SendNormalData

  InitCanConfig (Thumb, 44 bytes, Stack size 16 bytes, f_can_app.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = InitCanConfig ⇒ CanFilterConfigDeal ⇒ InitRecMbox ⇒ CAN_FilterInit
  [Calls]
  - >> InitCanDrive
  - >> CanFilterConfigDeal
  [Called By]
  - >> CanMainProcess

  CanMainProcess (Thumb, 204 bytes, Stack size 8 bytes, f_can_app.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = CanMainProcess ⇒ InitCanConfig ⇒ CanFilterConfigDeal ⇒ InitRecMbox ⇒ CAN_FilterInit
  [Calls]
  - >> InitCanConfig
  [Called By]
  - >> userMainProc

  CANRxdDataDeal (Thumb, 132 bytes, Stack size 16 bytes, f_can_app.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CANRxdDataDeal
  [Called By]
  - >> CANIntHook

  CANIntHook (Thumb, 16 bytes, Stack size 12 bytes, f_can_app.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = CANIntHook ⇒ CANRxdDataDeal
  [Calls]
  - >> CANRxdDataDeal
  [Called By]
  - >> CAN1_RX1_IRQHandler
  - >> CAN1_RX0_IRQHandler

  eCanDataTran (Thumb, 228 bytes, Stack size 40 bytes, f_can_drive.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = eCanDataTran ⇒ CAN_Transmit
  [Calls]
  - >> CAN_ITConfig
  - >> CAN_Transmit
  - >> __aeabi_memclr4
  - >> __aeabi_memcpy4
  - >> NVIC_EnableIRQ
  [Called By]
  - >> CanDataSendDemo

  CAN1_RX0_IRQHandler (Thumb, 264 bytes, Stack size 8 bytes, f_can_drive.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = CAN1_RX0_IRQHandler ⇒ CanDataSendDemo ⇒ eCanDataTran ⇒ CAN_Transmit
  [Calls]
  - >> CanDataSendDemo
  - >> CANIntHook
  [Address Reference Count : 1]
  - startup_stm32f407.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 264 bytes, Stack size 8 bytes, f_can_drive.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = CAN1_RX1_IRQHandler ⇒ CanDataSendDemo ⇒ eCanDataTran ⇒ CAN_Transmit
  [Calls]
  - >> CanDataSendDemo
  - >> CANIntHook
  [Address Reference Count : 1]
  - startup_stm32f407.o(RESET)

  CAN1_TX_IRQHandler (Thumb, 104 bytes, Stack size 8 bytes, f_can_drive.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CAN1_TX_IRQHandler ⇒ CAN_Transmit
  [Calls]
  - >> CAN_ITConfig
  - >> CAN_Transmit
  [Address Reference Count : 1]
  - startup_stm32f407.o(RESET)

  InitCANIO (Thumb, 58 bytes, Stack size 16 bytes, f_can_drive.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = InitCANIO ⇒ GPIO_PinAFConfig
  [Calls]
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  [Called By]
  - >> InitCanDrive

  InitCanDrive (Thumb, 802 bytes, Stack size 24 bytes, f_can_drive.o(.text))
  [Stack]

  - Max Depth = 60
  - Call Chain = InitCanDrive ⇒ InitCANIO ⇒ GPIO_PinAFConfig
  [Calls]
  - >> RCC_APB1PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  - >> CAN_ITConfig
  - >> CAN_StructInit
  - >> CAN_DeInit
  - >> NVIC_Init
  - >> InitCANIO
  [Called By]
  - >> InitCanConfig

  InitRecMbox (Thumb, 160 bytes, Stack size 48 bytes, f_can_drive.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = InitRecMbox ⇒ CAN_FilterInit
  [Calls]
  - >> CAN_FilterInit
  [Called By]
  - >> CanFilterConfigDeal

  userInitProc (Thumb, 2 bytes, Stack size 0 bytes, f_user_main.o(.text))
  [Called By]

  - >> main

  UserLedCtrlTest (Thumb, 54 bytes, Stack size 8 bytes, f_user_main.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = UserLedCtrlTest
  [Calls]
  - >> ModuleLed3GreenDispSet
  [Called By]
  - >> userMainProc

  userMainProc (Thumb, 42 bytes, Stack size 8 bytes, f_user_main.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = userMainProc ⇒ CanMainProcess ⇒ InitCanConfig ⇒ CanFilterConfigDeal ⇒ InitRecMbox ⇒ CAN_FilterInit
  [Calls]
  - >> UserLedCtrlTest
  - >> CanMainProcess
  - >> GetSysLoadMax
  - >> GetSysLoadRealTime
  [Called By]
  - >> UsersMainLoop

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> eCanDataTran
  - >> Ino_RxDataProcess

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> eCanDataTran

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  ### Local Symbols

  CheckITStatus (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_can.o(.text), UNUSED)
  [Called By]

  - >> CAN_GetITStatus

  TI4_Config (Thumb, 80 bytes, Stack size 20 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TI3_Config (Thumb, 72 bytes, Stack size 20 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TI2_Config (Thumb, 90 bytes, Stack size 20 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TI1_Config (Thumb, 58 bytes, Stack size 20 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  ModuleLedCtrl (Thumb, 220 bytes, Stack size 8 bytes, f_main.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = ModuleLedCtrl ⇒ LED_Ctrl
  [Calls]
  - >> LED_Ctrl
  [Called By]
  - >> ModuleLedDeal

  ModuleLedDeal (Thumb, 40 bytes, Stack size 8 bytes, f_main.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = ModuleLedDeal ⇒ ModuleLedCtrl ⇒ LED_Ctrl
  [Calls]
  - >> ModuleLedCtrl
  [Called By]
  - >> ManufacMainLoop

  UpdateLedStatus (Thumb, 156 bytes, Stack size 4 bytes, f_main.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = UpdateLedStatus
  [Calls]
  - >> ModuleLed2RedDispSet
  - >> ModuleLed2OrangeDispSet
  - >> ModuleLed2GreenDispSet
  [Called By]
  - >> ManufacMainLoop

  UpdateDataToUserApp (Thumb, 182 bytes, Stack size 0 bytes, f_main.o(.text))
  [Called By]

  - >> ManufacMainLoop

  SetSysClock (Thumb, 190 bytes, Stack size 12 bytes, f_rcc.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClock
  [Called By]
  - >> ClolkInit

  CrcCaculate (Thumb, 68 bytes, Stack size 12 bytes, f_inobus.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = CrcCaculate
  [Called By]
  - >> Ino_RxDataProcess
  - >> Ino_SendHandshake
  - >> Ino_SendNormalData

  Ino_SendNormalData (Thumb, 296 bytes, Stack size 16 bytes, f_inobus.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = Ino_SendNormalData ⇒ Uart6DmaSend ⇒ DMA_ITConfig
  [Calls]
  - >> Uart6DmaSend
  - >> CrcCaculate
  [Called By]
  - >> UartTranOverCallback
  - >> TIM1_BRK_TIM9_IRQHandler

  TIM3_Configuration (Thumb, 58 bytes, Stack size 16 bytes, f_inobus.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = TIM3_Configuration ⇒ TIM_DeInit
  [Calls]
  - >> TIM_Cmd
  - >> TIM_TimeBaseInit
  - >> TIM_DeInit
  - >> RCC_APB1PeriphClockCmd
  [Called By]
  - >> InobusInitDsp

  InobusInitDsp (Thumb, 12 bytes, Stack size 8 bytes, f_inobus.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = InobusInitDsp ⇒ Uart_Init ⇒ Uart6InitDma ⇒ NVIC_Init
  [Calls]
  - >> Uart_Init
  - >> TIM3_Configuration
  [Called By]
  - >> InobusMainLoop

  Ino_SendHandshake (Thumb, 68 bytes, Stack size 24 bytes, f_inobus.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = Ino_SendHandshake ⇒ Uart6DmaSend ⇒ DMA_ITConfig
  [Calls]
  - >> Uart6DmaSend
  - >> GetCardVesion
  - >> GetCardType
  - >> CrcCaculate
  [Called By]
  - >> InobusMainLoop

  GetSyncPeriod (Thumb, 12 bytes, Stack size 8 bytes, f_inobus.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = GetSyncPeriod
  [Calls]
  - >> TIM_GetCounter
  [Called By]
  - >> Ino_SendSync

  Ino_MsgWatchDog (Thumb, 114 bytes, Stack size 0 bytes, f_inobus.o(.text))
  [Called By]

  - >> InobusMainLoop

  InoProcessNormal (Thumb, 246 bytes, Stack size 48 bytes, f_inobus.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = InoProcessNormal ⇒ InoMsgRspCallbackFunc ⇒ C_Read_Func_Response
  [Calls]
  - >> InoMsgRspCallbackFunc
  [Called By]
  - >> Ino_RxDataProcess

  Ino_RxDataProcess (Thumb, 298 bytes, Stack size 1040 bytes, f_inobus.o(.text))
  [Stack]

  - Max Depth = 1144
  - Call Chain = Ino_RxDataProcess ⇒ InoProcessNormal ⇒ InoMsgRspCallbackFunc ⇒ C_Read_Func_Response
  [Calls]
  - >> __aeabi_memcpy4
  - >> InoProcessNormal
  - >> CrcCaculate
  [Called By]
  - >> InobusMainLoop

  CanFilterConfigDeal (Thumb, 122 bytes, Stack size 32 bytes, f_can_app.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = CanFilterConfigDeal ⇒ InitRecMbox ⇒ CAN_FilterInit
  [Calls]
  - >> InitRecMbox
  [Called By]
  - >> InitCanConfig

  CanDataSendDemo (Thumb, 110 bytes, Stack size 24 bytes, f_can_drive.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = CanDataSendDemo ⇒ eCanDataTran ⇒ CAN_Transmit
  [Calls]
  - >> eCanDataTran
  [Called By]
  - >> CAN1_RX1_IRQHandler
  - >> CAN1_RX0_IRQHandler

  NVIC_EnableIRQ (Thumb, 24 bytes, Stack size 0 bytes, f_can_drive.o(.text))
  [Called By]

  - >> eCanDataTran

  ### Undefined Global Symbols