#

##

##

    µVision Build Log
    Project:
    E:\12_CAN_USER\HCAN_User_defined_Ex\4_Project\HCAN_User.uvproj
    Project File Date:  05/08/2018

    Output:
    Rebuild target 'Target 1'
    assembling startup_stm32f407.s...
    compiling system_stm32f4xx.c...
    compiling misc.c...
    compiling stm32f4xx_can.c...
    compiling stm32f4xx_dbgmcu.c...
    compiling stm32f4xx_dma.c...
    compiling stm32f4xx_exti.c...
    compiling stm32f4xx_flash.c...
    compiling stm32f4xx_gpio.c...
    compiling stm32f4xx_pwr.c...
    compiling stm32f4xx_rcc.c...
    compiling stm32f4xx_syscfg.c...
    compiling stm32f4xx_tim.c...
    compiling stm32f4xx_usart.c...
    compiling stm32f4xx_wwdg.c...
    compiling f_CAN_app.c...
    compiling f_CAN_drive.c...
    compiling f_user_main.c...
    linking...
    Program Size: Code=19020 RO-data=556 RW-data=172 ZI-data=7124
    FromELF: creating hex file...
    "..\5_Output\Objects\HCAN_User.axf" - 0 Error(s), 0 Warning(s).
    Load "..\\5_Output\\Objects\\HCAN_User.axf"
    Set JLink Project File to "E:\12_CAN_USER\HCAN_User_defined_Ex\4_Project\JLinkSettings.ini"
    * JLink Info: Device "STM32F407VG" selected (1024 KB flash, 128 KB RAM).

    JLink info:
    ------------
    DLL: V4.80g, compiled Feb 13 2014 20:50:02
    Firmware: J-Link V9 compiled Dec  1 2017 14:40:21
    Hardware: V9.40
    S/N : 59425868
    Feature(s) : RDI, GDB, FlashDL, FlashBP, JFlash, RDDI

    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: TotalIRLen = 9, IRPrint = 0x0011
    * JLink Info: Found Cortex-M4 r0p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F407VG
    VTarget = 3.330V
    State of Pins:
    TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 2000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...

s\\HCAN_User.axf" Set JLink Project File to "E:\12_CAN_USER\HCAN_User_defined_Ex\4_Project\JLinkSettings.ini" * JLink Info: Device "STM32F407VG" selected (1024 KB flash, 128 KB RAM). JLink info: ------------ DLL: V4.80g, compiled Feb 13 2014 20:50:02 Firmware: J-Link V9 compiled Dec 1 2017 14:40:21 Hardware: V9.40 S/N : 59425868 Feature(s) : RDI, GDB, FlashDL, FlashBP, JFlash, RDDI * JLink Info: TotalIRLen = 9, IRPrint = 0x0011 * JLink Info: TotalIRLen = 9, IRPrint = 0x0011 * JLink Info: Found Cortex-M4 r0p1, Little endian. * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots * JLink Info: TPIU fitted. * JLink Info: ETM fitted. ROMTableAddr = 0xE00FF003 Target info: ------------ Device: STM32F407VG VTarget = 3.333V State of Pins: TCK: 1, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1 Hardware-Breakpoints: 6 Software-Breakpoints: 8192 Watchpoints: 4 JTAG speed: 2000 kHz Erase Done. Programming Done. Verify OK. Application running ...