English

i550 Note:
- The PROFINET interface of the i550 cabinet firmware version 6.x supports a higher specification version than before
  This leads to an incompatibility between firmware versions 5.x and 6.x.
  The GSDML file 'GSDML-V2.3-Lenze-I550PN100-20170505.xml' is valid for the firmware version 5.x onwards of the i550 cabinet.
  The GSDML file 'GSDML-V2.4-Lenze-I550PN100-20200925.xml' is valid for the firmware version 6.x onwards of the i550 cabinet.

9400 Note:
- The GSDML file 'GSDML-V2.0-Lenze-9400PN-20070102.xml' can be used for firmware version 0.50 of the E94AYCER Profinet I/O communication module.

- Due to the integration of the 'PROFIsafe' safety protocol the new GSDML device description file, GSDML-V2.0-Lenze-9400PN100-20070901.xml, has been created for firmware versions 0.70 and 1.01.
  It is not possible to exchange modules equipped with different firmware versions. Every firmware version can only be operated in combination with the corresponding GSDML file! 
  As a result, the Profinet master must be reconfigured when a module with firmware version 0.50 is exchanged for a module equipped with 0.70 or 1.01.
  Due to the integration of the internal Ethernet Switch functionality and the Networktopologyidentification the new GSDML device description file, 
  GSDML-V2.1-Lenze-9400PN110-20081118.xml, has been created for firmware versions 1.10.

- The GSDM file GSDML-V2.2-Lenze-9400PN130-20110331.xml can be used with firmware version 1.10 and 1.30 and has only new error text included. 
  Moduls with firmware version 1.30 can also work with the GSDML file  GSDML-V2.1-Lenze-9400PN110-20081118.xml.

8400 Protec Note:
- The GSDML file 'GSDML-V2.2-Lenze-8420PN120-20100330.xml' can be used with Protec-Profinet firmware version 01.04 and the GSDML file GSDML-V2.2-Lenze-8420PN120-20101207.xml 
  can be used with Protec-Profinet firmware version 02.00 onwards.
  The GSDML file 'GSDML-V2.32-Lenze-8420PN120-20161213.xml' is valid for module firmware version 03.00 onwards.

8400 StateLineC, HighLineC and TopLineC Note:
- The GSDML file 'GSDML-V2.2-Lenze-8400PN100-20100423.xml' can be used with MCI-Profinet firmware version 01.00 and the GSDML file 'GSDML-V2.2-Lenze-8400PN100-20110406.xml'
  can be used with MCI-Profinet firmware version 02.01 onwards.
  The GSDML file 'GSDML-V2.35-Lenze-8400PN100-20190408.xml' is valid for module firmware version 04.00 onwards.

8400 Motec Note:
- The GSDML file 'GSDML-V2.2-Lenze-8440PN200-20110713.xml' can be used with 8400 Motec Profinet firmware version 02.02 onwards.
  The GSDML file 'GSDML-V2.32-Lenze-8440PN200-20161214.xml' is valid for module firmware version 03.00 onwards.



German

Hinweis i550
- Die Profinet Schnittstelle des i550 cabinet Firmware Version 6.x unterstützt eine höhere Spezifikations Version.
  Dies führt zu einer Inkompatibilität zwsichen der Firmware Version 5.x und 6.x.
  Die GSDML-Datei 'GSDML-V2.3-Lenze-I550PN100-20170505.xml' ist ab der Firmware Version 5.x des i550 cabinet verwendbar.
  Die GSDML-Datei 'GSDML-V2.4-Lenze-I550PN100-20200925.xml' ist ab der Firmware Version 6.x des i550 cabinet verwendbar.

Hinweis 9400:
- Die GSDML-Datei 'GSDML-V2.0-Lenze-9400PN-20070102.xml' ist für den Firmware V0.50 des Kommunikationsmoduls Profinet I/O E94AYCER.

- Durch die Integration des Sicherheitsprotokolls PROFIsafe gibt es für die Firmware V0.70 und V1.01 eine neue GSDML-Gerätebeschreibungsdatei 'GSDML-V2.0-Lenze-9400PN100-20070901.xml'. 
  Ein Wechsel des Gerätemoduls mit unterschiedlichen Firmwareversionen ist nicht möglich. Jede Firmwareversion kann nur mit der passenden GSDML-Datei betrieben werden! 
  Damit ist es bei einem Gerätemodulwechsel vom Firmware V0.50 auf V0.70 oder V1.01 notwendig, den Profinet-Master neu zu konfigurieren.

- Durch die Integration einer integrierten Ethernet-Switch-Funktionalität für 2 Ports und der Netzwerktopologieerkennung gibt es für die Firmware V1.10 
  eine neue GSDML-Gerätebeschreibungsdatei 'GSDML-V2.1-Lenze-9400PN110-20081118.xml'.

- Die GSDML-Datei 'GSDML-V2.2-Lenze-9400PN130-20110331.xml' kann für die Firmware V1.10 und V1.30 eingesetzt werden und wurde zur Vorgängerversion nur um neue Fehlertexte erweitert.
  Gerätemodule mit der Firmware V1.30 können auch mit der Vorgängerversion der GSDML-Datei 'GSDML-V2.1-Lenze-9400PN110-20081118.xml' betrieben werden.

Hinweis 8400 protec:
- Die GSDML-Datei 'GSDML-V2.2-LENZE-8420PN120-20100330.xml' ist ab der 8400 protec Profinet Firmware V01.04 und die GSDML-Datei 'GSDML-V2.3-Lenze-8420PN120-20150923.xml'
   ist ab der 8400 protec Profinet Firmware V02.00 verwendbar.
  Die GSDML-Datei 'GSDML-V2.32-Lenze-8420PN120-20161213.xml' ist ab der Module Firmware Version 03.00 verwendbar.

Hinweis 8400 StateLine C, HighLine C und TopLine C:
- Die GSDML-Datei 'GSDML-V2.2-Lenze-8400PN100-20100423.xml' ist ab der 8400 MCI Profinet Firmware V01.00 und die GSDML-Datei 'GSDML-V2.3-Lenze-8400PN100-20150923.xml'
   ist ab der 8400 MCI Profinet Firmware V02.01 verwendbar.
  Die GSDML-Datei 'GSDML-V2.35-Lenze-8400PN100-20190408.xml' ist ab der Module Firmware Version 04.00 verwendbar.


Hinweis 8400 motec:
- Die GSDML-Datei 'GSDML-V2.3-Lenze-8440PN200-20150923.xml' ist ab der 8400 Motec Profinet Firmware V02.02 verwendbar.
  Die GSDML-Datei 'GSDML-V2.32-Lenze-8440PN200-20161214.xml' ist ab der Module Firmware Version 03.00 verwendbar.

