
Kit description: 5-face toolsetting for Fanuc & Meldas controls

Kit number: A-4012-0584

Disc number: A-4012-0583

File number: F-4012-0584

Doc number:

H-2000-6525 (EN) Programming manual
H-2000-6535 (FR)
H-2000-6536 (DE)
H-2000-6537 (IT)
H-2000-6551 (R)
H-2000-6591 (ES)
H-2000-6631 (NL)
H-2000-6888 (JA)
H-2000-6826 (EN) GoProbe programming manual

++++++++++++++++++++++++++++++++++++++++++++

First issue date: 1992
Latest update date: Nov 2018

++++++++++++++++++++++++++++++++++++++++++++

Warnings and known issues

The software Installation Wizard continues to accept inch
or metric values, however all setting data in macro O9750
and calibration data (#5xx) are stored in metric, irrespective
of the machine units. During measurement the above values are
converted automatically ensuring inch customers receive the
same levels of performance.

This development simplifies the software structure, reduces
testing time and will be rolled out across all inspection and
tool setting packages when appropriate.

Parameter P6000.3 (V15) is known to switch the wear and
geometry variables for the tool offsets. If the parameter cannot
be changed then edits must be made in O9750 to change the offset
base numbers.

++++++++++++++++++++++++++++++++++++++++++++

Change Log (History)

Revision - AG
Date: Nov 2018
Engineer: HW

Additional check added to O9851 for length offset =0 when off-centre 
Check for R input greater than max tool diameter added to O9857
Program number variable introduced (#119) to O9855-O9859 
Japanese Manual added 
Minor wizard edits


Issue raised to AF
Date: Sept 2015
GoProbe tool setting cycle O9921 added and option added to the wizard.
Wizard setting of #112 adjusted and extra warning of parameter 6019.4 added.
Y input in O9857 adjusted to match programming manual.
Multi-axis issue resolved in O9752.
Parameter P6000.3 (V15) warning added to readme.

-----------------------------------------------------------------

Issue raised to AE
Date: February 2015
Calibration cycle modified so only the top and one side face is measured,
all subsequent measurement cycles will only use these faces.
New input added to the installation wizard to reflect this change. 
This new option not currently described in programming guide, to follow later.

Settings for #104 single sided below, #103 automatically set to 0 when selected.
#104 = -100 (Tool approaches from the X positive direction) 
#104 = +100 (Tool approaches from the X negative direction)
#104 = -200 (Tool approaches from the Y positive direction)
#104 = +200 (Tool approaches from the Y negative direction)
Use +1,-1, 2 and -2 for standard Five face.

Install Wizard amended for Meldas type 2 tool offsets
Air blasted option added to installation wizard.
Parameter 6019.4 option added to installation wizard.
Automatic lenght measure, complusory Y input removed.

-----------------------------------------------------------------

Issue raised to AD
* Amendment to second probe calibration storage variable in O9750
* Install Wizard option added for more than 200 tool offsets  
Date: January 2015

-----------------------------------------------------------------

Issue raised to AC
Install Wizard modified for European Windows setting.
Date: October 2014

-----------------------------------------------------------------

Issue raised to AB
Calibration data is stored as metric values irrespective of machine units.
Minor issues in O9755, O9856, O9857 and O9858 addressed.
O9856 B3 cycle inputs same as O9857 B3.
Date: October 2014

-----------------------------------------------------------------
Issue raised to AA
07/08/14
*#149 replaced with #107 (Alarm flag)
*New Wizard template 1.5.6 used
*Meldas compatiblity added via wizard
*Program structure changed
*Program 9755 added for dia
*Dia setting added to manual cycle O9856
*Inch\Metric conversion changed, settings now all in Metric
-----------------------------------------------------------------
Issue raised to OY
21/01/13
*Feed rate modified in 4 places to incorporate inch feed rate F[2000*#129] was F2000
*Reset #21 input before loop now #21=0
------------------------------------------------
Changes for A-4012-0584-0X 17/01/12
Optional 'B' and 'F' inputs changed to 'U' and 'V'

http://renport/MTPD/Apps/Lists/EFI%20Application%20List/DispForm.aspx?ID=1&Source=http%3A%2F%2Frenport%2FMTPD%2FApps%2FLists%2FEFI%2520Application%2520List%2FEFI%2520List%2Easpx
-------------------------------------------------------------------------------------------
END OF FILE
-------------------------------------------------------------------------------------------
