Controller type
Select the controller type.
Note about Fanuc options:
It is advisable to check the following parameter to establish which setting to use!
Example: Fanuc 0i, 16i, 18i, 21i and 3xi series
If P6000.3=0 (V15) - select 'Fanuc 16i, 18i, 21i, 0i-Mx, 3xi A/B series' option
If P6000.3=1 - select the 'Fanuc 10-15M series' option.
For other controls refer to the machine parameter manual for an equivalent parameter.
When 'Meldas M80, M800 Series' is selected, the generated code will have the O removed from the program names and no program number at the beginning of the files. Cycles will then be M80/M800 ready.