Number of probes or axis configurations
Select the number of tool setters or axis configurations that are required (maximum of 4).
Tip: Use one tool setter configuration where possible!
Additional probes with alternative switch on /off methods and stylus configurations can be supported for special applications. This is best avoided to minimise the settings information required and complexity of supporting multiple probes!
The default selection is '1'.