# LGF_typeActDeactMonitorDeviceParameter (UDT / V2.0.0)

Overview

## Description

This UDT belongs to the Module `LGF_ActDeactMonitorDeviceParameter` and lists all possible parameter to configure its behavior.

## Parameter description

Identifier | Data type | Default value | Description
--- | --- | --- | ---
activationRetries | SInt | 100 | Number of activation & deactiviation retries until an error is set.
timeOutActDeact | Time | T#5S | Time to monitor the commands `activate` and `deactivate` should be greater than the configured `configuration time` in the PLC hardware configuration section `Startup`
timeOutStateMonitoring | Time | T#100ms | Time to monitor the device state while the device is activated After time has expired an error is present as long as the state is faulty.
enableAndDeactivate | Bool | TRUE | TRUE: Disable / Deactivate device during startup / enabling (prior to `enableAndActive`) FALSE: Keep actual state or `enableAndActivate`
enableAndActivate | Bool | FALSE | TRUE: Enable / Activate device during startup / enabling FALSE: Keep actual state or `enableAndDeactivate`
disableAndDeactivate | Bool | TRUE | TRUE: Disable / Deactivate device during disabling of the module FALSE: Keep actual state