# LGF_typeActDeactDeviceParameter (UDT / V2.0.0)

Overview

## Description

This UDT belongs to the Module `LGF_ActDeactDeviceParameter` and lists all possible parameters to configure its behavior.

## Parameter description

Identifier | Data type | Default value | Description
--- | --- | --- | ---
activationRetries | SInt | 100 | Number of activation & deactiviation retries until an error is set.
timeOutActDeact | Time | T#5S | Time to monitor the commands `activate` and `deactivate` should be greater than the configured `configuration time` in the PLC hardware configuration section `Startup`