# LGF_typeMeasureCpuLoad_Configuration (UDT / V1.0.0)

Overview

## Description

This UDT belongs to the Module `LGF_MeasureCpuLoad` and lists all possible parameter to configure its behavior.

## Parameter description

Identifier | Data type | Default value | Description
--- | --- | --- | ---
cfcRun | Bool | FALSE | CFC Run (OB No is shifted to 10xx)
averagingValues | USInt | 0 | Averaging the measured values by building the arithmetic average value
comLoadSim | UInt | 0 | Com Load Simulation [%] IF > 0.0 used as value for calculation IF <= 0.0 take real com load value read from PLC
limitWarning | Real | 70.0 | Warning threshold value [%]
limitAlarm | Real | 100.0 | Alarming threshold value [%]
organizationBlocksCyclic | Array[0..10] of LGF_typeMeasureCpuLoad_ConfigurationBlock | --- | Cyclic Blocks to measure
organizationBlocks | Array[0..30] of LGF_typeMeasureCpuLoad_ConfigurationBlock | --- | NON-Cyclic Blocks to measure