$ EZ-EDS Version 3.27.1.20191218 Generated Electronic Data Sheet

[File]
        DescText = "EIP_Card";
        CreateDate = 10-22-2020;
        CreateTime = 08:37:08;
        ModDate = 05-10-2021;
        ModTime = 19:09:57;
        Revision = 1.0;
        HomeURL = "http://www.inovance.cn";

[Device]
        VendCode = 1660;
        VendName = "Inovance";
        ProdType = 150;
        ProdTypeStr = "Frequency converter to Ethernet/IP";
        ProdCode = 1;
        MajRev = 1;
        MinRev = 1;
        ProdName = "EIP_Card";
        Catalog = "MD500-EN1";

[Device Classification]
        Class1 = EtherNetIP;

[Params]
        Param1 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0004,                 $ Descriptor
                0xC8,                   $ Data Type
                4,                      $ Data Size in bytes
                "RPI Range",            $ name
                "",                     $ units
                "",                     $ help string
                1000,20000000,20000,    $ min, max, default data values
                1,1000,1,0,             $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                1;                      $ decimal places
        Param2 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input Assembly Size",  $ name
                "",                     $ units
                "",                     $ help string
                24,24,24,               $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param3 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output Assembly Size", $ name
                "",                     $ units
                "",                     $ help string
                24,24,24,               $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param4 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0004,                 $ Descriptor
                0xC6,                   $ Data Type
                1,                      $ Data Size in bytes
                "Producer ID",          $ name
                "",                     $ units
                "",                     $ help string
                0,255,101,              $ min, max, default data values
                1,1,1,0,                $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param5 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0004,                 $ Descriptor
                0xC6,                   $ Data Type
                1,                      $ Data Size in bytes
                "Consumer ID",          $ name
                "",                     $ units
                "",                     $ help string
                0,255,100,              $ min, max, default data values
                1,1,1,0,                $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param100 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Inverter State",       $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param101 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output Frq",           $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param102 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input I/O Messages[2]",$ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param103 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input I/O Messages[3]",$ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param104 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input I/O Messages[4]",$ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param105 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input I/O Messages[5]",$ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param106 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input I/O Messages[6]",$ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param107 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input I/O Messages[7]",$ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param108 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input I/O Messages[8]",$ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param109 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input I/O Messages[9]",$ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param110 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input I/O Messages[10]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param111 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input I/O Messages[11]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param200 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Control Command",      $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param201 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Written Freq",         $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param202 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output I/O Messages[2]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param203 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output I/O Messages[3]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param204 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output I/O Messages[4]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param205 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output I/O Messages[5]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param206 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output I/O Messages[6]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param207 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output I/O Messages[7]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param208 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output I/O Messages[8]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param209 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output I/O Messages[9]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param210 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output I/O Messages[10]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param211 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output I/O Messages[11]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param300 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input I/O Messages Mapping(T->O)[0]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,28740,          $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param301 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input I/O Messages Mapping(T->O)[1]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,28741,          $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param302 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input I/O Messages Mapping(T->O)[2]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,61440,          $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param303 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input I/O Messages Mapping(T->O)[3]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,61440,          $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param304 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input I/O Messages Mapping(T->O)[4]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,61440,          $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param305 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input I/O Messages Mapping(T->O)[5]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,61440,          $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param306 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input I/O Messages Mapping(T->O)[6]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,61440,          $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param307 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input I/O Messages Mapping(T->O)[7]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,61440,          $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param308 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input I/O Messages Mapping(T->O)[8]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,61440,          $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param309 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input I/O Messages Mapping(T->O)[9]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,61440,          $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param310 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input I/O Messages Mapping(T->O)[10]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,61440,          $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param311 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input I/O Messages Mapping(T->O)[11]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,61440,          $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param400 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output I/O Messages Mapping(O->T)[0]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,29457,          $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param401 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output I/O Messages Mapping(O->T)[1]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,29456,          $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param402 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output I/O Messages Mapping(O->T)[2]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,61440,          $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param403 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output I/O Messages Mapping(O->T)[3]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,61440,          $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param404 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output I/O Messages Mapping(O->T)[4]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,61440,          $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param405 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output I/O Messages Mapping(O->T)[5]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,61440,          $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param406 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output I/O Messages Mapping(O->T)[6]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,61440,          $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param407 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output I/O Messages Mapping(O->T)[7]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,61440,          $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param408 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output I/O Messages Mapping(O->T)[8]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,61440,          $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param409 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output I/O Messages Mapping(O->T)[9]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,61440,          $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param410 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output I/O Messages Mapping(O->T)[10]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,61440,          $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param411 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output I/O Messages Mapping(O->T)[11]",    $ name
                "",                     $ units
                "New Help String",      $ help string
                0,65535,61440,          $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places

[Assembly]
        Object_Name = "Assembly Object";
        Object_Class_Code = 0x04;
        Assem1 =
                "Input I/O Messages",
                ,
                ,
                0x0000,
                ,,
                16,Param100,
                16,Param101,
                16,Param102,
                16,Param103,
                16,Param104,
                16,Param105,
                16,Param106,
                16,Param107,
                16,Param108,
                16,Param109,
                16,Param110,
                16,Param111;
        Assem2 =
                "Output I/O Messages",
                ,
                ,
                0x0000,
                ,,
                16,Param200,
                16,Param201,
                16,Param202,
                16,Param203,
                16,Param204,
                16,Param205,
                16,Param206,
                16,Param207,
                16,Param208,
                16,Param209,
                16,Param210,
                16,Param211;
        Assem3 =
                "I/O Messages Mapping",
                ,
                ,
                0x0000,
                ,,
                16,Param300,
                16,Param301,
                16,Param302,
                16,Param303,
                16,Param304,
                16,Param305,
                16,Param306,
                16,Param307,
                16,Param308,
                16,Param309,
                16,Param310,
                16,Param311,
                16,Param400,
                16,Param401,
                16,Param402,
                16,Param403,
                16,Param404,
                16,Param405,
                16,Param406,
                16,Param407,
                16,Param408,
                16,Param409,
                16,Param410,
                16,Param411;

[Connection Manager]
        Object_Name = "Connection Manager Object";
        Object_Class_Code = 0x06;
        Connection1 =                   $ Exclusive Owner
                0x04010002,             $ trigger & transport
                                        $   0-15   = supported transport classes (class 1)
                                        $   16     = trigger: cyclic (1=supported)
                                        $   17     = trigger: change of state (0=not supported)
                                        $   18     = trigger: application (0=not supported)
                                        $   19-23  = trigger: reserved (must be zero)
                                        $   24     = application type: listen-only (0=not supported)
                                        $   25     = application type: input-only (0=not supported)
                                        $   26     = application type: exclusive-owner (1=supported)
                                        $   27     = application type: redundant-owner (0=not supported)
                                        $   28-30  = reserved (must be zero)
                                        $   31     = Direction: Client=0, Server=1 (don't care for classes 0 and 1)
                0x44640405,             $ point/multicast & priority & realtime format
                                        $   0      = O->T fixed size (1=supported)
                                        $   1      = O->T variable size (0=not supported)
                                        $   2      = T->O fixed size (1=supported)
                                        $   3      = T->O variable size (0=not supported)
                                        $   4-5    = O->T number of bytes per slot (obsolete)
                                        $   6-7    = T->O number of bytes per slot (obsolete)
                                        $   8-10   = O->T Real time transfer format (4 byte run/idle)
                                        $   11     = reserved (must be zero)
                                        $   12-14  = T->O Real time transfer format (4 byte run/idle)
                                        $   15     = reserved (must be zero)
                                        $   16     = O->T connection type: Null (0=not supported)
                                        $   17     = O->T connection type: Multicast (0=not supported)
                                        $   18     = O->T connection type: Point-to-point (1=supported)
                                        $   19     = O->T connection type: reserved
                                        $   20     = T->O connection type: Null (0=not supported)
                                        $   21     = T->O connection type: Multicast (1=supported)
                                        $   22     = T->O connection type: Point-to-point (1=supported)
                                        $   23     = T->O connection type: reserved
                                        $   24     = O->T priority: Low (0=not supported)
                                        $   25     = O->T priority: High (0=not supported)
                                        $   26     = O->T priority: Scheduled (1=supported)
                                        $   27     = O->T priority: reserved
                                        $   28     = T->O priority: Low (0=not supported)
                                        $   29     = T->O priority: High (0=not supported)
                                        $   30     = T->O priority: Scheduled (1=supported)
                                        $   31     = T->O priority: reserved
                Param1,24,Assem2,       $ O->T RPI, size, format
                Param1,24,Assem1,       $ T->O RPI, size, format
                ,,                      $ proxy config size, format
                48,Assem3,              $ target config size, format
                "Exclusive Owner",      $ connection name
                "",                     $ help string
                "20 04 24 66 2C 64 2C 65";    $ path

[Port]
        Object_Name = "Port Object";
        Object_Class_Code = 0xF4;
        Port1 =
                TCP,
                "EtherNet/IP Port",
                "20 F5 24 01",
                2,
                0x00,
                ;

[Capacity]
        ConnOverhead = .0;              $ Requires Measurement
        MaxIOConnections = 1;           $ Max I/O connections
        MaxMsgConnections = 16;         $ Max Explicit connections
        MaxConsumersPerMcast = 1;

        TSpec1 = TxRx, 2, 1000;         $ Assume default size
        TSpec2 = TxRx, 24, 1000;        $ Assume maximum size

[TCP/IP Interface Class]
        Revision = 2;
        Object_Name = "TCP/IP Interface Object";
        Object_Class_Code = 0xF5;
        MaxInst = 1;
        Number_Of_Static_Instances = 1;
        Max_Number_Of_Dynamic_Instances = 0;

[Ethernet Link Class]
        Revision = 3;
        Object_Name = "Ethernet Link Object";
        Object_Class_Code = 0xF6;
        MaxInst = 2;
        Number_Of_Static_Instances = 2;
        Max_Number_Of_Dynamic_Instances = 0;
        InterfaceLabel1 = "1";
        InterfaceLabel2 = "2";
        InterfaceType1 = 2;             $ 2=Twisted Pair
        InterfaceType2 = 2;             $ 2=Twisted Pair

