# LGF_StoreMinMax (FB / V3.0.1)

Autor: Siemens Digital Industries

## Kurzbeschreibung

Dieser Baustein liest bei jedem Aufruf einen Wert einer Variablen ein und gibt den maximalen und minimalen Wert aus, der seit dem ersten Aufruf eingelesen wurde.
Die Auswertung kann bei Bedarf zurückgesetzt werden. Der Baustein unterstützt den Datentyp LReal.

### Baustein Schnittstelle

| LGF_StoreMinMax (FB) |
--- | --- | ---
LReal |  |  | value |  | minValue |  |  | LReal
Bool |  |  | reset |  | maxValue |  |  | LReal

### Input Parameter

Bezeichner | Datentyp | Default Wert | Beschreibung
--- | --- | --- | ---
value | LReal | 0.0 | Wert der auf Min- und Maximum geprüft wird.
reset | Bool | false | TRUE: Die min/max Historie wird zurückgesetzt und die Auswertung beginnt von vorne.

### Output Parameter

Bezeichner | Datentyp | Beschreibung
--- | --- | ---
minValue | LReal | Minimaler Wert seit erstem Aufruf oder einem `reset`.
maxValue | LReal | Maximaler Wert seit erstem Aufruf oder einem `reset`.

## Änderungshistorie

Version & Datum | Änderungsbeschreibung
--- | ---
| 01.00.00 | Siemens Industry Online Support
| 19.08.2015 | First released version
| 01.00.01 | Siemens Industry Online Support
| 02.01.2017 | Upgrade: TIA Portal V14 Update 1 Code optimization
| 01.00.02 | Siemens Industry Online Support
| 17.08.2018 | Upgrade: TIA V15 Update 2
| 01.00.03 | Siemens Industry Online Support
| 23.11.2018 | Upgrade: TIA V15.1
| 01.00.04 | Simatic Systems Support
| 09.10.2019 | Regions, comments and constants are added
| 03.00.00 | Simatic Systems Support
| 23.04.2020 | Set version to V3.0.0, harmonize the version of the whole library
| 03.00.01 | Simatic Systems Support
| 04.02.2021 | Insert documentation