# LGF_IecTimerOnOff (FB / 1.0.0)

Overview

Author: Siemens Industry Support

## Short description

The Block implements an IEC_Timer TON and TOF

### Block Interface

| LGF_IecTimerOnOff (FB) |
--- | --- | ---
Bool |  |  | in |  | out |  |  | Bool
Time |  |  | timeOnDelay |  |  |  |  |
Time |  |  | timeOffDelay |  |  |  |  |

### Input parameter

Identifier | Data type | Default value | Description
--- | --- | --- | ---
in | Bool | FALSE | Boolean Input value
timeOnDelay | Time | T#0s | Preset Time on Delay
timeOffDelay | Time | T#0s | Preset Time off Delay

### Output parameter

Identifier | Data type | Description
--- | --- | ---
out | Bool | Delayed Input signal from input `in`

## Change log

Version & Date | Change description
--- | ---
| 1.0.0 | Siemens Industry Support
| 2022-05-01 | First released version