# LGF_typeRampTimeTable (UDT / V3.0.1)

Overview

## Description

Data type to setup a speed curve based on a setpoint table for the function `LGF_RampCI`

## Parameter description

Identifier | Data type | Default value | Description
--- | --- | --- | ---
outputValue | LReal | 0.0 | Setpoint Value to reach by the interpolation curve
time | Time | T#0s | Time until the interpolation point is reached