# LGF_StringToTime (FC / 3.1.0)

Übersicht

Autor: Siemens Digital Industry

## Kurzbeschreibung

Diese Funktion konvertiert eine Variable vom Datentyp `String` in eine Variable des Systemdatentyp `Time`.

### Baustein Schnittstelle

| LGF_StringToTime (FC) |
--- | --- | ---
String |  |  | timeValue |  | Ret_Val |  |  | Time

### Input Parameter

Bezeichner | Datentyp | Beschreibung
--- | --- | ---
timeValue | String | Zu konvertierte Zeit als String Beispiel: `1D3H45M6S0MS`

### Output Parameter

Bezeichner | Datentyp | Beschreibung
--- | --- | ---
Ret_Val | Time | Konvertierter Zeit-Wert Beispiel: `T#1D_3H_45M_6S`

## Änderungshistorie

Version & Datum | Änderungsbeschreibung
--- | ---
| 1.0.0 | Simatic Systems Support
| 02.07.2019 | First released version
| 1.0.1 | Simatic Systems Support
| 09.07.2019 | Further improvements and code optimization
| 1.0.2 | Simatic Systems Support
| 30.07.2019 | Add ENO handling
| 3.0.0 | Simatic Systems Support
| 23.04.2020 | Set version to V3.0.0 Harmonize the version of the whole library
| 3.0.1 | Simatic Systems Support
| 23.02.2021 | Insert documentation
| 3.1.0 | Simatic Systems Support
| 17.07.2025 | Implemented separator functionality