# LGF_IntToString (FC / 3.0.1)

Übersicht

Autor: Siemens Digital Industry

## Kurzbeschreibung

Diese Funktion konvertiert eine Variable vom Datentyp `DInt` in eine Variable vom Datentyp `String`.

### Baustein Schnittstelle

| LGF_IntToString (FC) |
--- | --- | ---
DInt |  |  | value |  | Ret_Val |  |  | String

### Input Parameter

Bezeichner | Datentyp | Beschreibung
--- | --- | ---
value | DInt | Doppel-Integer Wert zur Konvertierung

### Output Parameter

Bezeichner | Datentyp | Beschreibung
--- | --- | ---
Ret_Val | String | Konvertierter Wert als String. Beispiel: ‘+16927’

## Änderungshistorie

Version & Datum | Änderungsbeschreibung
--- | ---
| 1.0.0 | Siemens Industry Online Support
| 04.07.2018 | First released version
| 1.0.1 | Siemens Industry Online Support
| 17.08.2018 | Upgrade: TIA V15 Update 2
| 1.0.2 | Siemens Industry Online Support
| 23.11.2018 | Upgrade: TIA V15.1
| 1.0.5 | Simatic Systems Support
| 07.06.2019 | Standard header and block parameters update Program changed to VAL_STRG wrapper
| 1.0.6 | Simatic Systems Support
| 30.07.2019 | Add ENO handling
| 3.0.0 | Simatic Systems Support
| 23.04.2020 | Set version to V3.0.0 Harmonize the version of the whole library
| 3.0.1 | Simatic Systems Support
| 23.02.2021 | Insert documentation