# LGF_StringToDTL_US (FC / 1.0.0)

Overview

Author: Siemens Digital Industry

## Short description

This function converts a character string in American format (US) with date and time components into the data type DTL.

### Block Interface

| LGF_StringToDTL_US (FC) |
--- | --- | ---
String |  |  | date |  | Ret_Val |  |  | DTL
|  |  |  |  | error |  |  | Bool
|  |  |  |  | status |  |  | Word

### Input parameter

Identifier | Data type | Description
--- | --- | ---
date | String | Date as a character string according to the format. Example: `01-22-2019 14:07:57.696417000`.

### Output parameter

Identifier | Data type | Description
--- | --- | ---
Ret_Val | DTL |
error | Bool | FALSE: No error TRUE: An error occurred during the execution of the FB
status | Word | 16#0000-16#7FFF: Status of the FB 16#8000-16#FFFF: Error identification (see following Table)

### Status & Error codes

Code / Value | Identifier / Description
--- | ---
16#0000 | STATUS_FINISHED_NO_ERROR Status: Execution finished without errors
16#7000 | STATUS_NO_JOB Status: No current job processed
16#8201 | ERR_FORMAT_YEAR Error: YEAR out of range of DTL - YEAR value does not correspond to the format or specification (outside the value range of DTL)
16#8202 | ERR_FORMAT_MONTH Error: MONTH out of range of DTL - MONTH value does not correspond to the format or specification (outside the value range of DTL)
16#8203 | ERR_FORMAT_DAY Error: DAY out of range of DTL - DAY value does not correspond to the format or specification (outside the value range of DTL)
16#8204 | ERR_FORMAT_HOUR Error: HOUR out of range of DTL - HOUR value does not correspond to the format or specification (outside the value range of DTL)
16#8205 | ERR_FORMAT_MINUTE Error: MINUTE out of range of DTL - MINUTE value does not correspond to the format or specification (outside the value range of DTL)
16#8206 | ERR_FORMAT_SECOND Error: SECOND out of range of DTL - SECOND value does not correspond to the format or specification (outside the value range of DTL)
16#8207 | ERR_FORMAT_NANOSECOND Error: NANOSECOND out of range of DTL - NANOSECOND value does not correspond to the format or specification (outside the value range of DTL)
16#8400 | ERR_DATE_STRING_EMPTY Error: Input String `date` is empty
16#8401 | ERR_DATE_STRING_TO_SHORT Error: Input String `date` is too short - minimum is 'MM-DD-YYYY HH:MM:SS'

## Functional description

The block reads a date as a character string and converts it to the data type DTL. The individual date components in the character string are separated according to the American format. The separator between the components in the character string is irrelevant.

### American format (US):

## Change log

Version & Date | Change description
--- | ---
| 1.0.0 | Siemens Industry Online Support
| 28.07.2025 | First released version